[
{"data":{"title":"IOReportLegend"},"attr":{"id":"7147","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7148","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"7150","ColType":"String","ColValue":"PWRB 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"7152","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7153","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7154","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"7155","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7156","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"7157","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7158","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"7159","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7160","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"7161","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7162","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"7163","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7164","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"7165","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7166","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"7167","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7168","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"7169","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7170","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"7171","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7172","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"7174","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"7176","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"7178","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"7180","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7181","ColType":"Data","ColValue":"&lt;0200000000000000&gt;"}}]},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"7183","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"7185","ColType":"Data","ColValue":"&lt;\"PNP0C0C\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"7187","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"7189","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7190","ColType":"String","ColValue":"ACPIEventController"}}]},
{"data":{"title":"_STA"},"attr":{"id":"7192","ColType":"Number","ColValue":"18446744073709551615"}}
]
