[
{"data":{"title":"built-in"},"attr":{"id":"5899","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5901","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5902","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5903","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5905","ColType":"Number","ColValue":"549775867904"}},{"data":{"title":"length"},"attr":{"id":"5907","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"5909","ColType":"Data","ColValue":"&lt;21200000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"5911","ColType":"Data","ColValue":"&lt;\"pci8086,2021\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5913","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/CB0D@40003"}},
{"data":{"title":"IOName"},"attr":{"id":"5915","ColType":"String","ColValue":"pci8086,2021"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5917","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5919","ColType":"Data","ColValue":"&lt;04000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5921","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5923","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5925","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5927","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5928","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"5929","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5931","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5933","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5935","ColType":"String","ColValue":"0:4:3"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5937","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5939","ColType":"Number","ColValue":"146"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5941","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5943","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5945","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5947","ColType":"Number","ColValue":"3"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5949","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5951","ColType":"Data","ColValue":"&lt;00800800&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"5953","ColType":"Data","ColValue":"&lt;\"pci8086,0\",\"pci8086,2021\",\"pciclass,088000\",\"CB0D\"&gt;"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"5955","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"5957","ColType":"Data","ColValue":"&lt;1023008280000000000032010000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5959","ColType":"Data","ColValue":"&lt;00230000000000000000000000000000000000001023000200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5961","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5962","ColType":"Data","ColValue":"&lt;1300000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"5963","ColType":"Data","ColValue":"&lt;0700000000000100&gt;"}}]}
]
