[
{"data":{"title":"_STA"},"attr":{"id":"4561","ColType":"Number","ColValue":"15"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"4563","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4564","ColType":"Data","ColValue":"&lt;1500000007000000&gt;"}}]},
{"data":{"title":"_ADR"},"attr":{"id":"4566","ColType":"Number","ColValue":"1638400"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"4568","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4569","ColType":"String","ColValue":"io-apic-0"}}]},
{"data":{"title":"device-properties"},"attr":{"id":"4571","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-device"},"attr":{"id":"4573","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},{"data":{"title":"uart-channel-number"},"attr":{"id":"4575","ColType":"Data","ColValue":"&lt;0200000000000000&gt;"}},{"data":{"title":"acpi-path"},"attr":{"id":"4577","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/URT2@190000"}}]}
]
