[
{"data":{"title":"_STA"},"attr":{"id":"3986","ColType":"Number","ColValue":"15"}},
{"data":{"title":"_ADR"},"attr":{"id":"3988","ColType":"Number","ColValue":"3"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"3990","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"MaxPowerState"},"attr":{"id":"3992","ColType":"Number","ColValue":"2"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"3994","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"3996","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"device-properties"},"attr":{"id":"3998","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-path"},"attr":{"id":"4000","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/ADIO@3"}},{"data":{"title":"acpi-device"},"attr":{"id":"4002","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}}]},
{"data":{"title":"acpi-pci-pm"},"attr":{"id":"4004","ColType":"Boolean","ColValue":"Yes"}}
]
