[
{"data":{"title":"_STA"},"attr":{"id":"6346","ColType":"Number","ColValue":"15"}},
{"data":{"title":"_ADR"},"attr":{"id":"6348","ColType":"Number","ColValue":"131072"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"6350","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"MaxPowerState"},"attr":{"id":"6352","ColType":"Number","ColValue":"2"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"6354","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"6356","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"device-properties"},"attr":{"id":"6358","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-device"},"attr":{"id":"6360","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},{"data":{"title":"acpi-path"},"attr":{"id":"6362","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000"}},{"data":{"title":"PCIHotplugCapable"},"attr":{"id":"6364","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"acpi-pci-pm"},"attr":{"id":"6366","ColType":"Boolean","ColValue":"Yes"}}
]
