[
{"data":{"title":"assigned-addresses"},"attr":{"id":"9391","ColType":"Data","ColValue":"&lt;10007d8200000000000010900000000000000100&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"9393","ColType":"String","ColValue":"125:0:0"}},
{"data":{"title":"IOPCITunnelL1Enable"},"attr":{"id":"9395","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"9397","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"9399","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9400","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"9401","ColType":"Data","ColValue":"&lt;2900000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"9403","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000/XHC2@0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"9405","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"9407","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9408","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"9409","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"USBBusNumber"},"attr":{"id":"9411","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"9413","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"9415","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"9417","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"9419","ColType":"Data","ColValue":"&lt;22220000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"9421","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"9423","ColType":"Data","ColValue":"&lt;\"pci8086,15d4\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"9425","ColType":"Number","ColValue":"2"}},
{"data":{"title":"compatible"},"attr":{"id":"9427","ColType":"Data","ColValue":"&lt;\"pci2222,1111\",\"pci8086,15d4\",\"pciclass,0c0330\",\"XHC2\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"9429","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"9431","ColType":"Number","ColValue":"0"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"9433","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"9435","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"9437","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"9439","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"9441","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"9443","ColType":"Number","ColValue":"4545601"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"9445","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AAPL,xhci-clock-id"},"attr":{"id":"9447","ColType":"Number","ColValue":"1"}},
{"data":{"title":"built-in"},"attr":{"id":"9449","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"9451","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"9453","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9454","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9455","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"9457","ColType":"Number","ColValue":"2416967680"}},{"data":{"title":"length"},"attr":{"id":"9459","ColType":"Number","ColValue":"65536"}}]}]}]},
{"data":{"title":"IOName"},"attr":{"id":"9461","ColType":"String","ColValue":"pci8086,15d4"}},
{"data":{"title":"acpi-device"},"attr":{"id":"9463","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"9465","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"9467","ColType":"Data","ColValue":"&lt;11110000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"9469","ColType":"Data","ColValue":"&lt;00007d000000000000000000000000000000000010007d0200000000000000000000000000000100&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"9471","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9472","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"9474","ColType":"String","ColValue":"XHC2 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"9476","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9477","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9478","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"9479","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9480","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"9481","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9482","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"9483","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9484","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"9485","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9486","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"9487","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9488","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"9489","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9490","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"9491","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9492","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"9493","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9494","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"9495","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9496","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"9498","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"9500","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"9502","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"9504","ColType":"Data","ColValue":"&lt;30030c00&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"9506","ColType":"Data","ColValue":"&lt;d4150000&gt;"}}
]
