[
{"data":{"title":"_STA"},"attr":{"id":"5274","ColType":"Number","ColValue":"15"}},
{"data":{"title":"_ADR"},"attr":{"id":"5276","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5278","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"MaxPowerState"},"attr":{"id":"5280","ColType":"Number","ColValue":"2"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"5282","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5284","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"device-properties"},"attr":{"id":"5286","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-device"},"attr":{"id":"5288","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},{"data":{"title":"PCI-Thunderbolt"},"attr":{"id":"5290","ColType":"Number","ColValue":"1"}},{"data":{"title":"acpi-path"},"attr":{"id":"5292","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0"}}]},
{"data":{"title":"acpi-pci-pm"},"attr":{"id":"5294","ColType":"Boolean","ColValue":"Yes"}}
]
