[
{"data":{"title":"IOPCITunnelLinkChange"},"attr":{"id":"38446","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"ranges"},"attr":{"id":"38448","ColType":"Data","ColValue":"&lt;0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"38450","ColType":"String","ColValue":"7:4:0(10:10)"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"38452","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"38454","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38455","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"38456","ColType":"Data","ColValue":"&lt;1500000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"38458","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000"}},
{"data":{"title":"Thunderbolt Path"},"attr":{"id":"38460","ColType":"String","ColValue":"IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2D@3/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@7"}},
{"data":{"title":"IOPCIExpressSlotCapabilities"},"attr":{"id":"38462","ColType":"Number","ColValue":"2359392"}},
{"data":{"title":"IOPCIExpressSlotStatus"},"attr":{"id":"38464","ColType":"Number","ColValue":"0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"38466","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"38468","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38469","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"38470","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"38472","ColType":"Number","ColValue":"354"}},
{"data":{"title":"AAPL,slot-name"},"attr":{"id":"38474","ColType":"Data","ColValue":"&lt;\"PCI Slot 2\"&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"38476","ColType":"Number","ColValue":"4"}},
{"data":{"title":"IOPCITunnelID"},"attr":{"id":"38478","ColType":"Number","ColValue":"4294968446"}},
{"data":{"title":"IOPCIConfigured"},"attr":{"id":"38480","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"38482","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IODTPersist"},"attr":{"id":"38484","ColType":"Number","ColValue":"0"}},
{"data":{"title":"#size-cells"},"attr":{"id":"38486","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"38488","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"38490","ColType":"Data","ColValue":"&lt;\"pci-bridge\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"38492","ColType":"Number","ColValue":"48"}},
{"data":{"title":"compatible"},"attr":{"id":"38494","ColType":"Data","ColValue":"&lt;\"pci8086,15d3\",\"pciclass,060400\",\"DSB4\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"38496","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"DevicePowerState"},"attr":{"id":"38498","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"38500","ColType":"Number","ColValue":"0"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"38502","ColType":"Number","ColValue":"0"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"38504","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"38506","ColType":"Number","ColValue":"2"}},{"data":{"title":"PowerOverrideOn"},"attr":{"id":"38508","ColType":"Boolean","ColValue":"Yes"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"38510","ColType":"Number","ColValue":"2"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"38512","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"38514","ColType":"Number","ColValue":"74538049"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"38516","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"38518","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"#address-cells"},"attr":{"id":"38520","ColType":"Data","ColValue":"&lt;03000000&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"38522","ColType":"String","ColValue":"pci-bridge"}},
{"data":{"title":"acpi-device"},"attr":{"id":"38524","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"38526","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"reg"},"attr":{"id":"38528","ColType":"Data","ColValue":"&lt;0020070000000000000000000000000000000000&gt;"}},
{"data":{"title":"Thunderbolt Entry ID"},"attr":{"id":"38530","ColType":"Number","ColValue":"4294968480"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"38532","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38533","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"38535","ColType":"String","ColValue":"DSB4 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"38537","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38538","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38539","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"38540","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38541","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"38542","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38543","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"38544","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38545","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"38546","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38547","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"38548","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38549","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"38550","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38551","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"38552","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38553","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"38554","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38555","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"38556","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38557","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"38559","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"38561","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"38563","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"38565","ColType":"Data","ColValue":"&lt;00040600&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"38567","ColType":"Data","ColValue":"&lt;d3150000&gt;"}}
]
