[
{"data":{"title":"built-in"},"attr":{"id":"5647","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"5649","ColType":"Data","ColValue":"&lt;20200000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"5651","ColType":"Data","ColValue":"&lt;\"pci8086,2020\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5653","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/DMI0@0"}},
{"data":{"title":"IOName"},"attr":{"id":"5655","ColType":"String","ColValue":"pci8086,2020"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5657","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5659","ColType":"Data","ColValue":"&lt;04000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5661","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5663","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5665","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5667","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5668","ColType":"String","ColValue":"io-apic-0"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5670","ColType":"Number","ColValue":"8009795"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5672","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5674","ColType":"String","ColValue":"0:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5676","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5678","ColType":"Number","ColValue":"66"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5680","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5682","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5684","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5686","ColType":"Number","ColValue":"3"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5688","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5690","ColType":"Data","ColValue":"&lt;00000600&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"5692","ColType":"Data","ColValue":"&lt;\"pci8086,0\",\"pci8086,2020\",\"pciclass,060000\",\"DMI0\"&gt;"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"5694","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5696","ColType":"Data","ColValue":"&lt;0000000000000000000000000000000000000000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5698","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5699","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}}]}
]
