[
{"data":{"title":"built-in"},"attr":{"id":"5833","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5835","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5836","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5837","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5839","ColType":"Number","ColValue":"549775884288"}},{"data":{"title":"length"},"attr":{"id":"5841","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"5843","ColType":"Data","ColValue":"&lt;21200000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"5845","ColType":"Data","ColValue":"&lt;\"pci8086,2021\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5847","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/CB0C@40002"}},
{"data":{"title":"IOName"},"attr":{"id":"5849","ColType":"String","ColValue":"pci8086,2021"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5851","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5853","ColType":"Data","ColValue":"&lt;04000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5855","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5857","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5859","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5861","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5862","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"5863","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5865","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5867","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5869","ColType":"String","ColValue":"0:4:2"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5871","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5873","ColType":"Number","ColValue":"146"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5875","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5877","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5879","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5881","ColType":"Number","ColValue":"3"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5883","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5885","ColType":"Data","ColValue":"&lt;00800800&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"5887","ColType":"Data","ColValue":"&lt;\"pci8086,0\",\"pci8086,2021\",\"pciclass,088000\",\"CB0C\"&gt;"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"5889","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"5891","ColType":"Data","ColValue":"&lt;1022008280000000004032010000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5893","ColType":"Data","ColValue":"&lt;00220000000000000000000000000000000000001022000200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5895","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5896","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"5897","ColType":"Data","ColValue":"&lt;0200000000000100&gt;"}}]}
]
