[
{"data":{"title":"IOPowerManagement"},"attr":{"id":"6368","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"MaxPowerState"},"attr":{"id":"6370","ColType":"Number","ColValue":"2"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"6372","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"6374","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"_ADR"},"attr":{"id":"6376","ColType":"Number","ColValue":"0"}},
{"data":{"title":"acpi-wake-gpe"},"attr":{"id":"6378","ColType":"Number","ColValue":"105"}},
{"data":{"title":"acpi-pci-pm"},"attr":{"id":"6380","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOGeneralInterest"},"attr":{"id":"6382","ColType":"String","ColValue":"IOCommand is not serializable"}},
{"data":{"title":"_STA"},"attr":{"id":"6384","ColType":"Number","ColValue":"18446744073709551615"}},
{"data":{"title":"device-properties"},"attr":{"id":"6386","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-device"},"attr":{"id":"6388","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},{"data":{"title":"USBBusNumber"},"attr":{"id":"6390","ColType":"Number","ColValue":"1"}},{"data":{"title":"acpi-path"},"attr":{"id":"6392","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000/XHC3@0"}},{"data":{"title":"AAPL,xhci-clock-id"},"attr":{"id":"6394","ColType":"Number","ColValue":"1"}}]}
]
