[
{"data":{"title":"built-in"},"attr":{"id":"43782","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"43784","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43785","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43786","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"43788","ColType":"Number","ColValue":"4029284352"}},{"data":{"title":"length"},"attr":{"id":"43790","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"43792","ColType":"Number","ColValue":"80"}},
{"data":{"title":"layout-id"},"attr":{"id":"43794","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"hda-gfx"},"attr":{"id":"43796","ColType":"Data","ColValue":"&lt;\"onboard-1\"&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"43798","ColType":"Data","ColValue":"&lt;f8aa0000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"43800","ColType":"Number","ColValue":"2"}},
{"data":{"title":"name"},"attr":{"id":"43802","ColType":"Data","ColValue":"&lt;\"pci1002,aaf8\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"43804","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC03@0/BR3A@0/EGP0@0/EGP1@0/HDAU@1"}},
{"data":{"title":"IOName"},"attr":{"id":"43806","ColType":"String","ColValue":"pci1002,aaf8"}},
{"data":{"title":"vendor-id"},"attr":{"id":"43808","ColType":"Data","ColValue":"&lt;02100000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"43810","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"43812","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"43814","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"43816","ColType":"Data","ColValue":"&lt;02100000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"43818","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43819","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"43820","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"43822","ColType":"Number","ColValue":"4459779"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"43824","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43825","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"43827","ColType":"String","ColValue":"HDAU 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"43829","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43830","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43831","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"43832","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"43833","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"43834","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43835","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"43836","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"43837","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"43838","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43839","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"43840","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"43841","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"43842","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43843","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"43844","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"43845","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"43846","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43847","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"43848","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"43849","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"43851","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"43853","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"43855","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"43857","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"43859","ColType":"String","ColValue":"243:0:1"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"43861","ColType":"Number","ColValue":"4355"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"43863","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"43865","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"43867","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"43869","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"43871","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"43873","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"43875","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"43877","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"43879","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"43881","ColType":"Data","ColValue":"&lt;\"pci1002,aaf8\",\"pciclass,040300\",\"HDAU\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"43883","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"43885","ColType":"Data","ColValue":"&lt;f8aa0000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"43887","ColType":"Data","ColValue":"&lt;1001f3820000000000002af00000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"43889","ColType":"Data","ColValue":"&lt;0001f300000000000000000000000000000000001001f30200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"43891","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"43892","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"43893","ColType":"Data","ColValue":"&lt;2b00000000000100&gt;"}}]}
]
