# dmidecode 2.12b
Handle 0x0000, DMI type 16, 23 bytes
0000: 10 17 00 00 03 03 03 00 00 00 02 fe ff 04 00 00 
0010: 00 00 00 00 00 00 00 

Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 32 GB
	Error Information Handle: Not Provided
	Number Of Devices: 4

Handle 0x0001, DMI type 17, 40 bytes
0000: 11 28 01 00 00 00 fe ff 40 00 40 00 00 10 0d 00 
0010: 01 02 1a 80 00 60 09 03 04 05 06 01 00 00 00 00 
0020: 60 09 00 00 00 00 b0 04 

Memory Device
	Array Handle: 0x0000
	Error Information Handle: Not Provided
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 4096 MB
	Form Factor: SODIMM
	Set: None
	Locator: DIMM0
	Bank Locator: BANK 0
	Type: <OUT OF SPEC>
	Type Detail: Synchronous
	Speed: 2400 MHz (0.4 ns)
	Manufacturer: 0x802C
	Serial Number: 0x21122632
	Asset Tag:  
	Part Number: 0x344154463531323634485A2D3247334232202020
	Rank: 1
	Configured Clock Speed: 2400 MHz (0.4 ns)
	Minimum voltage:  Unknown
	Maximum voltage:  Unknown
	Configured voltage:  1.200 V

Handle 0x0002, DMI type 130, 186 bytes
0000: 82 ba 02 00 01 00 00 00 b0 00 23 11 0c 03 45 21 
0010: 00 08 00 60 00 03 02 03 00 00 00 00 07 0d f8 7f 
0020: 00 00 6e 6e 6e 11 00 6e f0 0a 20 08 00 05 00 f0 
0030: 2b 34 28 00 78 00 14 3c 00 00 00 00 00 00 00 00 
0040: 00 00 00 00 00 00 16 36 0b 35 16 36 0b 35 00 00 
0050: 16 36 0b 35 16 36 0b 35 00 00 00 00 00 00 00 00 
0060: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0070: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0080: 9c b5 00 00 00 00 e7 d6 b5 ed 0f 01 02 00 00 00 
0090: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00a0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00b0: 00 00 00 00 00 00 00 00 00 00 

Apple specific SPD
	000082ba020001000000b00023110c034521
	0010000800600003020300000000070df87f
	002000006e6e6e11006ef00a2008000500f0
	00302b3428007800143c0000000000000000
	004000000000000016360b3516360b350000
	005016360b3516360b350000000000000000
	006000000000000000000000000000000000
	007000000000000000000000000000000000
	00809cb500000000e7d6b5ed0f0102000000
	009000000000000000000000000000000000
	00a000000000000000000000000000000000
	00b000000000000000000000000011280300
	00c00000feff000000000000020001020200
	00d000000000000000000000000000000000
	00e00000000044494d4d310042414e4b2030
	00f00020000082ba040003000000b0000000

Handle 0x0003, DMI type 17, 40 bytes
0000: 11 28 03 00 00 00 fe ff 00 00 00 00 00 00 02 00 
0010: 01 02 02 00 00 00 00 00 00 00 00 00 00 00 00 00 
0020: 00 00 00 00 00 00 00 00 

Memory Device
	Array Handle: 0x0000
	Error Information Handle: Not Provided
	Total Width: Unknown
	Data Width: Unknown
	Size: No Module Installed
	Form Factor: Unknown
	Set: None
	Locator: DIMM1
	Bank Locator: BANK 0
	Type: Unknown
	Type Detail: None
	Speed: Unknown
	Manufacturer: Not Specified
	Serial Number: Not Specified
	Asset Tag: Not Specified
	Part Number: Not Specified
	Rank: Unknown
	Configured Clock Speed: Unknown
	Minimum voltage:  Unknown
	Maximum voltage:  Unknown
	Configured voltage:  Unknown

Handle 0x0004, DMI type 130, 186 bytes
0000: 82 ba 04 00 03 00 00 00 b0 00 00 00 00 00 00 00 
0010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0040: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0050: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0060: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0070: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0080: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0090: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00a0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00b0: 00 00 00 00 00 00 00 00 00 00 

Apple specific SPD
	000082ba040003000000b000000000000000
	001000000000000000000000000000000000
	002000000000000000000000000000000000
	003000000000000000000000000000000000
	004000000000000000000000000000000000
	005000000000000000000000000000000000
	006000000000000000000000000000000000
	007000000000000000000000000000000000
	008000000000000000000000000000000000
	009000000000000000000000000000000000
	00a000000000000000000000000000000000
	00b000000000000000000000000011280500
	00c00000feff4000400000100d0001021a80
	00d000600903040506010000000060090000
	00e00000b00444494d4d300042414e4b2031
	00f000307838303243003078323131323236

Handle 0x0005, DMI type 17, 40 bytes
0000: 11 28 05 00 00 00 fe ff 40 00 40 00 00 10 0d 00 
0010: 01 02 1a 80 00 60 09 03 04 05 06 01 00 00 00 00 
0020: 60 09 00 00 00 00 b0 04 

Memory Device
	Array Handle: 0x0000
	Error Information Handle: Not Provided
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 4096 MB
	Form Factor: SODIMM
	Set: None
	Locator: DIMM0
	Bank Locator: BANK 1
	Type: <OUT OF SPEC>
	Type Detail: Synchronous
	Speed: 2400 MHz (0.4 ns)
	Manufacturer: 0x802C
	Serial Number: 0x21122605
	Asset Tag:  
	Part Number: 0x344154463531323634485A2D3247334232202020
	Rank: 1
	Configured Clock Speed: 2400 MHz (0.4 ns)
	Minimum voltage:  Unknown
	Maximum voltage:  Unknown
	Configured voltage:  1.200 V

Handle 0x0006, DMI type 130, 186 bytes
0000: 82 ba 06 00 05 00 00 00 b0 00 23 11 0c 03 45 21 
0010: 00 08 00 60 00 03 02 03 00 00 00 00 07 0d f8 7f 
0020: 00 00 6e 6e 6e 11 00 6e f0 0a 20 08 00 05 00 f0 
0030: 2b 34 28 00 78 00 14 3c 00 00 00 00 00 00 00 00 
0040: 00 00 00 00 00 00 16 36 0b 35 16 36 0b 35 00 00 
0050: 16 36 0b 35 16 36 0b 35 00 00 00 00 00 00 00 00 
0060: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0070: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0080: 9c b5 00 00 00 00 e7 d6 b5 ed 0f 01 02 00 00 00 
0090: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00a0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00b0: 00 00 00 00 00 00 00 00 00 00 

Apple specific SPD
	000082ba060005000000b00023110c034521
	0010000800600003020300000000070df87f
	002000006e6e6e11006ef00a2008000500f0
	00302b3428007800143c0000000000000000
	004000000000000016360b3516360b350000
	005016360b3516360b350000000000000000
	006000000000000000000000000000000000
	007000000000000000000000000000000000
	00809cb500000000e7d6b5ed0f0102000000
	009000000000000000000000000000000000
	00a000000000000000000000000000000000
	00b000000000000000000000000011280700
	00c00000feff000000000000020001020200
	00d000000000000000000000000000000000
	00e00000000044494d4d310042414e4b2031
	00f00020000082ba080007000000b0000000

Handle 0x0007, DMI type 17, 40 bytes
0000: 11 28 07 00 00 00 fe ff 00 00 00 00 00 00 02 00 
0010: 01 02 02 00 00 00 00 00 00 00 00 00 00 00 00 00 
0020: 00 00 00 00 00 00 00 00 

Memory Device
	Array Handle: 0x0000
	Error Information Handle: Not Provided
	Total Width: Unknown
	Data Width: Unknown
	Size: No Module Installed
	Form Factor: Unknown
	Set: None
	Locator: DIMM1
	Bank Locator: BANK 1
	Type: Unknown
	Type Detail: None
	Speed: Unknown
	Manufacturer: Not Specified
	Serial Number: Not Specified
	Asset Tag: Not Specified
	Part Number: Not Specified
	Rank: Unknown
	Configured Clock Speed: Unknown
	Minimum voltage:  Unknown
	Maximum voltage:  Unknown
	Configured voltage:  Unknown

Handle 0x0008, DMI type 130, 186 bytes
0000: 82 ba 08 00 07 00 00 00 b0 00 00 00 00 00 00 00 
0010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0040: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0050: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0060: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0070: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0080: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0090: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00a0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00b0: 00 00 00 00 00 00 00 00 00 00 

Apple specific SPD
	000082ba080007000000b000000000000000
	001000000000000000000000000000000000
	002000000000000000000000000000000000
	003000000000000000000000000000000000
	004000000000000000000000000000000000
	005000000000000000000000000000000000
	006000000000000000000000000000000000
	007000000000000000000000000000000000
	008000000000000000000000000000000000
	009000000000000000000000000000000000
	00a000000000000000000000000000000000
	00b0000000000000000000000000131f0900
	00c000000000ffff7f000000020000000000
	00d00000000000000000000000000000180a
	00e00001020000037f809801000000000081
	00f00a0001ffff4170706c6520496e632e00

Handle 0x0009, DMI type 19, 31 bytes
0000: 13 1f 09 00 00 00 00 00 ff ff 7f 00 00 00 02 00 
0010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 

Memory Array Mapped Address
	Starting Address: 0x00000000000
	Ending Address: 0x001FFFFFFFF
	Range Size: 8 GB
	Physical Array Handle: 0x0000
	Partition Width: 2

Handle 0x000A, DMI type 0, 24 bytes
0000: 00 18 0a 00 01 02 00 00 03 7f 80 98 01 00 00 00 
0010: 00 00 81 0a 00 01 ff ff 

BIOS Information
	Vendor: Apple Inc.
	Version: IM183.88Z.0145.B02.1703311945
	Release Date: 03/31/2017
	ROM Size: 8192 kB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		ACPI is supported
		Smart battery is supported
		Function key-initiated network boot is supported
		UEFI is supported
	BIOS Revision: 0.1

Handle 0x000B, DMI type 1, 27 bytes
0000: 01 1b 0b 00 01 02 03 04 27 23 2a b2 46 5f 6d 51 
0010: be 36 bb 7e 83 d3 e6 61 06 05 06 

System Information
	Manufacturer: Apple Inc.
	Product Name: iMac18,3
	Version: 1.0
	Serial Number: C**********G
	UUID: 00000000-0000-0000-0000-000000000000
	Wake-up Type: Power Switch
	SKU Number:  
	Family: iMac

Handle 0x000C, DMI type 2, 17 bytes
0000: 02 11 0c 00 01 02 03 04 05 01 06 0d 00 0a 00 00 
0010: 00 

Base Board Information
	Manufacturer: Apple Inc.
	Product Name: Mac-BE088AF8C5EB4FA2
	Version: iMac18,3
	Serial Number: C0000000000000004
	Asset Tag:  
	Features:
		Board is a hosting board
	Location In Chassis:  
	Chassis Handle: 0x000D
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000D, DMI type 3, 24 bytes
0000: 03 18 0d 00 01 09 02 03 04 03 03 03 03 00 00 00 
0010: 00 00 00 00 00 00 00 00 

Chassis Information
	Manufacturer: Apple Inc.
	Type: Laptop
	Lock: Not Present
	Version: Mac-BE088AF8C5EB4FA2
	Serial Number: C**********G
	Asset Tag:  
	Boot-up State: Safe
	Power Supply State: Safe
	Thermal State: Safe
	Security Status: None
	OEM Information: 0x00000000
	Height: Unspecified
	Number Of Power Cords: Unspecified
	Contained Elements: 0
	SKU Number: Not Specified

Handle 0x000E, DMI type 8, 9 bytes
0000: 08 09 0e 00 00 00 01 12 10 

Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: USB0
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x000F, DMI type 8, 9 bytes
0000: 08 09 0f 00 00 00 01 12 10 

Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: USB1
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x0010, DMI type 8, 9 bytes
0000: 08 09 10 00 00 00 01 1f 1d 

Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Audio Line In
	External Connector Type: Mini Jack (headphones)
	Port Type: Audio Port

Handle 0x0011, DMI type 8, 9 bytes
0000: 08 09 11 00 00 00 01 00 ff 

Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Thunderbolt
	External Connector Type: None
	Port Type: Other

Handle 0x0012, DMI type 8, 9 bytes
0000: 08 09 12 00 01 ff 00 00 00 

Port Connector Information
	Internal Reference Designator: Microphone
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: None

Handle 0x0013, DMI type 8, 9 bytes
0000: 08 09 13 00 01 ff 00 00 00 

Port Connector Information
	Internal Reference Designator: Speaker
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: None

Handle 0x0014, DMI type 11, 5 bytes
0000: 0b 05 14 00 01 

OEM Strings
	String 1: Apple ROM Version.  BIOS ID:      IM183.88Z.0145.B02.1703311945.  Built by:     _atsserver@xapp157.  Date:         Fri Mar 31 19:45:54 2017.  Revision:     145.2 (B&I).  ROM Version:  0145_B02.  Build Type:   Official Build.  Compiler:     Apple LLVM version 6.1.0 (clang-602.0.53) (based on LLVM 3.6.0svn).

Handle 0x0015, DMI type 41, 11 bytes
0000: 29 0b 15 00 01 83 01 00 00 00 00 

Onboard Device
	Reference Designation: Integrated Video Controller
	Type: Video
	Status: Enabled
	Type Instance: 1
	Bus Address: 0000:00:00.0

Handle 0x0016, DMI type 41, 11 bytes
0000: 29 0b 16 00 01 87 01 00 00 00 00 

Onboard Device
	Reference Designation: Azalia Audio Codec
	Type: Sound
	Status: Enabled
	Type Instance: 1
	Bus Address: 0000:00:00.0

Handle 0x0017, DMI type 41, 11 bytes
0000: 29 0b 17 00 01 89 01 00 00 00 00 

Onboard Device
	Reference Designation: SATA
	Type: SATA Controller
	Status: Enabled
	Type Instance: 1
	Bus Address: 0000:00:00.0

Handle 0x0018, DMI type 13, 22 bytes
0000: 0d 16 18 00 01 01 00 00 00 00 00 00 00 00 00 00 
0010: 00 00 00 00 00 01 

BIOS Language Information
	Installable Languages: 1
		en
	Currently Installed Language: en

Handle 0x0019, DMI type 22, 26 bytes
0000: 16 1a 19 00 00 00 00 00 00 02 00 00 00 00 00 00 
0010: 00 00 00 00 00 00 00 00 00 00 

Portable Battery
	Location: Not Specified
	Manufacturer: Not Specified
	Name: Not Specified
	Design Capacity: Unknown
	Design Voltage: Unknown
	SBDS Version: Not Specified
	Maximum Error: 0%
	SBDS Serial Number: 0000
	SBDS Manufacture Date: 1980-00-00
	SBDS Chemistry: Not Specified
	OEM-specific Information: 0x00000000

Handle 0x001A, DMI type 32, 11 bytes
0000: 20 0b 1a 00 00 00 00 00 00 00 00 

System Boot Information
	Status: No errors detected

Handle 0x001B, DMI type 131, 6 bytes
0000: 83 06 1b 00 05 06 

Apple specific Processor Type
	 cpu=0605

Handle 0x001C, DMI type 133, 12 bytes
0000: 85 0c 1c 00 00 00 00 00 00 00 00 00 

OEM-specific Type
	Header and Data:
		85 0C 1C 00 00 00 00 00 00 00 00 00

Handle 0x001D, DMI type 128, 96 bytes
0000: 80 60 1d 00 03 00 00 00 36 f5 07 fd 3f ff 1f ff 
0010: 02 00 03 00 00 00 00 00 00 90 96 ff ff 3f ad ff 
0020: 00 40 ad ff ff df d0 ff 00 90 93 ff ff 8f 96 ff 
0030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0040: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0050: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0060: 

Apple specific FirmwareVolume
	FirmwareFeatures: fd07f536
	FirmwareFeaturesMask: ff1fff3f
	Region Type:02 Start:ff969000 End:ffad3fff
	Region Type:00 Start:ffad4000 End:ffd0dfff
	Region Type:03 Start:ff939000 End:ff968fff

Handle 0x001E, DMI type 134, 20 bytes
0000: 86 14 1e 00 32 2e 34 31 46 30 31 00 00 00 00 00 
0010: 00 00 00 00 

OEM-specific Type
	Header and Data:
		86 14 1E 00 32 2E 34 31 46 30 31 00 00 00 00 00
		00 00 00 00

Handle 0x001F, DMI type 7, 19 bytes
0000: 07 13 1f 00 01 80 01 00 01 00 01 20 00 20 00 00 
0010: 04 05 07 

Cache Information
	Socket Designation: L1 Cache
	Configuration: Enabled, Not Socketed, Level 1
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 256 kB
	Maximum Size: 256 kB
	Supported SRAM Types:
		Synchronous
	Installed SRAM Type: Synchronous
	Speed: Unknown
	Error Correction Type: Parity
	System Type: Unified
	Associativity: 8-way Set-associative

Handle 0x0020, DMI type 7, 19 bytes
0000: 07 13 20 00 01 81 01 00 04 00 04 20 00 20 00 00 
0010: 05 05 05 

Cache Information
	Socket Designation: L2 Cache
	Configuration: Enabled, Not Socketed, Level 2
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 1024 kB
	Maximum Size: 1024 kB
	Supported SRAM Types:
		Synchronous
	Installed SRAM Type: Synchronous
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Unified
	Associativity: 4-way Set-associative

Handle 0x0021, DMI type 7, 19 bytes
0000: 07 13 21 00 01 82 01 00 18 00 18 20 00 20 00 00 
0010: 06 05 09 

Cache Information
	Socket Designation: L3 Cache
	Configuration: Enabled, Not Socketed, Level 3
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 6144 kB
	Maximum Size: 6144 kB
	Supported SRAM Types:
		Synchronous
	Installed SRAM Type: Synchronous
	Speed: Unknown
	Error Correction Type: Multi-bit ECC
	System Type: Unified
	Associativity: 12-way Set-associative

Handle 0x0022, DMI type 4, 48 bytes
0000: 04 30 22 00 01 03 cd 02 e9 06 09 00 ff fb eb bf 
0010: 03 8a 19 00 48 0d 48 0d 41 01 1f 00 20 00 21 00 
0020: 04 05 06 04 04 04 ec 00 cd 00 04 00 04 00 04 00 
0030: 

Processor Information
	Socket Designation: U3E1
	Type: Central Processor
	Family: Core i5
	Manufacturer: Intel(R) Corporation
	ID: E9 06 09 00 FF FB EB BF
	Signature: Type 0, Family 6, Model 158, Stepping 9
	Flags:
		FPU (Floating-point unit on-chip)
		VME (Virtual mode extension)
		DE (Debugging extension)
		PSE (Page size extension)
		TSC (Time stamp counter)
		MSR (Model specific registers)
		PAE (Physical address extension)
		MCE (Machine check exception)
		CX8 (CMPXCHG8 instruction supported)
		APIC (On-chip APIC hardware supported)
		SEP (Fast system call)
		MTRR (Memory type range registers)
		PGE (Page global enable)
		MCA (Machine check architecture)
		CMOV (Conditional move instruction supported)
		PAT (Page attribute table)
		PSE-36 (36-bit page size extension)
		CLFSH (CLFLUSH instruction supported)
		DS (Debug store)
		ACPI (ACPI supported)
		MMX (MMX technology supported)
		FXSR (FXSAVE and FXSTOR instructions supported)
		SSE (Streaming SIMD extensions)
		SSE2 (Streaming SIMD extensions 2)
		SS (Self-snoop)
		HTT (Multi-threading)
		TM (Thermal monitor supported)
		PBE (Pending break enabled)
	Version: Intel(R) Core(TM) i5-7500 CPU @ 3.40GHz
	Voltage: 1.0 V
	External Clock: 25 MHz
	Max Speed: 3400 MHz
	Current Speed: 3400 MHz
	Status: Populated, Enabled
	Upgrade: Other
	L1 Cache Handle: 0x001F
	L2 Cache Handle: 0x0020
	L3 Cache Handle: 0x0021
	Serial Number: To Be Filled By O.E.M.
	Asset Tag: To Be Filled By O.E.M.
	Part Number: To Be Filled By O.E.M.
	Core Count: 4
	Core Enabled: 4
	Thread Count: 4
	Characteristics:
		64-bit capable
		Multi-Core
		Execute Protection
		Enhanced Virtualization
		Power/Performance Control

Handle 0x0023, DMI type 14, 8 bytes
0000: 0e 08 23 00 01 db 00 00 

Group Associations
	Name: $MEI
	Items: 1
		0x0000 (<OUT OF SPEC>)

Handle 0x0024, DMI type 219, 81 bytes
0000: db 51 24 00 01 03 01 55 00 00 90 06 01 8a 30 10 
0010: 00 00 00 00 40 00 00 00 00 00 00 00 00 00 40 02 
0020: ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
0030: ff ff ff ff ff ff ff ff 03 00 00 00 80 00 00 00 
0040: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
0050: 00 

OEM-specific Type
	Header and Data:
		DB 51 24 00 01 03 01 55 00 00 90 06 01 8A 30 10
		00 00 00 00 40 00 00 00 00 00 00 00 00 00 40 02
		FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
		FF FF FF FF FF FF FF FF 03 00 00 00 80 00 00 00
		00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
		00
	Strings:
		MEI1
		MEI2
		MEI3

Handle 0xFEFF, DMI type 127, 4 bytes
0000: 7f 04 ff fe 

End Of Table

