+-o Root  <class IORegistryEntry, id 0x100000100, retain 9>
  | {
  |   "IOKitBuildVersion" = "Darwin Kernel Version 13.2.0: Thu Apr 17 23:03:13 PDT 2014; root:xnu-2422.100.13~1/RELEASE_X86_64"
  |   "OS Build Version" = "13D65"
  |   "IONDRVFramebufferGeneration" = <0300000003000000>
  |   "OSKernelCPUSubtype" = 3
  |   "OSKernelCPUType" = 16777223
  |   "OSPrelinkKextCount" = 253
  |   "IOConsoleLocked" = No
  |   "IORegistryPlanes" = {"IOACPIPlane"="IOACPIPlane","IOPower"="IOPower","IODeviceTree"="IODeviceTree","IOService"="IOService","IOUSB"="IOUSB"}
  |   "IOConsoleUsers" = ({"kCGSSessionOnConsoleKey"=Yes,"kCGSSessionLoginwindowSafeLogin"=No,"kSCSecuritySessionID"=100004,"kCGSessionLongUserNameKey"=,"kCGSSessionUserIDKey"=501,"kCGSSessionSystemSafeBoot"=No,"kCGSSessionUserNameKey"="plievasabina","kCGSSessionIDKey"=256,"kCGSessionLoginDoneKey"=Yes,"kCGSSessionGroupIDKey"=20,"kCGSSessionAuditIDKey"=100004})
  |   "IOKitDiagnostics" = {"Container allocation"=3634707,"Instance allocation"=4790752,"Pageable allocation"=101642996,"Classes"={"AppleACPIButton"=2,"IOHDIXCommand"=0,"_IOConfigThread"=0,"nvVirtualAddress"=780,"IOInterleavedMemoryDescriptor"=0,"IOAGPDevice"=0,"IOHIDPointing"=1,"IOHIDEventRepairDriver"=0,"IOSMBusController"=1,"IOGraphicsAccelerator2"=1,"AppleACPICPUInterruptController"=1,"IOUSBRootHubDevice"=2,"AppleHDAFunctionGroupATI_RS710"=0,"OSSerialize"=1,"IOBreaker"=0,"IO80211Peer"=0,"IGAccelEventMachine"=1,"IGSubStolenMemoryDescriptor"=0,"AppleXsanFilter"=1,"IGRangeAllocator"=2,"DspParameter"=161,"BroadcomBluetoothHostControllerUSBTransport"=1,"AppleThunderboltNHITransmitRing"=12,"IOMemoryCursor"=1,"AppleThunderboltDPOutAdapter"=1,"IOUserClient"=26,"AppleMCP89AHCIPort"=0,"nvDevice"=5,"IOThunderboltTransmitQueue"=1,"IORegistryIterator"=0,"IOBluetoothHostController"=0,"IOThunderboltFindCapabilityCommand"=2,"IOAccelShared"=1,"IOServicePM"=89,"IOUSBLog"=1,"IOBluetoothObject"=2,"IOAccelResource2"=0,"AppleHDAWidgetATI_Park"=0,"nvTextureBuffer"=515,"AppleSMBusPCI"=1,"OSArray"=4096,"AppleLMUClient"=1,"AppleMikeyDevice_CD3282"=1,"AppleIntelFramebuffer"=0,"IOSubMemoryDescriptor"=12,"AppleAHCIDiskPolledInterface"=1,"IOAccelMemory"=1,"OSObject"=128,"PMEventDetails"=0,"IOThunderboltPath"=0,"IOApplePartitionScheme"=0,"PMHaltWorker"=0,"DspFuncPreGain"=0,"IOTimerEventSource"=105,"IOPCIMessagedInterruptController"=1,"AppleHDAFunctionGroup_10DE0014"=0,"IOThunderboltConfigPrepareToSleepCommand"=1,"IOMemoryDescriptor"=2,"AppleMCP89AHCI"=0,"MEIDriverIOEventSource"=3,"nvTeslaGT21AHAL"=0,"AppleHDAAudioSelectorControlDP"=0,"IOThunderboltConfigReadQuadletCommand"=3,"IGAccelDisplayMachine"=1,"__GLNVEvoBasePushBuf"=1,"AppleIntelPanelA"=1,"AppleACPILid"=0,"IOBluetoothHIDDriver"=1,"IODTPlatformExpert"=1,"IOConditionLock"=0,"IOUSBInterfaceIterator"=0,"AppleMultitouchHIDEventDriver"=1,"mDNSHandoff"=0,"IO80211NetBootNub"=0,"DspFuncClientGainAdjust"=1,"IOUSBControllerV2"=1,"AppleEFIRuntime"=1,"IOAppleLabelScheme"=0,"AppleHDAWidgetALC885"=0,"IOAccelEventMachine"=1,"AirPort_Brcm4360_P2PInterface"=1,"IOBluetoothDevice"=2,"IOAHCIPort"=1,"AppleXHCIAsyncTransferDescriptor"=53,"AppleMultitouchEventDriverWrapper"=1,"com_belkin_f2cd0007_adapter"=0,"AirPort_Brcm4360_InputQueue"=1,"IO80211ScanManager"=1,"IOAccelGPURestartReport"=0,"nvFermiGLContext"=4,"IOHIDWorkLoop"=1,"_IOFramebufferNotifier"=12,"IGHardwareRingBufferBlit"=1,"nvTeslaG82HAL"=0,"AppleThunderboltNHIType1"=0,"CamelliaTcon"=0,"AppleHDAWidgetWM8800"=0,"DspFuncMultiBandCompressor"=0,"IOHIDUserClient"=1,"IOCommandPool"=8,"IOMultiMemoryDescriptor"=0,"DspFuncLoudness"=1,"IOAccelStatistics"=1,"AppleUSBHSHubUserClient"=0,"nvFermiHAL"=1,"DspFuncAudioMeter"=0,"IOThunderboltPacketLoggerNub"=0,"IOBluetoothRFCOMMConnectionUserClient"=0,"IOHIDKeyboard"=1,"IOThunderboltArray"=5,"OSNumber"=10295,"IOAccelAllocation"=1,"IOAccelCLContext"=0,"IOHIDElement"=1,"IOPacketQueue"=1,"PMAssertionsTracker"=1,"AppleGraphicsDeviceControlClient"=0,"nvKeplerSharedPixels"=1,"IOPlatformExpert"=1,"IOHIDResourceDeviceUserClient"=0,"IOServiceMessageUserNotification"=188,"AppleMCCSControlModule"=3,"IOHDACodecFunction"=2,"IODisplayConnect"=1,"IOHDIXHDDriveOutKernel"=0,"IOUSBControllerListElement"=0,"AppleMultitouchEventServiceWrapper"=0,"LogManagerDevice"=3,"AppleBacklightDisplay"=1,"IGAccelCLContext"=0,"IOOutputQueue"=1,"IOThunderboltIECSCommand"=0,"IOEventSource"=15,"AppleSMBusDevice"=2,"com_apple_AppleFSCompression_AppleFSCompressionTypeDataless"=1,"IOHWSensor"=1,"nvVirtualAddressSpace"=6,"AppleUSBMergeNub"=1,"AppleHDAWidgetAD1984"=0,"AirPort_Brcm4360"=1,"AppleGraphicsDeviceControl"=2,"AppleThunderboltEDMSinkUserClient"=0,"AppleHDACodec"=1,"IOFramebufferParameterHandler"=3,"IOPanicPlatform"=0,"IOBluetoothL2CAPSupervisoryFrameMemoryBlock"=0,"IOUSBControllerV3"=1,"IOGraphicsAccelerator"=1,"IO80211VirtualInterfaceNamer"=1,"AppleSMC"=1,"OSKext"=122,"X86PlatformShim"=1,"AppleSMBusControllerUserClient"=0,"IOThunderboltConfigXDomainLinkChangeRequestCommand"=0,"IOSCSIPeripheralDeviceType07"=0,"IOBluetoothHCIUserClient"=4,"BluetoothMultitouchTransport"=1,"IOThunderboltConfigMultiReadCommand"=2,"AppleAHCIPortPolledAdapter"=1,"AppleEmbeddedKeyboard"=1,"IOUSBBus"=1,"IOBootFramebuffer"=0,"AppleHDAControllerUserClient"=0,"IOBluetoothLocalUtilityEventSource"=0,"AppleHDAWorkLoop"=2,"AppleSDXCSlot"=1,"AppleHDAFunctionGroupGK10X"=1,"nvGpFifoChannel"=21,"AppleHDAWidgetSTAC9220"=0,"IORootParent"=1,"AppleMikeyACPIFactory"=0,"IOAccelChannel2"=1,"nvHAL"=1,"IOBluetoothSerialClientModemStreamSync"=1,"IOAccelCommandBufferPool2"=3,"IOAccelContext2"=0,"ApplePlatformEnablerUserClient"=0,"IOThunderboltControlPathListener"=7,"IO80211ServiceRequestDescriptor"=0,"AppleHDAWidgetFactory"=0,"ApplePlatformEnabler"=1,"nvSemaphoreManager"=5,"IOHIDResource"=1,"DspFunc2To6Splitter"=0,"IOAccelMemoryMap"=1,"IOMemoryMap"=632,"IO80211Interface"=1,"IOCharacterDevice"=3,"AppleHDAWidget_80862807"=0,"IOThunderboltConfigCommand"=11,"IOAccelSharedNamespace"=3,"IOThunderboltEEPROM"=2,"IGAccelMemoryMap"=16,"IOAudioDevice"=1,"IOI2CInterface"=1,"IOAccelFIFOChannel"=0,"IOSCSIMultipathedLogicalUnit"=0,"IOPMPowerSourceList"=0,"IOThunderboltXDPropertiesEntry"=11,"IO80211P2PInterface"=1,"IOAccelShared2"=0,"IGHardwareRingBuffer"=4,"IOAudioToggleControl"=7,"IOAudioStream"=1,"AppleXHCIIsochTransferDescriptor"=0,"AppleMikeyDevice"=1,"IOThunderboltConfigXDomainUUIDRequestCommand"=1,"DspFuncBuzzKill"=0,"IOSCSILogicalUnitNub"=2,"IOReportLegend"=3,"nvGpFifoChannelInterface"=21,"BNBMouseDevice"=1,"IOAccelContext"=2,"AppleUSBComposite"=0,"IOAccelDisplayMachine2"=1,"IOPowerConnection"=82,"AppleThunderboltIPEventSource"=1,"RSNSupplicant"=0,"AppleHDAWidget_1002AAA0"=0,"IOPCIBridge"=2,"AppleThunderboltNHIReceiveRingManager"=1,"AppleHDAPathControl"=10,"_IOServiceNotifier"=204,"AppleHDAEngine"=2,"IOHIDKeyboardDevice"=0,"AppleThunderboltNHIUserClient"=0,"IOHDAController"=1,"AppleEFINVRAM"=1,"DspFuncVirtualization"=0,"IOPCIDevice"=25,"IOGraphicsDevice"=1,"IOAudioPort"=0,"IOBluetoothDataQueue"=0,"IOThunderboltLocalNode"=1,"IOThunderboltXDPropertiesImmediateValue"=7,"IOThunderboltConfigWriteQuadletCommand"=2,"IOInterruptEventSource"=78,"nvDebugClient"=0,"nvVidmemPushBuffer"=0,"AGPMController"=1,"AppleACPIEventController"=1,"IOHDAStream"=3,"IOHIDevice"=2,"IOPlatformPluginFamily"=1,"IOPMRequest"=0,"DspFuncMozartCompressorDualBand"=1,"IOThunderboltUserObjectExporter"=0,"IOPlatformExpertDevice"=1,"IOHITabletPointer"=0,"IOThunderboltI2CCommandQueue"=1,"IORegistryPlane"=5,"IOUSBInterface"=12,"AppleAHCIPolledAdapter"=1,"AppleThunderboltNHIReceiveRing"=12,"DspFuncDelay"=0,"AppleMikeyACPIHeadsetA"=1,"AppleMikeyHIDDriver"=1,"IOLittleMemoryCursor"=0,"IOAccelMemoryInfoUserClient"=1,"IOThunderboltControlPath"=1,"IOAHCIDiskQueueManager"=1,"IOHIDEventDriver"=3,"AppleHDAFunctionGroupATI_Park"=0,"HDCPCtrl"=0,"IOSurfaceRootUserClient"=2,"IOMbufMemoryCursor"=1,"IGAccelVideoContext"=0,"IOBluetoothACLMemoryDescriptor"=0,"IOThunderboltUserProtocolListener"=0,"IOThunderboltFamilyUserClient"=0,"AppleMikeyDeviceFactory"=0,"IOAudioControlUserClient"=19,"IGHardwareRingBufferMedia"=1,"AudioAUUC"=0,"BroadcomBluetoothHostController"=0,"AppleHDAFunctionGroupExternalControl_GPIO"=1,"AppleThunderboltIPReceiveCommand"=0,"IOAccelBlockFencePort2"=0,"IOAccelSharedNamespace2"=0,"AppleBluetoothHIDKeyboard"=1,"IO80211PeerExtendedStats"=0,"OSData"=23497,"IOUSBUserClientInit"=1,"AppleThunderboltEDMSink"=1,"IOThunderboltConfigModifyQuadletCommand"=1,"AppleThunderboltNHIType2"=1,"IOHIDDeviceShim"=0,"IODMACommand"=138,"IOMbufNaturalMemoryCursor"=3,"IOPlatformDevice"=4,"IOPCI2PCIBridge"=11,"IOUSBHubDevice"=2,"IOBluetoothMemoryBlockQueue"=2,"AppleMikeyI2C_CD3282"=1,"IOThunderboltXDPropertiesLeafText"=2,"IOPartitionScheme"=2,"IOBufferMemoryDescriptor"=529,"IOBluetoothL2CAPChannel"=5,"IOUSBController"=1,"IOAccelDisplayPipeGammaTable2"=0,"IOWatchDogTimer"=1,"OSIterator"=2,"IOGeneralMemoryDescriptor"=479,"DspFuncMozartCompressor"=1,"OSMetaClass"=0,"SCSITaskUserClient"=0,"AppleHDAFunctionGroupCS4206"=1,"IOBluetoothDeviceUserClient"=2,"OSSymbol"=4849,"OSString"=5719,"EFIData"=44,"DspFunc6ChOutput"=0,"IOHistogramReporter"=0,"IO80211VirtualInterface"=1,"IOHIDLibUserClient"=6,"_IOServiceInterestNotifier"=223,"IOMapper"=1,"DspFunc2To4Splitter"=1,"AppleHDAFunctionGroupGT216"=0,"IOAccelEventMachine2"=1,"DspFunc"=8,"IOHIKeyboardMapper"=2,"IOBluetoothL2CAPSignalChannel"=2,"BNBDevice"=1,"AppleHDADriverUserClient"=0,"AppleIntelPanel"=1,"RootHubPortTable"=0,"IOSerialATARequestFIS"=68,"DspFuncAutoGainControl"=0,"IOAccelVideoContext"=0,"DspFuncChOutput"=1,"com_apple_AppleFSCompression_AppleFSCompressionTypeZlib"=1,"AppleMikeyI2C_TS3A8235"=1,"DspFuncSplineLimiter"=2,"IOUSBCompositeDriver"=3,"IOThunderboltCommand"=5,"IOPMTimeline"=0,"IOThunderboltConfigXDomainPathTeardownRequestCommand"=0,"AppleIntelPAVPEventSource"=0,"nvEvoChannel"=1,"IOAccelDrawable"=6,"DirectHWService"=1,"IO80211QueueDescriptor"=0,"IOThunderboltAbstractPath"=0,"IOUSBMassStorageUFIDevice"=0,"IOThunderboltData"=0,"nv2DContext"=3,"IOAHCIPollerInterface"=1,"AirPort_Brcm4360_Interface"=1,"AppleSMBusControllerMCP"=0,"nvApiClient"=0,"IOCommandGate"=209,"IOHIDConsumer"=1,"IO80211AWDLPeerManager"=0,"AppleHDAFunctionGroupExternalControlFactory"=0,"IOAccelChannel"=1,"AppleMikeyDriver"=1,"AppleHDAWidget_10DE0014"=0,"IOPMRequestQueue"=2,"IOAccelDisplayPipeTransaction"=0,"IOThunderboltReceiveCommand"=16,"AppleSCSISubsystemGlobals"=1,"IOSerialBSDClient"=2,"IOMediaBSDClient"=15,"IOSCSIProtocolServices"=2,"IOBluetoothRFCOMMConnection"=0,"IOUFIStorageServices"=0,"IOHIDPointingDevice"=0,"AppleHDACodecGeneric"=2,"IONetworkController"=1,"IOThunderboltXDomainService"=0,"nvHandleManager"=1,"AppleMikeyI2CFactory"=0,"IOThunderboltNHITransmitRing"=1,"IONDRVFramebuffer"=1,"SMCPolledInterface"=1,"IOThunderboltNumber"=205,"AppleIntelMCEReporting"=0,"IOAppleBluetoothHIDDriver"=2,"IODTNVRAM"=1,"AppleUpstreamUserClientDriver"=3,"IOACPIPlatformExpert"=1,"IOAccelEventMachineList"=1,"nvChannelManager"=1,"IOGraphicsWorkLoop"=2,"IOThunderboltConfigReadCommand"=9,"X86PlatformPlugin"=1,"IOHDIXController"=1,"IOSCSIPeripheralDeviceType00"=1,"IOBluetoothHCIPacketLogUserClient"=0,"IOKDP"=0,"nvTimerManager"=1,"IOHIDEventServiceQueue"=0,"nvAccelerator"=1,"IOInterruptController"=5,"IOBluetoothHCIController"=1,"AGPMHeuristic1"=0,"IOAccelerationUserClient"=1,"IOAccel2DContext"=1,"AppleSMBusController"=1,"AppleMCCSControlCello"=0,"AppleHDAWidgetCS4206"=23,"IOThunderboltDispatchQueue"=2,"AppleHDAFunctionGroupATI_RS780"=0,"IOThunderboltNHIReceiveRing"=1,"AppleHDAWidgetAD1988"=0,"IOUSBCommand"=50,"IGAccel2DContext"=0,"IOHIDElementPrivate"=385,"AGPMHeuristic3"=0,"AppleThunderboltDPPathManager"=4,"IOFramebufferUserClient"=3,"IOThunderboltXDomainLink"=0,"AppleSDXC"=1,"IOStateReporter"=3,"AppleHDAFunctionGroupALC262"=0,"IOUSBMassStorageUFISubclass"=0,"CSRBluetoothHostController"=0,"nvVideoContext"=0,"AppleAHCIRequestTimer"=1,"IOHIDSystem"=1,"AGPMClient"=2,"AppleHDAMikeyInternal"=0,"IOAccelRestartUserClient2"=0,"nvTeslaHAL"=1,"SCSITask"=0,"AppleMCP79AHCIPort"=0,"IGAccelStatistics"=1,"NVDAStartup"=0,"IOAccelSurface"=1,"IOThunderboltString"=42,"AppleHWAccessUserClient"=0,"IOFilterScheme"=0,"IOAccelDisplayPipeUserClient"=0,"IOCPU"=1,"AHCIRequest"=33,"AppleThunderboltIPTransmitCommand"=0,"AppleHDAFunctionGroupExternalControl"=2,"IGHardwareContext"=3,"IOAccelEventMachineBasic"=0,"nvAllocation"=347,"RootDomainUserClient"=35,"OSCollectionIterator"=9,"AppleACPIACAdapter"=0,"IOHIDDevice"=2,"AppleKeyStore"=1,"IO80211PeerManager"=0,"OSSerializer"=16,"IOBlockStorageDevice"=3,"AppleSATLSMARTUserClient"=0,"IOUSBNotification"=0,"nvFermiSharedPixels"=1,"AppleSDXCBlockStorageDevice"=1,"PMTraceWorker"=1,"IOAHCIBlockStorageDevice"=1,"AppleAHCIWorkLoop"=1,"IOAccelEventMachineEqual2"=0,"IOAccelSurface2"=0,"AppleMultitouchDevice"=1,"IOBluetoothL2CAPChannelUserClient"=0,"IOUserEthernetResourceUserClient"=0,"mDNSOffloadUserClient"=0,"OSDictionary"=10036,"AppleMCCSParameterHandler"=3,"DspFunc2Dot2Crossover"=0,"TTBandwidthTable"=0,"IOReportHub"=1,"AppleICH8AHCI"=0,"IOAccelBlockFencePort"=0,"AppleMCCSUserClient"=0,"IOThunderboltConfigXDomainResponseCommand"=7,"IOThunderboltLinkController"=2,"IOHIDEventQueue"=1,"AppleThunderboltIPConnection"=0,"DspFunc4ChOutput"=1,"PMSettingObject"=4,"IOThunderboltConfigXDomainCommand"=2,"IOThunderboltStatistics"=1,"AppleSDXCWorkLoop"=1,"IOAudioLevelControl"=3,"IOAudioClientBufferSet"=0,"IOHDIXCommandQueue"=0,"IO80211AWDLMulticastPeer"=0,"AppleACPIEC"=1,"IGAccelDevice"=0,"AppleSMCClient"=1,"IOEthernetInterface"=4,"IOAudioEngineUserClient"=15,"IOHDIXControllerUserClient"=0,"IOAudioTimeIntervalFilter"=1,"AppleMultitouchDeviceIODataQueue"=1,"IOController"=6,"IOThunderboltTransmitCommand"=3,"IOThunderboltConfigNotifyAckCommand"=0,"AppleHDAFunctionGroup_80862805"=0,"IOHDIXHDDriveOutKernelUserClient"=0,"AppleHDAWidgetATI_RS730"=0,"IONetworkUserClient"=0,"AppleHDAFunctionGroupExternalControl_VirtualGPO"=1,"IOHIDStackShotUserClient"=1,"AppleThunderboltDPOutAdapterUserClient"=0,"IOSCSIPeripheralDeviceNub"=1,"nvMemory"=1,"AppleMCCSControlFamily"=1,"IOPMinformeeList"=89,"nvCudaContext"=0,"DspFuncMultiBandDRC"=0,"IOAudioControl"=3,"IOBluetoothSerialClient"=2,"IOAudioTimeIntervalFilterIIR"=3,"AppleHDAPath"=7,"AppleHDAFunctionGroupFactory"=0,"IOAccelStatistics2"=1,"AppleXHCIIsochEndpoint"=2,"IOBluetoothRFCOMMChannel"=0,"IOThunderboltNub"=2,"IOHIKeyboard"=2,"IOThunderboltFrameList"=18,"IOFilterInterruptEventSource"=11,"AppleThunderboltIPTransmitter"=0,"AppleXHCIDiagnostics"=1,"IOUSBControllerUserClient"=0,"IOAccelMemoryAllocator"=0,"IOHITablet"=1,"AppleACPICPU"=4,"IOSurfaceRoot"=1,"IOThunderboltSwitchType1"=0,"NVDA"=3,"AppleMikeyACPI"=1,"DspFuncStereoEnhancer"=0,"AppleMikeyACPIHeadsetB"=0,"AppleSMBusControllerICH"=1,"nvSurface"=6,"IOGUIDPartitionScheme"=2,"IOSerialStreamSync"=2,"AppleThunderboltHAL"=1,"AppleIntelPchSeriesAHCI"=1,"AppleACPIEventPoller"=1,"IOHIDEventSystemUserClient"=3,"IOPlatformPluginFamilyPriv"=1,"IOSCSITargetDevice"=0,"IORS232SerialStreamSync"=1,"AppleHDAWidgetCS4208"=0,"IOSimpleReporter"=0,"IODeblocker"=0,"AppleDisplay"=0,"IOAccelEventMachineList2"=0,"IOUSBControllerIsochEndpoint"=1,"IOBluetoothGamepadHIDDriver"=0,"NVDC"=1,"nvGLContext"=1,"IOUSBPipe"=1,"IOAccelMemoryAllocator2"=0,"IOAccelDevice2"=0,"IOSurface"=0,"IOBluetoothHostControllerTransport"=1,"IGAccelDisplayPipe"=0,"IGHardwareRingBufferMain"=1,"nvDisplayManager"=1,"IOThunderboltConnectionManager"=1,"IOGatedOutputQueue"=11,"IOSurfaceSendRight"=0,"IOUSBMassStorageClass"=1,"IOThunderboltXDPropertiesDirectory"=2,"IOThunderboltTimerCommandQueue"=1,"_IOOpenServiceIterator"=0,"AppleAHCIWatchdogTimer"=1,"IOThunderboltPortMicro"=0,"IODisplayParameterHandler"=3,"IONetworkStackUserClient"=1,"IOCommand"=85,"DspPatchPoint"=64,"AppleACPIPowerResource"=0,"DspFunc3ChOutput"=0,"IOReportUserClient"=1,"AppleThunderboltNHIMemoryBlock"=0,"IOPMPowerSource"=0,"IOHIDResourceQueue"=0,"DISPLAYPATH"=0,"SMCWatchDogTimer"=1,"AppleMCP79AHCI"=0,"MEICompletion"=0,"IOBluetoothRFCOMMChannelUserClient"=0,"IO80211ActionFrameDescriptor"=0,"AppleHDAWidget"=2,"IOAccelGLContext2"=0,"AppleHWAccess"=1,"AppleHDAFunctionGroupSTAC9220"=0,"IOThunderboltConfigCompareSwapCommand"=0,"SCSITaskUserClientIniter"=1,"AppleThunderboltDPAdapterFamily"=2,"IOBacklightDisplay"=1,"IOUSBPipeV2"=19,"IOThunderboltPort"=12,"OSBoolean"=2,"nvTeslaGLContext"=1,"DspFuncCrossover"=0,"IOUSBDevice"=5,"IOHIDParamUserClient"=1,"nvCLContext"=0,"IOHIDAsyncReportQueue"=0,"IOAudioEngineEntry"=0,"DspFuncVolume_4ch"=0,"AppleHDAFunctionGroupAD1988"=0,"AppleBacklightParameterHandler"=1,"IOBasicOutputQueue"=1,"DspFuncStereoToMono"=0,"AppleSMCFamily"=1,"IOSCSIPrimaryCommandsDevice"=1,"AppleHDAFunctionGroup_80862807"=0,"IOThunderboltReceiveQueue"=1,"AppleHDAFunctionGroup_1002AAA0"=0,"IOAHCIBlockStorageDriver"=1,"IOAccelDisplayPipe2"=0,"DspFunc2WayCrossover"=0,"IOHDIXHDDriveNub"=0,"IOBluetoothInactivityTimerEventSource"=3,"IOThunderboltProtocolListener"=1,"IONDRVDevice"=3,"IOMbufLittleMemoryCursor"=0,"IOUserNotification"=2,"AppleAHCIDiskQueueManager"=1,"IOBluetoothHostControllerUSBTransport"=1,"nvEventManager"=1,"nvPushBuffer"=1,"AppleThunderboltIPControlCommand"=0,"AppleHIDKeyboardEventDriverV2"=0,"IOThunderboltIECSCommandQueue"=1,"IOBlockStorageDriver"=3,"IOService"=146,"IGAccelSurface"=0,"IOHIDEvent"=0,"AGPMEventSource"=1,"IONetworkStack"=1,"IOBluetoothTimerEventSource"=0,"IOSerialDriverSync"=1,"IOThunderboltConfigWriteCommand"=6,"Dont_Steal_Mac_OS_X"=1,"IORegistryEntry"=68,"IOThunderboltController"=1,"IODMAController"=0,"IOBootNDRV"=0,"IGAccelTask"=1,"AppleXHCIAsyncEndpoint"=13,"IOHIPointing"=1,"IOServiceUserNotification"=143,"IOStorage"=3,"DspFuncNoiseCanceller"=1,"IOModemSerialStreamSync"=1,"IOHWControl"=0,"IOThunderboltCallbackEventSource"=5,"IOThunderboltSwitch"=1,"AppleThunderboltDPInAdapter"=2,"IOAccelCLContext2"=0,"IOHDACodecDevice"=2,"IOAccelDevice"=1,"AppleAPICInterruptController"=1,"IOSMBusRequest"=0,"AppleHDAEngineUserClient"=0,"IOUSBInterfaceUserClientV3"=0,"IOAccelDrawable2"=0,"DspFuncUserClient"=0,"IOBigMemoryCursor"=0,"AppleHDAFunctionGroupATI_Broadway"=0,"nvEvoChannelInterface"=1,"DspFuncLimiter"=0,"AGPM"=1,"AppleHDAFunctionGroupALC885"=0,"OSCollection"=5,"AppleUSBXHCI"=1,"AppleHDAFunctionGroupCS4208"=0,"IOThunderboltXDPropertiesLeafData"=0,"AppleRTC"=1,"IOSCSIBlockCommandsDevice"=1,"AppleIntelAzulController"=1,"AppleACPIPlatformExpert"=1,"IOHDIXHDDrive"=0,"AppleAHCIWorkLoopLock"=1,"PMSettingHandle"=4,"nvTimerAction"=4,"IOSyncer"=0,"IOAccelerator"=2,"nvRingBuffer"=21,"DirectHWUserClient"=0,"AppleHDAMikeyInternalCS4208"=0,"MEIClientList"=1,"IONaturalMemoryCursor"=0,"IOSurfaceClient"=0,"AppleThunderboltNHITransmitRingManager"=1,"IOThunderboltConfigXDomainROMChangedRequestCommand"=0,"nvTeslaSharedPixels"=1,"IOBluetoothHCIRequest"=0,"AHCISMARTUserClient"=0,"IONotifier"=3,"IOCatalogue"=1,"nvChannelInterface"=2,"EupDSP"=0,"AppleHDAWidgetGT216"=0,"IOUserEthernetResource"=1,"AirPort_Brcm4360_Timer"=22,"IOAccelCommandBuffer"=0,"IOUSBWorkLoop"=1,"IOPolledInterface"=5,"NVDAGK100HAL"=1,"IOSCSIProtocolInterface"=2,"AudioAUUCDriver"=1,"IOKernelDebugger"=0,"IOUSBIsocCommand"=50,"IOMedia"=15,"AppleACPIInterruptLink"=0,"IOThunderboltCommandGate"=8,"nvKeplerHAL"=1,"nvShared"=3,"IOHIDInterface"=3,"IOAudioTimeIntervalFilterFIR"=0,"AppleThunderboltIPPort"=2,"IOAccelAllocationInfo"=0,"BNBTrackpadDevice"=0,"AppleHDAWidgetGK10X"=8,"IOThunderboltConfigXDomainLinkStatusRequestCommand"=0,"AppleHDAFunctionGroupWM8800"=0,"IOThunderboltSwitchType2"=1,"IOThunderboltNHI"=1,"AppleHDAController"=2,"AppleHDAFunctionGroupMCP89"=0,"IOEthernetAVBInterface"=1,"AppleThunderboltPCIDownAdapter"=4,"AppleLPC"=1,"AppleHDAWidgetMCP79"=0,"IOAccelDisplayPipeGammaTable"=0,"IOUserEthernetInterface"=0,"IONDRV"=0,"IOThunderboltConfigCMOverrideCommand"=1,"AppleThunderboltNHI"=1,"IOAccelDisplayPipeUserClient2"=0,"AppleMultitouchHIDEventDriverV2"=0,"IOAccelGLContext"=1,"AppleAHCIDiskDriver"=1,"IOThunderboltConfigPollQuadletCommand"=1,"AppleSDXCCommand"=64,"IOUSBDeviceUserClientV2"=0,"AppleHDAWidgetATI_RS710"=0,"IOThunderboltConfigXDomainROMReadRequestCommand"=0,"IOHIDEventSystemQueue"=0,"IOEthernetAVBController"=1,"IOAudioEngine"=1,"AppleMultitouchDeviceUserClient"=1,"IOPMWorkQueue"=1,"AppleMultitouchHIDEventService"=0,"BCM5701Enet"=1,"IOAccelEventMachineBasic2"=1,"IOWorkLoop"=35,"IO80211CommandQueue"=0,"IOUSBLowLatencyCommand"=0,"IOPMinformee"=55,"IGAccelGLContext"=0,"AppleHDAFunctionGroup"=2,"AppleHDAWidgetALC262"=0,"IOThunderboltXDomainPath"=0,"IOThunderboltTunnelDriver"=2,"IOUSBNub"=2,"IOUserEthernetController"=0,"IO80211Controller"=1,"AppleThunderboltIPService"=1,"AppleIntelMEIDriver"=1,"DspBuffer"=10,"IGAccelStolenMemoryPool"=1,"IOPCIConfigurator"=1,"DspFuncGain"=1,"IOThunderboltConfigXDomainRequestCommand"=0,"nvEvoManager"=1,"IOThunderboltDictionary"=12,"IOFramebufferSharedUserClient"=1,"IOThunderboltWorkLoop"=1,"AppleMikeyDriverUserClient"=0,"IOBluetoothWorkLoop"=0,"AppleHDAMikeyInternalFactory"=0,"IOSurfaceDeviceCache"=0,"OSSet"=813,"IOAccelResource"=2,"AppleMikeyI2C"=2,"IOThunderboltConfigXDomainPathSetupRequestCommand"=0,"AppleHDADriver"=2,"AppleUSBDiagnostics"=1,"IOAccelTask"=1,"NVDAUser"=0,"nvSysmemPushBuffer"=22,"DspFuncEQ"=5,"IOAccelRestartUserClient"=0,"IGAccelVideoContextVEBox"=0,"IOThunderboltXDPropertiesCache"=1,"LogManager"=1,"com_apple_BootCache"=1,"IODisplay"=1,"IO80211WorkLoop"=1,"KDIURL"=0,"AppleHDANode"=2,"AppleHDAStream"=4,"AppleHDAEngineOutput"=1,"IOUSBCommandPool"=2,"IO80211DriverCommandDescriptor"=0,"nvGpFifoBuffer"=21,"AppleLMUController"=1,"AppleAHCIEventSource"=1,"IOAccelSharedUserClient"=1,"AppleSNBFBUserClient"=0,"IOMbufBigMemoryCursor"=0,"AppleCSRBluetoothHostController"=0,"IOUSBHubPolicyMaker"=1,"IOUSBInterfaceUserClientV2"=0,"IOFramebufferI2CInterface"=3,"IOAccelVidMemory"=0,"ApplePMTGraphicsInformation"=0,"IGAccelSharedUserClient"=0,"IOAccelEventMachineSingle"=0,"IOPMCompletionQueue"=1,"AppleHDAFunctionGroupAD1984"=0,"AppleHDAFunctionGroupMCP79"=0,"DspFunc2Dot1Crossover"=0,"AppleUpstreamUserClient"=0,"AppleKeyStoreUserClient"=3,"AppleAHCIPort"=1,"IOBluetoothSerialManager"=1,"IOSharedDataQueue"=0,"IOBlockStorageServices"=1,"IONetworkMedium"=23,"IGAccelFIFOChannel"=4,"IOBluetoothL2CAPInformationFrameMemoryBlock"=0,"nvStatistics"=1,"IOBluetoothSerialClientSerialStreamSync"=1,"IOHDACodecDriver"=2,"IOThunderboltCommandQueue"=8,"AppleRTCUserClient"=0,"IOAccelDisplayPipeTransaction2"=0,"IOThunderboltXDDirectory"=0,"IOThunderboltTimerCommand"=8,"IOSCSIHierarchicalLogicalUnit"=0,"IGAccelVideoContextMedia"=0,"IONetworkData"=19,"AppleECSMBusController"=0,"IGAccelVideoContextMain"=0,"IntelFBClientControl"=1,"IOBluetoothRFCOMMMemoryBlock"=0,"nvSharedUserClient"=3,"IOAccel2DContext2"=0,"nvPTEEntry"=87,"AppleBroadcomBluetoothHostController"=0,"IntelAccelerator"=1,"IOI2CInterfaceUserClient"=0,"IOCPUInterruptController"=1,"AppleHDAWidgetATI_RS780"=0,"IOAccelSysMemory"=1,"IOAccelSharedUserClient2"=0,"IOReporter"=1,"IOAHCIDevice"=1,"IODataQueue"=2,"BCM5701UserClient"=0,"IOThunderboltXDLocalPropertiesCache"=1,"IOHWMonitor"=1,"DspFuncSum"=0,"IOThunderboltHopSet"=24,"IOHIDUserDevice"=0,"DspFuncBiquad"=0,"IOAHCIPortMultiplier"=0,"IODisplayWrangler"=1,"AppleMikeyWorkLoop"=1,"IOPMPowerStateQueue"=1,"IOAudioSelectorControl"=5,"AppleUSBiPod"=0,"DspFuncDRC"=0,"AppleIntelPAVP"=0,"IGAccelSysMemory"=16,"IOAccelEventMachineEqual"=0,"nvSharedPixels"=1,"AppleUSBHubPort"=23,"AppleHPET"=1,"AppleHDAWidgetMCP89"=0,"IOThunderboltConfigErrorCommand"=1,"AppleUSBHub"=3,"IOAudioTimerEvent"=0,"AGPMHeuristic0"=0,"IOAccelFIFOChannel2"=1,"IGHardwareRingBufferVEBox"=1,"AppleHIDKeyboardEventDriver"=0,"RadeonPCI"=0,"AppleSMBIOS"=1,"AppleMikeyI2C_CD3275"=0,"AppleIntelMCE_InterruptController"=0,"IO80211AWDLPeer"=0,"AppleVTD"=1,"DspFuncVolume_3ch"=0,"STUCWorkLoopLock"=0,"IONetworkInterface"=1,"IOPMrootDomain"=1,"AppleAHCI"=1,"IOFDiskPartitionScheme"=0,"IOEthernetController"=3,"IOAccelGPURestartReport2"=0,"IOResources"=1,"IOAccelDisplayPipe"=3,"DspFuncBeamFormer"=0,"AGPMHeuristic2"=0,"IODMAEventSource"=0,"IOUSBControllerIsochListElement"=0,"IGAccelResource"=0,"AppleHDAHardwareConfigDriverLoader"=0,"AppleHDAEngineInput"=2,"IOAccelDisplayMachine"=1,"OSOrderedSet"=223,"IOSharedInterruptController"=1,"_IOServiceJob"=0,"AGPMHeuristic"=1,"AppleMultitouchEventDriverV2Wrapper"=0,"RadeonPCIUserClient"=0,"AppleIntelPchSeriesAHCIPort"=1,"AppleHDAEngineOutputDP"=0,"IOHIDEventService"=1,"IOPlatformPluginDevice"=2,"AGPMHeuristic4"=1,"IOAccelVideoContext2"=0,"IOBluetoothL2CAPMemoryBlock"=0,"MEIEventSource"=1,"DspFuncSplitBand"=0,"IOAccelFrameDelimiter"=1,"IOThunderboltI2CCommand"=2,"IO80211PacketDescriptor"=0,"IOAccelEventMachineSingle2"=0,"DspFuncWithSharedMemory"=4,"AppleACPIPlatformUserClient"=0,"IOAccelCommandBufferPool"=0,"IOHIDSecurePromptClient"=0,"IOThunderboltDispatchCallback"=1,"AppleMEClientController"=1,"IOMachPort"=559,"IODiskImageBlockStorageDeviceOutKernel"=0,"IOHDACodecDeviceUserClient"=0,"IOBluetoothMemoryBlock"=0,"DspFuncVolume"=2,"AppleHDAFunctionGroupATI_RS730"=0,"IOThunderboltDispatchContext"=2,"AppleHDAWidget_80862805"=0,"IOAHCIPortInterface"=1,"AppleACPIPCI"=1,"DspFuncBeam2"=1,"AppleHDAPathSet"=6,"AppleMikeyDevice_CD3275"=0,"__GLNVEvoOverlayPushBuf"=0,"IOKitDiagnostics"=1,"IOWorkQueue"=4,"IOThunderboltSet"=25,"IOThunderboltConfigResetCommand"=2,"nvVidmemElementNode"=0,"IOACPIPlatformDevice"=139,"AppleFDEKeyStoreUserClient"=0,"DspFuncManager"=3,"IOFramebuffer"=1,"IORangeAllocator"=4,"AppleFDEKeyStore"=1},"IOMalloc allocation"=58232678}
  | }
  | 
  +-o /  <class IOPlatformExpertDevice, id 0x100000112, registered, matched, active, busy 0 (10969 ms), retain 40>
    | {
    |   "compatible" = <"iMac14,2">
    |   "version" = <"1.0">
    |   "board-id" = <"Mac-27ADBB7B4CEE8E61">
    |   "IOInterruptSpecifiers" = (<0900000005000000>)
    |   "platform-feature" = <0100000000000000>
    |   "serial-number" = <46384a350000000000000000004330324c3334364846384a35000000000000000000000000000000000000>
    |   "IOInterruptControllers" = ("io-apic-0")
    |   "IOPlatformUUID" = "1031E241-F1EB-5259-8978-BFC0255B451B"
    |   "clock-frequency" = <00e1f505>
    |   "IOPolledInterface" = "SMCPolledInterface is not serializable"
    |   "manufacturer" = <"Apple Inc.">
    |   "IOPlatformSystemSleepPolicy" = < >
    |   "IOPlatformSerialNumber" = "C02L346HF8J5"
    |   "system-type" = <01>
    |   "product-name" = <"iMac14,2">
    |   "model" = <"iMac14,2">
    |   "name" = <"/">
    |   "IOBusyInterest" = "IOCommand is not serializable"
    | }
    | 
    +-o chosen  <class IOService, id 0x100000101, !registered, !matched, active, busy 0, retain 6>
    | | {
    | |   "boot-file-path" = <040450005c00530079007300740065006d005c004c006900620072006100720079005c0043006f0072006500530065007200760069006300650073005c0062006f006f0074002e0065006600690000007fff0400>
    | |   "boot-args" = <00>
    | |   "machine-signature" = <00000000>
    | |   "IOScreenLockState" = <01000000>
    | |   "boot-uuid" = <"0A72ACE6-3CA9-3689-92AB-46C63CC23C2E">
    | |   "boot-kernelcache-adler32" = <5053e8c2>
    | |   "boot-file" = <"mach_kernel">
    | |   "name" = <"chosen">
    | |   "boot-device-path" = <02010c00d041030a0000000001010600021f03120a0000000000000004012a0002000000284006000000000040ce567400000000e03d0000820800008f5b0000fd01000002027fff0400>
    | | }
    | | 
    | +-o memory-map  <class IOService, id 0x100000102, !registered, !matched, active, busy 0, retain 6>
    |     {
    |       "name" = <"memory-map">
    |       "FailedCLUT" = <0030060a00030000>
    |       "FailedImage" = <0040060a30270000>
    |     }
    |     
    +-o efi  <class IOService, id 0x100000103, !registered, !matched, active, busy 0, retain 8>
    | | {
    | |   "firmware-revision" = <0a000100>
    | |   "device-properties" = < >
    | |   "firmware-abi" = <"EFI64">
    | |   "name" = <"efi">
    | |   "firmware-vendor" = <4100700070006c0065000000>
    | | }
    | | 
    | +-o kernel-compatibility  <class IOService, id 0x100000104, !registered, !matched, active, busy 0, retain 4>
    | |   {
    | |     "name" = <"kernel-compatibility">
    | |     "x86_64" = <01000000>
    | |   }
    | |   
    | +-o runtime-services  <class IOService, id 0x100000105, !registered, !matched, active, busy 0, retain 4>
    | |   {
    | |     "name" = <"runtime-services">
    | |     "table" = <90ebe88c00000000>
    | |   }
    | |   
    | +-o configuration-table  <class IOService, id 0x100000106, !registered, !matched, active, busy 0, retain 14>
    | | | {
    | | |   "name" = <"configuration-table">
    | | | }
    | | | 
    | | +-o EB9D2D31-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x100000107, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"EB9D2D31-2D88-11D3-9A16-0090273FC14D">
    | | |     "guid" = <312d9deb882dd3119a160090273fc14d>
    | | |     "table" = <0050d18c00000000>
    | | |   }
    | | |   
    | | +-o 8868E871-E4F1-11D3-BC22-0080C73C8881  <class IOService, id 0x100000108, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "alias" = <"ACPI_20">
    | | |     "name" = <"8868E871-E4F1-11D3-BC22-0080C73C8881">
    | | |     "table" = <14e0d88c00000000>
    | | |     "guid" = <71e86888f1e4d311bc220080c73c8881>
    | | |   }
    | | |   
    | | +-o EB9D2D30-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x100000109, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "alias" = <"ACPI">
    | | |     "name" = <"EB9D2D30-2D88-11D3-9A16-0090273FC14D">
    | | |     "table" = <00e0d88c00000000>
    | | |     "guid" = <302d9deb882dd3119a160090273fc14d>
    | | |   }
    | | |   
    | | +-o C5CFF4F1-379A-54E1-9EDD-93219C6AA4FE  <class IOService, id 0x10000010a, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"C5CFF4F1-379A-54E1-9EDD-93219C6AA4FE">
    | | |     "guid" = <f1f4cfc59a37e1549edd93219c6aa4fe>
    | | |     "table" = <b0caed8c00000000>
    | | |   }
    | | |   
    | | +-o F76761DC-FF89-44E4-9C0C-CD0ADA4EF983  <class IOService, id 0x10000010b, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"F76761DC-FF89-44E4-9C0C-CD0ADA4EF983">
    | | |     "guid" = <dc6167f789ffe4449c0ccd0ada4ef983>
    | | |     "table" = <a8c9e38c00000000>
    | | |   }
    | | |   
    | | +-o 026C0F80-22EC-11E2-AA02-3C07540E73B4  <class IOService, id 0x10000010c, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"026C0F80-22EC-11E2-AA02-3C07540E73B4">
    | | |     "guid" = <800f6c02ec22e211aa023c07540e73b4>
    | | |     "table" = <80c15a8c00000000>
    | | |   }
    | | |   
    | | +-o 49152E77-1ADA-4764-B7A2-7AFEFED95E8B  <class IOService, id 0x10000010d, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"49152E77-1ADA-4764-B7A2-7AFEFED95E8B">
    | | |     "guid" = <772e1549da1a6447b7a27afefed95e8b>
    | | |     "table" = <98015b8c00000000>
    | | |   }
    | | |   
    | | +-o 4C19049F-4137-4DD3-9C10-8B97A83FFDFA  <class IOService, id 0x10000010e, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"4C19049F-4137-4DD3-9C10-8B97A83FFDFA">
    | | |     "guid" = <9f04194c3741d34d9c108b97a83ffdfa>
    | | |     "table" = <e06c5a8c00000000>
    | | |   }
    | | |   
    | | +-o 7739F24C-93D7-11D4-9A3A-0090273FC14D  <class IOService, id 0x10000010f, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"7739F24C-93D7-11D4-9A3A-0090273FC14D">
    | | |     "guid" = <4cf23977d793d4119a3a0090273fc14d>
    | | |     "table" = <9001ff8c00000000>
    | | |   }
    | | |   
    | | +-o 05AD34BA-6F02-4214-952E-4DA0398E2BB9  <class IOService, id 0x100000110, !registered, !matched, active, busy 0, retain 4>
    | |     {
    | |       "name" = <"05AD34BA-6F02-4214-952E-4DA0398E2BB9">
    | |       "guid" = <ba34ad05026f1442952e4da0398e2bb9>
    | |       "table" = <78645a8c00000000>
    | |     }
    | |     
    | +-o platform  <class IOService, id 0x100000111, !registered, !matched, active, busy 0, retain 5>
    |     {
    |       "SystemSerialNumber" = <"C","0","2","L","3","4","6","H","F","8","J","5">
    |       "system-id" = <a40fde1738147e54bf68ac3a138ca5df>
    |       "StartupPowerEvents" = <0000000000000000>
    |       "FSBFrequency" = <dd5af20500000000>
    |       "Model" = <69004d0061006300310034002c0032000000>
    |       "DevicePathsSupported" = <01000000>
    |       "name" = <"platform">
    |     }
    |     
    +-o cpus  <class IOPlatformDevice, id 0x100000119, registered, matched, active, busy 0 (0 ms), retain 14>
    | | {
    | |   "name" = <"cpus">
    | | }
    | | 
    | +-o CPU0@0  <class IOACPIPlatformDevice, id 0x10000011a, registered, matched, active, busy 0 (99 ms), retain 8>
    | |   {
    | |     "processor-id" = 1
    | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     "cpu-type" = <0506>
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "device_type" = <"processor">
    | |     "clock-frequency" = <00e2a7ca>
    | |     "plugin-type" = 1
    | |     "processor-lapic" = 0
    | |     "processor-index" = 0
    | |     "bus-frequency" = <00e1f505>
    | |     "name" = <"CPU0">
    | |     "processor-number" = 0
    | |   }
    | |   
    | +-o CPU1@2  <class IOACPIPlatformDevice, id 0x10000011b, registered, matched, active, busy 0 (4 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 2
    | |     "clock-frequency" = <00e2a7ca>
    | |     "processor-number" = 1
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 2
    | |     "bus-frequency" = <00e1f505>
    | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     "cpu-type" = <0506>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 1
    | |     "name" = <"CPU1">
    | |   }
    | |   
    | +-o CPU2@4  <class IOACPIPlatformDevice, id 0x10000011c, registered, matched, active, busy 0 (4 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 4
    | |     "clock-frequency" = <00e2a7ca>
    | |     "processor-number" = 2
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 3
    | |     "bus-frequency" = <00e1f505>
    | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     "cpu-type" = <0506>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 2
    | |     "name" = <"CPU2">
    | |   }
    | |   
    | +-o CPU3@6  <class IOACPIPlatformDevice, id 0x10000011d, registered, matched, active, busy 0 (5 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 6
    | |     "clock-frequency" = <00e2a7ca>
    | |     "processor-number" = 3
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 4
    | |     "bus-frequency" = <00e1f505>
    | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     "cpu-type" = <0506>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 3
    | |     "name" = <"CPU3">
    | |   }
    | |   
    | +-o CPU4  <class IOACPIPlatformDevice, id 0x10000011e, registered, matched, active, busy 0 (5 ms), retain 7>
    | |   {
    | |     "processor-index" = 4
    | |     "processor-id" = 5
    | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     "name" = <"CPU4">
    | |     "cpu-type" = <0506>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o CPU5  <class IOACPIPlatformDevice, id 0x10000011f, registered, matched, active, busy 0 (5 ms), retain 7>
    | |   {
    | |     "processor-index" = 5
    | |     "processor-id" = 6
    | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     "name" = <"CPU5">
    | |     "cpu-type" = <0506>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o CPU6  <class IOACPIPlatformDevice, id 0x100000120, registered, matched, active, busy 0 (5 ms), retain 7>
    | |   {
    | |     "processor-index" = 6
    | |     "processor-id" = 7
    | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     "name" = <"CPU6">
    | |     "cpu-type" = <0506>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o CPU7  <class IOACPIPlatformDevice, id 0x100000121, registered, matched, active, busy 0 (5 ms), retain 7>
    |     {
    |       "processor-index" = 7
    |       "processor-id" = 8
    |       "IOGeneralInterest" = "IOCommand is not serializable"
    |       "name" = <"CPU7">
    |       "cpu-type" = <0506>
    |       "device_type" = <"processor">
    |     }
    |     
    +-o memory  <class IOService, id 0x100000137, !registered, !matched, active, busy 0, retain 4>
    |   {
    |     "dimm-part-number" = <3078343534323441333433303535343733383435343635353335324434373445344332443436003078343534323441333433303535343733383435343635353335324434373445344332443436000000>
    |     "dimm-types" = <"DDR3","DDR3","RAM","RAM">
    |     "slot-names" = <"   ","BANK 0/DIMM0","BANK 1/DIMM0","BANK 0/DIMM1","BANK 1/DIMM1">
    |     "dimm-speeds" = <"1600 MHz","1600 MHz","0 MHz","0 MHz">
    |     "dimm-manufacturer" = <30783032464500307830324645000000>
    |     "ecc-enabled" = No
    |     "reg" = <0100000000000000010000000000000000000000000000000000000000000000>
    |     "dimm-info" = < >
    |     "dimm-serial-number" = <307834373231303843300030784443454330364643000000>
    |   }
    |   
    +-o rom@0  <class IOService, id 0x100000138, !registered, !matched, active, busy 0, retain 4>
    |   {
    |     "vendor" = <"Apple Inc.">
    |     "fv-main-size" = 1703936
    |     "release-date" = <"06/27/2013">
    |     "rom-size" = 8388608
    |     "fv-main-address" = 18446744073702801408
    |     "apple-rom-info" = <4170706c6520524f4d2056657273696f6e0a202042494f532049443a202020202020494d3134320a20204275696c742062793a2020202020726f6f74407361756d6f6e0a2020446174653a202020202020202020546875204a756e2032372031313a32333a31392050445420323031330a20205265766973696f6e3a202020202073766e2033313538382028422649290a20204275696c64636176652049443a203839360a2020524f4d2056657273696f6e3a2020303130385f42303000>
    |     "version" = <"IM142.88Z.0108.B00.1306271125">
    |   }
    |   
    +-o PCI0@0  <class IOACPIPlatformDevice, id 0x10000013a, registered, matched, active, busy 0 (2258 ms), retain 39>
    | | {
    | |   "compatible" = <"PNP0A03">
    | |   "IODTPersist" = <>
    | |   "_STA" = 18446744073709551615
    | |   "IOPCIConfigured" = Yes
    | |   "acpi-address-spaces" = < >
    | |   "IODeviceMemory" = (({"address"=3320,"length"=8}))
    | |   "#size-cells" = <02000000>
    | |   "_UID" = "0"
    | |   "acpi-pci-routing-table" = < >
    | |   "_ADR" = 0
    | |   "device-properties" = {"acpi-device"="IOACPIPlatformDevice is not serializable","acpi-path"="IOACPIPlane:/_SB/PCI0@0"}
    | |   "#address-cells" = <03000000>
    | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0"
    | |   "name" = <"PNP0A08">
    | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | }
    | | 
    | +-o PDRC  <class IOACPIPlatformDevice, id 0x1000001a1, registered, matched, active, busy 0 (0 ms), retain 7>
    | |   {
    | |     "_STA" = 18446744073709551615
    | |     "_UID" = "1"
    | |     "IODeviceMemory" = (({"address"=4275159040,"length"=16384}),({"address"=4275109888,"length"=32768}),({"address"=4275142656,"length"=4096}),({"address"=4275146752,"length"=4096}),({"address"=3758096384,"length"=268435456}),({"address"=4275175424,"length"=131072}),({"address"=4275634176,"length"=16384}),({"address"=4275326976,"length"=307200}),({"address"=4278190080,"length"=16777216}),({"address"=4276092928,"length"=1048576}))
    | |     "name" = <"PNP0C02">
    | |   }
    | |   
    | +-o MCHC@0  <class IOPCIDevice, id 0x1000001ba, registered, matched, active, busy 0 (0 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,c00">
    | |     "compatible" = <"pci106b,123","pci8086,c00","pciclass,060000","MCHC">
    | |     "subsystem-vendor-id" = <6b100000>
    | |     "IOName" = "pci8086,c00"
    | |     "reg" = <0000000000000000000000000000000000000000>
    | |     "device-id" = <000c0000>
    | |     "IOPowerManagement" = {"MaxPowerState"=3,"ChildProxyPowerState"=2,"CurrentPowerState"=2}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <06000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:0:0"
    | |     "class-code" = <00000600>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/MCHC@0"
    | |     "subsystem-id" = <23010000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o P0P2@1  <class IOPCIDevice, id 0x1000001bb, registered, matched, active, busy 0 (270 ms), retain 13>
    | | | {
    | | |   "IOPCIPMCSState" = 0
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 64
    | | |   "subsystem-vendor-id" = <7f000000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "pci-aspm-default" = 3
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "built-in" = <00>
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <010c0000>
    | | |   "acpi-pmcap-offset" = 128
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci7f,0","pci8086,c01","pciclass,060400","P0P2">
    | | |   "ranges" = <0000008200000000000000b00000008200000000000000b00000000000001001000000c27f00000000000080000000c27f0000000000008000000000000000120000008100000000001000000000008100000000001000000000000000100000>
    | | |   "IOPCIExpressLinkCapabilities" = 39955715
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P2@10000"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <06000000>
    | | |   "IOPCIExpressLinkStatus" = 55553
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:1:0(1:1)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <0008000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 796032
    | | | }
    | | | 
    | | +-o GFX0@0  <class IOPCIDevice, id 0x1000001bc, registered, matched, active, busy 0 (240 ms), retain 25>
    | | | | {
    | | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | | |   "built-in" = <00>
    | | | |   "saved-config" = <0f084c032001000060001006b0050003027f000aa005a00a30005000c905030008000800565e000000000000010000000000000000040000010a0a0400000003000000000000000aa005000aa0050000007e7e00010000000000000f00800000000000000000000000000000000000000000000000000000010000000000000000000000000000000000000000000000ff000000000000000000000000000000020000000000000f00800000000000000000000000000000000000000000000000000000010000000000000000000000000000000000000000000000ff000000000000000000000000000000>
    | | | |   "NVDA,Features" = <ff162001>
    | | | |   "NVDAType" = "Official"
    | | | |   "rom-revision" = <"3745">
    | | | |   "IODeviceMemory" = (({"address"=2952790016,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=2969567232,"length"=524288}))
    | | | |   "NVArch" = "GK100"
    | | | |   "VRAM,totalMB" = <00080000>
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P2@10000/GFX0@0"
    | | | |   "pci-aspm-default" = 3
    | | | |   "reg" = <0000010000000000000000000000000000000000100001020000000000000000000000000000000114000142000000000000000000000000000000101c0001420000000000000000000000000000000224000101000000000000000000000000800000003000010200000000000000000000000000000800>
    | | | |   "NVCLASS" = "NVDA"
    | | | |   "hda-gfx" = <"onboard-1">
    | | | |   "IOName" = "display"
    | | | |   "graphic-options" = <0c000000>
    | | | |   "NVDA,invalid-config" = <00000000>
    | | | |   "IOPCIExpressLinkCapabilities" = 4537603
    | | | |   "IOChildIndex" = 1
    | | | |   "VRAM,memvendorID" = <0300>
    | | | |   "attached-gpu-control-path" = "IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/P0P2@1/IOPP/GFX0@0/NVDA,Display-A@0/NVDA/AGPM"
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "AAPL,iokit-ndrv" = <f0ec00887fffffff>
    | | | |   "vbios-revision" = <0100c40480>
    | | | |   "rm_board_number" = <00000000>
    | | | |   "class-code" = <00000300>
    | | | |   "IOPCIResourced" = Yes
    | | | |   "name" = <"display">
    | | | |   "NVCAP" = <0500000000000100060000000000000f00000000>
    | | | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0900000000000100>)
    | | | |   "IOPCIPMCSState" = 0
    | | | |   "compatible" = <"pci106b,120","pci10de,119d","pciclass,030000","GFX0">
    | | | |   "revision-id" = <a2000000>
    | | | |   "IOPCIMSIMode" = Yes
    | | | |   "subsystem-vendor-id" = <6b100000>
    | | | |   "VRAM,totalsize" = <0000008000000000>
    | | | |   "assigned-addresses" = <1000018200000000000000b00000000000000001140001c27f0000000000008000000000000000101c0001c27f00000000000090000000000000000224000181000000000010000000000000800000003000018200000000000000b10000000000000800>
    | | | |   "device-id" = <9d110000>
    | | | |   "AAPL,ndrv-dev" = Yes
    | | | |   "boot-gamma-restored" = <0000000000000000>
    | | | |   "IOPCIExpressLinkStatus" = 4353
    | | | |   "pcidebug" = "1:0:0"
    | | | |   "IOPCIExpressCapabilities" = 2
    | | | |   "NVKernelLoaded" = <01000000>
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | | |   "IONVRAMProperty" = Yes
    | | | |   "IOHibernateState" = <00000000>
    | | | |   "subsystem-id" = <10000000>
    | | | |   "device_type" = <"NVDA,Parent">
    | | | |   "vendor-id" = <de100000>
    | | | |   "model" = <"NVIDIA GeForce GTX 775M">
    | | | |   "IOPMIsPowerManaged" = Yes
    | | | |   "NVDAinitgl_created" = "yes"
    | | | |   "com-master-varp" = <00a0d4da80ffffff>
    | | | | }
    | | | | 
    | | | +-o LCD@80002400  <class IORegistryEntry, id 0x1000001bd, retain 4>
    | | | |   {
    | | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P2@10000/GFX0@0/LCD@80002400"
    | | | |   }
    | | | |   
    | | | +-o IOService@3  <class IOService, id 0x100000325, !registered, !matched, active, busy 0, retain 4>
    | | | |   {
    | | | |     "NVDA,UnderscanMin" = <52000000>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-A@0  <class IONDRVDevice, id 0x100000322, registered, matched, active, busy 0 (40 ms), retain 8>
    | | | |   {
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "use-backlight-blanking" = <>
    | | | |     "IODeviceMemory" = (({"address"=2952790016,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=2969567232,"length"=524288}))
    | | | |     "audio-codec-info" = <00010600>
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "built-in" = <>
    | | | |     "connector-type" = <00040000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "edid" = < >
    | | | |     "name" = <"NVDA,Display-A">
    | | | |     "IOFBDependentID" = 18446743524408053760
    | | | |     "display-cfg" = <03040800>
    | | | |     "NVMT" = <0e037f2000000000000aa005a00a300a500a0000c905a305a805000060ff640e00000001af00000000000000000000000000000000000000000000000000000000000000ffff0000000000000000000001000000000000ff00000000bc02014a0a04000000030000000aa005000aa005>
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "fboffset" = <00000200>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "NVDA,UnderscanMin" = <52000000>
    | | | |     "EDID" = < >
    | | | |     "AAPL,iokit-ndrv" = <f0ec00887fffffff>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "av-signal-type" = <10000000>
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "IOFBDependentIndex" = 0
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "port-number" = <00000000>
    | | | |     "AAPL,RegEntryID" = <0032db1b80ffffffffcd24e47f000000656d6953000000007a6c755200000000>
    | | | |     "device_type" = <"display">
    | | | |     "dp-device-id" = <41000000>
    | | | |     "AAPL,boot-display" = <>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-B@1  <class IONDRVDevice, id 0x100000323, registered, matched, active, busy 0 (1 ms), retain 8>
    | | | |   {
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "IODeviceMemory" = (({"address"=2952790016,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=2969567232,"length"=524288}))
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "connector-type" = <00040000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "IOFBDependentID" = 18446743524408053760
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "name" = <"NVDA,Display-B">
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "NVDA,UnderscanMin" = <52000000>
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "AAPL,iokit-ndrv" = <f0ec00887fffffff>
    | | | |     "IOFBDependentIndex" = 1
    | | | |     "can-hot-plug" = <>
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "port-number" = <01000000>
    | | | |     "AAPL,RegEntryID" = <002cef1b80ffffffffd310e47f000000656d6953000000007a6c755200000000>
    | | | |     "device_type" = <"display">
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-C@2  <class IONDRVDevice, id 0x100000324, registered, matched, active, busy 0 (9 ms), retain 8>
    | | |     {
    | | |       "nativeNDRV" = <"advn">
    | | |       "IODeviceMemory" = (({"address"=2952790016,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=2969567232,"length"=524288}))
    | | |       "AAPL,gray-page" = <01000000>
    | | |       "connector-type" = <00040000>
    | | |       "noNVRAM" = <01000000>
    | | |       "IOFBDependentID" = 18446743524408053760
    | | |       "NVDA,SubDeviceClass" = <80200000>
    | | |       "display-cfg" = <ffffffff>
    | | |       "name" = <"NVDA,Display-C">
    | | |       "AAPL,ndrv-dev" = Yes
    | | |       "compatible" = <"NVDA,NVMac">
    | | |       "NVDA,UnderscanMin" = <52000000>
    | | |       "display-connect-flags" = <00000000>
    | | |       "AAPL,iokit-ndrv" = <f0ec00887fffffff>
    | | |       "IOFBDependentIndex" = 2
    | | |       "NVDA,DeviceClass" = <80000000>
    | | |       "AAPL,gray-value" = <00000000>
    | | |       "port-number" = <02000000>
    | | |       "AAPL,RegEntryID" = <00dada1b80ffffffff2525e47f000000656d6953000000007a6c755200000000>
    | | |       "device_type" = <"display">
    | | |     }
    | | |     
    | | +-o HDAU@0,1  <class IOPCIDevice, id 0x1000001be, registered, matched, active, busy 0 (32 ms), retain 11>
    | |     {
    | |       "assigned-addresses" = <1001018200000000000008b10000000000400000>
    | |       "IOInterruptSpecifiers" = (<1100000007000000>,<0a00000000000100>)
    | |       "class-code" = <00030400>
    | |       "IODeviceMemory" = (({"address"=2970091520,"length"=16384}))
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "built-in" = <00>
    | |       "PinConfigurations" = <e0005628>
    | |       "pci-aspm-default" = 3
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "hda-gfx" = <"onboard-1">
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "IOPCIMSIMode" = Yes
    | |       "vendor-id" = <de100000>
    | |       "IOChildIndex" = 2
    | |       "device-id" = <0a0e0000>
    | |       "name" = <"pci10de,e0a">
    | |       "IOPCIResourced" = Yes
    | |       "layout-id" = <07000000>
    | |       "compatible" = <"pci10de,e0a","pciclass,040300","HDAU">
    | |       "IOPCIExpressLinkCapabilities" = 4537603
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P2@10000/HDAU@1"
    | |       "DigitalAudioCapabilities" = {"DisplayPort"=1,"HDMI"=1}
    | |       "revision-id" = <a1000000>
    | |       "IOPCIExpressLinkStatus" = 4353
    | |       "IOPCIExpressCapabilities" = 2
    | |       "pcidebug" = "1:0:1"
    | |       "IOName" = "pci10de,e0a"
    | |       "IOPCIPMCSState" = 0
    | |       "reg" = <00010100000000000000000000000000000000001001010200000000000000000000000000400000>
    | |     }
    | |     
    | +-o IGPU@2  <class IOPCIDevice, id 0x1000001bf, registered, matched, active, busy 0 (254 ms), retain 21>
    | | | {
    | | |   "assigned-addresses" = <1010008200000000000040b10000000000004000181000c27f0000000000009800000000000000082010008100000000002000000000000040000000>
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0500000000000100>)
    | | |   "class-code" = <00000300>
    | | |   "IODeviceMemory" = (({"address"=2973761536,"length"=4194304}),({"address"=548010983424,"length"=134217728}),"IOSubMemoryDescriptor is not serializable")
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <6b100000>
    | | |   "built-in" = <00>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOPCIMSIMode" = Yes
    | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | |   "name" = <"display">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <12040000>
    | | |   "IOPCIResourced" = Yes
    | | |   "compatible" = <"pci106b,123","pci8086,412","pciclass,030000","IGPU">
    | | |   "AAPL,iokit-ndrv" = <f0ec00887fffffff>
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000"
    | | |   "model" = <"Intel Iris Pro">
    | | |   "subsystem-id" = <23010000>
    | | |   "revision-id" = <06000000>
    | | |   "IOPCIPMCSState" = 0
    | | |   "AAPL,ig-platform-id" = <04001204>
    | | |   "pcidebug" = "0:2:0"
    | | |   "IOName" = "display"
    | | |   "reg" = <0010000000000000000000000000000000000000101000020000000000000000000000000000400018100042000000000000000000000000000000082010000100000000000000000000000040000000>
    | | |   "IOMemoryDescriptorOptions" = 2048
    | | | }
    | | | 
    | | +-o DD01@100  <class IORegistryEntry, id 0x1000001c0, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD01@100"
    | | |   }
    | | |   
    | | +-o DD02@400  <class IORegistryEntry, id 0x1000001c1, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD02@400"
    | | |   }
    | | |   
    | | +-o DD03@200  <class IORegistryEntry, id 0x1000001c2, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD03@200"
    | | |   }
    | | |   
    | | +-o DD04@4  <class IORegistryEntry, id 0x1000001c3, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD04@4"
    | | |   }
    | | |   
    | | +-o DD05@5  <class IORegistryEntry, id 0x1000001c4, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD05@5"
    | | |   }
    | | |   
    | | +-o DD06@6  <class IORegistryEntry, id 0x1000001c5, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD06@6"
    | | |   }
    | | |   
    | | +-o DD07@7  <class IORegistryEntry, id 0x1000001c6, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD07@7"
    | | |   }
    | | |   
    | | +-o DD08@8  <class IORegistryEntry, id 0x1000001c7, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD08@8"
    | | |   }
    | | |   
    | | +-o DD1F@1f  <class IORegistryEntry, id 0x1000001c8, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IGPU@20000/DD1F@1f"
    | |     }
    | |     
    | +-o XHC1@14  <class IOPCIDevice, id 0x100000214, registered, matched, active, busy 0 (678 ms), retain 22>
    | | | {
    | | |   "assigned-addresses" = <10a00082000000000000c0b10000000000000100>
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0200000000000100>)
    | | |   "AAPL,current-extra-in-sleep" = 2700
    | | |   "class-code" = <30030c00>
    | | |   "IODeviceMemory" = (({"address"=2982150144,"length"=65536}))
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <86800000>
    | | |   "built-in" = <00>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "AAPL,current-extra" = 2700
    | | |   "IOPCIMSIMode" = Yes
    | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | |   "USBBusNumber" = 10
    | | |   "name" = <"pci8086,8c31">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <318c0000>
    | | |   "acpi-pmcap-offset" = 112
    | | |   "IOPCIResourced" = Yes
    | | |   "AAPL,current-available" = 2100
    | | |   "compatible" = <"pci8086,7270","pci8086,8c31","pciclass,0c0330","XHC1">
    | | |   "AAPL,max-port-current-in-sleep" = 2100
    | | |   "locationID" = 335544320
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC1@140000"
    | | |   "subsystem-id" = <70720000>
    | | |   "revision-id" = <05000000>
    | | |   "pcidebug" = "0:20:0"
    | | |   "IOName" = "pci8086,8c31"
    | | |   "reg" = <00a000000000000000000000000000000000000010a0000200000000000000000000000000000100>
    | | | }
    | | | 
    | | +-o @2:0  <class IOMedia, id 0x1000002f2, registered, matched, active, busy 0 (55 ms), retain 11>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "GUID_partition_scheme"
    | | |     "Whole" = Yes
    | | |     "Leaf" = No
    | | |     "BSD Name" = "disk1"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 4
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "BSD Major" = 1
    | | |     "Size" = 500074283008
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = ""
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:1  <class IOMedia, id 0x1000002f8, registered, matched, active, busy 0 (0 ms), retain 9>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s1"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 5
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "14D3F574-A44E-4DD1-8B5C-5435D901F1D4"
    | | |     "Partition ID" = 1
    | | |     "BSD Major" = 1
    | | |     "Size" = 209715200
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = No
    | | |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:2  <class IOMedia, id 0x1000002f9, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s2"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 10
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "277BCBE8-8F60-48D8-82C8-72F452E937BA"
    | | |     "Partition ID" = 2
    | | |     "BSD Major" = 1
    | | |     "Size" = 10000003072
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:3  <class IOMedia, id 0x1000002fa, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s3"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 9
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "981AAB51-D316-4EA3-B8F2-0EA2E0FF9808"
    | | |     "Partition ID" = 3
    | | |     "BSD Major" = 1
    | | |     "Size" = 10000003072
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:4  <class IOMedia, id 0x1000002fb, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s4"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 12
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "FB7D9490-4D02-4E7E-9265-5B3A9D23922C"
    | | |     "Partition ID" = 4
    | | |     "BSD Major" = 1
    | | |     "Size" = 10000003072
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:5  <class IOMedia, id 0x1000002fc, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s5"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 13
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "87D392EA-85A0-4B85-9279-B1CC2A722229"
    | | |     "Partition ID" = 5
    | | |     "BSD Major" = 1
    | | |     "Size" = 10000003072
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:6  <class IOMedia, id 0x1000002fd, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s6"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 6
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "7E63A465-596B-4928-922A-3902AAB6A775"
    | | |     "Partition ID" = 6
    | | |     "BSD Major" = 1
    | | |     "Size" = 10000003072
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:7  <class IOMedia, id 0x1000002fe, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s7"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 11
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "9A3E6CCB-4702-4558-A1C1-4C62177DB15D"
    | | |     "Partition ID" = 7
    | | |     "BSD Major" = 1
    | | |     "Size" = 27786694656
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:8  <class IOMedia, id 0x1000002ff, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s8"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 14
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "56AC1AFD-5D8A-4591-A969-4B47EDF1CDD1"
    | | |     "Partition ID" = 8
    | | |     "BSD Major" = 1
    | | |     "Size" = 149999996928
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:9  <class IOMedia, id 0x100000300, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "Removable" = No
    | | |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "Whole" = No
    | | |     "Leaf" = Yes
    | | |     "BSD Name" = "disk1s9"
    | | |     "Ejectable" = No
    | | |     "Preferred Block Size" = 512
    | | |     "BSD Minor" = 7
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "UUID" = "E7A5A3D0-BE08-4412-9906-9F227F07D61D"
    | | |     "Partition ID" = 9
    | | |     "BSD Major" = 1
    | | |     "Size" = 135502036992
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |     "BSD Unit" = 1
    | | |   }
    | | |   
    | | +-o @2:10  <class IOMedia, id 0x100000301, registered, matched, active, busy 0 (0 ms), retain 10>
    | |     {
    | |       "Removable" = No
    | |       "Content" = "EBD0A0A2-B9E5-4433-87C0-68B6B72699C7"
    | |       "Whole" = No
    | |       "Leaf" = Yes
    | |       "BSD Name" = "disk1s10"
    | |       "Ejectable" = No
    | |       "Preferred Block Size" = 512
    | |       "BSD Minor" = 8
    | |       "IOGeneralInterest" = "IOCommand is not serializable"
    | |       "Writable" = Yes
    | |       "UUID" = "4E86257E-01DF-4B8A-B212-9ADF6670A3ED"
    | |       "Partition ID" = 10
    | |       "BSD Major" = 1
    | |       "Size" = 135500136448
    | |       "IOBusyInterest" = "IOCommand is not serializable"
    | |       "Open" = Yes
    | |       "Content Hint" = "EBD0A0A2-B9E5-4433-87C0-68B6B72699C7"
    | |       "BSD Unit" = 1
    | |     }
    | |     
    | +-o pci8086,8c3a@16  <class IOPCIDevice, id 0x10000022c, registered, matched, active, busy 0 (9 ms), retain 10>
    | |   {
    | |     "assigned-addresses" = <10b00082000000000059c1b10000000010000000>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>,<0300000000000100>)
    | |     "IODeviceMemory" = (({"address"=2982238464,"length"=16}))
    | |     "class-code" = <00800700>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOPCIMSIMode" = Yes
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "vendor-id" = <86800000>
    | |     "name" = <"pci8086,8c3a">
    | |     "acpi-pmcap-offset" = 80
    | |     "device-id" = <3a8c0000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,7270","pci8086,8c3a","pciclass,078000">
    | |     "subsystem-id" = <70720000>
    | |     "revision-id" = <05000000>
    | |     "IOPCIPMCSState" = 0
    | |     "pcidebug" = "0:22:0"
    | |     "IOName" = "pci8086,8c3a"
    | |     "reg" = <00b000000000000000000000000000000000000010b0000200000000000000000000000010000000>
    | |   }
    | |   
    | +-o HDEF@1B  <class IOPCIDevice, id 0x1000001d1, registered, matched, active, busy 0 (507 ms), retain 11>
    | |   {
    | |     "assigned-addresses" = <10d80082000000000000c1b10000000000400000>
    | |     "MaximumBootBeepVolumeAlt" = <4d>
    | |     "IOInterruptSpecifiers" = (<1600000007000000>,<0400000000000100>)
    | |     "class-code" = <00030400>
    | |     "IODeviceMemory" = (({"address"=2982215680,"length"=16384}))
    | |     "PinConfigurations" = <20402b00120110900001a69030e04b006090ab0110011090>
    | |     "subsystem-vendor-id" = <86800000>
    | |     "multiEQDevicePresence" = <00000100>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "MaximumBootBeepVolume" = <4d>
    | |     "pci-aspm-default" = 0
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,8c20">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <208c0000>
    | |     "acpi-pmcap-offset" = 80
    | |     "layout-id" = <07000000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,7270","pci8086,8c20","pciclass,040300","HDEF">
    | |     "IOPCIMSIMode" = Yes
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/HDEF@1b0000"
    | |     "subsystem-id" = <70720000>
    | |     "revision-id" = <05000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 145
    | |     "pcidebug" = "0:27:0"
    | |     "IOName" = "pci8086,8c20"
    | |     "IOPCIPMCSState" = 0
    | |     "reg" = <00d800000000000000000000000000000000000010d8000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o RP01@1C  <class IOPCIDevice, id 0x1000001d2, registered, matched, active, busy 0 (3 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "IOPCIPMCSState" = 0
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 0
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 3
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <108c0000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,8c10","pciclass,060400","RP01">
    | | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 20007970
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000"
    | | |   "revision-id" = <d5000000>
    | | |   "IOPCIExpressLinkStatus" = 4097
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:0(2:2)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e0000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 262240
    | | | }
    | | | 
    | | +-o SSD0@0  <class IORegistryEntry, id 0x1000001d3, retain 5>
    | |   | {
    | |   |   "use-msi" = 0
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/SSD0@0"
    | |   | }
    | |   | 
    | |   +-o PRT0@ffff  <class IORegistryEntry, id 0x1000001d4, retain 4>
    | |       {
    | |         "io-device-location" = <"SSD">
    | |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/SSD0@0/PRT0@ffff"
    | |       }
    | |       
    | +-o RP03@1C,2  <class IOPCIDevice, id 0x1000001d5, registered, matched, active, busy 0 (341 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1200000007000000>)
    | | |   "IOPCIPMCSState" = 0
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 64
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 3
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <148c0000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,8c14","pciclass,060400","RP03">
    | | |   "ranges" = <0000008200000000000080b10000008200000000000080b10000000000003000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 53623826
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP03@1c0002"
    | | |   "revision-id" = <d5000000>
    | | |   "IOPCIExpressLinkStatus" = 28689
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:2(3:3)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e2000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 1356288
    | | | }
    | | | 
    | | +-o ARPT@0  <class IOPCIDevice, id 0x1000001d6, registered, matched, active, busy 0 (333 ms), retain 12>
    | |     {
    | |       "assigned-addresses" = <10000382000000000000a0b100000000008000001800038200000000000080b10000000000002000>
    | |       "IOInterruptSpecifiers" = (<1200000007000000>,<0b00000000000100>)
    | |       "class-code" = <00800200>
    | |       "IODeviceMemory" = (({"address"=2980052992,"length"=32768}),({"address"=2977955840,"length"=2097152}))
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-vendor-id" = <6b100000>
    | |       "built-in" = <00>
    | |       "pci-aspm-default" = 3
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "IOPCIMSIMode" = Yes
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "name" = <"pci14e4,43a0">
    | |       "IOChildIndex" = 1
    | |       "device-id" = <a0430000>
    | |       "vendor-id" = <e4140000>
    | |       "acpi-pmcap-offset" = 72
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci106b,111","pci14e4,43a0","pciclass,028000","ARPT">
    | |       "IOPCIExpressLinkCapabilities" = 4643857
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP03@1c0002/ARPT@0"
    | |       "subsystem-id" = <11010000>
    | |       "revision-id" = <03000000>
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "IOPCIExpressCapabilities" = 2
    | |       "pcidebug" = "3:0:0"
    | |       "IOName" = "pci14e4,43a0"
    | |       "acpi-wake-type" = 2
    | |       "reg" = <000003000000000000000000000000000000000010000302000000000000000000000000008000001800030200000000000000000000000000002000>
    | |       "IOPCIPMCSState" = 0
    | |     }
    | |     
    | +-o RP04@1C,3  <class IOPCIDevice, id 0x1000001d7, registered, matched, active, busy 0 (494 ms), retain 13>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1300000007000000>)
    | | |   "IOPCIPMCSState" = 0
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 64
    | | |   "subsystem-vendor-id" = <7f000000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "pci-aspm-default" = 2
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "built-in" = <00>
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <168c0000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci7f,0","pci8086,8c16","pciclass,060400","RP04">
    | | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c27f00000000000092000000c27f0000000000009200000000000010000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 70401042
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP04@1c0003"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <d5000000>
    | | |   "IOPCIExpressLinkStatus" = 28689
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:3(4:4)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e3000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 1880576
    | | | }
    | | | 
    | | +-o GIGE@0  <class IOPCIDevice, id 0x1000001d8, registered, matched, active, busy 0 (486 ms), retain 11>
    | | |   {
    | | |     "assigned-addresses" = <100004c27f000000000000920000000000000100180004c27f000000000001920000000000000100>
    | | |     "IOInterruptSpecifiers" = (<1300000007000000>,<0700000000000100>)
    | | |     "class-code" = <00000200>
    | | |     "IODeviceMemory" = (({"address"=547910320128,"length"=65536}),({"address"=547910385664,"length"=65536}))
    | | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |     "subsystem-vendor-id" = <e4140000>
    | | |     "built-in" = <00>
    | | |     "pci-aspm-default" = 2
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "IOPCIMSIMode" = Yes
    | | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | |     "name" = <"ethernet">
    | | |     "IOChildIndex" = 1
    | | |     "device-id" = <86160000>
    | | |     "vendor-id" = <e4140000>
    | | |     "acpi-pmcap-offset" = 72
    | | |     "IOPCIResourced" = Yes
    | | |     "compatible" = <"pci14e4,1686","pciclass,020000","GIGE">
    | | |     "IOPCIPauseCompatible" = Yes
    | | |     "IOPCIExpressLinkCapabilities" = 4676625
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP04@1c0003/GIGE@0"
    | | |     "IOPMPCIConfigSpaceVolatile" = No
    | | |     "model" = "Broadcom 57766-A1"
    | | |     "subsystem-id" = <86160000>
    | | |     "revision-id" = <01000000>
    | | |     "IOPCIExpressLinkStatus" = 4113
    | | |     "IOPCIExpressCapabilities" = 2
    | | |     "pcidebug" = "4:0:0"
    | | |     "IOName" = "ethernet"
    | | |     "acpi-wake-type" = 2
    | | |     "reg" = <000004000000000000000000000000000000000010000442000000000000000000000000000001001800044200000000000000000000000000000100>
    | | |     "IOPCIPMCSState" = 0
    | | |   }
    | | |   
    | | +-o SDXC@0,1  <class IOPCIDevice, id 0x1000001d9, registered, matched, active, busy 0 (4 ms), retain 12>
    | |     {
    | |       "assigned-addresses" = <100104c27f000000000002920000000000000100>
    | |       "IOInterruptSpecifiers" = (<1000000007000000>,<0800000000000100>)
    | |       "class-code" = <01050800>
    | |       "IODeviceMemory" = (({"address"=547910451200,"length"=65536}))
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-vendor-id" = <e4140000>
    | |       "built-in" = <00>
    | |       "pci-aspm-default" = 2
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "IOPCIMSIMode" = Yes
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "name" = <"pci14e4,16bc">
    | |       "IOChildIndex" = 2
    | |       "device-id" = <bc160000>
    | |       "vendor-id" = <e4140000>
    | |       "acpi-pmcap-offset" = 72
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci14e4,0","pci14e4,16bc","pciclass,080501","SDXC">
    | |       "IOPCIExpressLinkCapabilities" = 4676625
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP04@1c0003/SDXC@1"
    | |       "IOPMPCIConfigSpaceVolatile" = No
    | |       "subsystem-id" = <00000000>
    | |       "revision-id" = <01000000>
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "IOPCIExpressCapabilities" = 2
    | |       "pcidebug" = "4:0:1"
    | |       "IOName" = "pci14e4,16bc"
    | |       "IOPCIPMCSState" = 8459
    | |       "reg" = <00010400000000000000000000000000000000001001044200000000000000000000000000000100>
    | |     }
    | |     
    | +-o RP05@1C,4  <class IOPCIDevice, id 0x1000001da, registered, matched, active, busy 0 (1109 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "IOPCIPMCSState" = 0
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 64
    | | |   "subsystem-vendor-id" = <7f000000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"DevicePowerState"=0,"CurrentPowerState"=0,"PowerOverrideOn"=Yes,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "built-in" = <00>
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <188c0000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci7f,0","pci8086,8c18","pciclass,060400","RP05">
    | | |   "ranges" = <00000082000000000000d0b100000082000000000000d0b1000000000000302e000000c27f000000000000a0000000c27f000000000000a000000000000000600000008100000000003000000000008100000000003000000000000000b00000>
    | | |   "IOPCIExpressLinkCapabilities" = 87182402
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <d5000000>
    | | |   "IOPCIExpressLinkStatus" = 28738
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:4(5:255)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e4000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 2424064
    | | | }
    | | | 
    | | +-o UPSB@0  <class IOPCIDevice, id 0x1000001db, registered, matched, active, busy 0 (1098 ms), retain 16>
    | |   | {
    | |   |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   |   "PCI-Thunderbolt" = 1
    | |   |   "#address-cells" = <03000000>
    | |   |   "class-code" = <00040600>
    | |   |   "IOPowerManagement" = {"ChildrenPowerState"=2,"DesiredPowerState"=2,"CurrentPowerState"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |   "subsystem-vendor-id" = <7f000000>
    | |   |   "built-in" = <00>
    | |   |   "pci-aspm-default" = 0
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "IOInterruptControllers" = ("io-apic-0")
    | |   |   "name" = <"pci-bridge">
    | |   |   "vendor-id" = <86800000>
    | |   |   "device-id" = <47150000>
    | |   |   "IOChildIndex" = 1
    | |   |   "acpi-pmcap-offset" = 128
    | |   |   "IOPCIResourced" = Yes
    | |   |   "compatible" = <"pci7f,0","pci8086,1547","pciclass,060400","UPSB">
    | |   |   "ranges" = <00000082000000000000d0b100000082000000000000d0b1000000000000302e000000c27f000000000000a0000000c27f000000000000a000000000000000600000008100000000003000000000008100000000003000000000000000b00000>
    | |   |   "IOPCIExpressLinkCapabilities" = 523330
    | |   |   "IODTPersist" = <>
    | |   |   "IOPCIConfigured" = Yes
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0"
    | |   |   "subsystem-id" = <00000000>
    | |   |   "revision-id" = <03000000>
    | |   |   "IOPCIExpressLinkStatus" = 4162
    | |   |   "IOPCIExpressCapabilities" = 82
    | |   |   "pcidebug" = "5:0:0(6:255)"
    | |   |   "IOName" = "pci-bridge"
    | |   |   "#size-cells" = <02000000>
    | |   |   "reg" = <0000050000000000000000000000000000000000>
    | |   |   "IOPCIPMCSState" = 0
    | |   | }
    | |   | 
    | |   +-o DSB0@0  <class IOPCIDevice, id 0x1000001dc, registered, matched, active, busy 0 (1097 ms), retain 12>
    | |   | | {
    | |   | |   "IOPCIPMCSState" = 0
    | |   | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "class-code" = <00040600>
    | |   | |   "IOPCIExpressSlotStatus" = 64
    | |   | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"DesiredPowerState"=2,"CurrentPowerState"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   | |   "built-in" = <00>
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "IOInterruptControllers" = ("io-apic-0")
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOChildIndex" = 1
    | |   | |   "device-id" = <47150000>
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "compatible" = <"pci8086,1547","pciclass,060400","DSB0">
    | |   | |   "ranges" = <00000082000000000000d0b100000082000000000000d0b10000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "IOPCIExpressLinkCapabilities" = 2358337
    | |   | |   "IODTPersist" = <>
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB0@0"
    | |   | |   "revision-id" = <03000000>
    | |   | |   "IOPCIExpressLinkStatus" = 4161
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "pcidebug" = "6:0:0(7:7)"
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "reg" = <0000060000000000000000000000000000000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 0
    | |   | | }
    | |   | | 
    | |   | +-o NHI0@0  <class IOPCIDevice, id 0x1000001dd, registered, matched, active, busy 0 (1096 ms), retain 11>
    | |   |     {
    | |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |       "IOPCIMSIMode" = Yes
    | |   |       "assigned-addresses" = <10000782000000000000d0b1000000000000040014000782000000000000d4b10000000000100000>
    | |   |       "class-code" = <00800800>
    | |   |       "subsystem-vendor-id" = <22220000>
    | |   |       "vendor-id" = <86800000>
    | |   |       "IOPCIExpressLinkCapabilities" = 523329
    | |   |       "IOName" = "pci8086,1547"
    | |   |       "pathcr" = <0400000000000000000007001000100005000000000000000000070010001000010000000b000e000e000000000000000200000000000000000004000200010003000000000000000000070002000100>
    | |   |       "IOPCIPMCSState" = 0
    | |   |       "TBTDPLowToHigh" = <01000000>
    | |   |       "power-save" = 1
    | |   |       "IOChildIndex" = 1
    | |   |       "pcidebug" = "7:0:0"
    | |   |       "IOPCIExpressLinkStatus" = 4161
    | |   |       "pci-aspm-default" = 0
    | |   |       "IOPCIExpressCapabilities" = 2
    | |   |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   |       "linkDetails" = <0800000003000000>
    | |   |       "IOPCITunnelControllerID" = 4294967926
    | |   |       "built-in" = <00>
    | |   |       "IOPCIResourced" = Yes
    | |   |       "IOPowerManagement" = {"ChildrenPowerState"=2,"DesiredPowerState"=2,"CurrentPowerState"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |       "IODeviceMemory" = (({"address"=2983198720,"length"=262144}),({"address"=2983460864,"length"=4096}))
    | |   |       "acpi-pmcap-offset" = 128
    | |   |       "name" = <"pci8086,1547">
    | |   |       "ThunderboltUUID" = <0e2e82108c67755cba54a49498600a08>
    | |   |       "subsystem-id" = <11110000>
    | |   |       "compatible" = <"pci2222,1111","pci8086,1547","pciclass,088000","NHI0">
    | |   |       "ThunderboltDROM" = <e900609d1b0d000100cc7c096e01650001000a00010a088180028000000008829001800000000883800480010000088490038001000008850000000000000386600387800388a00389c0058a500000058b500082058c5000840d014170706c6520496e632e000c024d6163696e746f736800>
    | |   |       "sscOffset" = <0007>
    | |   |       "reg" = <000007000000000000000000000000000000000010000702000000000000000000000000000004001400070200000000000000000000000000100000>
    | |   |       "device-id" = <47150000>
    | |   |       "ThunderboltConfig" = <0000ffff2500010026000200270001001600020001000200>
    | |   |       "revision-id" = <03000000>
    | |   |       "IOInterruptSpecifiers" = (<1000000007000000>,<1400000000000100>)
    | |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB0@0/NHI0@0"
    | |   |     }
    | |   |     
    | |   +-o DSB1@3  <class IOPCIDevice, id 0x1000001de, registered, matched, active, busy 0 (1 ms), retain 13>
    | |   | | {
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000"
    | |   | |   "IOPCIExpressLinkCapabilities" = 53738561
    | |   | |   "class-code" = <00040600>
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "IOPCIPMCSState" = 0
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 1572960
    | |   | |   "IOChildIndex" = 2
    | |   | |   "pcidebug" = "6:3:0(194:194)"
    | |   | |   "Thunderbolt Path" = "IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/RP05@1C,4/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType2/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType2/IOThunderboltPort@6"
    | |   | |   "IOPCIExpressLinkStatus" = 4161
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "IODTPersist" = <>
    | |   | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "Thunderbolt Entry ID" = 4294967983
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "AAPL,slot-name" = <"Thunderbolt Slot 1">
    | |   | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"DesiredPowerState"=2,"CurrentPowerState"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "IOPCITunnelLinkChange" = Yes
    | |   | |   "compatible" = <"pci8086,1547","pciclass,060400","DSB1">
    | |   | |   "IOPCIExpressSlotStatus" = 0
    | |   | |   "reg" = <0018060000000000000000000000000000000000>
    | |   | |   "device-id" = <47150000>
    | |   | |   "IOPCITunnelID" = 4294967926
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "IOInterruptSpecifiers" = (<1300000007000000>,<0c00000000000100>)
    | |   | |   "revision-id" = <03000000>
    | |   | |   "IOPCIMSIMode" = Yes
    | |   | | }
    | |   | | 
    | |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000001df, retain 9>
    | |   |   | {
    | |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0"
    | |   |   | }
    | |   |   | 
    | |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000001e0, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB0@0"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001e1, retain 4>
    | |   |   |     {
    | |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |     }
    | |   |   |     
    | |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000001e2, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000001e3, retain 9>
    | |   |   |   | {
    | |   |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0"
    | |   |   |   | }
    | |   |   |   | 
    | |   |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000001e4, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001e5, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000001e6, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001e7, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x1000001e8, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001e9, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x1000001ea, retain 4>
    | |   |   |   |   {
    | |   |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0/DSB5@50000"
    | |   |   |   |   }
    | |   |   |   |   
    | |   |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x1000001eb, retain 4>
    | |   |   |       {
    | |   |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB3@30000/UPS0@0/DSB6@60000"
    | |   |   |       }
    | |   |   |       
    | |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x1000001ec, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000001ed, retain 9>
    | |   |   |   | {
    | |   |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0"
    | |   |   |   | }
    | |   |   |   | 
    | |   |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000001ee, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001ef, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000001f0, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001f1, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x1000001f2, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001f3, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x1000001f4, retain 4>
    | |   |   |   |   {
    | |   |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0/DSB5@50000"
    | |   |   |   |   }
    | |   |   |   |   
    | |   |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x1000001f5, retain 4>
    | |   |   |       {
    | |   |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB4@40000/UPS0@0/DSB6@60000"
    | |   |   |       }
    | |   |   |       
    | |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x1000001f6, retain 4>
    | |   |   |   {
    | |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB5@50000"
    | |   |   |   }
    | |   |   |   
    | |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x1000001f7, retain 4>
    | |   |       {
    | |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB1@30000/UPS0@0/DSB6@60000"
    | |   |       }
    | |   |       
    | |   +-o DSB2@4  <class IOPCIDevice, id 0x1000001f8, registered, matched, active, busy 0 (1 ms), retain 13>
    | |   | | {
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000"
    | |   | |   "IOPCIExpressLinkCapabilities" = 70515777
    | |   | |   "class-code" = <00040600>
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "IOPCIPMCSState" = 0
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 2097248
    | |   | |   "IOChildIndex" = 3
    | |   | |   "pcidebug" = "6:4:0(132:132)"
    | |   | |   "Thunderbolt Path" = "IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/RP05@1C,4/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType2/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType2/IOThunderboltPort@7"
    | |   | |   "IOPCIExpressLinkStatus" = 4161
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "IODTPersist" = <>
    | |   | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "Thunderbolt Entry ID" = 4294967984
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "AAPL,slot-name" = <"Thunderbolt Slot 2">
    | |   | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"DesiredPowerState"=2,"CurrentPowerState"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "IOPCITunnelLinkChange" = Yes
    | |   | |   "compatible" = <"pci8086,1547","pciclass,060400","DSB2">
    | |   | |   "IOPCIExpressSlotStatus" = 0
    | |   | |   "reg" = <0020060000000000000000000000000000000000>
    | |   | |   "device-id" = <47150000>
    | |   | |   "IOPCITunnelID" = 4294967926
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0d00000000000100>)
    | |   | |   "revision-id" = <03000000>
    | |   | |   "IOPCIMSIMode" = Yes
    | |   | | }
    | |   | | 
    | |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000001f9, retain 9>
    | |   |   | {
    | |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0"
    | |   |   | }
    | |   |   | 
    | |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000001fa, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB0@0"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001fb, retain 4>
    | |   |   |     {
    | |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |     }
    | |   |   |     
    | |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000001fc, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000001fd, retain 9>
    | |   |   |   | {
    | |   |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0"
    | |   |   |   | }
    | |   |   |   | 
    | |   |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000001fe, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000001ff, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x100000200, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000201, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x100000202, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000203, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x100000204, retain 4>
    | |   |   |   |   {
    | |   |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0/DSB5@50000"
    | |   |   |   |   }
    | |   |   |   |   
    | |   |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x100000205, retain 4>
    | |   |   |       {
    | |   |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB3@30000/UPS0@0/DSB6@60000"
    | |   |   |       }
    | |   |   |       
    | |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x100000206, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o UPS0@0  <class IORegistryEntry, id 0x100000207, retain 9>
    | |   |   |   | {
    | |   |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0"
    | |   |   |   | }
    | |   |   |   | 
    | |   |   |   +-o DSB0@0  <class IORegistryEntry, id 0x100000208, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000209, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x10000020a, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x10000020b, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x10000020c, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x10000020d, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x10000020e, retain 4>
    | |   |   |   |   {
    | |   |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0/DSB5@50000"
    | |   |   |   |   }
    | |   |   |   |   
    | |   |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x10000020f, retain 4>
    | |   |   |       {
    | |   |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB4@40000/UPS0@0/DSB6@60000"
    | |   |   |       }
    | |   |   |       
    | |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x100000210, retain 4>
    | |   |   |   {
    | |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB5@50000"
    | |   |   |   }
    | |   |   |   
    | |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x100000211, retain 4>
    | |   |       {
    | |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB2@40000/UPS0@0/DSB6@60000"
    | |   |       }
    | |   |       
    | |   +-o DSB3@5  <class IOPCIDevice, id 0x100000212, registered, matched, active, busy 0 (1 ms), retain 12>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB3@50000"
    | |   |     "IOPCIExpressLinkCapabilities" = 87292993
    | |   |     "class-code" = <00040600>
    | |   |     "vendor-id" = <86800000>
    | |   |     "IOName" = "pci-bridge"
    | |   |     "IOPCIPMCSState" = 0
    | |   |     "#size-cells" = <02000000>
    | |   |     "IOPCIExpressSlotCapabilities" = 2621536
    | |   |     "IOChildIndex" = 4
    | |   |     "pcidebug" = "6:5:0(70:70)"
    | |   |     "Thunderbolt Path" = "IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/RP05@1C,4/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType2/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType2/IOThunderboltPort@8"
    | |   |     "IOPCIExpressLinkStatus" = 4161
    | |   |     "pci-aspm-default" = 0
    | |   |     "IODTPersist" = <>
    | |   |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   |     "IOPCIConfigured" = Yes
    | |   |     "IOPCIExpressCapabilities" = 354
    | |   |     "Thunderbolt Entry ID" = 4294967985
    | |   |     "IOPCIResourced" = Yes
    | |   |     "AAPL,slot-name" = <"Thunderbolt Slot 3">
    | |   |     "IOPowerManagement" = {"ChildrenPowerState"=2,"DesiredPowerState"=2,"CurrentPowerState"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |     "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   |     "acpi-pmcap-offset" = 128
    | |   |     "name" = <"pci-bridge">
    | |   |     "IOPCITunnelLinkChange" = Yes
    | |   |     "compatible" = <"pci8086,1547","pciclass,060400","DSB3">
    | |   |     "IOPCIExpressSlotStatus" = 0
    | |   |     "reg" = <0028060000000000000000000000000000000000>
    | |   |     "device-id" = <47150000>
    | |   |     "IOPCITunnelID" = 4294967926
    | |   |     "#address-cells" = <03000000>
    | |   |     "IOInterruptSpecifiers" = (<1100000007000000>,<0e00000000000100>)
    | |   |     "revision-id" = <03000000>
    | |   |     "IOPCIMSIMode" = Yes
    | |   |   }
    | |   |   
    | |   +-o DSB4@6  <class IOPCIDevice, id 0x100000213, registered, matched, active, busy 0 (1 ms), retain 12>
    | |       {
    | |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/UPSB@0/DSB4@60000"
    | |         "IOPCIExpressLinkCapabilities" = 104070209
    | |         "class-code" = <00040600>
    | |         "vendor-id" = <86800000>
    | |         "IOName" = "pci-bridge"
    | |         "IOPCIPMCSState" = 0
    | |         "#size-cells" = <02000000>
    | |         "IOPCIExpressSlotCapabilities" = 3145824
    | |         "IOChildIndex" = 5
    | |         "pcidebug" = "6:6:0(8:8)"
    | |         "Thunderbolt Path" = "IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/RP05@1C,4/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType2/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType2/IOThunderboltPort@9"
    | |         "IOPCIExpressLinkStatus" = 4161
    | |         "pci-aspm-default" = 0
    | |         "IODTPersist" = <>
    | |         "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |         "IOPCIConfigured" = Yes
    | |         "IOPCIExpressCapabilities" = 354
    | |         "Thunderbolt Entry ID" = 4294967986
    | |         "IOPCIResourced" = Yes
    | |         "AAPL,slot-name" = <"Thunderbolt Slot 4">
    | |         "IOPowerManagement" = {"ChildrenPowerState"=2,"DesiredPowerState"=2,"CurrentPowerState"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |         "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |         "acpi-pmcap-offset" = 128
    | |         "name" = <"pci-bridge">
    | |         "IOPCITunnelLinkChange" = Yes
    | |         "compatible" = <"pci8086,1547","pciclass,060400","DSB4">
    | |         "IOPCIExpressSlotStatus" = 0
    | |         "reg" = <0030060000000000000000000000000000000000>
    | |         "device-id" = <47150000>
    | |         "IOPCITunnelID" = 4294967926
    | |         "#address-cells" = <03000000>
    | |         "IOInterruptSpecifiers" = (<1200000007000000>,<1300000000000100>)
    | |         "revision-id" = <03000000>
    | |         "IOPCIMSIMode" = Yes
    | |       }
    | |       
    | +-o LPCB@1F  <class IOPCIDevice, id 0x1000001d0, registered, matched, active, busy 0 (97 ms), retain 22>
    | | | {
    | | |   "name" = <"pci8086,8c44">
    | | |   "compatible" = <"pci8086,7270","pci8086,8c44","pciclass,060100","LPCB">
    | | |   "subsystem-vendor-id" = <86800000>
    | | |   "IOName" = "pci8086,8c44"
    | | |   "reg" = <00f8000000000000000000000000000000000000>
    | | |   "device-id" = <448c0000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "IOPCIResourced" = Yes
    | | |   "revision-id" = <05000000>
    | | |   "vendor-id" = <86800000>
    | | |   "pcidebug" = "0:31:0"
    | | |   "class-code" = <00010600>
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/LPCB@1f0000"
    | | |   "subsystem-id" = <70720000>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | }
    | | | 
    | | +-o DMAC  <class IOACPIPlatformDevice, id 0x100000152, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0200">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=0,"length"=32}),({"address"=129,"length"=17}),({"address"=147,"length"=13}),({"address"=192,"length"=32}))
    | | |   }
    | | |   
    | | +-o FWHD  <class IOACPIPlatformDevice, id 0x100000153, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "name" = <"INT0800">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=4278190080,"length"=16777216}))
    | | |   }
    | | |   
    | | +-o HPET  <class IOACPIPlatformDevice, id 0x100000154, registered, matched, active, busy 0 (0 ms), retain 8>
    | | |   {
    | | |     "_STA" = 15
    | | |     "IODeviceMemory" = (({"address"=4275044352,"length"=1024}))
    | | |     "name" = <"PNP0103">
    | | |     "IOInterruptControllers" = ("io-apic-0","io-apic-0","io-apic-0","io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0200000000000000>,<0800000000000000>,<0b00000000000000>,<0c00000000000000>)
    | | |     "compatible" = <"PNP0C01">
    | | |   }
    | | |   
    | | +-o IPIC  <class IOACPIPlatformDevice, id 0x100000155, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0000">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=32,"length"=2}),({"address"=36,"length"=2}),({"address"=40,"length"=2}),({"address"=44,"length"=2}),({"address"=48,"length"=2}),({"address"=52,"length"=2}),({"address"=56,"length"=2}),({"address"=60,"length"=2}),({"address"=160,"length"=2}),({"address"=164,"length"=2}),({"address"=168,"length"=2}),({"address"=172,"length"=2}),({"address"=176,"length"=2}),({"address"=180,"length"=2}),({"address"=184,"length"=2}),({"address"=188,"length"=2}),({"address"=1232,"length"=2}))
    | | |   }
    | | |   
    | | +-o MATH  <class IOACPIPlatformDevice, id 0x100000156, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=240,"length"=1}))
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0d00000000000000>)
    | | |     "name" = <"PNP0C04">
    | | |   }
    | | |   
    | | +-o LDRC  <class IOACPIPlatformDevice, id 0x100000157, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "_UID" = "2"
    | | |     "IODeviceMemory" = (({"address"=46,"length"=2}),({"address"=78,"length"=2}),({"address"=97,"length"=1}),({"address"=99,"length"=1}),({"address"=101,"length"=1}),({"address"=103,"length"=1}),({"address"=128,"length"=1}),({"address"=146,"length"=1}),({"address"=178,"length"=2}),({"address"=65535,"length"=1}),({"address"=1024,"length"=128}),({"address"=2048,"length"=128}))
    | | |     "name" = <"PNP0C02">
    | | |   }
    | | |   
    | | +-o RTC  <class IOACPIPlatformDevice, id 0x100000158, registered, matched, active, busy 0 (7 ms), retain 9>
    | | |   {
    | | |     "IODeviceMemory" = (({"address"=112,"length"=8}))
    | | |     "_STA" = 18446744073709551615
    | | |     "IOInterruptSpecifiers" = (<0400000000000000>)
    | | |     "acpi-wake-type" = 4
    | | |     "name" = <"PNP0B00">
    | | |     "IOInterruptControllers" = ("ACPIEventController")
    | | |   }
    | | |   
    | | +-o TIMR  <class IOACPIPlatformDevice, id 0x100000159, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0100">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=64,"length"=4}),({"address"=80,"length"=4}))
    | | |   }
    | | |   
    | | +-o SMC  <class IOACPIPlatformDevice, id 0x10000015a, registered, matched, active, busy 0 (132 ms), retain 10>
    | | | | {
    | | | |   "_STA" = 11
    | | | |   "IODeviceMemory" = (({"address"=768,"length"=32}),({"address"=4277141504,"length"=65536}))
    | | | |   "name" = <"APP0001">
    | | | |   "IOInterruptControllers" = ("io-apic-0")
    | | | |   "IOInterruptSpecifiers" = (<0600000000000000>)
    | | | |   "compatible" = <"smc-huronriver">
    | | | | }
    | | | | 
    | | | +-o DPPT  <class IOACPIPlatformDevice, id 0x10000015b, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |     {
    | | |       "_STA" = 18446744073709551615
    | | |       "IOGeneralInterest" = "IOCommand is not serializable"
    | | |       "name" = <"APP000C">
    | | |       "compatible" = <"smc-dppt">
    | | |     }
    | | |     
    | | +-o ALS0  <class IOACPIPlatformDevice, id 0x10000015c, registered, matched, active, busy 0 (82 ms), retain 8>
    | | |   {
    | | |     "compatible" = <"smc-als">
    | | |     "_STA" = 15
    | | |     "name" = <"ACPI0008">
    | | |   }
    | | |   
    | | +-o EC  <class IOACPIPlatformDevice, id 0x10000015d, registered, matched, active, busy 0 (1 ms), retain 8>
    | |     {
    | |       "IODeviceMemory" = (({"address"=98,"length"=1}),({"address"=102,"length"=1}))
    | |       "_STA" = 18446744073709551615
    | |       "_UID" = "0"
    | |       "name" = <"PNP0C09">
    | |       "acpi-wake-gpe" = 35
    | |     }
    | |     
    | +-o SATA@1F,2  <class IOPCIDevice, id 0x1000001c9, registered, matched, active, busy 0 (345 ms), retain 13>
    | | | {
    | | |   "assigned-addresses" = <10fa00810000000088200000000000000800000014fa00810000000094200000000000000400000018fa0081000000008020000000000000080000001cfa00810000000090200000000000000400000020fa00810000000060200000000000002000000024fa0082000000000050c1b10000000000080000>
    | | |   "IOInterruptSpecifiers" = (<1300000007000000>,<0600000000000100>)
    | | |   "class-code" = <01060100>
    | | |   "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable",({"address"=2982236160,"length"=2048}))
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <86800000>
    | | |   "built-in" = <00>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOPCIMSIMode" = Yes
    | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | |   "name" = <"pci8086,8c02">
    | | |   "vendor-id" = <86800000>
    | | |   "acpi-pmcap-offset" = 112
    | | |   "device-id" = <028c0000>
    | | |   "IOPCIResourced" = Yes
    | | |   "compatible" = <"pci8086,7270","pci8086,8c02","pciclass,010601","SATA">
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002"
    | | |   "subsystem-id" = <70720000>
    | | |   "IOPCIPMCSState" = 0
    | | |   "revision-id" = <05000000>
    | | |   "pcidebug" = "0:31:2"
    | | |   "IOName" = "pci8086,8c02"
    | | |   "reg" = <00fa00000000000000000000000000000000000010fa00010000000000000000000000000800000014fa00010000000000000000000000000400000018fa0001000000000000000000000000080000001cfa00010000000000000000000000000400000020fa00010000000000000000000000002000000024fa000200000000000000000000000000080000>
    | | | }
    | | | 
    | | +-o PRT0@0  <class AppleIntelPchSeriesAHCIPort, id 0x1000001ca, registered, matched, active, busy 0 (303 ms), retain 11>
    | |   | {
    | |   |   "AHCI Port ALPM" = Yes
    | |   |   "IOPolledInterface" = "AppleAHCIPortPolledAdapter is not serializable"
    | |   |   "AHCI Port Hot Plug" = No
    | |   |   "IOMaximumSegmentByteCountRead" = 4194304
    | |   |   "64-bit" = Yes
    | |   |   "IOMaximumSegmentByteCountWrite" = 4194304
    | |   |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=2}
    | |   |   "AHCI-Built-In" = Yes
    | |   |   "Physical Interconnect Location" = "Internal"
    | |   |   "AHCI Port Optimized Device Number" = 0
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "IOMaximumSegmentCountRead" = 256
    | |   |   "AHCI Port SNotification" = No
    | |   |   "AHCI Port ESATA" = No
    | |   |   "IOMaximumSegmentCountWrite" = 256
    | |   |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.30 Supported","Product Name"="8 Series Chipset","Vendor Name"="Intel","Port Speed"="6 Gigabit"}
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002/PRT0@ffff"
    | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="Internal"}
    | |   |   "hdd-power-off" = 1
    | |   |   "AHCI-Ejectable" = No
    | |   | }
    | |   | 
    | |   +-o PMP@0  <class IOAHCIDevice, id 0x10000027f, registered, matched, active, busy 0 (303 ms), retain 14>
    | |     | {
    | |     |   "IOUnit" = 0
    | |     |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="3 Gigabit","Physical Interconnect Location"="Internal"}
    | |     | }
    | |     | 
    | |     +-o @0:0  <class IOMedia, id 0x100000285, registered, matched, active, busy 0 (301 ms), retain 11>
    | |     |   {
    | |     |     "Removable" = No
    | |     |     "Content" = "GUID_partition_scheme"
    | |     |     "Whole" = Yes
    | |     |     "Leaf" = No
    | |     |     "BSD Name" = "disk0"
    | |     |     "Ejectable" = No
    | |     |     "Preferred Block Size" = 512
    | |     |     "IOMediaIcon" = {"IOBundleResourceFile"="Internal.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | |     |     "BSD Minor" = 0
    | |     |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     |     "Writable" = Yes
    | |     |     "BSD Major" = 1
    | |     |     "Size" = 1000204886016
    | |     |     "IOBusyInterest" = "IOCommand is not serializable"
    | |     |     "Open" = Yes
    | |     |     "Content Hint" = ""
    | |     |     "BSD Unit" = 0
    | |     |   }
    | |     |   
    | |     +-o @0:1  <class IOMedia, id 0x10000029e, registered, matched, active, busy 0 (0 ms), retain 9>
    | |     |   {
    | |     |     "Removable" = No
    | |     |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | |     |     "Whole" = No
    | |     |     "Leaf" = Yes
    | |     |     "BSD Name" = "disk0s1"
    | |     |     "Ejectable" = No
    | |     |     "Preferred Block Size" = 512
    | |     |     "BSD Minor" = 1
    | |     |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     |     "Writable" = Yes
    | |     |     "UUID" = "0000765C-1B22-0000-335C-000048100000"
    | |     |     "Partition ID" = 1
    | |     |     "BSD Major" = 1
    | |     |     "Size" = 209715200
    | |     |     "IOBusyInterest" = "IOCommand is not serializable"
    | |     |     "Open" = No
    | |     |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | |     |     "BSD Unit" = 0
    | |     |   }
    | |     |   
    | |     +-o @0:2  <class IOMedia, id 0x10000029f, registered, matched, active, busy 0 (31 ms), retain 11>
    | |     |   {
    | |     |     "Removable" = No
    | |     |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | |     |     "Whole" = No
    | |     |     "Leaf" = Yes
    | |     |     "BSD Name" = "disk0s2"
    | |     |     "Ejectable" = No
    | |     |     "Preferred Block Size" = 512
    | |     |     "BSD Minor" = 2
    | |     |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |     |     "Writable" = Yes
    | |     |     "UUID" = "00003DE0-0882-0000-8F5B-0000FD010000"
    | |     |     "Partition ID" = 2
    | |     |     "BSD Major" = 1
    | |     |     "Size" = 999345127424
    | |     |     "IOBusyInterest" = "IOCommand is not serializable"
    | |     |     "Open" = Yes
    | |     |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | |     |     "BSD Unit" = 0
    | |     |   }
    | |     |   
    | |     +-o @0:3  <class IOMedia, id 0x1000002a0, registered, matched, active, busy 0 (31 ms), retain 9>
    | |         {
    | |           "Removable" = No
    | |           "Content" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | |           "Whole" = No
    | |           "Leaf" = Yes
    | |           "BSD Name" = "disk0s3"
    | |           "Ejectable" = No
    | |           "Preferred Block Size" = 512
    | |           "BSD Minor" = 3
    | |           "IOGeneralInterest" = "IOCommand is not serializable"
    | |           "Writable" = Yes
    | |           "UUID" = "2112F065-8502-49F8-A348-FDEB8D4FBE3A"
    | |           "Partition ID" = 3
    | |           "BSD Major" = 1
    | |           "Size" = 650002432
    | |           "IOBusyInterest" = "IOCommand is not serializable"
    | |           "Open" = No
    | |           "Content Hint" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | |           "BSD Unit" = 0
    | |         }
    | |         
    | +-o SBUS@1F,3  <class IOPCIDevice, id 0x1000001cb, registered, matched, active, busy 0 (210 ms), retain 13>
    |   | {
    |   |   "assigned-addresses" = <10fb0082000000000058c1b1000000000001000020fb008100000000a0ef00000000000020000000>
    |   |   "IOInterruptSpecifiers" = (<1200000007000000>)
    |   |   "IODeviceMemory" = (({"address"=2982238208,"length"=256}),"IOSubMemoryDescriptor is not serializable")
    |   |   "class-code" = <00050c00>
    |   |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    |   |   "subsystem-vendor-id" = <86800000>
    |   |   "built-in" = <00>
    |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |   |   "IOInterruptControllers" = ("io-apic-0")
    |   |   "name" = <"pci8086,8c22">
    |   |   "vendor-id" = <86800000>
    |   |   "device-id" = <228c0000>
    |   |   "IOPCIResourced" = Yes
    |   |   "compatible" = <"pci8086,7270","pci8086,8c22","pciclass,0c0500","SBUS">
    |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0003"
    |   |   "subsystem-id" = <70720000>
    |   |   "revision-id" = <05000000>
    |   |   "pcidebug" = "0:31:3"
    |   |   "IOName" = "pci8086,8c22"
    |   |   "reg" = <00fb00000000000000000000000000000000000010fb00020000000000000000000000000001000020fb000100000000000000000000000020000000>
    |   | }
    |   | 
    |   +-o BUS0@0  <class IORegistryEntry, id 0x1000001cc, retain 6>
    |   | | {
    |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0003/BUS0@0"
    |   | | }
    |   | | 
    |   | +-o MKY0@0  <class IORegistryEntry, id 0x1000001cd, retain 4>
    |   | |   {
    |   | |     "resprg" = 3
    |   | |     "refnum" = 0
    |   | |     "hdet" = 1
    |   | |     "ramp-control-address" = 59
    |   | |     "address" = 57
    |   | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0003/BUS0@0/MKY0@0"
    |   | |     "device-id" = 3285
    |   | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |   | |   }
    |   | |   
    |   | +-o BLC0@0  <class IORegistryEntry, id 0x1000001ce, retain 4>
    |   |     {
    |   |       "type" = 1296253779
    |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0003/BUS0@0/BLC0@0"
    |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |   |       "refnum" = 0
    |   |       "command" = 81
    |   |       "address" = 110
    |   |     }
    |   |     
    |   +-o BUS1@1  <class IORegistryEntry, id 0x1000001cf, retain 4>
    |       {
    |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0003/BUS1@1"
    |       }
    |       
    +-o MEM2  <class IOACPIPlatformDevice, id 0x1000001ae, registered, matched, active, busy 0 (0 ms), retain 7>
    |   {
    |     "_STA" = 18446744073709551615
    |     "_UID" = "2"
    |     "IODeviceMemory" = (({"address"=536870912,"length"=2097152}),({"address"=1073741824,"length"=2097152}))
    |     "name" = <"PNP0C01">
    |   }
    |   
    +-o LNKA  <class IOACPIPlatformDevice, id 0x1000001af, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "1"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKB  <class IOACPIPlatformDevice, id 0x1000001b0, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "2"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKC  <class IOACPIPlatformDevice, id 0x1000001b1, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "3"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKD  <class IOACPIPlatformDevice, id 0x1000001b2, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "4"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKE  <class IOACPIPlatformDevice, id 0x1000001b3, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "5"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKF  <class IOACPIPlatformDevice, id 0x1000001b4, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "6"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKG  <class IOACPIPlatformDevice, id 0x1000001b5, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "7"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKH  <class IOACPIPlatformDevice, id 0x1000001b6, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "8"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o PWRB  <class IOACPIPlatformDevice, id 0x1000001b7, registered, matched, active, busy 0 (0 ms), retain 9>
    |   {
    |     "_STA" = 18446744073709551615
    |     "IOInterruptSpecifiers" = (<0200000000000000>)
    |     "name" = <"PNP0C0C">
    |     "acpi-wake-type" = 1
    |     "IOInterruptControllers" = ("ACPIEventController")
    |   }
    |   
    +-o PNLF@0  <class IOACPIPlatformDevice, id 0x1000001b8, registered, matched, active, busy 0 (24 ms), retain 10>
    |   {
    |     "refnum" = 0
    |     "compatible" = <"backlight">
    |     "acpi-path" = "IOACPIPlane:/_SB/PNLF@0"
    |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |     "_UID" = "10"
    |     "device-properties" = {"acpi-device"="IOACPIPlatformDevice is not serializable","type"=1296253779,"refnum"=0,"acpi-path"="IOACPIPlane:/_SB/PNLF@0"}
    |     "_STA" = 11
    |     "type" = 1296253779
    |     "_ADR" = 0
    |     "name" = <"APP0002">
    |   }
    |   
    +-o SLPB  <class IOACPIPlatformDevice, id 0x1000001b9, registered, matched, active, busy 0 (0 ms), retain 8>
    |   {
    |     "name" = <"PNP0C0E">
    |     "_STA" = 11
    |   }
    |   
    +-o options  <class AppleEFINVRAM, id 0x10000022a, registered, matched, active, busy 0 (0 ms), retain 570>
        {
          "efi-boot-device" = <"<array><dict><key>IOMatch</key><dict><key>IOProviderClass</key><string>IOMedia</string><key>IOPropertyMatch</key><dict><key>UUID</key><string>00003DE0-0882-0000-8F5B-0000FD010000</string></dict></dict><key>BLLastBSDName</key><string>disk0s2</string></dict></array>">
          "boot-gamma" = <1006000005b00000000000006e0000000000000007000404db050b0bb20e1e1e952436366d3e57574f6077770980a1a187a807000404db050b0bb20e1e1e952436366d3e57574f6077770980a1a187a807000404db050b0bb20e1e1e952436366d3e57574f6077770980a1a187a8>
          "EFIBluetoothDelay" = <b80b>
          "backlight-level" = <df2c>
          "fmm-mobileme-token-FMM" = < >
          "prev-lang:kbd" = <"ru:0">
          "fmm-computer-name" = <"iMac - Plieva">
          "bluetoothActiveControllerInfo" = <8d82ac05020000008314c8e0eb2c72fe>
          "efi-boot-device-data" = <02010c00d041030a0000000001010600021f03120a0000000000000004012a0002000000284006000000000040ce567400000000e03d0000820800008f5b0000fd01000002027fff0400>
          "SystemAudioVolume" = <4d>
          "display-config" = <000025017308ffff0100>
          "LocationServicesEnabled" = <01>
        }
        
