flashrom v0.9.6.1-runknown on Darwin 13.2.0 (x86_64)
flashrom was built with libpci 3.1.9, GCC 4.0.1 (Apple Inc. build 5488), little endian
Command line (6 args): /Applications/DarwinDumper_v2.8.8/DarwinDumper.app/Contents/Resources/Tools/flashrom -p internal -r /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/BIOS/System/biosbackup.rom -o /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/BIOS/System/flashrom_log.txt
Calibrating delay loop... OS timer resolution is 1 usecs, 2930M loops per second, 10 myus = 18 us, 100 myus = 93 us, 1000 myus = 929 us, 10000 myus = 8652 us, 4 myus = 3 us, OK.
Initializing internal programmer
Mapping low megabyte at 0x00000400, unaligned size 0xffc00.
Mapping low megabyte, 0xffc00 bytes at unaligned 0x00000400.
No coreboot table found.
dmidecode execution unsuccessful - continuing without DMI info
Found chipset "Intel Lynx Point" with PCI ID 8086:8c44. 
This chipset is marked as untested. If you are using an up-to-date version
of flashrom *and* were (not) able to successfully update your firmware with it,
then please email a report to flashrom@flashrom.org including a verbose (-V) log.
Thank you!
Enabling flash write... enable_flash_ich_dc_spi: unknown ICH generation. Please report!

0xfff80000/0xffb80000 FWH IDSEL: 0x0
0xfff00000/0xffb00000 FWH IDSEL: 0x0
0xffe80000/0xffa80000 FWH IDSEL: 0x1
0xffe00000/0xffa00000 FWH IDSEL: 0x1
0xffd80000/0xff980000 FWH IDSEL: 0x2
0xffd00000/0xff900000 FWH IDSEL: 0x2
0xffc80000/0xff880000 FWH IDSEL: 0x3
0xffc00000/0xff800000 FWH IDSEL: 0x3
0xff700000/0xff300000 FWH IDSEL: 0x4
0xff600000/0xff200000 FWH IDSEL: 0x5
0xff500000/0xff100000 FWH IDSEL: 0x6
0xff400000/0xff000000 FWH IDSEL: 0x7
0xfff80000/0xffb80000 FWH decode enabled
0xfff00000/0xffb00000 FWH decode enabled
0xffe80000/0xffa80000 FWH decode enabled
0xffe00000/0xffa00000 FWH decode enabled
0xffd80000/0xff980000 FWH decode enabled
0xffd00000/0xff900000 FWH decode enabled
0xffc80000/0xff880000 FWH decode enabled
0xffc00000/0xff800000 FWH decode enabled
0xff700000/0xff300000 FWH decode disabled
0xff600000/0xff200000 FWH decode disabled
0xff500000/0xff100000 FWH decode disabled
0xff400000/0xff000000 FWH decode disabled
Maximum FWH chip size: 0x100000 bytes
BIOS_CNTL = 0x09: BIOS Lock Enable: disabled, BIOS Write Enable: enabled
Root Complex Register Block address = 0xfed1c000
GCS = 0xc21: BIOS Interface Lock-Down: enabled, Boot BIOS Straps: 0x3 (unknown)
Top Swap : not enabled
SPIBAR = 0xfed1c000 + 0x3800
0x04: 0xf008 (HSFS)
HSFS: FDONE=0, FCERR=0, AEL=0, BERASE=1, SCIP=0, FDOPSS=1, FDV=1, FLOCKDN=1
WARNING: SPI Configuration Lockdown activated.
Reading OPCODES... done
        OP        Type      Pre-OP
op[0]: 0x9f, read  w/o addr, none
op[1]: 0x02, write w/  addr, none
op[2]: 0x03, read  w/  addr, none
op[3]: 0x01, write w/o addr, none
op[4]: 0x05, read  w/o addr, none
op[5]: 0x20, write w/  addr, none
op[6]: 0xd8, write w/  addr, none
op[7]: 0xff, read  w/o addr, none
Pre-OP 0: 0x06, Pre-OP 1: 0x06
0x06: 0x0004 (HSFC)
HSFC: FGO=0, FCYCLE=2, FDBC=0, SME=0
0x08: 0x00616257 (FADDR)
0x50: 0x00004aff (FRAP)
BMWAG 0x00, BMRAG 0x00, BRWA 0x4a, BRRA 0xff
0x54: 0x00000000 FREG0: WARNING: Flash Descriptor region (0x00000000-0x00000fff) is read-only.
0x58: 0x07ff0190 FREG1: BIOS region (0x00190000-0x007fffff) is read-write.
0x5C: 0x018f0002 FREG2: WARNING: Management Engine region (0x00002000-0x0018ffff) is read-only.
0x60: 0x00007fff FREG3: Gigabit Ethernet region is unused.
0x64: 0x00010001 FREG4: WARNING: Platform Data region (0x00001000-0x00001fff) is read-only.
0x74: 0x80010000 PR0: WARNING: 0x00000000-0x00001fff is read-only.
0x78: 0x860f0190 PR1: WARNING: 0x00190000-0x0060ffff is read-only.
0x7C: 0x9fff0632 PR2: WARNING: 0x00632000-0x01ffffff is read-only.
0x80: 0x00000000 (PR3 is unused)
0x84: 0x00000000 (PR4 is unused)
Please send a verbose log to flashrom@flashrom.org if this board is not listed on
http://flashrom.org/Supported_hardware#Supported_mainboards yet.
Writes have been disabled. You can enforce write support with the
ich_spi_force programmer option, but it will most likely harm your hardware!
If you force flashrom you will get no support if something breaks.
0x90: 0xc0 (SSFS)
SSFS: SCIP=0, FDONE=0, FCERR=0, AEL=0
0x91: 0xfc7f00 (SSFC)
SSFC: SCGO=0, ACS=0, SPOP=0, COP=0, DBC=63, SME=0, SCF=4
0x94: 0x0606     (PREOP)
0x96: 0x3c6c     (OPTYPE)
0x98: 0x0103029f (OPMENU)
0x9C: 0xffd82005 (OPMENU+4)
0xA0: 0x00000000 (BBAR)
0xC4: 0x80802045 (LVSCC)
LVSCC: BES=0x1, WG=1, WSR=0, WEWS=0, EO=0x20, VCL=1
0xC8: 0x00000000 (UVSCC)
UVSCC: BES=0x0, WG=0, WSR=0, WEWS=0, EO=0x0, VCL=0
0xD0: 0x50444653 (FPB)

Reading flash descriptors mapped by the chipset via FDOC/FDOD... done.
=== Content Section ===
FLVALSIG 0x0ff0a55a
FLMAP0   0x03040003
FLMAP1   0x15100206
FLMAP2   0x00210120

--- Details ---
NR          (Number of Regions):                     4
FRBA        (Flash Region Base Address):         0x040
NC          (Number of Components):                  1
FCBA        (Flash Component Base Address):      0x030
ISL         (ICH/PCH Strap Length):                 21
FISBA/FPSBA (Flash ICH/PCH Strap Base Address):  0x100
NM          (Number of Masters):                     3
FMBA        (Flash Master Base Address):         0x060
MSL/PSL     (MCH/PROC Strap Length):                 1
FMSBA       (Flash MCH/PROC Strap Base Address): 0x200

=== Component Section ===
FLCOMP   0x64900044
FLILL    0x00000000

--- Details ---
Component 1 density:             8 MB
Component 2 is not used.
Read Clock Frequency:           20 MHz
Read ID and Status Clock Freq.: 50 MHz
Write and Erase Clock Freq.:    50 MHz
Fast Read is supported.
Fast Read Clock Frequency:      50 MHz
No forbidden opcodes.

=== Region Section ===
FLREG0   0x00000000
FLREG1   0x07ff0190
FLREG2   0x018f0002
FLREG3   0x00007fff
FLREG4   0x00010001

--- Details ---
Region 0 (Descr.) 0x00000000 - 0x00000fff
Region 1 (BIOS  ) 0x00190000 - 0x007fffff
Region 2 (ME    ) 0x00002000 - 0x0018ffff
Region 3 (GbE   ) is unused.
Region 4 (Platf.) 0x00001000 - 0x00001fff

=== Master Section ===
FLMSTR1  0x0aff0000
FLMSTR2  0x0c0d0000
FLMSTR3  0xffff0118

--- Details ---
      Descr. BIOS ME GbE Platf.
BIOS    r     rw  r   rw   r 
ME      r         rw  rw     
GbE     rw    rw  rw  rw   rw

SPI Read Configuration: prefetching enabled, caching enabled, OK.
The following protocols are supported: FWH, SPI.
Probing for AMIC A25L05PT, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L05PU, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L10PT, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L10PU, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L20PT, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L20PU, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L40PT, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L40PU, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L80P, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L16PT, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L16PU, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L512, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L010, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L020, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L040, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L080, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L016, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L032, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25LQ032, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF021, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF041A, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF081, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF081A, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF161, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF321, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF321A, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF641(A), 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DQ161, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25F512B, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25FS010, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25FS040, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26DF041, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26DF081A, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26DF161, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26DF161A, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26F004, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45CS1282, 16896 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB011D, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB021D, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB041D, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB081D, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB161D, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB321C, 4224 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB321D, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB642D, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for EMST F25L008A, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B05, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B05T, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B10, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B10T, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B20T, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B40T, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B80T, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B16T, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B32T, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B64T, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F05, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F10, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q80(A), 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q32(A/B), 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q128, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25QH16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25QH32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q128, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L512, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L1005, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L2005, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L4005, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L8005, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L1605, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L1635D, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L1635E, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L3205, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L3235D, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L6405, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Chip status register is 00
Chip status register: Status Register Write Disable (SRWD) is not set
Chip status register: Bit 6 is not set
Chip status register: Block Protect 3 (BP3) is not set
Chip status register: Block Protect 2 (BP2) is not set
Chip status register: Block Protect 1 (BP1) is not set
Chip status register: Block Protect 0 (BP0) is not set
Chip status register: Write Enable Latch (WEL) is not set
Chip status register: Write In Progress (WIP/BUSY) is not set
Found Macronix flash chip "MX25L6405" (8192 kB, SPI) at physical address 0xff800000.
Probing for Macronix MX25L12805, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE10, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx N25Q064, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV010, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV016B, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV020, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV040, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV080B, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV512, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Sanyo LF25FW203A, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL004A, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL008A, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL016A, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL032A, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL064A, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25LF040A, 512 kB: Invalid OPCODE 0xab, will not execute.
Probing for SST SST25LF080A, 1024 kB: Invalid OPCODE 0xab, will not execute.
Probing for SST SST25VF010, 128 kB: Invalid OPCODE 0x90, will not execute.
Probing for SST SST25VF016B, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25VF032B, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25VF064C, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25VF040, 512 kB: Invalid OPCODE 0x90, will not execute.
Probing for SST SST25VF040B, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25VF040B.REMS, 512 kB: Invalid OPCODE 0x90, will not execute.
Probing for SST SST25VF080B, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P05-A, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P05, 64 kB: Ignoring RES in favour of RDID.
Probing for ST M25P10-A, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P10, 128 kB: Ignoring RES in favour of RDID.
Probing for ST M25P20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P40-old, 512 kB: Ignoring RES in favour of RDID.
Probing for ST M25P80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P128, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25PX16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25PX32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25PX64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q128, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X10, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Unknown SFDP-capable chip, 0 kB: Invalid OPCODE 0x5a, will not execute.
Receiving SFDP signature failed.
Probing for AMIC unknown AMIC SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel unknown Atmel SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon unknown Eon SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix unknown Macronix SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC unknown PMC SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST unknown SST SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST unknown ST SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Sanyo unknown Sanyo SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Generic unknown SPI chip (RDID), 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Generic unknown SPI chip (REMS), 0 kB: Invalid OPCODE 0x90, will not execute.
Probing for Atmel AT49LH002, 256 kB: probe_82802ab: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 82802AB, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 82802AC, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm49FL002, 256 kB: probe_jedec_common: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm49FL004, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Sharp LHF00L04, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF002A/B, 256 kB: probe_jedec_common: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF003A/B, 384 kB: probe_jedec_common: id1 0xf0, id2 0xe2, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF004A/B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF004C, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF008A, 1024 kB: probe_jedec_common: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF008C, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF016C, 2048 kB: Chip size 2048 kB is bigger than supported size 1024 kB of chipset/board/programmer for FWH interface, probe/read/erase/write may fail. probe_82802ab: id1 0xf0, id2 0xe2, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW040A, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW040B, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW080A, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW080B, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW002, 256 kB: probe_82802ab: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW016, 2048 kB: Chip size 2048 kB is bigger than supported size 1024 kB of chipset/board/programmer for FWH interface, probe/read/erase/write may fail. probe_82802ab: id1 0xf0, id2 0xe2, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW040, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW080, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FA, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FB, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FC, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W49V002FA, 256 kB: probe_jedec_common: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V080FA, 1024 kB: probe_jedec_common: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V080FA (dual mode), 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Found Macronix flash chip "MX25L6405" (8192 kB, SPI).
Reading flash... done.
Restoring MMIO space at 0x858a0
Restoring PCI config space for 00:1f:0 reg 0xdc
