DarwinDumper Report Version: 2.8.8

Development location: http://www.projectosx.com
Date: Mon May 26 01:26:55 MSK 2014Mac Model: iMac14,2
CPU: Intel(R) Core(TM) i5-4670 CPU @ 3.40GHz
Graphics: NVIDIA GeForce GTX 775M
Audio: NVidia (Unknown)/ Cirrus Logic CS4206/
Operating System
Mavericks
Build: 13D65

Note: A complete dump contains more information than shown in this .htm report. If submitting a report for help then please supply the containing directory, not just this file.

ACPI Tables
APIC

View File APIC.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/APIC.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [APIC]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "APIC" [Multiple APIC Description Table (MADT)]
[004h 0004 4] Table Length : 000000BC
[008h 0008 1] Revision : 02
[009h 0009 1] Checksum : 59
[00Ah 0010 6] Oem ID : "APPLE "
[010h 0016 8] Oem Table ID : "Apple00"
[018h 0024 4] Oem Revision : 00000001
[01Ch 0028 4] Asl Compiler ID : "Loki"
[020h 0032 4] Asl Compiler Revision : 0000005F
[024h 0036 4] Local Apic Address : FEE00000
[028h 0040 4] Flags (decoded below) : 00000001
PC-AT Compatibility : 1
[02Ch 0044 1] Subtable Type : 00 [Processor Local APIC]
[02Dh 0045 1] Length : 08
[02Eh 0046 1] Processor ID : 01
[02Fh 0047 1] Local Apic ID : 00
[030h 0048 4] Flags (decoded below) : 00000001
Processor Enabled : 1
[034h 0052 1] Subtable Type : 00 [Processor Local APIC]
[035h 0053 1] Length : 08
[036h 0054 1] Processor ID : 02
[037h 0055 1] Local Apic ID : 02
[038h 0056 4] Flags (decoded below) : 00000001
Processor Enabled : 1
[03Ch 0060 1] Subtable Type : 00 [Processor Local APIC]
[03Dh 0061 1] Length : 08
[03Eh 0062 1] Processor ID : 03
[03Fh 0063 1] Local Apic ID : 04
[040h 0064 4] Flags (decoded below) : 00000001
Processor Enabled : 1
[044h 0068 1] Subtable Type : 00 [Processor Local APIC]
[045h 0069 1] Length : 08
[046h 0070 1] Processor ID : 04
[047h 0071 1] Local Apic ID : 06
[048h 0072 4] Flags (decoded below) : 00000001
Processor Enabled : 1
[04Ch 0076 1] Subtable Type : 00 [Processor Local APIC]
[04Dh 0077 1] Length : 08
[04Eh 0078 1] Processor ID : 05
[04Fh 0079 1] Local Apic ID : FF
[050h 0080 4] Flags (decoded below) : 00000000
Processor Enabled : 0
[054h 0084 1] Subtable Type : 00 [Processor Local APIC]
[055h 0085 1] Length : 08
[056h 0086 1] Processor ID : 06
[057h 0087 1] Local Apic ID : FF
[058h 0088 4] Flags (decoded below) : 00000000
Processor Enabled : 0
[05Ch 0092 1] Subtable Type : 00 [Processor Local APIC]
[05Dh 0093 1] Length : 08
[05Eh 0094 1] Processor ID : 07
[05Fh 0095 1] Local Apic ID : FF
[060h 0096 4] Flags (decoded below) : 00000000
Processor Enabled : 0
[064h 0100 1] Subtable Type : 00 [Processor Local APIC]
[065h 0101 1] Length : 08
[066h 0102 1] Processor ID : 08
[067h 0103 1] Local Apic ID : FF
[068h 0104 4] Flags (decoded below) : 00000000
Processor Enabled : 0
[06Ch 0108 1] Subtable Type : 01 [I/O APIC]
[06Dh 0109 1] Length : 0C
[06Eh 0110 1] I/O Apic ID : 02
[06Fh 0111 1] Reserved : 00
[070h 0112 4] Address : FEC00000
[074h 0116 4] Interrupt : 00000000
[078h 0120 1] Subtable Type : 02 [Interrupt Source Override]
[079h 0121 1] Length : 0A
[07Ah 0122 1] Bus : 00
[07Bh 0123 1] Source : 00
[07Ch 0124 4] Interrupt : 00000002
[080h 0128 2] Flags (decoded below) : 0000
Polarity : 0
Trigger Mode : 0
[082h 0130 1] Subtable Type : 02 [Interrupt Source Override]
[083h 0131 1] Length : 0A
[084h 0132 1] Bus : 00
[085h 0133 1] Source : 09
[086h 0134 4] Interrupt : 00000009
[08Ah 0138 2] Flags (decoded below) : 000D
Polarity : 1
Trigger Mode : 3
[08Ch 0140 1] Subtable Type : 04 [Local APIC NMI]
[08Dh 0141 1] Length : 06
[08Eh 0142 1] Processor ID : 01
[08Fh 0143 2] Flags (decoded below) : 0005
Polarity : 1
Trigger Mode : 1
[091h 0145 1] Interrupt Input LINT : 01
[092h 0146 1] Subtable Type : 04 [Local APIC NMI]
[093h 0147 1] Length : 06
[094h 0148 1] Processor ID : 02
[095h 0149 2] Flags (decoded below) : 0005
Polarity : 1
Trigger Mode : 1
[097h 0151 1] Interrupt Input LINT : 01
[098h 0152 1] Subtable Type : 04 [Local APIC NMI]
[099h 0153 1] Length : 06
[09Ah 0154 1] Processor ID : 03
[09Bh 0155 2] Flags (decoded below) : 0005
Polarity : 1
Trigger Mode : 1
[09Dh 0157 1] Interrupt Input LINT : 01
[09Eh 0158 1] Subtable Type : 04 [Local APIC NMI]
[09Fh 0159 1] Length : 06
[0A0h 0160 1] Processor ID : 04
[0A1h 0161 2] Flags (decoded below) : 0005
Polarity : 1
Trigger Mode : 1
[0A3h 0163 1] Interrupt Input LINT : 01
[0A4h 0164 1] Subtable Type : 04 [Local APIC NMI]
[0A5h 0165 1] Length : 06
[0A6h 0166 1] Processor ID : 05
[0A7h 0167 2] Flags (decoded below) : 0005
Polarity : 1
Trigger Mode : 1
[0A9h 0169 1] Interrupt Input LINT : 01
[0AAh 0170 1] Subtable Type : 04 [Local APIC NMI]
[0ABh 0171 1] Length : 06
[0ACh 0172 1] Processor ID : 06
[0ADh 0173 2] Flags (decoded below) : 0005
Polarity : 1
Trigger Mode : 1
[0AFh 0175 1] Interrupt Input LINT : 01
[0B0h 0176 1] Subtable Type : 04 [Local APIC NMI]
[0B1h 0177 1] Length : 06
[0B2h 0178 1] Processor ID : 07
[0B3h 0179 2] Flags (decoded below) : 0005
Polarity : 1
Trigger Mode : 1
[0B5h 0181 1] Interrupt Input LINT : 01
[0B6h 0182 1] Subtable Type : 04 [Local APIC NMI]
[0B7h 0183 1] Length : 06
[0B8h 0184 1] Processor ID : 08
[0B9h 0185 2] Flags (decoded below) : 0005
Polarity : 1
Trigger Mode : 1
[0BBh 0187 1] Interrupt Input LINT : 01
Raw Table Data: Length 188 (0xBC)
0000: 41 50 49 43 BC 00 00 00 02 59 41 50 50 4C 45 20 APIC.....YAPPLE
0010: 41 70 70 6C 65 30 30 00 01 00 00 00 4C 6F 6B 69 Apple00.....Loki
0020: 5F 00 00 00 00 00 E0 FE 01 00 00 00 00 08 01 00 _...............
0030: 01 00 00 00 00 08 02 02 01 00 00 00 00 08 03 04 ................
0040: 01 00 00 00 00 08 04 06 01 00 00 00 00 08 05 FF ................
0050: 00 00 00 00 00 08 06 FF 00 00 00 00 00 08 07 FF ................
0060: 00 00 00 00 00 08 08 FF 00 00 00 00 01 0C 02 00 ................
0070: 00 00 C0 FE 00 00 00 00 02 0A 00 00 02 00 00 00 ................
0080: 00 00 02 0A 00 09 09 00 00 00 0D 00 04 06 01 05 ................
0090: 00 01 04 06 02 05 00 01 04 06 03 05 00 01 04 06 ................
00A0: 04 05 00 01 04 06 05 05 00 01 04 06 06 05 00 01 ................
00B0: 04 06 07 05 00 01 04 06 08 05 00 01 ............

DMAR

View File DMAR.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/DMAR.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [DMAR]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "DMAR" [DMA Remapping table]
[004h 0004 4] Table Length : 00000088
[008h 0008 1] Revision : 01
[009h 0009 1] Checksum : DA
[00Ah 0010 6] Oem ID : "APPLE "
[010h 0016 8] Oem Table ID : "HSW "
[018h 0024 4] Oem Revision : 00000001
[01Ch 0028 4] Asl Compiler ID : "AAPL"
[020h 0032 4] Asl Compiler Revision : 00000001
[024h 0036 1] Host Address Width : 26
[025h 0037 1] Flags : 01
[026h 0038 10] Reserved : 00 00 00 00 00 00 00 00 00 00
[030h 0048 2] Subtable Type : 0000 [Hardware Unit Definition]
[032h 0050 2] Length : 0018
[034h 0052 1] Flags : 00
[035h 0053 1] Reserved : 00
[036h 0054 2] PCI Segment Number : 0000
[038h 0056 8] Register Base Address : 00000000FED90000
[040h 0064 1] Device Scope Entry Type : 01
[041h 0065 1] Entry Length : 08
[042h 0066 2] Reserved : 0000
[044h 0068 1] Enumeration ID : 00
[045h 0069 1] PCI Bus Number : 00
[046h 0070 2] PCI Path : 02,00
[048h 0072 2] Subtable Type : 0000 [Hardware Unit Definition]
[04Ah 0074 2] Length : 0020
[04Ch 0076 1] Flags : 01
[04Dh 0077 1] Reserved : 00
[04Eh 0078 2] PCI Segment Number : 0000
[050h 0080 8] Register Base Address : 00000000FED91000
[058h 0088 1] Device Scope Entry Type : 03
[059h 0089 1] Entry Length : 08
[05Ah 0090 2] Reserved : 0000
[05Ch 0092 1] Enumeration ID : 02
[05Dh 0093 1] PCI Bus Number : F0
[05Eh 0094 2] PCI Path : 1F,00
[060h 0096 1] Device Scope Entry Type : 04
[061h 0097 1] Entry Length : 08
[062h 0098 2] Reserved : 0000
[064h 0100 1] Enumeration ID : 00
[065h 0101 1] PCI Bus Number : F0
[066h 0102 2] PCI Path : 0F,00
[068h 0104 2] Subtable Type : 0001 [Reserved Memory Region]
[06Ah 0106 2] Length : 0020
[06Ch 0108 2] Reserved : 0000
[06Eh 0110 2] PCI Segment Number : 0000
[070h 0112 8] Base Address : 000000008D800000
[078h 0120 8] End Address (limit) : 000000008F9FFFFF
[080h 0128 1] Device Scope Entry Type : 01
[081h 0129 1] Entry Length : 08
[082h 0130 2] Reserved : 0000
[084h 0132 1] Enumeration ID : 00
[085h 0133 1] PCI Bus Number : 00
[086h 0134 2] PCI Path : 02,00
Raw Table Data: Length 136 (0x88)
0000: 44 4D 41 52 88 00 00 00 01 DA 41 50 50 4C 45 20 DMAR......APPLE
0010: 48 53 57 20 00 00 00 00 01 00 00 00 41 41 50 4C HSW ........AAPL
0020: 01 00 00 00 26 01 00 00 00 00 00 00 00 00 00 00 ....&...........
0030: 00 00 18 00 00 00 00 00 00 00 D9 FE 00 00 00 00 ................
0040: 01 08 00 00 00 00 02 00 00 00 20 00 01 00 00 00 .......... .....
0050: 00 10 D9 FE 00 00 00 00 03 08 00 00 02 F0 1F 00 ................
0060: 04 08 00 00 00 F0 0F 00 01 00 20 00 00 00 00 00 .......... .....
0070: 00 00 80 8D 00 00 00 00 FF FF 9F 8F 00 00 00 00 ................
0080: 01 08 00 00 00 00 02 00 ........

DSDT

View File DSDT.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/DSDT.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "DSDT"
* Length 0x0000663B (26171)
* Revision 0x03
* Checksum 0x05
* OEM ID "APPLE "
* OEM Table ID "iMac"
* OEM Revision 0x00410002 (4259842)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/DSDT.aml", "DSDT", 3, "APPLE ", "iMac", 0x00410002)
{
/*
* iASL Warning: There were 6 external control methods found during
* disassembly, but additional ACPI tables to resolve these externals
* were not specified. This resulting disassembler output file may not
* compile because the disassembler did not know how many arguments
* to assign to these methods. To specify the tables needed to resolve
* external control method references, use the one of the following
* example iASL invocations:
* iasl -e <ssdt1.aml,ssdt2.aml...> -d <dsdt.aml>
* iasl -e <dsdt.aml,ssdt2.aml...> -d <ssdt1.aml>
*/
External (_SB_.PCI0.DTLK, MethodObj) // Warning: Unresolved Method, guessing 0 arguments (may be incorrect, see warning above)
External (_SB_.PCI0.RMCR, MethodObj) // Warning: Unresolved Method, guessing 0 arguments (may be incorrect, see warning above)
External (_SB_.PCI0.RMCW, MethodObj) // Warning: Unresolved Method, guessing 0 arguments (may be incorrect, see warning above)
External (_SB_.PCI0.TGPE, MethodObj) // Warning: Unresolved Method, guessing 0 arguments (may be incorrect, see warning above)
External (HDOS, MethodObj) // Warning: Unresolved Method, guessing 0 arguments (may be incorrect, see warning above)
External (HNOT, MethodObj) // Warning: Unresolved Method, guessing 1 arguments (may be incorrect, see warning above)
External (_SB_.PCI0.DTBP)
External (_SB_.PCI0.P0P2.GFX0)
External (_SB_.PCI0.P0P2.GFX0.DID0)
External (_SB_.PCI0.P0P2.GFX0.VID0)
External (_SB_.PCI0.XHC1)
External (_SB_.SDTB, BuffObj)
External (IDAB)
External (PDC0)
External (PDC1)
External (PDC2)
External (PDC3)
External (PDC4)
External (PDC5)
External (PDC6)
External (PDC7)
External (SNXD)
Name (SP2O, 0x4E)
Name (SP1O, 0x164E)
Name (IO1B, 0x0600)
Name (IO1L, 0x70)
Name (IO2B, 0x0680)
Name (IO2L, 0x20)
Name (IO3B, 0x0290)
Name (IO3L, 0x10)
Name (SP3O, 0x2E)
Name (IO4B, 0x0A20)
Name (IO4L, 0x20)
Name (MCHB, 0xFED10000)
Name (MCHL, 0x4000)
Name (EGPB, 0xFED19000)
Name (EGPL, 0x1000)
Name (DMIB, 0xFED18000)
Name (DMIL, 0x1000)
Name (IFPB, 0xFED14000)
Name (IFPL, 0x1000)
Name (PEBS, 0xE0000000)
Name (PELN, 0x04000000)
Name (TTTB, 0xFED20000)
Name (TTTL, 0x00020000)
Name (SMBS, 0xEFA0)
Name (SMBL, 0x10)
Name (PBLK, 0x0410)
Name (PMLN, 0x80)
Name (LVL2, 0x0414)
Name (LVL3, 0x0415)
Name (LVL4, 0x0416)
Name (SMIP, 0xB2)
Name (GPBS, 0x0800)
Name (GPLN, 0x80)
Name (APCB, 0xFEC00000)
Name (APCL, 0x1000)
Name (PM30, 0x0430)
Name (SRCB, 0xFED1C000)
Name (SRCL, 0x4000)
Name (SUSW, 0xFF)
Name (HPTB, 0xFED00000)
Name (HPTC, 0xFED1F404)
Name (ACPH, 0xDE)
Name (ASSB, 0x00)
Name (AOTB, 0x00)
Name (AAXB, 0x00)
Name (PEHP, 0x01)
Name (SHPC, 0x01)
Name (PEPM, 0x01)
Name (PEER, 0x01)
Name (PECS, 0x01)
Name (ITKE, 0x00)
Name (DSSP, 0x00)
Name (FHPP, 0x01)
Name (FMBL, 0x01)
Name (FDTP, 0x02)
Name (BSH, 0x00)
Name (BEL, 0x01)
Name (BEH, 0x02)
Name (BRH, 0x03)
Name (BTF, 0x04)
Name (BHC, 0x05)
Name (BYB, 0x06)
Name (BPH, 0x07)
Name (BSHS, 0x08)
Name (BELS, 0x09)
Name (BRHS, 0x0A)
Name (BTFS, 0x0B)
Name (BEHS, 0x0C)
Name (BPHS, 0x0D)
Name (BTL, 0x10)
Name (BOF, 0x20)
Name (BEF, 0x21)
Name (BLLE, 0x22)
Name (BLLC, 0x23)
Name (BLCA, 0x24)
Name (TCGM, 0x01)
Name (TRTP, 0x01)
Name (TRTD, 0x02)
Name (TRTI, 0x03)
Name (GCDD, 0x01)
Name (DSTA, 0x0A)
Name (DSLO, 0x0C)
Name (DSLC, 0x0E)
Name (PITS, 0x10)
Name (SBCS, 0x12)
Name (SALS, 0x13)
Name (LSSS, 0x2A)
Name (SOOT, 0x35)
Name (PDBR, 0x4D)
Name (WOWE, 0x00)
Name (TAPD, 0x00)
OperationRegion (GNVS, SystemMemory, 0x8CD3EA90, 0x026D)
Field (GNVS, AnyAcc, Lock, Preserve)
{
OSYS, 16,
SMIF, 8,
PRM0, 8,
PRM1, 8,
SCIF, 8,
PRM2, 8,
PRM3, 8,
LCKF, 8,
PRM4, 8,
PRM5, 8,
P80D, 32,
LIDS, 8,
PWRS, 8,
DBGS, 8,
THOF, 8,
ACT1, 8,
ACTT, 8,
PSVT, 8,
TC1V, 8,
TC2V, 8,
TSPV, 8,
CRTT, 8,
DTSE, 8,
DTS1, 8,
DTS2, 8,
DTSF, 8,
Offset (0x25),
REVN, 8,
Offset (0x28),
APIC, 8,
TCNT, 8,
PCP0, 8,
PCP1, 8,
PPCM, 8,
PPMF, 32,
C67L, 8,
NATP, 8,
CMAP, 8,
CMBP, 8,
LPTP, 8,
FDCP, 8,
CMCP, 8,
CIRP, 8,
SMSC, 8,
W381, 8,
SMC1, 8,
EMAE, 8,
EMAP, 16,
EMAL, 16,
Offset (0x42),
MEFE, 8,
DSTS, 8,
Offset (0x46),
TPMP, 8,
TPME, 8,
MORD, 8,
TCGP, 8,
PPRP, 32,
PPRQ, 8,
LPPR, 8,
GTF0, 56,
GTF2, 56,
IDEM, 8,
GTF1, 56,
BDID, 8,
Offset (0x78),
OSCC, 8,
NEXP, 8,
SDGV, 8,
SDDV, 8,
Offset (0x81),
DSEN, 8,
ECON, 8,
GPIC, 8,
CTYP, 8,
L01C, 8,
VFN0, 8,
VFN1, 8,
ATMC, 8,
PTMC, 8,
ATRA, 8,
PTRA, 8,
PNHM, 32,
TBAB, 32,
TBAH, 32,
RTIP, 8,
TSOD, 8,
ATPC, 8,
PTPC, 8,
PFLV, 8,
BREV, 8,
DPBM, 8,
DPCM, 8,
DPDM, 8,
SDID, 8,
BLCP, 8,
BLCC, 8,
Offset (0xA5),
BLCT, 32,
BLCB, 32,
Offset (0xB2),
NHIB, 32,
GVNV, 32,
MM64, 8,
Offset (0x12C),
SARV, 32,
ASLB, 32,
IMON, 8,
IGDS, 8,
CADL, 8,
PADL, 8,
CSTE, 16,
NSTE, 16,
DID9, 32,
DIDA, 32,
DIDB, 32,
IBTT, 8,
IPAT, 8,
IPSC, 8,
IBLC, 8,
IBIA, 8,
ISSC, 8,
IPCF, 8,
IDMS, 8,
IF1E, 8,
HVCO, 8,
NXD1, 32,
NXD2, 32,
NXD3, 32,
NXD4, 32,
NXD5, 32,
NXD6, 32,
NXD7, 32,
NXD8, 32,
GSMI, 8,
PAVP, 8,
GLID, 8,
KSV0, 32,
KSV1, 8,
BBAR, 32,
BLCS, 8,
BRTL, 8,
ALSE, 8,
ALAF, 8,
LLOW, 8,
LHIH, 8,
ALFP, 8,
AUDA, 32,
AUDB, 32,
AUDC, 32,
DIDC, 32,
DIDD, 32,
DIDE, 32,
DIDF, 32,
CADR, 32,
CCNT, 8,
Offset (0x1F4),
SGMD, 8,
SGFL, 8,
PWOK, 8,
HLRS, 8,
PWEN, 8,
PRST, 8,
CPSP, 32,
EECP, 8,
EVCP, 16,
XBAS, 32,
GBAS, 16,
SGGP, 8,
NVGA, 32,
NVHA, 32,
AMDA, 32,
NDID, 8,
DID1, 32,
DID2, 32,
DID3, 32,
DID4, 32,
DID5, 32,
DID6, 32,
DID7, 32,
DID8, 32,
OBS1, 32,
OBS2, 32,
OBS3, 32,
OBS4, 32,
OBS5, 32,
OBS6, 32,
OBS7, 32,
OBS8, 32,
LTRA, 8,
OBFA, 8,
LTRB, 8,
OBFB, 8,
LTRC, 8,
OBFC, 8,
SMSL, 16,
SNSL, 16,
P0UB, 8,
P1UB, 8,
P2UB, 8,
EDPV, 8,
NXDX, 32,
DIDX, 32,
PCSL, 8,
SC7A, 8
}
Scope (\_SB)
{
Name (PR00, Package (0x1D)
{
Package (0x04)
{
0x001FFFFF,
0x00,
LNKF,
0x00
},
Package (0x04)
{
0x001FFFFF,
0x01,
LNKD,
0x00
},
Package (0x04)
{
0x001FFFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0x001FFFFF,
0x03,
LNKA,
0x00
},
Package (0x04)
{
0x0014FFFF,
0x00,
LNKA,
0x00
},
Package (0x04)
{
0x001DFFFF,
0x00,
LNKG,
0x00
},
Package (0x04)
{
0x001DFFFF,
0x01,
LNKD,
0x00
},
Package (0x04)
{
0x001DFFFF,
0x02,
LNKA,
0x00
},
Package (0x04)
{
0x001DFFFF,
0x03,
LNKC,
0x00
},
Package (0x04)
{
0x001AFFFF,
0x00,
LNKH,
0x00
},
Package (0x04)
{
0x001AFFFF,
0x01,
LNKF,
0x00
},
Package (0x04)
{
0x001AFFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0x001AFFFF,
0x03,
LNKD,
0x00
},
Package (0x04)
{
0x001BFFFF,
0x00,
LNKG,
0x00
},
Package (0x04)
{
0x0018FFFF,
0x00,
LNKE,
0x00
},
Package (0x04)
{
0x0019FFFF,
0x00,
LNKE,
0x00
},
Package (0x04)
{
0x0016FFFF,
0x00,
LNKA,
0x00
},
Package (0x04)
{
0x0016FFFF,
0x01,
LNKD,
0x00
},
Package (0x04)
{
0x0016FFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0x0016FFFF,
0x03,
LNKB,
0x00
},
Package (0x04)
{
0x001CFFFF,
0x00,
LNKA,
0x00
},
Package (0x04)
{
0x001CFFFF,
0x01,
LNKB,
0x00
},
Package (0x04)
{
0x001CFFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0x001CFFFF,
0x03,
LNKD,
0x00
},
Package (0x04)
{
0x0001FFFF,
0x00,
LNKA,
0x00
},
Package (0x04)
{
0x0001FFFF,
0x01,
LNKB,
0x00
},
Package (0x04)
{
0x0001FFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0x0001FFFF,
0x03,
LNKD,
0x00
},
Package (0x04)
{
0x0002FFFF,
0x00,
LNKA,
0x00
}
})
Name (AR00, Package (0x1D)
{
Package (0x04)
{
0x001FFFFF,
0x00,
0x00,
0x15
},
Package (0x04)
{
0x001FFFFF,
0x01,
0x00,
0x13
},
Package (0x04)
{
0x001FFFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0x001FFFFF,
0x03,
0x00,
0x10
},
Package (0x04)
{
0x0014FFFF,
0x00,
0x00,
0x10
},
Package (0x04)
{
0x001DFFFF,
0x00,
0x00,
0x16
},
Package (0x04)
{
0x001DFFFF,
0x01,
0x00,
0x13
},
Package (0x04)
{
0x001DFFFF,
0x02,
0x00,
0x10
},
Package (0x04)
{
0x001DFFFF,
0x03,
0x00,
0x12
},
Package (0x04)
{
0x001AFFFF,
0x00,
0x00,
0x17
},
Package (0x04)
{
0x001AFFFF,
0x01,
0x00,
0x15
},
Package (0x04)
{
0x001AFFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0x001AFFFF,
0x03,
0x00,
0x13
},
Package (0x04)
{
0x001BFFFF,
0x00,
0x00,
0x16
},
Package (0x04)
{
0x0018FFFF,
0x00,
0x00,
0x14
},
Package (0x04)
{
0x0019FFFF,
0x00,
0x00,
0x14
},
Package (0x04)
{
0x0016FFFF,
0x00,
0x00,
0x10
},
Package (0x04)
{
0x0016FFFF,
0x01,
0x00,
0x13
},
Package (0x04)
{
0x0016FFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0x0016FFFF,
0x03,
0x00,
0x11
},
Package (0x04)
{
0x001CFFFF,
0x00,
0x00,
0x10
},
Package (0x04)
{
0x001CFFFF,
0x01,
0x00,
0x11
},
Package (0x04)
{
0x001CFFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0x001CFFFF,
0x03,
0x00,
0x13
},
Package (0x04)
{
0x0001FFFF,
0x00,
0x00,
0x10
},
Package (0x04)
{
0x0001FFFF,
0x01,
0x00,
0x11
},
Package (0x04)
{
0x0001FFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0x0001FFFF,
0x03,
0x00,
0x13
},
Package (0x04)
{
0x0002FFFF,
0x00,
0x00,
0x10
}
})
Name (PR04, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKD,
0x00
}
})
Name (AR04, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x13
}
})
Name (PR05, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKD,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKA,
0x00
}
})
Name (AR05, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x13
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x10
}
})
Name (PR06, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKD,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKB,
0x00
}
})
Name (AR06, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x13
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x11
}
})
Name (PR07, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKD,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKC,
0x00
}
})
Name (AR07, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x13
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x12
}
})
Name (PR08, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKD,
0x00
}
})
Name (AR08, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x13
}
})
Name (PR09, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKD,
0x00
}
})
Name (AR09, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x13
}
})
Name (PR0E, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKD,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKB,
0x00
}
})
Name (AR0E, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x13
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x11
}
})
Name (PR0F, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKD,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKC,
0x00
}
})
Name (AR0F, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x13
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x12
}
})
Name (PR02, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKD,
0x00
}
})
Name (AR02, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x13
}
})
Name (PR0A, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKD,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKA,
0x00
}
})
Name (AR0A, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x13
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x10
}
})
Name (PR0B, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKC,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKD,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKB,
0x00
}
})
Name (AR0B, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x12
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x13
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x11
}
})
Name (PR0C, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKD,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKA,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKB,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKC,
0x00
}
})
Name (AR0C, Package (0x04)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x13
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x10
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x11
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x12
}
})
Name (PR01, Package (0x0C)
{
Package (0x04)
{
0xFFFF,
0x00,
LNKF,
0x00
},
Package (0x04)
{
0xFFFF,
0x01,
LNKG,
0x00
},
Package (0x04)
{
0xFFFF,
0x02,
LNKH,
0x00
},
Package (0x04)
{
0xFFFF,
0x03,
LNKE,
0x00
},
Package (0x04)
{
0x0001FFFF,
0x00,
LNKG,
0x00
},
Package (0x04)
{
0x0001FFFF,
0x01,
LNKF,
0x00
},
Package (0x04)
{
0x0001FFFF,
0x02,
LNKE,
0x00
},
Package (0x04)
{
0x0001FFFF,
0x03,
LNKH,
0x00
},
Package (0x04)
{
0x0005FFFF,
0x00,
LNKC,
0x00
},
Package (0x04)
{
0x0005FFFF,
0x01,
LNKE,
0x00
},
Package (0x04)
{
0x0005FFFF,
0x02,
LNKG,
0x00
},
Package (0x04)
{
0x0005FFFF,
0x03,
LNKF,
0x00
}
})
Name (AR01, Package (0x0C)
{
Package (0x04)
{
0xFFFF,
0x00,
0x00,
0x15
},
Package (0x04)
{
0xFFFF,
0x01,
0x00,
0x16
},
Package (0x04)
{
0xFFFF,
0x02,
0x00,
0x17
},
Package (0x04)
{
0xFFFF,
0x03,
0x00,
0x14
},
Package (0x04)
{
0x0001FFFF,
0x00,
0x00,
0x16
},
Package (0x04)
{
0x0001FFFF,
0x01,
0x00,
0x15
},
Package (0x04)
{
0x0001FFFF,
0x02,
0x00,
0x14
},
Package (0x04)
{
0x0001FFFF,
0x03,
0x00,
0x17
},
Package (0x04)
{
0x0005FFFF,
0x00,
0x00,
0x12
},
Package (0x04)
{
0x0005FFFF,
0x01,
0x00,
0x14
},
Package (0x04)
{
0x0005FFFF,
0x02,
0x00,
0x16
},
Package (0x04)
{
0x0005FFFF,
0x03,
0x00,
0x15
}
})
Name (PRSA, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, )
{3,4,5,6,7,10,11,12,14,15}
})
Alias (PRSA, PRSB)
Alias (PRSA, PRSC)
Alias (PRSA, PRSD)
Alias (PRSA, PRSE)
Alias (PRSA, PRSF)
Alias (PRSA, PRSG)
Alias (PRSA, PRSH)
Device (PCI0)
{
Name (_HID, EisaId ("PNP0A08")) // _HID: Hardware ID
Name (_CID, EisaId ("PNP0A03")) // _CID: Compatible ID
Name (_ADR, 0x00) // _ADR: Address
Method (^BN00, 0, NotSerialized)
{
Return (0x00)
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (BN00 ())
}
Name (_UID, 0x00) // _UID: Unique ID
Method (_PRT, 0, NotSerialized) // _PRT: PCI Routing Table
{
If (PICM)
{
Return (AR00 ())
}
Return (PR00 ())
}
OperationRegion (HBUS, PCI_Config, 0x00, 0x0100)
Field (HBUS, DWordAcc, NoLock, Preserve)
{
Offset (0x40),
EPEN, 1,
, 11,
EPBR, 20,
Offset (0x48),
MHEN, 1,
, 14,
MHBR, 17,
Offset (0x50),
GCLK, 1,
Offset (0x54),
D0EN, 1,
Offset (0x60),
PXEN, 1,
PXSZ, 2,
, 23,
PXBR, 6,
Offset (0x68),
DIEN, 1,
, 11,
DIBR, 20,
Offset (0x70),
, 20,
MEBR, 12,
Offset (0x80),
, 4,
PM0H, 2,
Offset (0x81),
PM1L, 2,
, 2,
PM1H, 2,
Offset (0x82),
PM2L, 2,
, 2,
PM2H, 2,
Offset (0x83),
PM3L, 2,
, 2,
PM3H, 2,
Offset (0x84),
PM4L, 2,
, 2,
PM4H, 2,
Offset (0x85),
PM5L, 2,
, 2,
PM5H, 2,
Offset (0x86),
PM6L, 2,
, 2,
PM6H, 2,
Offset (0x87),
Offset (0xA8),
, 20,
TUUD, 19,
Offset (0xBC),
, 20,
TLUD, 12,
Offset (0xC8),
, 7,
HTSE, 1
}
OperationRegion (MCHT, SystemMemory, 0xFED10000, 0x6000)
Field (MCHT, ByteAcc, NoLock, Preserve)
{
Offset (0x5994),
RPSL, 8,
Offset (0x5998),
RP0C, 8,
RP1C, 8,
RPNC, 8
}
Name (BUF0, ResourceTemplate ()
{
WordBusNumber (ResourceProducer, MinFixed, MaxFixed, PosDecode,
0x0000, // Granularity
0x0000, // Range Minimum
0x00FF, // Range Maximum
0x0000, // Translation Offset
0x0100, // Length
,, )
DWordIO (ResourceProducer, MinFixed, MaxFixed, PosDecode, EntireRange,
0x00000000, // Granularity
0x00000000, // Range Minimum
0x00000CF7, // Range Maximum
0x00000000, // Translation Offset
0x00000CF8, // Length
,, , TypeStatic)
IO (Decode16,
0x0CF8, // Range Minimum
0x0CF8, // Range Maximum
0x01, // Alignment
0x08, // Length
)
DWordIO (ResourceProducer, MinFixed, MaxFixed, PosDecode, EntireRange,
0x00000000, // Granularity
0x00000D00, // Range Minimum
0x0000FFFF, // Range Maximum
0x00000000, // Translation Offset
0x0000F300, // Length
,, , TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000A0000, // Range Minimum
0x000BFFFF, // Range Maximum
0x00000000, // Translation Offset
0x00020000, // Length
,, , AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000C0000, // Range Minimum
0x000C3FFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y00, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000C4000, // Range Minimum
0x000C7FFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y01, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000C8000, // Range Minimum
0x000CBFFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y02, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000CC000, // Range Minimum
0x000CFFFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y03, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000D0000, // Range Minimum
0x000D3FFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y04, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000D4000, // Range Minimum
0x000D7FFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y05, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000D8000, // Range Minimum
0x000DBFFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y06, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000DC000, // Range Minimum
0x000DFFFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y07, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000E0000, // Range Minimum
0x000E3FFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y08, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000E4000, // Range Minimum
0x000E7FFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y09, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000E8000, // Range Minimum
0x000EBFFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y0A, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000EC000, // Range Minimum
0x000EFFFF, // Range Maximum
0x00000000, // Translation Offset
0x00004000, // Length
,, _Y0B, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x000F0000, // Range Minimum
0x000FFFFF, // Range Maximum
0x00000000, // Translation Offset
0x00010000, // Length
,, _Y0C, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0x00000000, // Range Minimum
0xFEAFFFFF, // Range Maximum
0x00000000, // Translation Offset
0xFEB00000, // Length
,, _Y0D, AddressRangeMemory, TypeStatic)
DWordMemory (ResourceProducer, PosDecode, MinFixed, MaxFixed, Cacheable, ReadWrite,
0x00000000, // Granularity
0xFED40000, // Range Minimum
0xFED44FFF, // Range Maximum
0x00000000, // Translation Offset
0x00005000, // Length
,, , AddressRangeMemory, TypeStatic)
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
If (PM1L)
{
CreateDWordField (BUF0, \_SB.PCI0._Y00._LEN, C0LN) // _LEN: Length
Store (Zero, C0LN)
}
If (LEqual (PM1L, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y00._RW, C0RW) // _RW_: Read-Write Status
Store (Zero, C0RW)
}
If (PM1H)
{
CreateDWordField (BUF0, \_SB.PCI0._Y01._LEN, C4LN) // _LEN: Length
Store (Zero, C4LN)
}
If (LEqual (PM1H, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y01._RW, C4RW) // _RW_: Read-Write Status
Store (Zero, C4RW)
}
If (PM2L)
{
CreateDWordField (BUF0, \_SB.PCI0._Y02._LEN, C8LN) // _LEN: Length
Store (Zero, C8LN)
}
If (LEqual (PM2L, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y02._RW, C8RW) // _RW_: Read-Write Status
Store (Zero, C8RW)
}
If (PM2H)
{
CreateDWordField (BUF0, \_SB.PCI0._Y03._LEN, CCLN) // _LEN: Length
Store (Zero, CCLN)
}
If (LEqual (PM2H, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y03._RW, CCRW) // _RW_: Read-Write Status
Store (Zero, CCRW)
}
If (PM3L)
{
CreateDWordField (BUF0, \_SB.PCI0._Y04._LEN, D0LN) // _LEN: Length
Store (Zero, D0LN)
}
If (LEqual (PM3L, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y04._RW, D0RW) // _RW_: Read-Write Status
Store (Zero, D0RW)
}
If (PM3H)
{
CreateDWordField (BUF0, \_SB.PCI0._Y05._LEN, D4LN) // _LEN: Length
Store (Zero, D4LN)
}
If (LEqual (PM3H, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y05._RW, D4RW) // _RW_: Read-Write Status
Store (Zero, D4RW)
}
If (PM4L)
{
CreateDWordField (BUF0, \_SB.PCI0._Y06._LEN, D8LN) // _LEN: Length
Store (Zero, D8LN)
}
If (LEqual (PM4L, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y06._RW, D8RW) // _RW_: Read-Write Status
Store (Zero, D8RW)
}
If (PM4H)
{
CreateDWordField (BUF0, \_SB.PCI0._Y07._LEN, DCLN) // _LEN: Length
Store (Zero, DCLN)
}
If (LEqual (PM4H, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y07._RW, DCRW) // _RW_: Read-Write Status
Store (Zero, DCRW)
}
If (PM5L)
{
CreateDWordField (BUF0, \_SB.PCI0._Y08._LEN, E0LN) // _LEN: Length
Store (Zero, E0LN)
}
If (LEqual (PM5L, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y08._RW, E0RW) // _RW_: Read-Write Status
Store (Zero, E0RW)
}
If (PM5H)
{
CreateDWordField (BUF0, \_SB.PCI0._Y09._LEN, E4LN) // _LEN: Length
Store (Zero, E4LN)
}
If (LEqual (PM5H, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y09._RW, E4RW) // _RW_: Read-Write Status
Store (Zero, E4RW)
}
If (PM6L)
{
CreateDWordField (BUF0, \_SB.PCI0._Y0A._LEN, E8LN) // _LEN: Length
Store (Zero, E8LN)
}
If (LEqual (PM6L, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y0A._RW, E8RW) // _RW_: Read-Write Status
Store (Zero, E8RW)
}
If (PM6H)
{
CreateDWordField (BUF0, \_SB.PCI0._Y0B._LEN, ECLN) // _LEN: Length
Store (Zero, ECLN)
}
If (LEqual (PM6H, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y0B._RW, ECRW) // _RW_: Read-Write Status
Store (Zero, ECRW)
}
If (PM0H)
{
CreateDWordField (BUF0, \_SB.PCI0._Y0C._LEN, F0LN) // _LEN: Length
Store (Zero, F0LN)
}
If (LEqual (PM0H, 0x01))
{
CreateBitField (BUF0, \_SB.PCI0._Y0C._RW, F0RW) // _RW_: Read-Write Status
Store (Zero, F0RW)
}
CreateDWordField (BUF0, \_SB.PCI0._Y0D._MIN, M1MN) // _MIN: Minimum Base Address
CreateDWordField (BUF0, \_SB.PCI0._Y0D._MAX, M1MX) // _MAX: Maximum Base Address
CreateDWordField (BUF0, \_SB.PCI0._Y0D._LEN, M1LN) // _LEN: Length
ShiftLeft (TLUD, 0x14, M1MN)
Add (Subtract (M1MX, M1MN), 0x01, M1LN)
Return (BUF0)
}
Name (GUID, Buffer (0x10)
{
/* 0000 */ 0x5B, 0x4D, 0xDB, 0x33, 0xF7, 0x1F, 0x1C, 0x40,
/* 0008 */ 0x96, 0x57, 0x74, 0x41, 0xC0, 0x3D, 0xD7, 0x66
})
Name (SUPP, 0x00)
Name (CTRL, 0x00)
Method (_OSC, 4, Serialized) // _OSC: Operating System Capabilities
{
Store (Arg3, Local0)
CreateDWordField (Local0, 0x00, CDW1)
CreateDWordField (Local0, 0x04, CDW2)
CreateDWordField (Local0, 0x08, CDW3)
Store (CDW2, SUPP)
Store (CDW3, CTRL)
If (LEqual (0x01, OSDW ()))
{
If (LAnd (LEqual (Arg0, GUID), NEXP))
{
If (Not (And (CDW1, 0x01)))
{
If (And (CTRL, 0x02))
{
NHPG ()
}
If (And (CTRL, 0x04))
{
NPME ()
}
}
If (LNotEqual (Arg1, One))
{
Or (CDW1, 0x08, CDW1)
}
If (LNotEqual (CDW3, CTRL))
{
Or (CDW1, 0x10, CDW1)
}
Store (CTRL, CDW3)
Store (CTRL, OSCC)
Return (Local0)
}
Else
{
Or (CDW1, 0x04, CDW1)
Return (Local0)
}
}
Else
{
If (LEqual (Arg0, GUID))
{
If (LEqual (\_SB.PCI0.DTBP, 0x01))
{
And (CDW3, 0xFFFFFFFB, CDW3)
}
}
Return (Local0)
}
}
Scope (\_SB.PCI0)
{
Method (AR00, 0, NotSerialized)
{
Return (\_SB.AR00)
}
Method (PR00, 0, NotSerialized)
{
Return (\_SB.PR00)
}
Method (AR01, 0, NotSerialized)
{
Return (\_SB.AR01)
}
Method (PR01, 0, NotSerialized)
{
Return (\_SB.PR01)
}
Method (AR02, 0, NotSerialized)
{
Return (\_SB.AR02)
}
Method (PR02, 0, NotSerialized)
{
Return (\_SB.PR02)
}
Method (AR04, 0, NotSerialized)
{
Return (\_SB.AR04)
}
Method (PR04, 0, NotSerialized)
{
Return (\_SB.PR04)
}
Method (AR05, 0, NotSerialized)
{
Return (\_SB.AR05)
}
Method (PR05, 0, NotSerialized)
{
Return (\_SB.PR05)
}
Method (AR06, 0, NotSerialized)
{
Return (\_SB.AR06)
}
Method (PR06, 0, NotSerialized)
{
Return (\_SB.PR06)
}
Method (AR07, 0, NotSerialized)
{
Return (\_SB.AR07)
}
Method (PR07, 0, NotSerialized)
{
Return (\_SB.PR07)
}
Method (AR08, 0, NotSerialized)
{
Return (\_SB.AR08)
}
Method (PR08, 0, NotSerialized)
{
Return (\_SB.PR08)
}
Method (AR09, 0, NotSerialized)
{
Return (\_SB.AR09)
}
Method (PR09, 0, NotSerialized)
{
Return (\_SB.PR09)
}
Method (AR0A, 0, NotSerialized)
{
Return (\_SB.AR0A)
}
Method (PR0A, 0, NotSerialized)
{
Return (\_SB.PR0A)
}
Method (AR0B, 0, NotSerialized)
{
Return (\_SB.AR0B)
}
Method (PR0B, 0, NotSerialized)
{
Return (\_SB.PR0B)
}
}
Device (MCHC)
{
Name (_ADR, 0x00) // _ADR: Address
}
Device (P0P2)
{
Name (_ADR, 0x00010000) // _ADR: Address
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x03
})
}
}
Method (_PRT, 0, NotSerialized) // _PRT: PCI Routing Table
{
If (PICM)
{
Return (AR02 ())
}
Return (PR02 ())
}
}
Device (IGPU)
{
Name (_ADR, 0x00020000) // _ADR: Address
OperationRegion (GFXH, PCI_Config, 0x00, 0x40)
Field (GFXH, ByteAcc, NoLock, Preserve)
{
VID0, 16,
DID0, 16
}
Method (PCPC, 0, NotSerialized)
{
}
Method (PAPR, 0, NotSerialized)
{
Return (0x00)
}
Method (_DOS, 1, NotSerialized) // _DOS: Disable Output Switching
{
Store (And (Arg0, 0x07), DSEN)
If (LEqual (And (Arg0, 0x03), 0x00))
{
If (CondRefOf (HDOS))
{
HDOS ()
}
}
}
Method (_DOD, 0, NotSerialized) // _DOD: Display Output Devices
{
If (CondRefOf (IDAB)) {}
Else
{
Store (0x00, NDID)
If (LNotEqual (DIDL, Zero))
{
Store (SDDL (DIDL), DID1)
}
If (LNotEqual (DDL2, Zero))
{
Store (SDDL (DDL2), DID2)
}
If (LNotEqual (DDL3, Zero))
{
Store (SDDL (DDL3), DID3)
}
If (LNotEqual (DDL4, Zero))
{
Store (SDDL (DDL4), DID4)
}
If (LNotEqual (DDL5, Zero))
{
Store (SDDL (DDL5), DID5)
}
If (LNotEqual (DDL6, Zero))
{
Store (SDDL (DDL6), DID6)
}
If (LNotEqual (DDL7, Zero))
{
Store (SDDL (DDL7), DID7)
}
If (LNotEqual (DDL8, Zero))
{
Store (SDDL (DDL8), DID8)
}
}
If (LEqual (NDID, 0x01))
{
Name (TMP1, Package (0x01)
{
0xFFFFFFFF
})
Store (Or (0x00010000, DID1), Index (TMP1, 0x00))
Return (TMP1)
}
If (LEqual (NDID, 0x02))
{
Name (TMP2, Package (0x02)
{
0xFFFFFFFF,
0xFFFFFFFF
})
Store (Or (0x00010000, DID1), Index (TMP2, 0x00))
Store (Or (0x00010000, DID2), Index (TMP2, 0x01))
Return (TMP2)
}
If (LEqual (NDID, 0x03))
{
Name (TMP3, Package (0x03)
{
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF
})
Store (Or (0x00010000, DID1), Index (TMP3, 0x00))
Store (Or (0x00010000, DID2), Index (TMP3, 0x01))
Store (Or (0x00010000, DID3), Index (TMP3, 0x02))
Return (TMP3)
}
If (LEqual (NDID, 0x04))
{
Name (TMP4, Package (0x04)
{
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF
})
Store (Or (0x00010000, DID1), Index (TMP4, 0x00))
Store (Or (0x00010000, DID2), Index (TMP4, 0x01))
Store (Or (0x00010000, DID3), Index (TMP4, 0x02))
Store (Or (0x00010000, DID4), Index (TMP4, 0x03))
Return (TMP4)
}
If (LEqual (NDID, 0x05))
{
Name (TMP5, Package (0x05)
{
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF
})
Store (Or (0x00010000, DID1), Index (TMP5, 0x00))
Store (Or (0x00010000, DID2), Index (TMP5, 0x01))
Store (Or (0x00010000, DID3), Index (TMP5, 0x02))
Store (Or (0x00010000, DID4), Index (TMP5, 0x03))
Store (Or (0x00010000, DID5), Index (TMP5, 0x04))
Return (TMP5)
}
If (LEqual (NDID, 0x06))
{
Name (TMP6, Package (0x06)
{
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF
})
Store (Or (0x00010000, DID1), Index (TMP6, 0x00))
Store (Or (0x00010000, DID2), Index (TMP6, 0x01))
Store (Or (0x00010000, DID3), Index (TMP6, 0x02))
Store (Or (0x00010000, DID4), Index (TMP6, 0x03))
Store (Or (0x00010000, DID5), Index (TMP6, 0x04))
Store (Or (0x00010000, DID6), Index (TMP6, 0x05))
Return (TMP6)
}
If (LEqual (NDID, 0x07))
{
Name (TMP7, Package (0x07)
{
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF
})
Store (Or (0x00010000, DID1), Index (TMP7, 0x00))
Store (Or (0x00010000, DID2), Index (TMP7, 0x01))
Store (Or (0x00010000, DID3), Index (TMP7, 0x02))
Store (Or (0x00010000, DID4), Index (TMP7, 0x03))
Store (Or (0x00010000, DID5), Index (TMP7, 0x04))
Store (Or (0x00010000, DID6), Index (TMP7, 0x05))
Store (Or (0x00010000, DID7), Index (TMP7, 0x06))
Return (TMP7)
}
If (LEqual (NDID, 0x08))
{
Name (TMP8, Package (0x08)
{
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF,
0xFFFFFFFF
})
Store (Or (0x00010000, DID1), Index (TMP8, 0x00))
Store (Or (0x00010000, DID2), Index (TMP8, 0x01))
Store (Or (0x00010000, DID3), Index (TMP8, 0x02))
Store (Or (0x00010000, DID4), Index (TMP8, 0x03))
Store (Or (0x00010000, DID5), Index (TMP8, 0x04))
Store (Or (0x00010000, DID6), Index (TMP8, 0x05))
Store (Or (0x00010000, DID7), Index (TMP8, 0x06))
Store (Or (0x00010000, DID8), Index (TMP8, 0x07))
Return (TMP8)
}
Return (Package (0x01)
{
0x0400
})
}
Name (EDPV, 0x00)
Name (DIDX, 0x00)
Name (NXDX, 0x00)
Name (BRTN, Package (0x12)
{
0x50,
0x2F,
0x01,
0x04,
0x06,
0x09,
0x0E,
0x13,
0x1A,
0x21,
0x28,
0x2E,
0x34,
0x3A,
0x41,
0x47,
0x4E,
0x55
})
Method (ABCL, 0, NotSerialized)
{
Store (DerefOf (Index (BRTN, 0x0F)), Index (BRTN, 0x00))
Store (DerefOf (Index (BRTN, 0x0A)), Index (BRTN, 0x01))
Return (BRTN)
}
Method (ABCM, 1, NotSerialized)
{
If (LAnd (LGreaterEqual (Arg0, 0x00), LLessEqual (Arg0, 0x64)))
{
Store (Arg0, BRTL)
If (BLCP)
{
\_SB.PCI0.SBUS.BUS0.BLC0.BSET (Arg0)
Return (Zero)
}
\_SB.PCI0.IGPU.AINT (0x01, Arg0)
}
Return (Zero)
}
Method (ABQC, 0, NotSerialized)
{
Return (BRTL)
}
Device (DD01)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (And (0x0F00, DID1), 0x0302))
{
Store (0x01, EDPV)
Store (NXD1, NXDX)
Store (DID1, DIDX)
Return (0x01)
}
If (LEqual (DID1, 0x00))
{
Return (0x01)
}
Else
{
Return (And (0xFFFF, DID1))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
Return (CDDS (DID1))
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXD1)
}
Return (NDDS (DID1))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Device (DD02)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (And (0x0F00, DID2), 0x0302))
{
Store (0x02, EDPV)
Store (NXD2, NXDX)
Store (DID2, DIDX)
Return (0x02)
}
If (LEqual (DID2, 0x00))
{
Return (0x02)
}
Else
{
Return (And (0xFFFF, DID2))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
If (LEqual (LIDS, 0x00))
{
Return (0x00)
}
Return (CDDS (DID2))
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXD2)
}
Return (NDDS (DID2))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Device (DD03)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (And (0x0F00, DID3), 0x0302))
{
Store (0x03, EDPV)
Store (NXD3, NXDX)
Store (DID3, DIDX)
Return (0x03)
}
If (LEqual (DID3, 0x00))
{
Return (0x03)
}
Else
{
Return (And (0xFFFF, DID3))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
If (LEqual (DID3, 0x00))
{
Return (0x0B)
}
Else
{
Return (CDDS (DID3))
}
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXD3)
}
Return (NDDS (DID3))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Device (DD04)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (And (0x0F00, DID4), 0x0302))
{
Store (0x04, EDPV)
Store (NXD4, NXDX)
Store (DID4, DIDX)
Return (0x04)
}
If (LEqual (DID4, 0x00))
{
Return (0x04)
}
Else
{
Return (And (0xFFFF, DID4))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
If (LEqual (DID4, 0x00))
{
Return (0x0B)
}
Else
{
Return (CDDS (DID4))
}
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXD4)
}
Return (NDDS (DID4))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Device (DD05)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (And (0x0F00, DID5), 0x0302))
{
Store (0x05, EDPV)
Store (NXD5, NXDX)
Store (DID5, DIDX)
Return (0x05)
}
If (LEqual (DID5, 0x00))
{
Return (0x05)
}
Else
{
Return (And (0xFFFF, DID5))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
If (LEqual (DID5, 0x00))
{
Return (0x0B)
}
Else
{
Return (CDDS (DID5))
}
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXD5)
}
Return (NDDS (DID5))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Device (DD06)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (And (0x0F00, DID6), 0x0302))
{
Store (0x06, EDPV)
Store (NXD6, NXDX)
Store (DID6, DIDX)
Return (0x06)
}
If (LEqual (DID6, 0x00))
{
Return (0x06)
}
Else
{
Return (And (0xFFFF, DID6))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
If (LEqual (DID6, 0x00))
{
Return (0x0B)
}
Else
{
Return (CDDS (DID6))
}
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXD6)
}
Return (NDDS (DID6))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Device (DD07)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (And (0x0F00, DID7), 0x0302))
{
Store (0x07, EDPV)
Store (NXD7, NXDX)
Store (DID7, DIDX)
Return (0x07)
}
If (LEqual (DID7, 0x00))
{
Return (0x07)
}
Else
{
Return (And (0xFFFF, DID7))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
If (LEqual (DID7, 0x00))
{
Return (0x0B)
}
Else
{
Return (CDDS (DID7))
}
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXD7)
}
Return (NDDS (DID7))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Device (DD08)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (And (0x0F00, DID8), 0x0302))
{
Store (0x08, EDPV)
Store (NXD8, NXDX)
Store (DID8, DIDX)
Return (0x08)
}
If (LEqual (DID8, 0x00))
{
Return (0x08)
}
Else
{
Return (And (0xFFFF, DID8))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
If (LEqual (DID8, 0x00))
{
Return (0x0B)
}
Else
{
Return (CDDS (DID8))
}
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXD8)
}
Return (NDDS (DID8))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Device (DD1F)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
If (LEqual (EDPV, 0x00))
{
Return (0x1F)
}
Else
{
Return (And (0xFFFF, DIDX))
}
}
Method (_DCS, 0, NotSerialized) // _DCS: Display Current Status
{
If (LEqual (EDPV, 0x00))
{
Return (0x00)
}
Else
{
Return (CDDS (DIDX))
}
}
Method (_DGS, 0, NotSerialized) // _DGS: Display Graphics State
{
If (CondRefOf (SNXD))
{
Return (NXDX)
}
Return (NDDS (DIDX))
}
Method (_DSS, 1, NotSerialized) // _DSS: Device Set State
{
If (LEqual (And (Arg0, 0xC0000000), 0xC0000000))
{
Store (NSTE, CSTE)
}
}
}
Method (SDDL, 1, NotSerialized)
{
Increment (NDID)
Store (And (Arg0, 0x0F0F), Local0)
Or (0x80000000, Local0, Local1)
If (LEqual (DIDL, Local0))
{
Return (Local1)
}
If (LEqual (DDL2, Local0))
{
Return (Local1)
}
If (LEqual (DDL3, Local0))
{
Return (Local1)
}
If (LEqual (DDL4, Local0))
{
Return (Local1)
}
If (LEqual (DDL5, Local0))
{
Return (Local1)
}
If (LEqual (DDL6, Local0))
{
Return (Local1)
}
If (LEqual (DDL7, Local0))
{
Return (Local1)
}
If (LEqual (DDL8, Local0))
{
Return (Local1)
}
Return (0x00)
}
Method (CDDS, 1, NotSerialized)
{
Store (And (Arg0, 0x0F0F), Local0)
If (LEqual (0x00, Local0))
{
Return (0x1D)
}
If (LEqual (CADL, Local0))
{
Return (0x1F)
}
If (LEqual (CAL2, Local0))
{
Return (0x1F)
}
If (LEqual (CAL3, Local0))
{
Return (0x1F)
}
If (LEqual (CAL4, Local0))
{
Return (0x1F)
}
If (LEqual (CAL5, Local0))
{
Return (0x1F)
}
If (LEqual (CAL6, Local0))
{
Return (0x1F)
}
If (LEqual (CAL7, Local0))
{
Return (0x1F)
}
If (LEqual (CAL8, Local0))
{
Return (0x1F)
}
Return (0x1D)
}
Method (NDDS, 1, NotSerialized)
{
Store (And (Arg0, 0x0F0F), Local0)
If (LEqual (0x00, Local0))
{
Return (0x00)
}
If (LEqual (NADL, Local0))
{
Return (0x01)
}
If (LEqual (NDL2, Local0))
{
Return (0x01)
}
If (LEqual (NDL3, Local0))
{
Return (0x01)
}
If (LEqual (NDL4, Local0))
{
Return (0x01)
}
If (LEqual (NDL5, Local0))
{
Return (0x01)
}
If (LEqual (NDL6, Local0))
{
Return (0x01)
}
If (LEqual (NDL7, Local0))
{
Return (0x01)
}
If (LEqual (NDL8, Local0))
{
Return (0x01)
}
Return (0x00)
}
Scope (\_SB.PCI0)
{
OperationRegion (MCHP, PCI_Config, 0x40, 0xC0)
Field (MCHP, AnyAcc, NoLock, Preserve)
{
Offset (0x14),
AUDE, 8,
Offset (0x60),
TASM, 10,
Offset (0x62)
}
}
OperationRegion (IGDP, PCI_Config, 0x40, 0xC0)
Field (IGDP, AnyAcc, NoLock, Preserve)
{
Offset (0x12),
, 1,
GIVD, 1,
, 2,
GUMA, 3,
Offset (0x14),
, 4,
GMFN, 1,
Offset (0x18),
Offset (0xA4),
ASLE, 8,
Offset (0xA8),
GSSE, 1,
GSSB, 14,
GSES, 1,
Offset (0xB0),
, 12,
CDVL, 1,
Offset (0xB2),
Offset (0xB5),
LBPC, 8,
Offset (0xBC),
ASLS, 32
}
OperationRegion (IGDM, SystemMemory, ASLB, 0x2000)
Field (IGDM, AnyAcc, NoLock, Preserve)
{
SIGN, 128,
SIZE, 32,
OVER, 32,
SVER, 256,
VVER, 128,
GVER, 128,
MBOX, 32,
DMOD, 32,
Offset (0x100),
DRDY, 32,
CSTS, 32,
CEVT, 32,
Offset (0x120),
DIDL, 32,
DDL2, 32,
DDL3, 32,
DDL4, 32,
DDL5, 32,
DDL6, 32,
DDL7, 32,
DDL8, 32,
CPDL, 32,
CPL2, 32,
CPL3, 32,
CPL4, 32,
CPL5, 32,
CPL6, 32,
CPL7, 32,
CPL8, 32,
CADL, 32,
CAL2, 32,
CAL3, 32,
CAL4, 32,
CAL5, 32,
CAL6, 32,
CAL7, 32,
CAL8, 32,
NADL, 32,
NDL2, 32,
NDL3, 32,
NDL4, 32,
NDL5, 32,
NDL6, 32,
NDL7, 32,
NDL8, 32,
ASLP, 32,
TIDX, 32,
CHPD, 32,
CLID, 32,
CDCK, 32,
SXSW, 32,
EVTS, 32,
CNOT, 32,
NRDY, 32,
Offset (0x200),
SCIE, 1,
GEFC, 4,
GXFC, 3,
GESF, 8,
Offset (0x204),
PARM, 32,
DSLP, 32,
Offset (0x300),
ARDY, 32,
ASLC, 32,
TCHE, 32,
ALSI, 32,
BCLP, 32,
PFIT, 32,
CBLV, 32,
BCLM, 320,
CPFM, 32,
EPFM, 32,
PLUT, 592,
PFMB, 32,
CCDV, 32,
PCFT, 32,
Offset (0x400),
GVD1, 49152,
PHED, 32,
BDDC, 2048
}
Name (DBTB, Package (0x15)
{
0x00,
0x07,
0x38,
0x01C0,
0x0E00,
0x3F,
0x01C7,
0x0E07,
0x01F8,
0x0E38,
0x0FC0,
0x00,
0x00,
0x00,
0x00,
0x00,
0x7000,
0x7007,
0x7038,
0x71C0,
0x7E00
})
Name (CDCT, Package (0x05)
{
Package (0x02)
{
0xE4,
0x0140
},
Package (0x02)
{
0xDE,
0x014D
},
Package (0x02)
{
0xDE,
0x014D
},
Package (0x02)
{
0x00,
0x00
},
Package (0x02)
{
0xDE,
0x014D
}
})
Name (SUCC, 0x01)
Name (NVLD, 0x02)
Name (CRIT, 0x04)
Name (NCRT, 0x06)
Method (GSCI, 0, Serialized)
{
Method (GBDA, 0, Serialized)
{
If (LEqual (GESF, 0x00))
{
Store (0x00020000, PARM)
Store (Zero, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x01))
{
Store (0x00200000, PARM)
Store (Zero, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x04))
{
And (PARM, 0xEFFF0000, PARM)
And (PARM, ShiftLeft (DerefOf (Index (DBTB, IBTT)), 0x10),
PARM)
Or (IBTT, PARM, PARM)
Store (Zero, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x05))
{
Store (IPSC, PARM)
Or (PARM, ShiftLeft (IPAT, 0x08), PARM)
Add (PARM, 0x0100, PARM)
Or (PARM, ShiftLeft (LIDS, 0x10), PARM)
Add (PARM, 0x00010000, PARM)
Or (PARM, ShiftLeft (IBIA, 0x14), PARM)
Store (Zero, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x06))
{
Store (Zero, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x07))
{
Store (GIVD, PARM)
XOr (PARM, 0x01, PARM)
Or (PARM, ShiftLeft (GMFN, 0x01), PARM)
Or (PARM, ShiftLeft (0x03, 0x0B), PARM)
Or (PARM, ShiftLeft (IDMS, 0x11), PARM)
Or (ShiftLeft (DerefOf (Index (DerefOf (Index (CDCT, HVCO)), CDVL
)), 0x15), PARM, PARM)
Store (0x01, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x0A))
{
Store (0x00, PARM)
If (ISSC)
{
Or (PARM, 0x03, PARM)
}
Store (0x00, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x0B))
{
Store (KSV0, PARM)
Store (KSV1, GESF)
Return (SUCC)
}
Store (Zero, GESF)
Return (CRIT)
}
Method (SBCB, 0, Serialized)
{
If (LEqual (GESF, 0x00))
{
Store (0x00, PARM)
Store (0x00020000, PARM)
Store (Zero, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x01))
{
Store (0x00, PARM)
Store (Zero, GESF)
Store (0x00200000, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x03))
{
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x04))
{
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x05))
{
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x06))
{
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x07))
{
If (LEqual (PARM, 0x00))
{
Store (CLID, Local0)
If (And (0x80000000, Local0))
{
And (CLID, 0x0F, CLID)
GLID (CLID)
}
}
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x08))
{
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x09))
{
And (PARM, 0xFF, IBTT)
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x0A))
{
And (PARM, 0xFF, IPSC)
If (And (ShiftRight (PARM, 0x08), 0xFF))
{
And (ShiftRight (PARM, 0x08), 0xFF, IPAT)
Decrement (IPAT)
}
And (ShiftRight (PARM, 0x14), 0x07, IBIA)
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x0B))
{
And (ShiftRight (PARM, 0x01), 0x01, IF1E)
If (And (PARM, ShiftLeft (0x0F, 0x0D)))
{
And (ShiftRight (PARM, 0x0D), 0x0F, IDMS)
}
Else
{
And (ShiftRight (PARM, 0x11), 0x0F, IDMS)
}
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x10))
{
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x11))
{
Store (ShiftLeft (LIDS, 0x08), PARM)
Add (PARM, 0x0100, PARM)
Store (Zero, GESF)
Return (SUCC)
}
If (LEqual (GESF, 0x12))
{
If (And (PARM, 0x01))
{
If (LEqual (ShiftRight (PARM, 0x01), 0x01))
{
Store (0x01, ISSC)
}
Else
{
Store (Zero, GESF)
Return (CRIT)
}
}
Else
{
Store (0x00, ISSC)
}
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x13))
{
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x14))
{
And (PARM, 0x0F, PAVP)
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
If (LEqual (GESF, 0x15))
{
If (LEqual (PARM, 0x01))
{
Or (\_SB.PCI0.AUDE, 0x20, \_SB.PCI0.AUDE)
Notify (\_SB.PCI0, 0x00)
}
If (LEqual (PARM, 0x00))
{
And (\_SB.PCI0.AUDE, 0xDF, \_SB.PCI0.AUDE)
Notify (\_SB.PCI0, 0x00)
}
Store (Zero, GESF)
Store (Zero, PARM)
Return (SUCC)
}
Store (Zero, GESF)
Return (SUCC)
}
If (LEqual (GEFC, 0x04))
{
Store (GBDA (), GXFC)
}
If (LEqual (GEFC, 0x06))
{
Store (SBCB (), GXFC)
}
Store (0x00, GEFC)
Store (0x01, SCIS)
Store (0x00, GSSE)
Store (0x00, SCIE)
Return (Zero)
}
Method (PDRD, 0, NotSerialized)
{
If (LNot (DRDY))
{
Sleep (ASLP)
}
Return (LNot (DRDY))
}
Method (PSTS, 0, NotSerialized)
{
If (LGreater (CSTS, 0x02))
{
Sleep (ASLP)
}
Return (LEqual (CSTS, 0x03))
}
Method (GNOT, 2, NotSerialized)
{
If (PDRD ())
{
Return (0x01)
}
Store (Arg0, CEVT)
Store (0x03, CSTS)
If (LAnd (LEqual (CHPD, 0x00), LEqual (Arg1, 0x00)))
{
If (LOr (LGreater (OSYS, 0x07D0), LLess (OSYS, 0x07D6)))
{
Notify (\_SB.PCI0, Arg1)
}
Else
{
Notify (\_SB.PCI0.IGPU, Arg1)
}
}
If (CondRefOf (HNOT))
{
HNOT (Arg0)
}
Else
{
Notify (\_SB.PCI0.IGPU, 0x80)
}
Return (0x00)
}
Method (GHDS, 1, NotSerialized)
{
Store (Arg0, TIDX)
Return (GNOT (0x01, 0x00))
}
Method (GLID, 1, NotSerialized)
{
If (LEqual (Arg0, 0x01))
{
Store (0x03, CLID)
}
Else
{
Store (Arg0, CLID)
}
Return (GNOT (0x02, 0x00))
}
Method (GDCK, 1, NotSerialized)
{
Store (Arg0, CDCK)
Return (GNOT (0x04, 0x00))
}
Method (PARD, 0, NotSerialized)
{
If (LNot (ARDY))
{
Sleep (ASLP)
}
Return (LNot (ARDY))
}
Method (AINT, 2, NotSerialized)
{
If (LNot (And (TCHE, ShiftLeft (0x01, Arg0))))
{
Return (0x01)
}
If (PARD ())
{
Return (0x01)
}
If (LEqual (Arg0, 0x02))
{
If (CPFM)
{
And (CPFM, 0x0F, Local0)
And (EPFM, 0x0F, Local1)
If (LEqual (Local0, 0x01))
{
If (And (Local1, 0x06))
{
Store (0x06, PFIT)
}
Else
{
If (And (Local1, 0x08))
{
Store (0x08, PFIT)
}
Else
{
Store (0x01, PFIT)
}
}
}
If (LEqual (Local0, 0x06))
{
If (And (Local1, 0x08))
{
Store (0x08, PFIT)
}
Else
{
If (And (Local1, 0x01))
{
Store (0x01, PFIT)
}
Else
{
Store (0x06, PFIT)
}
}
}
If (LEqual (Local0, 0x08))
{
If (And (Local1, 0x01))
{
Store (0x01, PFIT)
}
Else
{
If (And (Local1, 0x06))
{
Store (0x06, PFIT)
}
Else
{
Store (0x08, PFIT)
}
}
}
}
Else
{
XOr (PFIT, 0x07, PFIT)
}
Or (PFIT, 0x80000000, PFIT)
Store (0x04, ASLC)
}
Else
{
If (LEqual (Arg0, 0x01))
{
Store (Divide (Multiply (Arg1, 0xFF), 0x64, ), BCLP)
Or (BCLP, 0x80000000, BCLP)
Store (0x02, ASLC)
}
Else
{
If (LEqual (Arg0, 0x00))
{
Store (Arg1, ALSI)
Store (0x01, ASLC)
}
Else
{
Return (0x01)
}
}
}
Store (0x01, ASLE)
Return (0x00)
}
Method (SCIP, 0, NotSerialized)
{
If (LNotEqual (OVER, 0x00))
{
Return (LNot (GSMI))
}
Return (0x00)
}
Device (\_SB.MEM2)
{
Name (_HID, EisaId ("PNP0C01")) // _HID: Hardware ID
Name (_UID, 0x02) // _UID: Unique ID
Name (CRS, ResourceTemplate ()
{
Memory32Fixed (ReadWrite,
0x20000000, // Address Base
0x00200000, // Address Length
)
Memory32Fixed (ReadWrite,
0x40000000, // Address Base
0x00200000, // Address Length
)
})
Method (_CRS, 0, NotSerialized) // _CRS: Current Resource Settings
{
Return (CRS)
}
}
}
Device (SATA)
{
Name (_ADR, 0x001F0002) // _ADR: Address
}
Device (SBUS)
{
Name (_ADR, 0x001F0003) // _ADR: Address
OperationRegion (SMBP, PCI_Config, 0x40, 0xC0)
Field (SMBP, DWordAcc, NoLock, Preserve)
{
, 2,
I2CE, 1
}
OperationRegion (SMPB, PCI_Config, 0x20, 0x04)
Field (SMPB, DWordAcc, NoLock, Preserve)
{
, 5,
SBAR, 11
}
OperationRegion (SMBI, SystemIO, ShiftLeft (SBAR, 0x05), 0x10)
Field (SMBI, ByteAcc, NoLock, Preserve)
{
HSTS, 8,
Offset (0x02),
HCON, 8,
HCOM, 8,
TXSA, 8,
DAT0, 8,
DAT1, 8,
HBDR, 8,
PECR, 8,
RXSA, 8,
SDAT, 16
}
Method (SSXB, 2, Serialized)
{
If (STRT ())
{
Return (0x00)
}
Store (0x00, I2CE)
Store (0xBF, HSTS)
Store (Arg0, TXSA)
Store (Arg1, HCOM)
Store (0x48, HCON)
If (COMP ())
{
Or (HSTS, 0xFF, HSTS)
Return (0x01)
}
Return (0x00)
}
Method (SRXB, 1, Serialized)
{
If (STRT ())
{
Return (0xFFFF)
}
Store (0x00, I2CE)
Store (0xBF, HSTS)
Store (Or (Arg0, 0x01), TXSA)
Store (0x44, HCON)
If (COMP ())
{
Or (HSTS, 0xFF, HSTS)
Return (DAT0)
}
Return (0xFFFF)
}
Method (SWRB, 3, Serialized)
{
If (STRT ())
{
Return (0x00)
}
Store (0x00, I2CE)
Store (0xBF, HSTS)
Store (Arg0, TXSA)
Store (Arg1, HCOM)
Store (Arg2, DAT0)
Store (0x48, HCON)
If (COMP ())
{
Or (HSTS, 0xFF, HSTS)
Return (0x01)
}
Return (0x00)
}
Method (SRDB, 2, Serialized)
{
If (STRT ())
{
Return (0xFFFF)
}
Store (0x00, I2CE)
Store (0xBF, HSTS)
Store (Or (Arg0, 0x01), TXSA)
Store (Arg1, HCOM)
Store (0x48, HCON)
If (COMP ())
{
Or (HSTS, 0xFF, HSTS)
Return (DAT0)
}
Return (0xFFFF)
}
Method (SWRW, 3, Serialized)
{
If (STRT ())
{
Return (0x00)
}
Store (0x00, I2CE)
Store (0xBF, HSTS)
Store (Arg0, TXSA)
Store (Arg1, HCOM)
And (Arg2, 0xFF, DAT1)
And (ShiftRight (Arg2, 0x08), 0xFF, DAT0)
Store (0x4C, HCON)
If (COMP ())
{
Or (HSTS, 0xFF, HSTS)
Return (0x01)
}
Return (0x00)
}
Method (SRDW, 2, Serialized)
{
If (STRT ())
{
Return (0xFFFF)
}
Store (0x00, I2CE)
Store (0xBF, HSTS)
Store (Or (Arg0, 0x01), TXSA)
Store (Arg1, HCOM)
Store (0x4C, HCON)
If (COMP ())
{
Or (HSTS, 0xFF, HSTS)
Return (Or (ShiftLeft (DAT0, 0x08), DAT1))
}
Return (0xFFFFFFFF)
}
Method (SBLW, 4, Serialized)
{
If (STRT ())
{
Return (0x00)
}
Store (Arg3, I2CE)
Store (0xBF, HSTS)
Store (Arg0, TXSA)
Store (Arg1, HCOM)
Store (SizeOf (Arg2), DAT0)
Store (0x00, Local1)
Store (DerefOf (Index (Arg2, 0x00)), HBDR)
Store (0x54, HCON)
While (LGreater (SizeOf (Arg2), Local1))
{
Store (0x4E20, Local0)
While (LAnd (LNot (And (HSTS, 0x80)), Local0))
{
Decrement (Local0)
}
If (LNot (Local0))
{
KILL ()
Return (0x00)
}
Increment (Local1)
If (LGreater (SizeOf (Arg2), Local1))
{
Store (DerefOf (Index (Arg2, Local1)), HBDR)
Store (0x80, HSTS)
}
}
Store (0x80, HSTS)
If (COMP ())
{
Or (HSTS, 0xFF, HSTS)
Return (0x01)
}
Return (0x00)
}
Method (SBLR, 3, Serialized)
{
Name (TBUF, Buffer (0x0100) {})
If (STRT ())
{
Return (0x00)
}
Store (Arg2, I2CE)
Store (0xBF, HSTS)
Store (Or (Arg0, 0x01), TXSA)
Store (Arg1, HCOM)
Store (0x54, HCON)
Store (0x0FA0, Local0)
While (LAnd (LNot (And (HSTS, 0x80)), Local0))
{
Decrement (Local0)
Stall (0x32)
}
If (LNot (Local0))
{
KILL ()
Return (0x00)
}
Store (DAT0, Index (TBUF, 0x00))
Store (0x80, HSTS)
Store (0x01, Local1)
While (LLess (Local1, DerefOf (Index (TBUF, 0x00))))
{
Store (0x0FA0, Local0)
While (LAnd (LNot (And (HSTS, 0x80)), Local0))
{
Decrement (Local0)
Stall (0x32)
}
If (LNot (Local0))
{
KILL ()
Return (0x00)
}
Store (HBDR, Index (TBUF, Local1))
Store (0x80, HSTS)
Increment (Local1)
}
If (COMP ())
{
Or (HSTS, 0xFF, HSTS)
Return (TBUF)
}
Return (0x00)
}
Method (STRT, 0, Serialized)
{
Store (0xC8, Local0)
While (Local0)
{
If (And (HSTS, 0x40))
{
Decrement (Local0)
Sleep (0x01)
If (LEqual (Local0, 0x00))
{
Return (0x01)
}
}
Else
{
Store (0x00, Local0)
}
}
Store (0x0FA0, Local0)
While (Local0)
{
If (And (HSTS, 0x01))
{
Decrement (Local0)
Stall (0x32)
If (LEqual (Local0, 0x00))
{
KILL ()
}
}
Else
{
Return (0x00)
}
}
Return (0x01)
}
Method (COMP, 0, Serialized)
{
Store (0x0FA0, Local0)
While (Local0)
{
If (And (HSTS, 0x02))
{
Return (0x01)
}
Else
{
Decrement (Local0)
Stall (0x32)
If (LEqual (Local0, 0x00))
{
KILL ()
}
}
}
Return (0x00)
}
Method (KILL, 0, Serialized)
{
Or (HCON, 0x02, HCON)
Or (HSTS, 0xFF, HSTS)
}
Device (BUS0)
{
Name (_CID, "smbus") // _CID: Compatible ID
Name (_ADR, 0x00) // _ADR: Address
Device (MKY0)
{
Name (_ADR, 0x00) // _ADR: Address
Name (_CID, "mikey") // _CID: Compatible ID
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
Store (Package (0x0C)
{
"refnum",
0x00,
"address",
0x39,
"device-id",
0x0CD5,
"ramp-control-address",
0x3B,
"resprg",
0x03,
"hdet",
0x01
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3, RefOf (Local0))
Return (Local0)
}
Method (H1EN, 1, Serialized)
{
If (LLessEqual (Arg0, 0x01))
{
If (LEqual (Arg0, 0x01))
{
Or (GP52, 0x01, GP52)
}
Else
{
And (GP52, 0x00, GP52)
}
}
}
Method (H1IL, 0, Serialized)
{
Store (GP05, Local0)
Return (Local0)
}
Method (H1IP, 1, Serialized)
{
Store (Arg0, Local0)
If (LLessEqual (Arg0, 0x01))
{
Not (Arg0, Arg0)
Store (Arg0, GI05)
}
}
Name (H1IN, 0x15)
Scope (\_GPE)
{
Method (_L15, 0, NotSerialized) // _Lxx: Level-Triggered GPE
{
If (OSDW ())
{
Notify (\_SB.PCI0.SBUS.BUS0.MKY0, 0x80)
}
Else
{
Store (0x00, GI05)
Store (0x00, GU05)
Notify (\_SB.PWRB, 0x02)
}
}
}
Method (P1IL, 0, Serialized)
{
Store (GP03, Local0)
Return (Local0)
}
Method (P1IP, 1, Serialized)
{
If (LLessEqual (Arg0, 0x01))
{
Not (Arg0, Arg0)
Store (Arg0, GI03)
}
}
Name (P1IN, 0x13)
Scope (\_GPE)
{
Method (_L13, 0, NotSerialized) // _Lxx: Level-Triggered GPE
{
XOr (GI03, 0x01, GI03)
If (OSDW ())
{
Notify (\_SB.PCI0.SBUS.BUS0.MKY0, 0x81)
}
Else
{
Notify (\_SB.PWRB, 0x02)
}
}
}
}
Device (BLC0)
{
Name (_ADR, 0x00) // _ADR: Address
Name (_CID, "smbus-blc") // _CID: Compatible ID
OperationRegion (BLCM, SystemMemory, BLCB, 0x0100)
Field (BLCM, AnyAcc, NoLock, Preserve)
{
CSIZ, 8,
CBUF, 112
}
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
Store (Package (0x08)
{
"refnum",
0x00,
"address",
BLCP,
"command",
BLCC,
"type",
BLCT
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3, RefOf (Local0))
Return (Local0)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW ())
{
Return (0x0F)
}
Else
{
Return (0x0B)
}
}
Method (BSET, 1, Serialized)
{
If (LNot (BLCP))
{
Return (Zero)
}
If (LLessEqual (Arg0, 0x00))
{
Store (0x00, Local0)
}
Else
{
If (LGreater (Arg0, 0x64))
{
Store (0xFFFF, Local0)
}
Else
{
Multiply (0x028F, Arg0, Local0)
}
}
If (LEqual (BLCT, 0x4D434353))
{
Name (BUFR, Buffer (0x06) {})
CreateByteField (BUFR, 0x00, SIZE)
CreateByteField (BUFR, 0x01, VSET)
CreateByteField (BUFR, 0x02, VOPC)
CreateByteField (BUFR, 0x03, VALH)
CreateByteField (BUFR, 0x04, VALL)
CreateByteField (BUFR, 0x05, CKSM)
Store (0x84, SIZE)
Store (0x03, VSET)
Store (0x10, VOPC)
Store (ShiftRight (Local0, 0x08), VALH)
Store (And (Local0, 0xFF), VALL)
Store (XOr (0xA8, VALH), CKSM)
Store (XOr (CKSM, VALL), CKSM)
\_SB.PCI0.SBUS.SBLW (BLCP, BLCC, BUFR, 0x01)
Return (Zero)
}
If (LEqual (BLCT, 0x49324300))
{
\_SB.PCI0.SBUS.SWRW (ShiftLeft (BLCP, 0x01), BLCC, Local0)
}
Return (Zero)
}
Method (BCAL, 0, Serialized)
{
If (LNot (BLCP))
{
Return (Zero)
}
If (LAnd (LEqual (BLCT, 0x4D434353), CSIZ))
{
\_SB.PCI0.SBUS.SBLW (BLCP, BLCC, ToBuffer (CBUF), 0x01)
}
Return (Zero)
}
}
}
Device (BUS1)
{
Name (_CID, "smbus") // _CID: Compatible ID
Name (_ADR, 0x01) // _ADR: Address
}
}
Device (LPCB)
{
Name (_ADR, 0x001F0000) // _ADR: Address
Scope (\_SB)
{
OperationRegion (\_SB.PCI0.LPCB.LPC1, PCI_Config, 0x40, 0xC0)
Field (\_SB.PCI0.LPCB.LPC1, AnyAcc, NoLock, Preserve)
{
Offset (0x20),
PARC, 8,
PBRC, 8,
PCRC, 8,
PDRC, 8,
Offset (0x28),
PERC, 8,
PFRC, 8,
PGRC, 8,
PHRC, 8
}
Device (LNKA)
{
Name (_HID, EisaId ("PNP0C0F")) // _HID: Hardware ID
Name (_UID, 0x01) // _UID: Unique ID
Method (_DIS, 0, Serialized) // _DIS: Disable Device
{
Or (PARC, 0x80, PARC)
}
Name (_PRS, ResourceTemplate () // _PRS: Possible Resource Settings
{
IRQ (Level, ActiveLow, Shared, )
{1,3,4,5,6,7,10,12,14,15}
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
Name (RTLA, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, _Y0E)
{}
})
CreateWordField (RTLA, \_SB.LNKA._CRS._Y0E._INT, IRQ0) // _INT: Interrupts
Store (Zero, IRQ0)
ShiftLeft (0x01, And (PARC, 0x0F), IRQ0)
Return (RTLA)
}
Method (_SRS, 1, Serialized) // _SRS: Set Resource Settings
{
CreateWordField (Arg0, 0x01, IRQ0)
FindSetRightBit (IRQ0, Local0)
Decrement (Local0)
Store (Local0, PARC)
}
Method (_STA, 0, Serialized) // _STA: Status
{
If (And (PARC, 0x80))
{
Return (0x09)
}
Else
{
Return (0x0B)
}
}
}
Device (LNKB)
{
Name (_HID, EisaId ("PNP0C0F")) // _HID: Hardware ID
Name (_UID, 0x02) // _UID: Unique ID
Method (_DIS, 0, Serialized) // _DIS: Disable Device
{
Or (PBRC, 0x80, PBRC)
}
Name (_PRS, ResourceTemplate () // _PRS: Possible Resource Settings
{
IRQ (Level, ActiveLow, Shared, )
{1,3,4,5,6,7,11,12,14,15}
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
Name (RTLB, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, _Y0F)
{}
})
CreateWordField (RTLB, \_SB.LNKB._CRS._Y0F._INT, IRQ0) // _INT: Interrupts
Store (Zero, IRQ0)
ShiftLeft (0x01, And (PBRC, 0x0F), IRQ0)
Return (RTLB)
}
Method (_SRS, 1, Serialized) // _SRS: Set Resource Settings
{
CreateWordField (Arg0, 0x01, IRQ0)
FindSetRightBit (IRQ0, Local0)
Decrement (Local0)
Store (Local0, PBRC)
}
Method (_STA, 0, Serialized) // _STA: Status
{
If (And (PBRC, 0x80))
{
Return (0x09)
}
Else
{
Return (0x0B)
}
}
}
Device (LNKC)
{
Name (_HID, EisaId ("PNP0C0F")) // _HID: Hardware ID
Name (_UID, 0x03) // _UID: Unique ID
Method (_DIS, 0, Serialized) // _DIS: Disable Device
{
Or (PCRC, 0x80, PCRC)
}
Name (_PRS, ResourceTemplate () // _PRS: Possible Resource Settings
{
IRQ (Level, ActiveLow, Shared, )
{1,3,4,5,6,7,10,12,14,15}
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
Name (RTLC, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, _Y10)
{}
})
CreateWordField (RTLC, \_SB.LNKC._CRS._Y10._INT, IRQ0) // _INT: Interrupts
Store (Zero, IRQ0)
ShiftLeft (0x01, And (PCRC, 0x0F), IRQ0)
Return (RTLC)
}
Method (_SRS, 1, Serialized) // _SRS: Set Resource Settings
{
CreateWordField (Arg0, 0x01, IRQ0)
FindSetRightBit (IRQ0, Local0)
Decrement (Local0)
Store (Local0, PCRC)
}
Method (_STA, 0, Serialized) // _STA: Status
{
If (And (PCRC, 0x80))
{
Return (0x09)
}
Else
{
Return (0x0B)
}
}
}
Device (LNKD)
{
Name (_HID, EisaId ("PNP0C0F")) // _HID: Hardware ID
Name (_UID, 0x04) // _UID: Unique ID
Method (_DIS, 0, Serialized) // _DIS: Disable Device
{
Or (PDRC, 0x80, PDRC)
}
Name (_PRS, ResourceTemplate () // _PRS: Possible Resource Settings
{
IRQ (Level, ActiveLow, Shared, )
{1,3,4,5,6,7,11,12,14,15}
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
Name (RTLD, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, _Y11)
{}
})
CreateWordField (RTLD, \_SB.LNKD._CRS._Y11._INT, IRQ0) // _INT: Interrupts
Store (Zero, IRQ0)
ShiftLeft (0x01, And (PDRC, 0x0F), IRQ0)
Return (RTLD)
}
Method (_SRS, 1, Serialized) // _SRS: Set Resource Settings
{
CreateWordField (Arg0, 0x01, IRQ0)
FindSetRightBit (IRQ0, Local0)
Decrement (Local0)
Store (Local0, PDRC)
}
Method (_STA, 0, Serialized) // _STA: Status
{
If (And (PDRC, 0x80))
{
Return (0x09)
}
Else
{
Return (0x0B)
}
}
}
Device (LNKE)
{
Name (_HID, EisaId ("PNP0C0F")) // _HID: Hardware ID
Name (_UID, 0x05) // _UID: Unique ID
Method (_DIS, 0, Serialized) // _DIS: Disable Device
{
Or (PERC, 0x80, PERC)
}
Name (_PRS, ResourceTemplate () // _PRS: Possible Resource Settings
{
IRQ (Level, ActiveLow, Shared, )
{1,3,4,5,6,7,10,12,14,15}
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
Name (RTLE, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, _Y12)
{}
})
CreateWordField (RTLE, \_SB.LNKE._CRS._Y12._INT, IRQ0) // _INT: Interrupts
Store (Zero, IRQ0)
ShiftLeft (0x01, And (PERC, 0x0F), IRQ0)
Return (RTLE)
}
Method (_SRS, 1, Serialized) // _SRS: Set Resource Settings
{
CreateWordField (Arg0, 0x01, IRQ0)
FindSetRightBit (IRQ0, Local0)
Decrement (Local0)
Store (Local0, PERC)
}
Method (_STA, 0, Serialized) // _STA: Status
{
If (And (PERC, 0x80))
{
Return (0x09)
}
Else
{
Return (0x0B)
}
}
}
Device (LNKF)
{
Name (_HID, EisaId ("PNP0C0F")) // _HID: Hardware ID
Name (_UID, 0x06) // _UID: Unique ID
Method (_DIS, 0, Serialized) // _DIS: Disable Device
{
Or (PFRC, 0x80, PFRC)
}
Name (_PRS, ResourceTemplate () // _PRS: Possible Resource Settings
{
IRQ (Level, ActiveLow, Shared, )
{1,3,4,5,6,7,11,12,14,15}
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
Name (RTLF, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, _Y13)
{}
})
CreateWordField (RTLF, \_SB.LNKF._CRS._Y13._INT, IRQ0) // _INT: Interrupts
Store (Zero, IRQ0)
ShiftLeft (0x01, And (PFRC, 0x0F), IRQ0)
Return (RTLF)
}
Method (_SRS, 1, Serialized) // _SRS: Set Resource Settings
{
CreateWordField (Arg0, 0x01, IRQ0)
FindSetRightBit (IRQ0, Local0)
Decrement (Local0)
Store (Local0, PFRC)
}
Method (_STA, 0, Serialized) // _STA: Status
{
If (And (PFRC, 0x80))
{
Return (0x09)
}
Else
{
Return (0x0B)
}
}
}
Device (LNKG)
{
Name (_HID, EisaId ("PNP0C0F")) // _HID: Hardware ID
Name (_UID, 0x07) // _UID: Unique ID
Method (_DIS, 0, Serialized) // _DIS: Disable Device
{
Or (PGRC, 0x80, PGRC)
}
Name (_PRS, ResourceTemplate () // _PRS: Possible Resource Settings
{
IRQ (Level, ActiveLow, Shared, )
{1,3,4,5,6,7,10,12,14,15}
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
Name (RTLG, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, _Y14)
{}
})
CreateWordField (RTLG, \_SB.LNKG._CRS._Y14._INT, IRQ0) // _INT: Interrupts
Store (Zero, IRQ0)
ShiftLeft (0x01, And (PGRC, 0x0F), IRQ0)
Return (RTLG)
}
Method (_SRS, 1, Serialized) // _SRS: Set Resource Settings
{
CreateWordField (Arg0, 0x01, IRQ0)
FindSetRightBit (IRQ0, Local0)
Decrement (Local0)
Store (Local0, PGRC)
}
Method (_STA, 0, Serialized) // _STA: Status
{
If (And (PGRC, 0x80))
{
Return (0x09)
}
Else
{
Return (0x0B)
}
}
}
Device (LNKH)
{
Name (_HID, EisaId ("PNP0C0F")) // _HID: Hardware ID
Name (_UID, 0x08) // _UID: Unique ID
Method (_DIS, 0, Serialized) // _DIS: Disable Device
{
Or (PHRC, 0x80, PHRC)
}
Name (_PRS, ResourceTemplate () // _PRS: Possible Resource Settings
{
IRQ (Level, ActiveLow, Shared, )
{1,3,4,5,6,7,11,12,14,15}
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
Name (RTLH, ResourceTemplate ()
{
IRQ (Level, ActiveLow, Shared, _Y15)
{}
})
CreateWordField (RTLH, \_SB.LNKH._CRS._Y15._INT, IRQ0) // _INT: Interrupts
Store (Zero, IRQ0)
ShiftLeft (0x01, And (PHRC, 0x0F), IRQ0)
Return (RTLH)
}
Method (_SRS, 1, Serialized) // _SRS: Set Resource Settings
{
CreateWordField (Arg0, 0x01, IRQ0)
FindSetRightBit (IRQ0, Local0)
Decrement (Local0)
Store (Local0, PHRC)
}
Method (_STA, 0, Serialized) // _STA: Status
{
If (And (PHRC, 0x80))
{
Return (0x09)
}
Else
{
Return (0x0B)
}
}
}
}
OperationRegion (LPC0, PCI_Config, 0x40, 0xC0)
Field (LPC0, AnyAcc, NoLock, Preserve)
{
Offset (0x40),
IOD0, 8,
IOD1, 8,
Offset (0xB0),
RAEN, 1,
, 13,
RCBA, 18
}
Device (DMAC)
{
Name (_HID, EisaId ("PNP0200")) // _HID: Hardware ID
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
IO (Decode16,
0x0000, // Range Minimum
0x0000, // Range Maximum
0x01, // Alignment
0x20, // Length
)
IO (Decode16,
0x0081, // Range Minimum
0x0081, // Range Maximum
0x01, // Alignment
0x11, // Length
)
IO (Decode16,
0x0093, // Range Minimum
0x0093, // Range Maximum
0x01, // Alignment
0x0D, // Length
)
IO (Decode16,
0x00C0, // Range Minimum
0x00C0, // Range Maximum
0x01, // Alignment
0x20, // Length
)
DMA (Compatibility, NotBusMaster, Transfer8_16, )
{4}
})
}
Device (FWHD)
{
Name (_HID, EisaId ("INT0800")) // _HID: Hardware ID
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
Memory32Fixed (ReadOnly,
0xFF000000, // Address Base
0x01000000, // Address Length
)
})
}
Device (HPET)
{
Name (_HID, EisaId ("PNP0103")) // _HID: Hardware ID
Name (_CID, EisaId ("PNP0C01")) // _CID: Compatible ID
Name (BUF0, ResourceTemplate ()
{
IRQNoFlags ()
{0}
IRQNoFlags ()
{8}
Memory32Fixed (ReadWrite,
0xFED00000, // Address Base
0x00000400, // Address Length
_Y16)
})
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (LGreaterEqual (OSYS, 0x07D1))
{
If (HPAE)
{
Return (0x0F)
}
}
Else
{
If (HPAE)
{
Return (0x0B)
}
}
Return (0x00)
}
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
If (HPAE)
{
CreateDWordField (BUF0, \_SB.PCI0.LPCB.HPET._Y16._BAS, HPT0) // _BAS: Base Address
If (LEqual (HPAS, 0x01))
{
Store (0xFED01000, HPT0)
}
If (LEqual (HPAS, 0x02))
{
Store (0xFED02000, HPT0)
}
If (LEqual (HPAS, 0x03))
{
Store (0xFED03000, HPT0)
}
}
Return (BUF0)
}
}
Device (IPIC)
{
Name (_HID, EisaId ("PNP0000")) // _HID: Hardware ID
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
IO (Decode16,
0x0020, // Range Minimum
0x0020, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x0024, // Range Minimum
0x0024, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x0028, // Range Minimum
0x0028, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x002C, // Range Minimum
0x002C, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x0030, // Range Minimum
0x0030, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x0034, // Range Minimum
0x0034, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x0038, // Range Minimum
0x0038, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x003C, // Range Minimum
0x003C, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x00A0, // Range Minimum
0x00A0, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x00A4, // Range Minimum
0x00A4, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x00A8, // Range Minimum
0x00A8, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x00AC, // Range Minimum
0x00AC, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x00B0, // Range Minimum
0x00B0, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x00B4, // Range Minimum
0x00B4, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x00B8, // Range Minimum
0x00B8, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x00BC, // Range Minimum
0x00BC, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x04D0, // Range Minimum
0x04D0, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IRQNoFlags ()
{2}
})
}
Device (MATH)
{
Name (_HID, EisaId ("PNP0C04")) // _HID: Hardware ID
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
IO (Decode16,
0x00F0, // Range Minimum
0x00F0, // Range Maximum
0x01, // Alignment
0x01, // Length
)
IRQNoFlags ()
{13}
})
}
Device (LDRC)
{
Name (_HID, EisaId ("PNP0C02")) // _HID: Hardware ID
Name (_UID, 0x02) // _UID: Unique ID
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
IO (Decode16,
0x002E, // Range Minimum
0x002E, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x004E, // Range Minimum
0x004E, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0x0061, // Range Minimum
0x0061, // Range Maximum
0x01, // Alignment
0x01, // Length
)
IO (Decode16,
0x0063, // Range Minimum
0x0063, // Range Maximum
0x01, // Alignment
0x01, // Length
)
IO (Decode16,
0x0065, // Range Minimum
0x0065, // Range Maximum
0x01, // Alignment
0x01, // Length
)
IO (Decode16,
0x0067, // Range Minimum
0x0067, // Range Maximum
0x01, // Alignment
0x01, // Length
)
IO (Decode16,
0x0080, // Range Minimum
0x0080, // Range Maximum
0x01, // Alignment
0x01, // Length
)
IO (Decode16,
0x0092, // Range Minimum
0x0092, // Range Maximum
0x01, // Alignment
0x01, // Length
)
IO (Decode16,
0x00B2, // Range Minimum
0x00B2, // Range Maximum
0x01, // Alignment
0x02, // Length
)
IO (Decode16,
0xFFFF, // Range Minimum
0xFFFF, // Range Maximum
0x01, // Alignment
0x01, // Length
)
IO (Decode16,
0x0400, // Range Minimum
0x0400, // Range Maximum
0x01, // Alignment
0x80, // Length
)
IO (Decode16,
0x0800, // Range Minimum
0x0800, // Range Maximum
0x01, // Alignment
0x80, // Length
)
})
}
Device (RTC)
{
Name (_HID, EisaId ("PNP0B00")) // _HID: Hardware ID
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
IO (Decode16,
0x0070, // Range Minimum
0x0070, // Range Maximum
0x01, // Alignment
0x08, // Length
)
})
OperationRegion (CMS0, SystemCMOS, 0x00, 0x40)
Field (CMS0, ByteAcc, NoLock, Preserve)
{
Offset (0x38),
ISTB, 1,
Offset (0x39)
}
}
Device (TIMR)
{
Name (_HID, EisaId ("PNP0100")) // _HID: Hardware ID
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
IO (Decode16,
0x0040, // Range Minimum
0x0040, // Range Maximum
0x01, // Alignment
0x04, // Length
)
IO (Decode16,
0x0050, // Range Minimum
0x0050, // Range Maximum
0x10, // Alignment
0x04, // Length
)
})
}
Device (SMC)
{
Name (_HID, EisaId ("APP0001")) // _HID: Hardware ID
Name (_CID, "smc-huronriver") // _CID: Compatible ID
Name (_STA, 0x0B) // _STA: Status
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
IO (Decode16,
0x0300, // Range Minimum
0x0300, // Range Maximum
0x01, // Alignment
0x20, // Length
)
Memory32Fixed (ReadWrite,
0xFEF00000, // Address Base
0x00010000, // Address Length
)
IRQNoFlags ()
{6}
})
}
Device (ALS0)
{
Name (_HID, "ACPI0008") // _HID: Hardware ID
Name (_CID, "smc-als") // _CID: Compatible ID
Name (BUFF, Buffer (0x02) {})
CreateByteField (BUFF, 0x00, OB0)
CreateByteField (BUFF, 0x01, OB1)
CreateWordField (BUFF, 0x00, ALSI)
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (LGreaterEqual (OSYS, 0x07D9))
{
Return (0x0F)
}
Else
{
Return (0x00)
}
}
Method (_ALI, 0, NotSerialized) // _ALI: Ambient Light Illuminance
{
Store (\_SB.PCI0.LPCB.EC.ALB0, OB0)
Store (\_SB.PCI0.LPCB.EC.ALB1, OB1)
Store (ALSI, Local0)
Return (Local0)
}
Name (_ALR, Package (0x05) // _ALR: Ambient Light Response
{
Package (0x02)
{
0x0A,
0x00
},
Package (0x02)
{
0x14,
0x0A
},
Package (0x02)
{
0x32,
0x50
},
Package (0x02)
{
0x5A,
0x012C
},
Package (0x02)
{
0x64,
0x03E8
}
})
}
Device (EC)
{
Name (_HID, EisaId ("PNP0C09")) // _HID: Hardware ID
Name (_UID, 0x00) // _UID: Unique ID
Name (_CRS, ResourceTemplate () // _CRS: Current Resource Settings
{
IO (Decode16,
0x0062, // Range Minimum
0x0062, // Range Maximum
0x00, // Alignment
0x01, // Length
)
IO (Decode16,
0x0066, // Range Minimum
0x0066, // Range Maximum
0x00, // Alignment
0x01, // Length
)
})
Name (_GPE, 0x17) // _GPE: General Purpose Events
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x23,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x23,
0x03
})
}
}
Name (ECOK, 0x00)
OperationRegion (ECOR, EmbeddedControl, 0x00, 0xFF)
Field (ECOR, ByteAcc, Lock, Preserve)
{
ECVS, 8,
Offset (0x02),
Offset (0x03),
G3HT, 1,
Offset (0x04),
WBCB, 1,
DSLP, 1,
Offset (0x05),
Offset (0x06),
WKRS, 8,
Offset (0x10),
ECSS, 8,
PLIM, 8,
ALB0, 8,
ALB1, 8,
WTLB, 8,
WTMB, 8,
Offset (0x20),
SPTR, 8,
SSTS, 8,
SADR, 8,
SCMD, 8,
SBFR, 256,
SCNT, 8,
SAAD, 8,
SAD0, 8,
SAD1, 8,
SMUX, 8,
Offset (0x60),
ELSW, 1,
EACP, 1,
ECDI, 1,
ENMI, 1,
Offset (0x61),
EMHP, 1,
Offset (0x62),
Offset (0x63),
Offset (0x64),
SWLO, 1,
SWLC, 1,
SWAI, 1,
SWAR, 1,
SWCI, 1,
SWCE, 1,
SWMI, 1,
SWMR, 1,
SWPB, 1,
SWGP, 1,
SWPM, 1,
SWWT, 1,
SWLB, 1,
Offset (0x66),
Offset (0x67),
Offset (0x68),
EWLO, 1,
EWLC, 1,
EWAI, 1,
EWAR, 1,
EWCI, 1,
EWCE, 1,
EWMI, 1,
EWMR, 1,
EWPB, 1,
EWGP, 1,
EWPM, 1,
ENWT, 1,
EWLB, 1,
Offset (0x6A),
Offset (0x6B),
Offset (0x6C),
LWLO, 1,
LWLC, 1,
LWAI, 1,
LWAR, 1,
LWCI, 1,
LWCE, 1,
LWMI, 1,
LWMR, 1,
LWPB, 1,
LWGP, 1,
LWPM, 1,
LWWT, 1,
LWLB, 1,
Offset (0x6E),
Offset (0x6F),
Offset (0x70)
}
Field (ECOR, ByteAcc, Lock, Preserve)
{
Offset (0x03),
G3AD, 1,
BLOD, 1,
S4WE, 1,
APWC, 1,
Offset (0x04),
Offset (0x6C),
LWE0, 8,
LWE1, 8,
LWE2, 8,
LWE3, 8
}
Field (ECOR, ByteAcc, Lock, Preserve)
{
Offset (0x24),
SBDW, 16,
Offset (0x46),
SADW, 16
}
Method (WAKE, 0, NotSerialized)
{
If (ECOK)
{
Return (WKRS)
}
Else
{
Return (0x00)
}
}
Method (_Q40, 0, NotSerialized) // _Qxx: EC Query
{
Notify (\_SB.PCI0.LPCB.ALS0, 0x80)
}
Method (_Q5A, 0, NotSerialized) // _Qxx: EC Query
{
Notify (\_SB.SLPB, 0x80)
}
Method (_Q80, 0, NotSerialized) // _Qxx: EC Query
{
Notify (\_PR.CPU0, 0x80)
Notify (\_PR.CPU1, 0x80)
Notify (\_PR.CPU2, 0x80)
Notify (\_PR.CPU3, 0x80)
Notify (\_PR.CPU4, 0x80)
Notify (\_PR.CPU5, 0x80)
Notify (\_PR.CPU6, 0x80)
Notify (\_PR.CPU7, 0x80)
Store (EGPS, Local0)
If (LEqual (\_SB.PCI0.P0P2.GFX0.VID0, 0x10DE))
{
If (LEqual (\_SB.PCI0.P0P2.GFX0.DID0, 0x0FEA))
{
If (LLessEqual (Local0, 0x03))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD1)
}
Else
{
If (LAnd (LGreater (Local0, 0x03), LLessEqual (Local0, 0x08)))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD2)
}
If (LAnd (LGreater (Local0, 0x08), LLessEqual (Local0, 0x0D)))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD3)
}
If (LAnd (LGreater (Local0, 0x0D), LLessEqual (Local0, 0x11)))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD4)
}
If (LGreater (Local0, 0x11))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD5)
}
}
}
Else
{
If (LLessEqual (Local0, 0x02))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD1)
}
Else
{
If (LAnd (LGreater (Local0, 0x02), LLessEqual (Local0, 0x05)))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD2)
}
If (LAnd (LGreater (Local0, 0x05), LLessEqual (Local0, 0x08)))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD3)
}
If (LAnd (LGreater (Local0, 0x08), LLessEqual (Local0, 0x0B)))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD4)
}
If (LGreater (Local0, 0x0B))
{
Notify (\_SB.PCI0.P0P2.GFX0, 0xD5)
}
}
}
}
}
Method (_REG, 2, NotSerialized) // _REG: Region Availability
{
If (LOr (LEqual (Arg0, 0x03), LGreaterEqual (OSYS, 0x07D6)))
{
Store (Arg1, ECOK)
If (LEqual (Arg1, 0x01))
{
Store (0x00, ECSS)
}
}
}
}
}
Device (HDEF)
{
Name (_ADR, 0x001B0000) // _ADR: Address
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x03
})
}
}
}
Device (RP01)
{
Name (_ADR, 0x001C0000) // _ADR: Address
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x03
})
}
}
Method (_PRT, 0, NotSerialized) // _PRT: PCI Routing Table
{
If (PICM)
{
Return (AR04 ())
}
Return (PR04 ())
}
}
Device (RP03)
{
Name (_ADR, 0x001C0002) // _ADR: Address
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x04
})
}
}
Method (_PRT, 0, NotSerialized) // _PRT: PCI Routing Table
{
If (PICM)
{
Return (AR06 ())
}
Return (PR06 ())
}
}
Device (RP04)
{
Name (_ADR, 0x001C0003) // _ADR: Address
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x04
})
}
}
Method (_PRT, 0, NotSerialized) // _PRT: PCI Routing Table
{
If (PICM)
{
Return (AR07 ())
}
Return (PR07 ())
}
}
Device (RP05)
{
Name (_ADR, 0x001C0004) // _ADR: Address
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x03
})
}
}
Method (_PRT, 0, NotSerialized) // _PRT: PCI Routing Table
{
If (PICM)
{
Return (AR08 ())
}
Return (PR08 ())
}
}
Scope (\_SB.PCI0.RP04)
{
OperationRegion (A1E0, PCI_Config, 0x00, 0x60)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
Offset (0x04),
BMIE, 3,
Offset (0x19),
SECB, 8,
SBBN, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x4A),
, 5,
TPEN, 1,
Offset (0x50),
, 4,
LDIS, 1,
, 24,
LACT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
If (LAnd (LEqual (BMIE, 0x00), LEqual (SECB, 0xFF)))
{
Return (SNBS)
}
Else
{
Return (SECB)
}
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Name (BMIS, 0x00)
Name (SNBS, 0x00)
Name (SOBS, 0x00)
Name (LPFL, 0x00)
Method (C4PU, 0, Serialized)
{
Store (SOBS, SBBN)
Store (SNBS, SECB)
Store (BMIS, BMIE)
Store (0x00, LDIS)
Store (0x00, Local0)
Store (Or (LPFL, 0x20), LPFL)
Store (0x00, GP50)
While (0x01)
{
Sleep (0x05)
Sleep (0x64)
Store (0x00, Local1)
Add (Timer, 0x00989680, Local2)
While (LLessEqual (Timer, Local2))
{
If (LAnd (LEqual (LACT, 0x01), LAnd (LNotEqual (\_SB.PCI0.RP04.GIGE.AVND, 0xFFFF),
LNotEqual (\_SB.PCI0.RP04.SDXC.AVND, 0xFFFF))))
{
Store (0x01, Local1)
Break
}
Sleep (0x0A)
}
If (LEqual (Local1, 0x01))
{
Store (And (LPFL, Not (0x20)), LPFL)
Store (0x01, MABT)
Break
}
If (LEqual (Local0, 0x04))
{
Store (Or (LPFL, Or (0x20, 0x80)), LPFL)
Break
}
Increment (Local0)
Store (0x01, GP50)
Sleep (0x64)
Store (0x00, GP50)
}
Return (Zero)
}
Method (C4PD, 0, Serialized)
{
Store (Or (LPFL, 0x10), LPFL)
Store (BMIE, BMIS)
Store (SECB, SNBS)
Store (SBBN, SOBS)
Store (0x00, BMIE)
Store (0xFF, SECB)
Store (0xFE, SBBN)
Store (TPEN, Local0)
Store (0x01, LDIS)
Add (Timer, 0x00989680, Local0)
While (LLessEqual (Timer, Local0))
{
If (LEqual (LACT, 0x00))
{
Store (And (LPFL, Not (0x10)), LPFL)
Break
}
Sleep (0x0A)
}
If (And (LPFL, 0x10))
{
Store (Or (LPFL, Or (0x10, 0x40)), LPFL)
}
Store (0x01, GP50)
Sleep (0x32)
}
Method (C4LP, 0, Serialized)
{
If (LNot (OSDW ()))
{
Return (Zero)
}
If (LAnd (LEqual (And (LPFL, 0x04), 0x00), LEqual (And (
LPFL, 0x03), 0x03)))
{
Store (And (LPFL, Not (0x10)), LPFL)
C4PD ()
Store (Or (LPFL, 0x04), LPFL)
Return (Zero)
}
If (LAnd (LEqual (And (LPFL, 0x04), 0x04), LNotEqual (
And (LPFL, 0x03), 0x03)))
{
Store (And (LPFL, Not (0x20)), LPFL)
C4PU ()
Store (And (LPFL, Not (0x04)), LPFL)
Return (Zero)
}
Return (Zero)
}
Device (GIGE)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (ARE0, PCI_Config, 0x00, 0x04)
Field (ARE0, ByteAcc, NoLock, Preserve)
{
AVND, 16
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x04
})
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
Method (_PSW, 1, NotSerialized) // _PSW: Power State Wake
{
If (Arg0)
{
Store (0x01, GP12)
}
Else
{
Store (0x00, GP12)
}
}
Name (_GPE, 0x1D) // _GPE: General Purpose Events
Method (ELPR, 1, Serialized)
{
If (Arg0)
{
Store (Or (LPFL, 0x01), LPFL)
}
Else
{
Store (And (LPFL, Not (0x01)), LPFL)
}
C4LP ()
}
Method (EDET, 0, NotSerialized)
{
Return (GP13)
}
}
Device (SDXC)
{
Name (_ADR, 0x01) // _ADR: Address
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x1E,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x1E,
0x03
})
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
OperationRegion (ARE1, PCI_Config, 0x00, 0x20)
Field (ARE1, ByteAcc, NoLock, Preserve)
{
AVND, 16,
Offset (0x10),
BARL, 32,
BARH, 32
}
Name (SDAF, 0x0B)
Name (_GPE, 0x1E) // _GPE: General Purpose Events
Method (SLPR, 1, Serialized)
{
If (Arg0)
{
Store (Or (LPFL, 0x02), LPFL)
}
Else
{
Store (And (LPFL, Not (0x02)), LPFL)
}
C4LP ()
Return (LPFL)
}
Method (_PS0, 0, NotSerialized) // _PS0: Power State 0
{
Add (PEBS, ShiftLeft (^^SECB, 0x14), Local0)
Add (Local0, ShiftLeft (_ADR, 0x0C), Local0)
OperationRegion (SDEA, SystemMemory, Local0, 0x20)
Field (SDEA, ByteAcc, NoLock, Preserve)
{
Offset (0x04),
, 1,
MEMD, 1,
BMEN, 1
}
If (LEqual (MEMD, 0x01))
{
STBP (0x01)
}
Else
{
Store (0x01, MEMD)
STBP (0x01)
If (LNotEqual (BMEN, 0x01))
{
Store (0x00, MEMD)
}
}
}
Method (_PS3, 0, NotSerialized) // _PS3: Power State 3
{
STBP (0x03)
}
Method (STPE, 2, NotSerialized)
{
Multiply (Arg0, 0x0D, Local0)
Increment (Local0)
If (LEqual (Arg1, 0x00))
{
CreateByteField (\_SB.SDTB, Local0, ETAG)
Return (ETAG)
}
Else
{
Subtract (Multiply (Arg1, 0x04), 0x03, Local1)
CreateDWordField (\_SB.SDTB, Add (Local0, Local1), EFLD)
Return (EFLD)
}
}
Method (STPR, 1, NotSerialized)
{
Or (ShiftLeft (BARH, 0x20), And (BARL, 0xFFFFFFF0), Local0)
Add (Local0, STPE (Arg0, 0x01), Local0)
OperationRegion (SDRG, SystemMemory, Local0, 0x04)
Field (SDRG, DWordAcc, NoLock, Preserve)
{
RG32, 32
}
Or (And (RG32, STPE (Arg0, 0x02)), STPE (Arg0, 0x03),
RG32)
}
Method (STBP, 1, NotSerialized)
{
Store (0x00, Local0)
Store (DerefOf (Index (\_SB.SDTB, 0x00)), Local1)
While (LLess (Local0, Local1))
{
If (LEqual (STPE (Local0, 0x00), Arg0))
{
STPR (Local0)
}
Increment (Local0)
}
}
}
}
Scope (\_SB.PCI0.RP03)
{
OperationRegion (A1E0, PCI_Config, 0x00, 0x0380)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
Offset (0x04),
BMIE, 3,
Offset (0x19),
SECB, 8,
SBBN, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x4A),
, 5,
TPEN, 1,
Offset (0x50),
, 4,
LDIS, 1,
, 24,
LACT, 1,
Offset (0xA4),
PSTA, 2,
Offset (0xE2),
, 2,
L23E, 1,
L23D, 1,
Offset (0x324),
, 3,
LEDM, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
If (LAnd (LEqual (BMIE, 0x00), LEqual (SECB, 0xFF)))
{
Return (SNBS)
}
Else
{
Return (SECB)
}
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Name (BMIS, 0x00)
Name (SNBS, 0x00)
Name (SOBS, 0x00)
Method (APPD, 0, Serialized)
{
If (LOr (LNot (OSDW ()), LOr (LEqual (WOWE, 0x01), LNotEqual (
TAPD, 0x01))))
{
Return (Zero)
}
Store (0x03, \_SB.PCI0.RP03.ARPT.PSTA)
If (LAnd (LAnd (LNotEqual (BMIE, 0x00), LNotEqual (BMIE,
BMIS)), LAnd (LAnd (LNotEqual (SECB, 0x00), LNotEqual (SECB, SNBS)),
LAnd (LNotEqual (SBBN, 0x00), LNotEqual (SBBN, SOBS)))))
{
Store (BMIE, BMIS)
Store (SECB, SNBS)
Store (SBBN, SOBS)
}
Store (0x00, BMIE)
Store (0xFF, SECB)
Store (0xFE, SBBN)
Store (TPEN, Local0)
Store (0x03, PSTA)
Store (TPEN, Local0)
Store (0x01, LDIS)
Add (Timer, 0x00989680, Local0)
While (LLessEqual (Timer, Local0))
{
If (LEqual (LACT, 0x00))
{
Break
}
Sleep (0x0A)
}
If (LEqual (TAPD, 0x01))
{
Store (0x00, \_SB.PCI0.LPCB.EC.APWC)
Sleep (0x5A)
}
Return (Zero)
}
Method (APPU, 0, Serialized)
{
If (LOr (LNot (OSDW ()), LOr (LEqual (WOWE, 0x01), LNotEqual (
TAPD, 0x01))))
{
Store (0x00, WOWE)
Return (Zero)
}
Store (0x00, PSTA)
If (LNotEqual (SECB, 0xFF))
{
Return (Zero)
}
Store (SOBS, SBBN)
Store (SNBS, SECB)
Store (0x00, LDIS)
Store (0x00, WOWE)
If (LEqual (\_SB.PCI0.LPCB.EC.APWC, 0x01))
{
Return (Zero)
}
Store (0x00, Local0)
While (0x01)
{
Store (0x01, \_SB.PCI0.LPCB.EC.APWC)
Sleep (0xFA)
Store (0x00, Local1)
Add (Timer, 0x00989680, Local2)
While (LLessEqual (Timer, Local2))
{
If (LAnd (LEqual (LACT, 0x01), LNotEqual (\_SB.PCI0.RP03.ARPT.AVND, 0xFFFF)))
{
Store (0x01, Local1)
Break
}
Sleep (0x0A)
}
If (LEqual (Local1, 0x01))
{
Store (0x01, MABT)
Break
}
If (LEqual (Local0, 0x04))
{
Break
}
Increment (Local0)
Store (0x00, \_SB.PCI0.LPCB.EC.APWC)
Sleep (0x5A)
}
Return (Zero)
}
Method (ALPR, 1, NotSerialized)
{
If (LEqual (Arg0, 0x01))
{
APPD ()
}
Else
{
APPU ()
}
}
Method (_PS0, 0, Serialized) // _PS0: Power State 0
{
If (OSDW ())
{
ALPR (0x00)
}
}
Method (_PS3, 0, Serialized) // _PS3: Power State 3
{
If (OSDW ())
{
ALPR (0x01)
}
}
Device (ARPT)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (ARE2, PCI_Config, 0x00, 0xFF)
Field (ARE2, ByteAcc, NoLock, Preserve)
{
AVND, 16,
ADID, 16,
Offset (0x44),
PSTA, 2
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW ())
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x04
})
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
Method (WWEN, 1, NotSerialized)
{
If (LNotEqual (Arg0, 0x00))
{
Store (Arg0, WOWE)
}
}
Method (PDEN, 1, NotSerialized)
{
Store (Arg0, TAPD)
}
}
}
Scope (\_SB.PCI0.RP01)
{
OperationRegion (A1E0, PCI_Config, 0x00, 0x0380)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
Offset (0x04),
BMIE, 3,
Offset (0x19),
SECB, 8,
SBBN, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x4A),
, 5,
TPEN, 1,
Offset (0x50),
ASPM, 2,
, 2,
LDIS, 1,
Offset (0x52),
, 13,
LACT, 1,
Offset (0xA4),
PSTA, 2,
Offset (0xE2),
, 2,
L23E, 1,
L23D, 1,
Offset (0x324),
, 3,
LEDM, 1
}
Device (SSD0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
Store (Package (0x02)
{
"use-msi",
0x00
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3, RefOf (Local0))
Return (Local0)
}
}
}
}
Device (PWRB)
{
Name (_HID, EisaId ("PNP0C0C")) // _HID: Hardware ID
}
}
Scope (\_PR)
{
Processor (CPU0, 0x01, 0x00000410, 0x06) {}
Processor (CPU1, 0x02, 0x00000410, 0x06) {}
Processor (CPU2, 0x03, 0x00000410, 0x06) {}
Processor (CPU3, 0x04, 0x00000410, 0x06) {}
Processor (CPU4, 0x05, 0x00000410, 0x06) {}
Processor (CPU5, 0x06, 0x00000410, 0x06) {}
Processor (CPU6, 0x07, 0x00000410, 0x06) {}
Processor (CPU7, 0x08, 0x00000410, 0x06) {}
}
Mutex (MUTX, 0x00)
Name (SLTP, 0x00)
OperationRegion (PRT0, SystemIO, 0x80, 0x04)
Field (PRT0, DWordAcc, Lock, Preserve)
{
P80H, 32
}
OperationRegion (PLMT, SystemIO, 0x0310, 0x0A)
Field (PLMT, WordAcc, Lock, Preserve)
{
CPLT, 8,
IGPS, 8,
MPLT, 8,
CFIL, 8,
EGPS, 8
}
OperationRegion (S0BA, SystemMemory, 0xE00A8084, 0x04)
Field (S0BA, DWordAcc, Lock, Preserve)
{
S0D3, 2
}
OperationRegion (S4BA, SystemMemory, 0xE00AC084, 0x04)
Field (S4BA, DWordAcc, Lock, Preserve)
{
S4D3, 2
}
OperationRegion (TCOI, SystemIO, 0x0460, 0x08)
Field (TCOI, WordAcc, NoLock, Preserve)
{
Offset (0x04),
, 9,
SCIS, 1,
Offset (0x06)
}
Method (P8XH, 2, Serialized)
{
If (LEqual (Arg0, 0x00))
{
Store (Or (And (P80D, 0xFFFFFF00), Arg1), P80D)
}
If (LEqual (Arg0, 0x01))
{
Store (Or (And (P80D, 0xFFFF00FF), ShiftLeft (Arg1, 0x08)
), P80D)
}
If (LEqual (Arg0, 0x02))
{
Store (Or (And (P80D, 0xFF00FFFF), ShiftLeft (Arg1, 0x10)
), P80D)
}
If (LEqual (Arg0, 0x03))
{
Store (Or (And (P80D, 0x00FFFFFF), ShiftLeft (Arg1, 0x18)
), P80D)
}
Store (P80D, P80H)
}
OperationRegion (SPRT, SystemIO, 0xB2, 0x02)
Field (SPRT, ByteAcc, Lock, Preserve)
{
SSMP, 8,
SSMY, 8
}
Method (\_PIC, 1, NotSerialized) // _PIC: Interrupt Model
{
Store (Arg0, GPIC)
Store (Arg0, PICM)
}
Method (GETB, 3, Serialized)
{
Multiply (Arg0, 0x08, Local0)
Multiply (Arg1, 0x08, Local1)
CreateField (Arg2, Local0, Local1, TBF3)
Return (TBF3)
}
Method (PNOT, 0, Serialized)
{
If (LGreater (TCNT, 0x01))
{
If (And (PDC0, 0x08))
{
Notify (\_PR.CPU0, 0x80)
If (And (PDC0, 0x10))
{
Notify (\_PR.CPU0, 0x81)
}
}
If (And (PDC1, 0x08))
{
Notify (\_PR.CPU1, 0x80)
If (And (PDC1, 0x10))
{
Notify (\_PR.CPU1, 0x81)
}
}
If (And (PDC2, 0x08))
{
Notify (\_PR.CPU2, 0x80)
If (And (PDC2, 0x10))
{
Notify (\_PR.CPU2, 0x81)
}
}
If (And (PDC3, 0x08))
{
Notify (\_PR.CPU3, 0x80)
If (And (PDC3, 0x10))
{
Notify (\_PR.CPU3, 0x81)
}
}
If (And (PDC4, 0x08))
{
Notify (\_PR.CPU4, 0x80)
If (And (PDC4, 0x10))
{
Notify (\_PR.CPU4, 0x81)
}
}
If (And (PDC5, 0x08))
{
Notify (\_PR.CPU5, 0x80)
If (And (PDC5, 0x10))
{
Notify (\_PR.CPU5, 0x81)
}
}
If (And (PDC6, 0x08))
{
Notify (\_PR.CPU6, 0x80)
If (And (PDC6, 0x10))
{
Notify (\_PR.CPU6, 0x81)
}
}
If (And (PDC7, 0x08))
{
Notify (\_PR.CPU7, 0x80)
If (And (PDC7, 0x10))
{
Notify (\_PR.CPU7, 0x81)
}
}
}
Else
{
Notify (\_PR.CPU0, 0x80)
Notify (\_PR.CPU0, 0x81)
}
}
Method (DSPI, 0, Serialized)
{
If (LNot (OSDW ()))
{
Store (0x03, S0D3)
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
While (LNotEqual (Local1, 0x00))
{
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
}
Store (0xCE00AA07, IOIR)
Store (0x0600, IOSR)
Store (0xF000, IONR)
Store (IOSR, Local0)
Or (Local0, 0x01, Local0)
Store (Local0, IOSR)
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
While (LNotEqual (Local1, 0x00))
{
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
}
And (Local0, 0x06, Local1)
If (LEqual (Local1, 0x00))
{
Store (IODR, Local3)
}
Or (Local3, 0x0100, Local3)
Store (0x0700, IOSR)
Store (Local3, IODR)
Store (0xF000, IONR)
Store (IOSR, Local0)
Or (Local0, 0x01, Local0)
Store (Local0, IOSR)
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
While (LNotEqual (Local1, 0x00))
{
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
}
And (Local0, 0x06, Local1)
If (LEqual (Local1, 0x00)) {}
Store (0x03, S4D3)
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
While (LNotEqual (Local1, 0x00))
{
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
}
Store (0xCE00AB07, IOIR)
Store (0x0600, IOSR)
Store (0xF000, IONR)
Store (IOSR, Local0)
Or (Local0, 0x01, Local0)
Store (Local0, IOSR)
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
While (LNotEqual (Local1, 0x00))
{
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
}
And (Local0, 0x06, Local1)
If (LEqual (Local1, 0x00))
{
Store (IODR, Local3)
}
Or (Local3, 0x0100, Local3)
Store (0x0700, IOSR)
Store (Local3, IODR)
Store (0xF000, IONR)
Store (IOSR, Local0)
Or (Local0, 0x01, Local0)
Store (Local0, IOSR)
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
While (LNotEqual (Local1, 0x00))
{
Store (IOSR, Local0)
And (Local0, 0x01, Local1)
}
And (Local0, 0x06, Local1)
If (LEqual (Local1, 0x00)) {}
}
}
Method (TRAP, 2, Serialized)
{
Store (Arg1, SMIF)
If (LEqual (Arg0, \TRTP))
{
Store (0x00, TRP0)
}
If (LEqual (Arg0, \TRTD))
{
Store (Arg1, DTSF)
Store (0x00, TRPD)
Return (DTSF)
}
If (LEqual (Arg0, \TRTI))
{
Store (0x00, TRPH)
}
Return (SMIF)
}
Scope (\_SB)
{
Method (_INI, 0, NotSerialized) // _INI: Initialize
{
PINI ()
}
Device (PNLF)
{
Name (_ADR, 0x00) // _ADR: Address
Name (_HID, EisaId ("APP0002")) // _HID: Hardware ID
Name (_CID, "backlight") // _CID: Compatible ID
Name (_UID, 0x0A) // _UID: Unique ID
Name (_STA, 0x0B) // _STA: Status
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
Store (Package (0x04)
{
"refnum",
0x00,
"type",
BLCT
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3, RefOf (Local0))
Return (Local0)
}
}
Device (SLPB)
{
Name (_HID, EisaId ("PNP0C0E")) // _HID: Hardware ID
Name (_STA, 0x0B) // _STA: Status
}
}
Scope (\_SB.PCI0)
{
Method (_INI, 0, NotSerialized) // _INI: Initialize
{
\_SB.PCI0.RMCR ()
Store (0x07DC, OSYS)
If (CondRefOf (\_OSI, Local0))
{
If (_OSI ("Darwin"))
{
Store (0x2710, OSYS)
}
If (\_OSI ("Linux"))
{
Store (0x03E8, OSYS)
}
If (\_OSI ("Windows 2009"))
{
Store (0x07D9, OSYS)
}
If (\_OSI ("Windows 2012"))
{
Store (0x07DC, OSYS)
}
}
}
Method (NHPG, 0, Serialized)
{
}
Method (NPME, 0, Serialized)
{
}
}
Scope (\)
{
Name (PICM, 0x00)
Method (OSDW, 0, NotSerialized)
{
If (LEqual (OSYS, 0x2710))
{
Return (0x01)
}
Else
{
Return (0x00)
}
}
Method (PINI, 0, NotSerialized)
{
Store (0x07DC, OSYS)
If (CondRefOf (_OSI, Local0))
{
If (_OSI ("Darwin"))
{
Store (0x2710, OSYS)
}
Else
{
If (_OSI ("Linux"))
{
Store (0x03E8, OSYS)
}
Else
{
If (_OSI ("Windows 2009"))
{
Store (0x07D9, OSYS)
}
Else
{
If (_OSI ("Windows 2012"))
{
Store (0x07DC, OSYS)
}
}
}
}
}
Else
{
Store (0x07DC, OSYS)
}
}
}
Scope (\_SB.PCI0)
{
Device (PDRC)
{
Name (_HID, EisaId ("PNP0C02")) // _HID: Hardware ID
Name (_UID, 0x01) // _UID: Unique ID
Name (BUF0, ResourceTemplate ()
{
Memory32Fixed (ReadWrite,
0x00000000, // Address Base
0x00004000, // Address Length
_Y17)
Memory32Fixed (ReadWrite,
0x00000000, // Address Base
0x00008000, // Address Length
_Y19)
Memory32Fixed (ReadWrite,
0x00000000, // Address Base
0x00001000, // Address Length
_Y1A)
Memory32Fixed (ReadWrite,
0x00000000, // Address Base
0x00001000, // Address Length
_Y1B)
Memory32Fixed (ReadWrite,
0x00000000, // Address Base
0x00000000, // Address Length
_Y1C)
Memory32Fixed (ReadWrite,
0xFED20000, // Address Base
0x00020000, // Address Length
)
Memory32Fixed (ReadOnly,
0xFED90000, // Address Base
0x00004000, // Address Length
)
Memory32Fixed (ReadWrite,
0xFED45000, // Address Base
0x0004B000, // Address Length
)
Memory32Fixed (ReadOnly,
0xFF000000, // Address Base
0x01000000, // Address Length
)
Memory32Fixed (ReadOnly,
0xFEE00000, // Address Base
0x00100000, // Address Length
)
Memory32Fixed (ReadWrite,
0x00000000, // Address Base
0x00001000, // Address Length
_Y18)
})
Method (_CRS, 0, Serialized) // _CRS: Current Resource Settings
{
CreateDWordField (BUF0, \_SB.PCI0.PDRC._Y17._BAS, RBR0) // _BAS: Base Address
ShiftLeft (\_SB.PCI0.LPCB.RCBA, 0x0E, RBR0)
CreateDWordField (BUF0, \_SB.PCI0.PDRC._Y18._BAS, TBR0) // _BAS: Base Address
Store (TBAB, TBR0)
CreateDWordField (BUF0, \_SB.PCI0.PDRC._Y18._LEN, TBLN) // _LEN: Length
If (LEqual (TBAB, 0x00))
{
Store (0x00, TBLN)
}
CreateDWordField (BUF0, \_SB.PCI0.PDRC._Y19._BAS, MBR0) // _BAS: Base Address
ShiftLeft (\_SB.PCI0.MHBR, 0x0F, MBR0)
CreateDWordField (BUF0, \_SB.PCI0.PDRC._Y1A._BAS, DBR0) // _BAS: Base Address
ShiftLeft (\_SB.PCI0.DIBR, 0x0C, DBR0)
CreateDWordField (BUF0, \_SB.PCI0.PDRC._Y1B._BAS, EBR0) // _BAS: Base Address
ShiftLeft (\_SB.PCI0.EPBR, 0x0C, EBR0)
CreateDWordField (BUF0, \_SB.PCI0.PDRC._Y1C._BAS, XBR0) // _BAS: Base Address
ShiftLeft (\_SB.PCI0.PXBR, 0x1A, XBR0)
CreateDWordField (BUF0, \_SB.PCI0.PDRC._Y1C._LEN, XSZ0) // _LEN: Length
ShiftRight (0x10000000, \_SB.PCI0.PXSZ, XSZ0)
Return (BUF0)
}
}
}
Scope (\)
{
OperationRegion (IO_T, SystemIO, 0x0800, 0x10)
Field (IO_T, ByteAcc, NoLock, Preserve)
{
TRPI, 16,
Offset (0x04),
Offset (0x06),
Offset (0x08),
TRP0, 8,
Offset (0x0A),
Offset (0x0B),
Offset (0x0C),
Offset (0x0D),
Offset (0x0E),
Offset (0x0F),
Offset (0x10)
}
OperationRegion (IO_D, SystemIO, 0x0810, 0x04)
Field (IO_D, ByteAcc, NoLock, Preserve)
{
TRPD, 8
}
OperationRegion (IO_H, SystemIO, 0x1000, 0x04)
Field (IO_H, ByteAcc, NoLock, Preserve)
{
TRPH, 8
}
OperationRegion (RCRB, SystemMemory, \SRCB, 0x4000)
Field (RCRB, DWordAcc, Lock, Preserve)
{
Offset (0x1000),
Offset (0x2330),
IOIR, 32,
IODR, 32,
IOSR, 16,
IONR, 16,
Offset (0x3000),
Offset (0x3404),
HPAS, 2,
, 5,
HPAE, 1,
Offset (0x3418),
, 1,
, 1,
SATD, 1,
SMBD, 1,
HDAD, 1,
, 2,
UH6D, 1,
UH1D, 1,
UH2D, 1,
UH3D, 1,
UH4D, 1,
UH5D, 1,
Offset (0x341A),
RP1D, 1,
RP2D, 1,
RP3D, 1,
RP4D, 1,
RP5D, 1,
RP6D, 1,
RP7D, 1,
RP8D, 1,
, 4,
UH7D, 1
}
}
Scope (\_GPE)
{
Method (_L07, 0, NotSerialized) // _Lxx: Level-Triggered GPE
{
Store (0x20, \_SB.PCI0.SBUS.HSTS)
}
Method (_L06, 0, NotSerialized) // _Lxx: Level-Triggered GPE
{
If (LAnd (\_SB.PCI0.IGPU.GSSE, LNot (GSMI)))
{
\_SB.PCI0.IGPU.GSCI ()
}
Else
{
Store (0x00, \_SB.PCI0.IGPU.GEFC)
Store (0x01, SCIS)
Store (0x00, \_SB.PCI0.IGPU.GSSE)
Store (0x00, \_SB.PCI0.IGPU.SCIE)
}
}
Method (_L09, 0, NotSerialized) // _Lxx: Level-Triggered GPE
{
Notify (\_SB.PCI0.P0P2, 0x02)
Notify (\_SB.PCI0.RP01, 0x02)
Notify (\_SB.PCI0.RP03, 0x02)
Notify (\_SB.PCI0.RP04, 0x02)
Notify (\_SB.PCI0.RP05, 0x02)
\_SB.PCI0.TGPE ()
Notify (\_SB.PCI0.RP04.GIGE, 0x02)
Notify (\_SB.PCI0.RP03.ARPT, 0x02)
}
Method (_L0D, 0, NotSerialized) // _Lxx: Level-Triggered GPE
{
Notify (\_SB.PWRB, 0x02)
Notify (\_SB.PCI0.XHC1, 0x02)
If (OSDW ())
{
Notify (\_SB.PCI0.HDEF, 0x02)
}
}
}
Method (DTGP, 5, NotSerialized)
{
If (LEqual (Arg0, Buffer (0x10)
{
/* 0000 */ 0xC6, 0xB7, 0xB5, 0xA0, 0x18, 0x13, 0x1C, 0x44,
/* 0008 */ 0xB0, 0xC9, 0xFE, 0x69, 0x5E, 0xAF, 0x94, 0x9B
}))
{
If (LEqual (Arg1, One))
{
If (LEqual (Arg2, Zero))
{
Store (Buffer (0x01)
{
0x03
}, Arg4)
Return (One)
}
If (LEqual (Arg2, One))
{
Return (One)
}
}
}
Store (Buffer (0x01)
{
0x00
}, Arg4)
Return (Zero)
}
Name (_S0, Package (0x03) // _S0_: S0 System State
{
0x00,
0x00,
0x00
})
Name (_S4, Package (0x03) // _S4_: S4 System State
{
0x06,
0x06,
0x00
})
Name (_S5, Package (0x03) // _S5_: S5 System State
{
0x07,
0x07,
0x00
})
Method (_TTS, 1, NotSerialized) // _TTS: Transition To State
{
Store (Arg0, SLTP)
}
Method (_PTS, 1, NotSerialized) // _PTS: Prepare To Sleep
{
Store (0x00, P80D)
P8XH (0x00, Arg0)
Store (Arg0, \_SB.PCI0.LPCB.EC.ECSS)
Store (0x00, GP50)
If (LNot (OSDW ()))
{
Store (0x01, GP12)
If (LOr (LEqual (Arg0, 0x04), LEqual (Arg0, 0x05)))
{
Store (0x01, GD24)
Sleep (0x64)
Sleep (0x64)
Store (0x0A, Local0)
While (LGreater (Local0, 0x00))
{
Decrement (Local0)
Sleep (0x64)
If (LEqual (GP24, 0x00))
{
Break
}
}
Store (0x00, GP23)
Sleep (0xFA)
}
}
If (LAnd (LNot (OSDW ()), LGreaterEqual (Arg0, 0x04)))
{
Store (0x00, \_SB.PCI0.LPCB.EC.EWLO)
}
}
Method (_WAK, 1, NotSerialized) // _WAK: Wake
{
P8XH (0x00, 0x00)
Store (0x00, \_SB.PCI0.LPCB.EC.ECSS)
If (OSDW ()) {}
\_SB.PCI0.SBUS.BUS0.BLC0.BCAL ()
Store (\_SB.PCI0.LPCB.EC.EACP, PWRS)
If (LNot (OSDW ()))
{
Store (0x00, \_SB.PCI0.LPCB.EC.LWE0)
Store (0x00, \_SB.PCI0.LPCB.EC.LWE1)
Store (0x00, \_SB.PCI0.LPCB.EC.LWE2)
Store (0x00, \_SB.PCI0.LPCB.EC.LWE3)
If (LEqual (Arg0, 0x03))
{
\_SB.PCI0.DTLK ()
}
If (LEqual (Arg0, 0x04))
{
\_SB.PCI0.RMCW ()
}
}
PNOT ()
Return (Package (0x02)
{
0x00,
0x00
})
}
Scope (\)
{
OperationRegion (GPIO, SystemIO, \GPBS, 0x64)
Field (GPIO, ByteAcc, NoLock, Preserve)
{
, 5,
GU05, 1,
Offset (0x01),
Offset (0x02),
Offset (0x03),
Offset (0x04),
GD00, 4,
GD04, 1,
, 5,
GD10, 1,
, 1,
GD12, 1,
, 1,
GD14, 1,
Offset (0x07),
GD24, 1,
Offset (0x08),
Offset (0x0C),
, 3,
GP03, 1,
GP04, 1,
GP05, 1,
GP06, 1,
GP07, 1,
GP08, 1,
GP09, 1,
GP10, 1,
GP11, 1,
GP12, 1,
GP13, 1,
GP14, 1,
GP15, 1,
GP16, 1,
GP17, 1,
GP18, 1,
GP19, 1,
GP20, 1,
GP21, 1,
GP22, 1,
GP23, 1,
GP24, 1,
, 2,
GP27, 1,
GP28, 1,
Offset (0x10),
Offset (0x18),
GB00, 8,
GB01, 8,
GB02, 8,
GB03, 8,
Offset (0x2C),
, 3,
GI03, 1,
GI04, 1,
GI05, 1,
GI06, 1,
Offset (0x2D),
GI08, 1,
GI09, 1,
GI10, 1,
GI11, 1,
Offset (0x2E),
Offset (0x2F),
Offset (0x30),
Offset (0x31),
Offset (0x32),
Offset (0x33),
Offset (0x34),
Offset (0x35),
GD40, 1,
GD41, 1,
GD42, 1,
, 1,
GD44, 1,
, 1,
GD46, 1,
Offset (0x36),
, 6,
GD54, 1,
, 4,
GD59, 1,
GD60, 1,
Offset (0x38),
, 1,
GP33, 1,
, 2,
GP36, 1,
Offset (0x39),
GP40, 1,
GP41, 1,
GP42, 1,
, 1,
GP44, 1,
GP45, 1,
GP46, 1,
Offset (0x3A),
GP48, 1,
GP49, 1,
GP50, 1,
GP51, 1,
GP52, 1,
GP53, 1,
GP54, 1,
, 4,
GP59, 1,
GP60, 1,
Offset (0x3C),
Offset (0x40),
Offset (0x41),
Offset (0x42),
Offset (0x43),
Offset (0x44),
, 4,
GD68, 1,
GD69, 1,
GD70, 1,
GD71, 1,
GD72, 1,
GD73, 1,
GD74, 1,
, 4,
, 8,
, 8,
Offset (0x48),
GP64, 1,
, 3,
GP68, 1,
GP69, 1,
Offset (0x49),
GP72, 1,
GP73, 1,
GP74, 1,
Offset (0x4A),
Offset (0x4B),
Offset (0x4C)
}
}
}

ECDT

View File ECDT.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/ECDT.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [ECDT]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "ECDT" [Embedded Controller Boot Resources Table]
[004h 0004 4] Table Length : 00000053
[008h 0008 1] Revision : 01
[009h 0009 1] Checksum : 39
[00Ah 0010 6] Oem ID : "APPLE "
[010h 0016 8] Oem Table ID : "Apple00"
[018h 0024 4] Oem Revision : 00000001
[01Ch 0028 4] Asl Compiler ID : "Loki"
[020h 0032 4] Asl Compiler Revision : 0000005F
[024h 0036 12] Command/Status Register : [Generic Address Structure]
[024h 0036 1] Space ID : 01 [SystemIO]
[025h 0037 1] Bit Width : 08
[026h 0038 1] Bit Offset : 00
[027h 0039 1] Encoded Access Width : 00 [Undefined/Legacy]
[028h 0040 8] Address : 0000000000000066
[030h 0048 12] Data Register : [Generic Address Structure]
[030h 0048 1] Space ID : 01 [SystemIO]
[031h 0049 1] Bit Width : 08
[032h 0050 1] Bit Offset : 00
[033h 0051 1] Encoded Access Width : 00 [Undefined/Legacy]
[034h 0052 8] Address : 0000000000000062
[03Ch 0060 4] UID : 00000000
[040h 0064 1] GPE Number : 17
[041h 0065 18] Namepath : "\_SB.PCI0.LPCB.EC"
Raw Table Data: Length 83 (0x53)
0000: 45 43 44 54 53 00 00 00 01 39 41 50 50 4C 45 20 ECDTS....9APPLE
0010: 41 70 70 6C 65 30 30 00 01 00 00 00 4C 6F 6B 69 Apple00.....Loki
0020: 5F 00 00 00 01 08 00 00 66 00 00 00 00 00 00 00 _.......f.......
0030: 01 08 00 00 62 00 00 00 00 00 00 00 00 00 00 00 ....b...........
0040: 17 5C 5F 53 42 2E 50 43 49 30 2E 4C 50 43 42 2E .\_SB.PCI0.LPCB.
0050: 45 43 00 EC.

FACP

View File FACP.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/FACP.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [FACP]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "FACP" [Fixed ACPI Description Table (FADT)]
[004h 0004 4] Table Length : 000000F4
[008h 0008 1] Revision : 05
[009h 0009 1] Checksum : 2F
[00Ah 0010 6] Oem ID : "APPLE "
[010h 0016 8] Oem Table ID : "Apple00"
[018h 0024 4] Oem Revision : 00000000
[01Ch 0028 4] Asl Compiler ID : "Loki"
[020h 0032 4] Asl Compiler Revision : 0000005F
[024h 0036 4] FACS Address : 8CD1C000
[028h 0040 4] DSDT Address : 8CD80000
[02Ch 0044 1] Model : 00
[02Dh 0045 1] PM Profile : 01 [Desktop]
[02Eh 0046 2] SCI Interrupt : 0009
[030h 0048 4] SMI Command Port : 000000B2
[034h 0052 1] ACPI Enable Value : F0
[035h 0053 1] ACPI Disable Value : F1
[036h 0054 1] S4BIOS Command : 00
[037h 0055 1] P-State Control : 00
[038h 0056 4] PM1A Event Block Address : 00000400
[03Ch 0060 4] PM1B Event Block Address : 00000000
[040h 0064 4] PM1A Control Block Address : 00000404
[044h 0068 4] PM1B Control Block Address : 00000000
[048h 0072 4] PM2 Control Block Address : 00000450
[04Ch 0076 4] PM Timer Block Address : 00000408
[050h 0080 4] GPE0 Block Address : 00000420
[054h 0084 4] GPE1 Block Address : 00000000
[058h 0088 1] PM1 Event Block Length : 04
[059h 0089 1] PM1 Control Block Length : 02
[05Ah 0090 1] PM2 Control Block Length : 01
[05Bh 0091 1] PM Timer Block Length : 04
[05Ch 0092 1] GPE0 Block Length : 10
[05Dh 0093 1] GPE1 Block Length : 00
[05Eh 0094 1] GPE1 Base Offset : 10
[05Fh 0095 1] _CST Support : 85
[060h 0096 2] C2 Latency : 0065
[062h 0098 2] C3 Latency : 03E9
[064h 0100 2] CPU Cache Size : 0000
[066h 0102 2] Cache Flush Stride : 0000
[068h 0104 1] Duty Cycle Offset : 01
[069h 0105 1] Duty Cycle Width : 03
[06Ah 0106 1] RTC Day Alarm Index : 0D
[06Bh 0107 1] RTC Month Alarm Index : 00
[06Ch 0108 1] RTC Century Index : 32
[06Dh 0109 2] Boot Flags (decoded below) : 0001
Legacy Devices Supported (V2) : 1
8042 Present on ports 60/64 (V2) : 0
VGA Not Present (V4) : 0
MSI Not Supported (V4) : 0
PCIe ASPM Not Supported (V4) : 0
CMOS RTC Not Present (V5) : 0
[06Fh 0111 1] Reserved : 00
[070h 0112 4] Flags (decoded below) : 0000C4A5
WBINVD instruction is operational (V1) : 1
WBINVD flushes all caches (V1) : 0
All CPUs support C1 (V1) : 1
C2 works on MP system (V1) : 0
Control Method Power Button (V1) : 0
Control Method Sleep Button (V1) : 1
RTC wake not in fixed reg space (V1) : 0
RTC can wake system from S4 (V1) : 1
32-bit PM Timer (V1) : 0
Docking Supported (V1) : 0
Reset Register Supported (V2) : 1
Sealed Case (V3) : 0
Headless - No Video (V3) : 0
Use native instr after SLP_TYPx (V3) : 0
PCIEXP_WAK Bits Supported (V4) : 1
Use Platform Timer (V4) : 1
RTC_STS valid on S4 wake (V4) : 0
Remote Power-on capable (V4) : 0
Use APIC Cluster Model (V4) : 0
Use APIC Physical Destination Mode (V4) : 0
Hardware Reduced (V5) : 0
Low Power S0 Idle (V5) : 0
[074h 0116 12] Reset Register : [Generic Address Structure]
[074h 0116 1] Space ID : 01 [SystemIO]
[075h 0117 1] Bit Width : 08
[076h 0118 1] Bit Offset : 00
[077h 0119 1] Encoded Access Width : 01 [Byte Access:8]
[078h 0120 8] Address : 0000000000000CF9
[080h 0128 1] Value to cause reset : 06
[081h 0129 3] Reserved : 000000
[084h 0132 8] FACS Address : 000000008CD1C000
[08Ch 0140 8] DSDT Address : 000000008CD80000
[094h 0148 12] PM1A Event Block : [Generic Address Structure]
[094h 0148 1] Space ID : 01 [SystemIO]
[095h 0149 1] Bit Width : 20
[096h 0150 1] Bit Offset : 00
[097h 0151 1] Encoded Access Width : 03 [DWord Access:32]
[098h 0152 8] Address : 0000000000000400
[0A0h 0160 12] PM1B Event Block : [Generic Address Structure]
[0A0h 0160 1] Space ID : 01 [SystemIO]
[0A1h 0161 1] Bit Width : 00
[0A2h 0162 1] Bit Offset : 00
[0A3h 0163 1] Encoded Access Width : 00 [Undefined/Legacy]
[0A4h 0164 8] Address : 0000000000000000
[0ACh 0172 12] PM1A Control Block : [Generic Address Structure]
[0ACh 0172 1] Space ID : 01 [SystemIO]
[0ADh 0173 1] Bit Width : 10
[0AEh 0174 1] Bit Offset : 00
[0AFh 0175 1] Encoded Access Width : 02 [Word Access:16]
[0B0h 0176 8] Address : 0000000000000404
[0B8h 0184 12] PM1B Control Block : [Generic Address Structure]
[0B8h 0184 1] Space ID : 01 [SystemIO]
[0B9h 0185 1] Bit Width : 00
[0BAh 0186 1] Bit Offset : 00
[0BBh 0187 1] Encoded Access Width : 00 [Undefined/Legacy]
[0BCh 0188 8] Address : 0000000000000000
[0C4h 0196 12] PM2 Control Block : [Generic Address Structure]
[0C4h 0196 1] Space ID : 01 [SystemIO]
[0C5h 0197 1] Bit Width : 08
[0C6h 0198 1] Bit Offset : 00
[0C7h 0199 1] Encoded Access Width : 00 [Undefined/Legacy]
[0C8h 0200 8] Address : 0000000000000450
[0D0h 0208 12] PM Timer Block : [Generic Address Structure]
[0D0h 0208 1] Space ID : 01 [SystemIO]
[0D1h 0209 1] Bit Width : 20
[0D2h 0210 1] Bit Offset : 00
[0D3h 0211 1] Encoded Access Width : 03 [DWord Access:32]
[0D4h 0212 8] Address : 0000000000000408
[0DCh 0220 12] GPE0 Block : [Generic Address Structure]
[0DCh 0220 1] Space ID : 01 [SystemIO]
[0DDh 0221 1] Bit Width : 00
[0DEh 0222 1] Bit Offset : 00
[0DFh 0223 1] Encoded Access Width : 01 [Byte Access:8]
[0E0h 0224 8] Address : 0000000000000420
[0E8h 0232 12] GPE1 Block : [Generic Address Structure]
[0E8h 0232 1] Space ID : 01 [SystemIO]
[0E9h 0233 1] Bit Width : 00
[0EAh 0234 1] Bit Offset : 00
[0EBh 0235 1] Encoded Access Width : 01 [Byte Access:8]
[0ECh 0236 8] Address : 0000000000000000
// ACPI Warning: FADT revision 5 does not match length: found F4 expected 10C
Raw Table Data: Length 244 (0xF4)
0000: 46 41 43 50 F4 00 00 00 05 2F 41 50 50 4C 45 20 FACP...../APPLE
0010: 41 70 70 6C 65 30 30 00 00 00 00 00 4C 6F 6B 69 Apple00.....Loki
0020: 5F 00 00 00 00 C0 D1 8C 00 00 D8 8C 00 01 09 00 _...............
0030: B2 00 00 00 F0 F1 00 00 00 04 00 00 00 00 00 00 ................
0040: 04 04 00 00 00 00 00 00 50 04 00 00 08 04 00 00 ........P.......
0050: 20 04 00 00 00 00 00 00 04 02 01 04 10 00 10 85 ...............
0060: 65 00 E9 03 00 00 00 00 01 03 0D 00 32 01 00 00 e...........2...
0070: A5 C4 00 00 01 08 00 01 F9 0C 00 00 00 00 00 00 ................
0080: 06 00 00 00 00 C0 D1 8C 00 00 00 00 00 00 D8 8C ................
0090: 00 00 00 00 01 20 00 03 00 04 00 00 00 00 00 00 ..... ..........
00A0: 01 00 00 00 00 00 00 00 00 00 00 00 01 10 00 02 ................
00B0: 04 04 00 00 00 00 00 00 01 00 00 00 00 00 00 00 ................
00C0: 00 00 00 00 01 08 00 00 50 04 00 00 00 00 00 00 ........P.......
00D0: 01 20 00 03 08 04 00 00 00 00 00 00 01 00 00 01 . ..............
00E0: 20 04 00 00 00 00 00 00 01 00 00 01 00 00 00 00 ...............
00F0: 00 00 00 00 ....

FACS

View File FACS.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/FACS.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [FACS]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "FACS"
[004h 0004 4] Length : 00000040
[008h 0008 4] Hardware Signature : 00000000
[00Ch 0012 4] 32 Firmware Waking Vector : 00000000
[010h 0016 4] Global Lock : 00000000
[014h 0020 4] Flags (decoded below) : 00000000
S4BIOS Support Present : 0
64-bit Wake Supported (V2) : 0
[018h 0024 8] 64 Firmware Waking Vector : 0000000000000000
[020h 0032 1] Version : 01
[021h 0033 3] Reserved : 000000
[024h 0036 4] OspmFlags (decoded below) : 00000000
64-bit Wake Env Required (V2) : 0
Raw Table Data: Length 64 (0x40)
0000: 46 41 43 53 40 00 00 00 00 00 00 00 00 00 00 00 FACS@...........
0010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................
0020: 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................
0030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

HPET

View File HPET.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/HPET.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [HPET]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "HPET" [High Precision Event Timer table]
[004h 0004 4] Table Length : 00000038
[008h 0008 1] Revision : 01
[009h 0009 1] Checksum : 8C
[00Ah 0010 6] Oem ID : "APPLE "
[010h 0016 8] Oem Table ID : "Apple00"
[018h 0024 4] Oem Revision : 00000001
[01Ch 0028 4] Asl Compiler ID : "Loki"
[020h 0032 4] Asl Compiler Revision : 0000005F
[024h 0036 4] Hardware Block ID : 8086A201
[028h 0040 12] Timer Block Register : [Generic Address Structure]
[028h 0040 1] Space ID : 00 [SystemMemory]
[029h 0041 1] Bit Width : 40
[02Ah 0042 1] Bit Offset : 00
[02Bh 0043 1] Encoded Access Width : 00 [Undefined/Legacy]
[02Ch 0044 8] Address : 00000000FED00000
[034h 0052 1] Sequence Number : 00
[035h 0053 2] Minimum Clock Ticks : 0080
[037h 0055 1] Flags (decoded below) : 00
4K Page Protect : 0
64K Page Protect : 0
Raw Table Data: Length 56 (0x38)
0000: 48 50 45 54 38 00 00 00 01 8C 41 50 50 4C 45 20 HPET8.....APPLE
0010: 41 70 70 6C 65 30 30 00 01 00 00 00 4C 6F 6B 69 Apple00.....Loki
0020: 5F 00 00 00 01 A2 86 80 00 40 00 00 00 00 D0 FE _........@......
0030: 00 00 00 00 00 80 00 00 ........

MCFG

View File MCFG.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/MCFG.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [MCFG]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "MCFG" [Memory Mapped Configuration table]
[004h 0004 4] Table Length : 0000003C
[008h 0008 1] Revision : 01
[009h 0009 1] Checksum : 58
[00Ah 0010 6] Oem ID : "APPLE "
[010h 0016 8] Oem Table ID : "Apple00"
[018h 0024 4] Oem Revision : 00000001
[01Ch 0028 4] Asl Compiler ID : "Loki"
[020h 0032 4] Asl Compiler Revision : 0000005F
[024h 0036 8] Reserved : 0000000000000000
[02Ch 0044 8] Base Address : 00000000E0000000
[034h 0052 2] Segment Group Number : 0000
[036h 0054 1] Start Bus Number : 00
[037h 0055 1] End Bus Number : 9B
[038h 0056 4] Reserved : 00000000
Raw Table Data: Length 60 (0x3C)
0000: 4D 43 46 47 3C 00 00 00 01 58 41 50 50 4C 45 20 MCFG<....XAPPLE
0010: 41 70 70 6C 65 30 30 00 01 00 00 00 4C 6F 6B 69 Apple00.....Loki
0020: 5F 00 00 00 00 00 00 00 00 00 00 00 00 00 00 E0 _...............
0030: 00 00 00 00 00 00 00 9B 00 00 00 00 ............

RSDT

View File RSDT.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/RSDT.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [XSDT]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "XSDT" [Extended System Description Table]
[004h 0004 4] Table Length : 0000009C
[008h 0008 1] Revision : 01
[009h 0009 1] Checksum : 59
[00Ah 0010 6] Oem ID : "APPLE "
[010h 0016 8] Oem Table ID : "Apple00"
[018h 0024 4] Oem Revision : 00000000
[01Ch 0028 4] Asl Compiler ID : " "
[020h 0032 4] Asl Compiler Revision : 01000013
[024h 0036 8] ACPI Table Address 0 : 000000008CD8C000
[02Ch 0044 8] ACPI Table Address 1 : 000000008CD8B000
[034h 0052 8] ACPI Table Address 2 : 000000008CD8A000
[03Ch 0060 8] ACPI Table Address 3 : 000000008CD88000
[044h 0068 8] ACPI Table Address 4 : 000000008CD87000
[04Ch 0076 8] ACPI Table Address 5 : 000000008CD7F000
[054h 0084 8] ACPI Table Address 6 : 000000008CD7E000
[05Ch 0092 8] ACPI Table Address 7 : 000000008CD7A000
[064h 0100 8] ACPI Table Address 8 : 000000008CD79000
[06Ch 0108 8] ACPI Table Address 9 : 000000008CD75000
[074h 0116 8] ACPI Table Address 10 : 000000008CD64000
[07Ch 0124 8] ACPI Table Address 11 : 000000008CD63000
[084h 0132 8] ACPI Table Address 12 : 000000008CD62000
[08Ch 0140 8] ACPI Table Address 13 : 000000008CD89000
[094h 0148 8] ACPI Table Address 14 : 000000008CD61000
Raw Table Data: Length 156 (0x9C)
0000: 58 53 44 54 9C 00 00 00 01 59 41 50 50 4C 45 20 XSDT.....YAPPLE
0010: 41 70 70 6C 65 30 30 00 00 00 00 00 20 20 20 20 Apple00.....
0020: 13 00 00 01 00 C0 D8 8C 00 00 00 00 00 B0 D8 8C ................
0030: 00 00 00 00 00 A0 D8 8C 00 00 00 00 00 80 D8 8C ................
0040: 00 00 00 00 00 70 D8 8C 00 00 00 00 00 F0 D7 8C .....p..........
0050: 00 00 00 00 00 E0 D7 8C 00 00 00 00 00 A0 D7 8C ................
0060: 00 00 00 00 00 90 D7 8C 00 00 00 00 00 50 D7 8C .............P..
0070: 00 00 00 00 00 40 D6 8C 00 00 00 00 00 30 D6 8C .....@.......0..
0080: 00 00 00 00 00 20 D6 8C 00 00 00 00 00 90 D8 8C ..... ..........
0090: 00 00 00 00 00 10 D6 8C 00 00 00 00 ............

SBST

View File SBST.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SBST.aml, Mon May 26 01:26:33 2014
*
* ACPI Data Table [SBST]
*
* Format: [HexOffset DecimalOffset ByteLength] FieldName : FieldValue
*/
[000h 0000 4] Signature : "SBST" [Smart Battery Specification Table]
[004h 0004 4] Table Length : 00000030
[008h 0008 1] Revision : 01
[009h 0009 1] Checksum : 84
[00Ah 0010 6] Oem ID : "APPLE "
[010h 0016 8] Oem Table ID : "Apple00"
[018h 0024 4] Oem Revision : 00000001
[01Ch 0028 4] Asl Compiler ID : "Loki"
[020h 0032 4] Asl Compiler Revision : 0000005F
[024h 0036 4] Warning Level : 0000001E
[028h 0040 4] Low Level : 00000014
[02Ch 0044 4] Critical Level : 0000000A
Raw Table Data: Length 48 (0x30)
0000: 53 42 53 54 30 00 00 00 01 84 41 50 50 4C 45 20 SBST0.....APPLE
0010: 41 70 70 6C 65 30 30 00 01 00 00 00 4C 6F 6B 69 Apple00.....Loki
0020: 5F 00 00 00 1E 00 00 00 14 00 00 00 0A 00 00 00 _...............

SSDT-1

View File SSDT-1.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-1.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "SSDT"
* Length 0x000000B1 (177)
* Revision 0x01
* Checksum 0x1B
* OEM ID "APPLE "
* OEM Table ID "SmcDppt"
* OEM Revision 0x00001000 (4096)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-1.aml", "SSDT", 1, "APPLE ", "SmcDppt", 0x00001000)
{
External (_SB_.PCI0.LPCB.EC__, DeviceObj)
External (_SB_.PCI0.LPCB.SMC_, DeviceObj)
Scope (\_SB.PCI0.LPCB.SMC)
{
Device (DPPT)
{
Name (_HID, EisaId ("APP000C")) // _HID: Hardware ID
Name (_CID, "smc-dppt") // _CID: Compatible ID
}
}
Scope (\_SB.PCI0.LPCB.EC)
{
Method (_Q30, 0, NotSerialized) // _Qxx: EC Query
{
Notify (\_SB.PCI0.LPCB.SMC.DPPT, 0x80)
}
Method (_Q31, 0, NotSerialized) // _Qxx: EC Query
{
Notify (\_SB.PCI0.LPCB.SMC.DPPT, 0x81)
}
}
}

SSDT-2

View File SSDT-2.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-2.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "SSDT"
* Length 0x0000065A (1626)
* Revision 0x01
* Checksum 0x53
* OEM ID "APPLE "
* OEM Table ID "UsbLpt"
* OEM Revision 0x00001000 (4096)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-2.aml", "SSDT", 1, "APPLE ", "UsbLpt", 0x00001000)
{
/*
* iASL Warning: There were 1 external control methods found during
* disassembly, but additional ACPI tables to resolve these externals
* were not specified. This resulting disassembler output file may not
* compile because the disassembler did not know how many arguments
* to assign to these methods. To specify the tables needed to resolve
* external control method references, use the one of the following
* example iASL invocations:
* iasl -e <ssdt1.aml,ssdt2.aml...> -d <dsdt.aml>
* iasl -e <dsdt.aml,ssdt2.aml...> -d <ssdt1.aml>
*/
External (DTGP, MethodObj) // Warning: Unresolved Method, guessing 4 arguments (may be incorrect, see warning above)
External (_SB_.PCI0, DeviceObj)
External (GD54)
External (GP54)
External (OSDW, IntObj)
Scope (\_SB.PCI0)
{
Device (XHC1)
{
Name (_ADR, 0x00140000) // _ADR: Address
OperationRegion (XH1C, PCI_Config, 0xD0, 0x10)
Field (XH1C, ByteAcc, NoLock, Preserve)
{
PAHC, 1,
PCHC, 1,
Offset (0x01),
PBHC, 1,
PDHC, 1,
Offset (0x08),
PASS, 1,
PBSS, 1,
PCSS, 1,
PDSS, 1
}
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW)
{
Return (Package (0x02)
{
0x0D,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x0D,
0x03
})
}
}
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
Store (Package (0x09)
{
"AAPL,current-available",
0x0834,
"AAPL,current-extra",
0x0A8C,
"AAPL,current-extra-in-sleep",
0x0A8C,
"AAPL,max-port-current-in-sleep",
0x0834,
Buffer (0x01)
{
0x00
}
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3)
RefOf (Local0)
Return (Local0)
}
Method (XHCA, 0, NotSerialized)
{
If (LNot (OSDW))
{
Store (0x01, \_SB.PCI0.XHC1.PASS)
}
Store (0x01, \_SB.PCI0.XHC1.PAHC)
}
Method (XHCB, 0, NotSerialized)
{
If (LNot (OSDW))
{
Store (0x01, \_SB.PCI0.XHC1.PBSS)
}
Store (0x01, \_SB.PCI0.XHC1.PBHC)
}
Method (XHCC, 0, NotSerialized)
{
If (LNot (OSDW))
{
Store (0x01, \_SB.PCI0.XHC1.PCSS)
}
Store (0x01, \_SB.PCI0.XHC1.PCHC)
}
Method (XHCD, 0, NotSerialized)
{
If (LNot (OSDW))
{
Store (0x01, \_SB.PCI0.XHC1.PDSS)
}
Store (0x01, \_SB.PCI0.XHC1.PDHC)
}
Method (EHCA, 0, NotSerialized)
{
If (LNot (OSDW))
{
Store (0x00, \_SB.PCI0.XHC1.PASS)
}
Store (0x00, \_SB.PCI0.XHC1.PAHC)
}
Method (EHCB, 0, NotSerialized)
{
If (LNot (OSDW))
{
Store (0x00, \_SB.PCI0.XHC1.PBSS)
}
Store (0x00, \_SB.PCI0.XHC1.PBHC)
}
Method (EHCC, 0, NotSerialized)
{
If (LNot (OSDW))
{
Store (0x00, \_SB.PCI0.XHC1.PCSS)
}
Store (0x00, \_SB.PCI0.XHC1.PCHC)
}
Method (EHCD, 0, NotSerialized)
{
If (LNot (OSDW))
{
Store (0x00, \_SB.PCI0.XHC1.PDSS)
}
Store (0x00, \_SB.PCI0.XHC1.PDHC)
}
Device (RHUB)
{
Name (_ADR, 0x00) // _ADR: Address
Device (HS01)
{
Name (_ADR, 0x01) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0x03,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x31,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
Name (MUXS, "EHCA")
}
Device (HS02)
{
Name (_ADR, 0x02) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0x03,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x30,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
Name (MUXS, "EHCC")
}
Device (HS05)
{
Name (_ADR, 0x05) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0x03,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x31,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
Name (MUXS, "EHCB")
}
Device (HS06)
{
Name (_ADR, 0x06) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0x03,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x30,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
Name (MUXS, "EHCD")
}
Device (HS07)
{
Name (_ADR, 0x07) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0xFF,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x30,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
}
Device (HS08)
{
Name (_ADR, 0x08) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0xFF,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x30,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
}
Device (SSP1)
{
Name (_ADR, 0x10) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0x03,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x31,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
Name (XHCP, 0x01)
}
Device (SSP2)
{
Name (_ADR, 0x11) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0x03,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x31,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
Name (XHCP, 0x05)
}
Device (SSP5)
{
Name (_ADR, 0x14) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0x03,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x31,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
Name (XHCP, 0x02)
}
Device (SSP6)
{
Name (_ADR, 0x15) // _ADR: Address
Name (_UPC, Package (0x04) // _UPC: USB Port Capabilities
{
0xFF,
0x03,
0x00,
0x00
})
Name (_PLD, Package (0x10) // _PLD: Physical Location of Device
{
0x81,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00,
0x31,
0x1C,
0x00,
0x00,
0x00,
0x00,
0x00,
0x00
})
Name (XHCP, 0x06)
}
}
Method (XEPC, 0, NotSerialized)
{
Return (0x60)
}
Method (MBSD, 0, NotSerialized)
{
Return (0x01)
}
Method (BTRS, 0, Serialized)
{
Store (0x00, GP54)
Store (0x00, GD54)
Sleep (0x05)
Store (0x01, GD54)
Sleep (0x01)
}
}
}
}

SSDT-3

View File SSDT-3.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-3.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "SSDT"
* Length 0x00000032 (50)
* Revision 0x01
* Checksum 0xB3
* OEM ID "APPLE "
* OEM Table ID "SsdtS3"
* OEM Revision 0x00001000 (4096)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-3.aml", "SSDT", 1, "APPLE ", "SsdtS3", 0x00001000)
{
Name (_S3, Package (0x03) // _S3_: S3 System State
{
0x05,
0x05,
0x00
})
}

SSDT-4

View File SSDT-4.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-4.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "SSDT"
* Length 0x000035EE (13806)
* Revision 0x01
* Checksum 0x94
* OEM ID "APPLE "
* OEM Table ID "PcieTbt"
* OEM Revision 0x00001000 (4096)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-4.aml", "SSDT", 1, "APPLE ", "PcieTbt", 0x00001000)
{
/*
* iASL Warning: There were 4 external control methods found during
* disassembly, but additional ACPI tables to resolve these externals
* were not specified. This resulting disassembler output file may not
* compile because the disassembler did not know how many arguments
* to assign to these methods. To specify the tables needed to resolve
* external control method references, use the one of the following
* example iASL invocations:
* iasl -e <ssdt1.aml,ssdt2.aml...> -d <dsdt.aml>
* iasl -e <dsdt.aml,ssdt2.aml...> -d <ssdt1.aml>
*/
External (_SB_.PCI0.SBUS.BUS0.BLC0.BSET, MethodObj) // Warning: Unresolved Method, guessing 1 arguments (may be incorrect, see warning above)
External (BLCP, MethodObj) // Warning: Unresolved Method, guessing 2 arguments (may be incorrect, see warning above)
External (DTGP, MethodObj) // Warning: Unresolved Method, guessing 4 arguments (may be incorrect, see warning above)
External (GVNV, MethodObj) // Warning: Unresolved Method, guessing 1 arguments (may be incorrect, see warning above)
External (_SB_.PCI0, DeviceObj)
External (_SB_.PCI0.LPCB.RTC_.ISTB)
External (_SB_.PCI0.P0P2, DeviceObj)
External (_SB_.PCI0.RP05, DeviceObj)
External (B0PD)
External (B1PD)
External (B2PD)
External (B3PD)
External (BRTL, IntObj)
External (C7AE)
External (EGPS, IntObj)
External (F004, IntObj)
External (F006)
External (F00C, IntObj)
External (F019, IntObj)
External (F01A, IntObj)
External (F01C, IntObj)
External (F01D, IntObj)
External (F01E)
External (F020, IntObj)
External (F022, IntObj)
External (F024, IntObj)
External (F026, IntObj)
External (F028, IntObj)
External (F02C, IntObj)
External (F03C, IntObj)
External (F03D, IntObj)
External (F03E, IntObj)
External (F084, IntObj)
External (F08C, IntObj)
External (F092, IntObj)
External (F094, IntObj)
External (F098, IntObj)
External (F0A2, IntObj)
External (F0A8, IntObj)
External (F0AA)
External (F0AC, IntObj)
External (F0B0, IntObj)
External (F0B2)
External (F0B4, IntObj)
External (F0BC, IntObj)
External (F0C0)
External (F0C8, IntObj)
External (F0D0, IntObj)
External (F0D2)
External (F0EC, IntObj)
External (F0F4, IntObj)
External (F114, IntObj)
External (F11A)
External (F144, IntObj)
External (F150, IntObj)
External (F158, IntObj)
External (F15C, IntObj)
External (F1C4)
External (F1CC, IntObj)
External (F1D0)
External (F1F0)
External (F1F8, IntObj)
External (F1FC, IntObj)
External (F200, IntObj)
External (F204, IntObj)
External (F208, IntObj)
External (F214)
External (F224, IntObj)
External (F228, IntObj)
External (F22C, IntObj)
External (F238, IntObj)
External (F240, IntObj)
External (F244, IntObj)
External (F250, IntObj)
External (F258, IntObj)
External (F25C, IntObj)
External (F260, IntObj)
External (F508)
External (F80C, IntObj)
External (F82C, IntObj)
External (F84C, IntObj)
External (F86C, IntObj)
External (F88C, IntObj)
External (F8AC, IntObj)
External (F8CC, IntObj)
External (F8EC, IntObj)
External (F900, IntObj)
External (F904, IntObj)
External (F908, IntObj)
External (F90C, IntObj)
External (F910, IntObj)
External (F918, IntObj)
External (F920, IntObj)
External (F924, IntObj)
External (F928, IntObj)
External (F92C, IntObj)
External (F930, IntObj)
External (F938, IntObj)
External (F940, IntObj)
External (F944, IntObj)
External (F948, IntObj)
External (F94C, IntObj)
External (F950, IntObj)
External (F958, IntObj)
External (F960, IntObj)
External (F964, IntObj)
External (F968, IntObj)
External (F96C, IntObj)
External (F970, IntObj)
External (F978, IntObj)
External (F980, IntObj)
External (F984, IntObj)
External (F988, IntObj)
External (F98C, IntObj)
External (F990, IntObj)
External (F998, IntObj)
External (F9A0, IntObj)
External (F9A4, IntObj)
External (F9A8, IntObj)
External (F9AC, IntObj)
External (F9B0, IntObj)
External (F9B8, IntObj)
External (F9C0, IntObj)
External (F9C4, IntObj)
External (F9C8, IntObj)
External (F9CC, IntObj)
External (F9D0, IntObj)
External (F9D8, IntObj)
External (F9E0, IntObj)
External (F9E4, IntObj)
External (F9E8, IntObj)
External (F9EC, IntObj)
External (F9F0, IntObj)
External (F9F8, IntObj)
External (FA00, IntObj)
External (FA04, IntObj)
External (FA08, IntObj)
External (FA0C, IntObj)
External (FA10, IntObj)
External (FA14, IntObj)
External (FA18, IntObj)
External (FA1C, IntObj)
External (FA20, IntObj)
External (FA24, IntObj)
External (FA28, IntObj)
External (FA2C, IntObj)
External (FA30, IntObj)
External (FA34, IntObj)
External (FA38, IntObj)
External (FA3C, IntObj)
External (FA40, IntObj)
External (FA44, IntObj)
External (FA48, IntObj)
External (FA4C, IntObj)
External (FA50, IntObj)
External (FA54, IntObj)
External (FA58, IntObj)
External (FA5C, IntObj)
External (FA60, IntObj)
External (FA64, IntObj)
External (FA68, IntObj)
External (FA6C, IntObj)
External (FA70, IntObj)
External (FA74, IntObj)
External (FA78, IntObj)
External (FA7C, IntObj)
External (FA80, IntObj)
External (FA84, IntObj)
External (FA88, IntObj)
External (FA8C, IntObj)
External (FA90, IntObj)
External (FA94, IntObj)
External (FA98, IntObj)
External (FA9C, IntObj)
External (FAA0, IntObj)
External (FAA4, IntObj)
External (FAA8, IntObj)
External (FAAC, IntObj)
External (FAB0, IntObj)
External (FAB4, IntObj)
External (FAB8, IntObj)
External (FABC, IntObj)
External (FAC0, IntObj)
External (FAC4, IntObj)
External (FAC8, IntObj)
External (FACC, IntObj)
External (FAD0, IntObj)
External (FAD4, IntObj)
External (FAD8, IntObj)
External (FADC, IntObj)
External (FAE0, IntObj)
External (FAE4, IntObj)
External (FAE8, IntObj)
External (FAEC, IntObj)
External (FAF0, IntObj)
External (FAF4, IntObj)
External (FAF8, IntObj)
External (FAFC, IntObj)
External (FC28, IntObj)
External (FC30, IntObj)
External (FC38, IntObj)
External (FCD0, IntObj)
External (FD14, IntObj)
External (FD34, IntObj)
External (FD94, IntObj)
External (FD98, IntObj)
External (FD9C)
External (FDA0, IntObj)
External (FDA4, IntObj)
External (FDA8, IntObj)
External (FDAC, IntObj)
External (FDB0, IntObj)
External (FDB4, IntObj)
External (FDB8, IntObj)
External (FDBC, IntObj)
External (FDD8, IntObj)
External (FLDS)
External (FSQ1)
External (FSQ2)
External (GD04)
External (GD24)
External (GI04)
External (GP04, IntObj)
External (GP23)
External (GP24, IntObj)
External (GP33, IntObj)
External (MUTX)
External (OSDW, IntObj)
External (SSMP)
External (SSMY)
External (V004, IntObj)
External (V00C, IntObj)
External (V019, IntObj)
External (V01A, IntObj)
External (V01C, IntObj)
External (V01D, IntObj)
External (V020, IntObj)
External (V022, IntObj)
External (V024, IntObj)
External (V026, IntObj)
External (V028, IntObj)
External (V02C, IntObj)
External (V03C, IntObj)
External (V03D, IntObj)
External (V03E, IntObj)
External (V084, IntObj)
External (V08C, IntObj)
External (V092, IntObj)
External (V094, IntObj)
External (V098, IntObj)
External (V0A2, IntObj)
External (V0A8, IntObj)
External (V0AC, IntObj)
External (V0B0, IntObj)
External (V0B4, IntObj)
External (V0BC, IntObj)
External (V0C8, IntObj)
External (V0D0, IntObj)
External (V0EC, IntObj)
External (V0F4, IntObj)
External (V114, IntObj)
External (V144, IntObj)
External (V150, IntObj)
External (V158, IntObj)
External (V15C, IntObj)
External (V1CC, IntObj)
External (V1F8, IntObj)
External (V1FC, IntObj)
External (V200, IntObj)
External (V204, IntObj)
External (V208, IntObj)
External (V224, IntObj)
External (V228, IntObj)
External (V22C, IntObj)
External (V238, IntObj)
External (V240, IntObj)
External (V244, IntObj)
External (V250, IntObj)
External (V258, IntObj)
External (V25C, IntObj)
External (V260, IntObj)
External (V80C, IntObj)
External (V82C, IntObj)
External (V84C, IntObj)
External (V86C, IntObj)
External (V88C, IntObj)
External (V8AC, IntObj)
External (V8CC, IntObj)
External (V8EC, IntObj)
External (V900, IntObj)
External (V904, IntObj)
External (V908, IntObj)
External (V90C, IntObj)
External (V910, IntObj)
External (V918, IntObj)
External (V920, IntObj)
External (V924, IntObj)
External (V928, IntObj)
External (V92C, IntObj)
External (V930, IntObj)
External (V938, IntObj)
External (V940, IntObj)
External (V944, IntObj)
External (V948, IntObj)
External (V94C, IntObj)
External (V950, IntObj)
External (V958, IntObj)
External (V960, IntObj)
External (V964, IntObj)
External (V968, IntObj)
External (V96C, IntObj)
External (V970, IntObj)
External (V978, IntObj)
External (V980, IntObj)
External (V984, IntObj)
External (V988, IntObj)
External (V98C, IntObj)
External (V990, IntObj)
External (V998, IntObj)
External (V9A0, IntObj)
External (V9A4, IntObj)
External (V9A8, IntObj)
External (V9AC, IntObj)
External (V9B0, IntObj)
External (V9B8, IntObj)
External (V9C0, IntObj)
External (V9C4, IntObj)
External (V9C8, IntObj)
External (V9CC, IntObj)
External (V9D0, IntObj)
External (V9D8, IntObj)
External (V9E0, IntObj)
External (V9E4, IntObj)
External (V9E8, IntObj)
External (V9EC, IntObj)
External (V9F0, IntObj)
External (V9F8, IntObj)
External (VA00, IntObj)
External (VA04, IntObj)
External (VA08, IntObj)
External (VA0C, IntObj)
External (VA10, IntObj)
External (VA14, IntObj)
External (VA18, IntObj)
External (VA1C, IntObj)
External (VA20, IntObj)
External (VA24, IntObj)
External (VA28, IntObj)
External (VA2C, IntObj)
External (VA30, IntObj)
External (VA34, IntObj)
External (VA38, IntObj)
External (VA3C, IntObj)
External (VA40, IntObj)
External (VA44, IntObj)
External (VA48, IntObj)
External (VA4C, IntObj)
External (VA50, IntObj)
External (VA54, IntObj)
External (VA58, IntObj)
External (VA5C, IntObj)
External (VA60, IntObj)
External (VA64, IntObj)
External (VA68, IntObj)
External (VA6C, IntObj)
External (VA70, IntObj)
External (VA74, IntObj)
External (VA78, IntObj)
External (VA7C, IntObj)
External (VA80, IntObj)
External (VA84, IntObj)
External (VA88, IntObj)
External (VA8C, IntObj)
External (VA90, IntObj)
External (VA94, IntObj)
External (VA98, IntObj)
External (VA9C, IntObj)
External (VAA0, IntObj)
External (VAA4, IntObj)
External (VAA8, IntObj)
External (VAAC, IntObj)
External (VAB0, IntObj)
External (VAB4, IntObj)
External (VAB8, IntObj)
External (VABC, IntObj)
External (VAC0, IntObj)
External (VAC4, IntObj)
External (VAC8, IntObj)
External (VACC, IntObj)
External (VAD0, IntObj)
External (VAD4, IntObj)
External (VAD8, IntObj)
External (VADC, IntObj)
External (VAE0, IntObj)
External (VAE4, IntObj)
External (VAE8, IntObj)
External (VAEC, IntObj)
External (VAF0, IntObj)
External (VAF4, IntObj)
External (VAF8, IntObj)
External (VAFC, IntObj)
External (VC28, IntObj)
External (VC30, IntObj)
External (VC38, IntObj)
External (VCD0, IntObj)
External (VD14, IntObj)
External (VD34, IntObj)
External (VD94, IntObj)
External (VD98, IntObj)
External (VDA0, IntObj)
External (VDA4, IntObj)
External (VDA8, IntObj)
External (VDAC, IntObj)
External (VDB0, IntObj)
External (VDB4, IntObj)
External (VDB8, IntObj)
External (VDBC, IntObj)
External (VDD8, IntObj)
Scope (\_SB.PCI0.P0P2)
{
Device (GFX0)
{
Method (PSSR, 1, Serialized)
{
If (LEqual (Arg0, 0x01))
{
Store (FDD8, VDD8)
Store (F900, V900)
Store (F904, V904)
Store (F908, V908)
Store (F90C, V90C)
Store (F910, V910)
Store (F80C, V80C)
Store (F920, V920)
Store (F924, V924)
Store (F928, V928)
Store (F92C, V92C)
Store (F930, V930)
Store (F82C, V82C)
Store (F940, V940)
Store (F944, V944)
Store (F948, V948)
Store (F94C, V94C)
Store (F950, V950)
Store (F84C, V84C)
Store (F960, V960)
Store (F964, V964)
Store (F968, V968)
Store (F96C, V96C)
Store (F970, V970)
Store (F86C, V86C)
Store (F980, V980)
Store (F984, V984)
Store (F988, V988)
Store (F98C, V98C)
Store (F990, V990)
Store (F88C, V88C)
Store (F9A0, V9A0)
Store (F9A4, V9A4)
Store (F9A8, V9A8)
Store (F9AC, V9AC)
Store (F9B0, V9B0)
Store (F8AC, V8AC)
Store (F9C0, V9C0)
Store (F9C4, V9C4)
Store (F9C8, V9C8)
Store (F9CC, V9CC)
Store (F9D0, V9D0)
Store (F8CC, V8CC)
Store (F9E0, V9E0)
Store (F9E4, V9E4)
Store (F9E8, V9E8)
Store (F9EC, V9EC)
Store (F9F0, V9F0)
Store (F8EC, V8EC)
Store (FC30, VC30)
Store (FA00, VA00)
Store (FA04, VA04)
Store (FA08, VA08)
Store (FA0C, VA0C)
Store (FA10, VA10)
Store (FA14, VA14)
Store (FA18, VA18)
Store (FA1C, VA1C)
Store (FA20, VA20)
Store (FA24, VA24)
Store (FA28, VA28)
Store (FA2C, VA2C)
Store (FA30, VA30)
Store (FA34, VA34)
Store (FA38, VA38)
Store (FA3C, VA3C)
Store (FA40, VA40)
Store (FA44, VA44)
Store (FA48, VA48)
Store (FA4C, VA4C)
Store (FA50, VA50)
Store (FA54, VA54)
Store (FA58, VA58)
Store (FA5C, VA5C)
Store (FA60, VA60)
Store (FA64, VA64)
Store (FA68, VA68)
Store (FA6C, VA6C)
Store (FA70, VA70)
Store (FA74, VA74)
Store (FA78, VA78)
Store (FA7C, VA7C)
Store (FA80, VA80)
Store (FA84, VA84)
Store (FA88, VA88)
Store (FA8C, VA8C)
Store (FA90, VA90)
Store (FA94, VA94)
Store (FA98, VA98)
Store (FA9C, VA9C)
Store (FAA0, VAA0)
Store (FAA4, VAA4)
Store (FAA8, VAA8)
Store (FAAC, VAAC)
Store (FAB0, VAB0)
Store (FAB4, VAB4)
Store (FAB8, VAB8)
Store (FABC, VABC)
Store (FAC0, VAC0)
Store (FAC4, VAC4)
Store (FAC8, VAC8)
Store (FACC, VACC)
Store (FAD0, VAD0)
Store (FAD4, VAD4)
Store (FAD8, VAD8)
Store (FADC, VADC)
Store (FAE0, VAE0)
Store (FAE4, VAE4)
Store (FAE8, VAE8)
Store (FAEC, VAEC)
Store (FAF0, VAF0)
Store (FAF4, VAF4)
Store (FAF8, VAF8)
Store (FAFC, VAFC)
Store (F918, V918)
Store (F938, V938)
Store (F958, V958)
Store (F978, V978)
Store (F998, V998)
Store (F9B8, V9B8)
Store (F9D8, V9D8)
Store (F9F8, V9F8)
Store (FDA0, VDA0)
Store (FDA4, VDA4)
Store (FDA8, VDA8)
Store (FDAC, VDAC)
Store (FDB0, VDB0)
Store (FDB4, VDB4)
Store (FDB8, VDB8)
Store (FDBC, VDBC)
}
Else
{
Store (VDD8, FDD8)
Store (V900, F900)
Store (V904, F904)
Store (V908, F908)
Store (V90C, F90C)
Store (V910, F910)
Store (V80C, F80C)
Store (V920, F920)
Store (V924, F924)
Store (V928, F928)
Store (V92C, F92C)
Store (V930, F930)
Store (V82C, F82C)
Store (V940, F940)
Store (V944, F944)
Store (V948, F948)
Store (V94C, F94C)
Store (V950, F950)
Store (V84C, F84C)
Store (V960, F960)
Store (V964, F964)
Store (V968, F968)
Store (V96C, F96C)
Store (V970, F970)
Store (V86C, F86C)
Store (V980, F980)
Store (V984, F984)
Store (V988, F988)
Store (V98C, F98C)
Store (V990, F990)
Store (V88C, F88C)
Store (V9A0, F9A0)
Store (V9A4, F9A4)
Store (V9A8, F9A8)
Store (V9AC, F9AC)
Store (V9B0, F9B0)
Store (V8AC, F8AC)
Store (V9C0, F9C0)
Store (V9C4, F9C4)
Store (V9C8, F9C8)
Store (V9CC, F9CC)
Store (V9D0, F9D0)
Store (V8CC, F8CC)
Store (V9E0, F9E0)
Store (V9E4, F9E4)
Store (V9E8, F9E8)
Store (V9EC, F9EC)
Store (V9F0, F9F0)
Store (V8EC, F8EC)
Store (VC30, FC30)
Store (VA00, FA00)
Store (VA04, FA04)
Store (VA08, FA08)
Store (VA0C, FA0C)
Store (VA10, FA10)
Store (VA14, FA14)
Store (VA18, FA18)
Store (VA1C, FA1C)
Store (VA20, FA20)
Store (VA24, FA24)
Store (VA28, FA28)
Store (VA2C, FA2C)
Store (VA30, FA30)
Store (VA34, FA34)
Store (VA38, FA38)
Store (VA3C, FA3C)
Store (VA40, FA40)
Store (VA44, FA44)
Store (VA48, FA48)
Store (VA4C, FA4C)
Store (VA50, FA50)
Store (VA54, FA54)
Store (VA58, FA58)
Store (VA5C, FA5C)
Store (VA60, FA60)
Store (VA64, FA64)
Store (VA68, FA68)
Store (VA6C, FA6C)
Store (VA70, FA70)
Store (VA74, FA74)
Store (VA78, FA78)
Store (VA7C, FA7C)
Store (VA80, FA80)
Store (VA84, FA84)
Store (VA88, FA88)
Store (VA8C, FA8C)
Store (VA90, FA90)
Store (VA94, FA94)
Store (VA98, FA98)
Store (VA9C, FA9C)
Store (VAA0, FAA0)
Store (VAA4, FAA4)
Store (VAA8, FAA8)
Store (VAAC, FAAC)
Store (VAB0, FAB0)
Store (VAB4, FAB4)
Store (VAB8, FAB8)
Store (VABC, FABC)
Store (VAC0, FAC0)
Store (VAC4, FAC4)
Store (VAC8, FAC8)
Store (VACC, FACC)
Store (VAD0, FAD0)
Store (VAD4, FAD4)
Store (VAD8, FAD8)
Store (VADC, FADC)
Store (VAE0, FAE0)
Store (VAE4, FAE4)
Store (VAE8, FAE8)
Store (VAEC, FAEC)
Store (VAF0, FAF0)
Store (VAF4, FAF4)
Store (VAF8, FAF8)
Store (VAFC, FAFC)
Store (V918, F918)
Store (V938, F938)
Store (V958, F958)
Store (V978, F978)
Store (V998, F998)
Store (V9B8, F9B8)
Store (V9D8, F9D8)
Store (V9F8, F9F8)
Store (VDA0, FDA0)
Store (VDA4, FDA4)
Store (VDA8, FDA8)
Store (VDAC, FDAC)
Store (VDB0, FDB0)
Store (VDB4, FDB4)
Store (VDB8, FDB8)
Store (VDBC, FDBC)
}
}
Method (P0SR, 1, Serialized)
{
If (LEqual (Arg0, 0x01))
{
Store (F224, V224)
Store (F1F8, V1F8)
Store (F260, V260)
Store (FC28, VC28)
Store (FC38, VC38)
Store (FD14, VD14)
Store (F004, V004)
Store (F00C, V00C)
Store (F019, V019)
Store (F01A, V01A)
Store (F01C, V01C)
Store (F01D, V01D)
Store (F020, V020)
Store (F022, V022)
Store (F024, V024)
Store (F026, V026)
Store (F028, V028)
Store (F02C, V02C)
Store (F03C, V03C)
Store (F03D, V03D)
Store (F03E, V03E)
Store (F084, V084)
Store (F08C, V08C)
Store (F092, V092)
Store (F094, V094)
Store (F098, V098)
Store (F0A2, V0A2)
Store (F0A8, V0A8)
Store (F0AC, V0AC)
Store (F0B0, V0B0)
Store (F0B4, V0B4)
Store (F0BC, V0BC)
Store (F0C8, V0C8)
Store (F0D0, V0D0)
Store (F0EC, V0EC)
Store (F114, V114)
Store (F144, V144)
Store (F150, V150)
Store (F158, V158)
Store (F15C, V15C)
Store (F1CC, V1CC)
Store (F1FC, V1FC)
Store (F200, V200)
Store (F204, V204)
Store (F208, V208)
Store (F228, V228)
Store (F22C, V22C)
Store (F238, V238)
Store (F240, V240)
Store (F244, V244)
Store (F250, V250)
Store (F258, V258)
Store (F25C, V25C)
Store (FCD0, VCD0)
Store (FD34, VD34)
Store (FD94, VD94)
Store (FD98, VD98)
Store (F0F4, V0F4)
Store (FDA0, VDA0)
Store (FDA4, VDA4)
Store (FDA8, VDA8)
Store (FDAC, VDAC)
Store (FDB0, VDB0)
Store (FDB4, VDB4)
Store (FDB8, VDB8)
Store (FDBC, VDBC)
}
Else
{
Store (V224, F224)
Store (V1F8, F1F8)
Store (V260, F260)
Store (VC28, FC28)
Store (VC38, FC38)
Store (VD14, FD14)
Store (V004, F004)
Store (V00C, F00C)
Store (V019, F019)
Store (V01A, F01A)
Store (V01C, F01C)
Store (V01D, F01D)
Store (V020, F020)
Store (V022, F022)
Store (V024, F024)
Store (V026, F026)
Store (V028, F028)
Store (V02C, F02C)
Store (V03C, F03C)
Store (V03D, F03D)
Store (V03E, F03E)
Store (V084, F084)
Store (V08C, F08C)
Store (V092, F092)
Store (V094, F094)
Store (V098, F098)
Store (V0A2, F0A2)
Store (V0A8, F0A8)
Store (V0AC, F0AC)
Store (V0B0, F0B0)
Store (V0B4, F0B4)
Store (V0BC, F0BC)
Store (V0C8, F0C8)
Store (V0D0, F0D0)
Store (V0EC, F0EC)
Store (V114, F114)
Store (V144, F144)
Store (V150, F150)
Store (V158, F158)
Store (V15C, F15C)
Store (V1CC, F1CC)
Store (V1FC, F1FC)
Store (V200, F200)
Store (V204, F204)
Store (V208, F208)
Store (V228, F228)
Store (V22C, F22C)
Store (V238, F238)
Store (V240, F240)
Store (V244, F244)
Store (V250, F250)
Store (V258, F258)
Store (V25C, F25C)
Store (VCD0, FCD0)
Store (VD34, FD34)
Store (VD94, FD94)
Store (VD98, FD98)
Store (V0F4, F0F4)
Store (VDA0, FDA0)
Store (VDA4, FDA4)
Store (VDA8, FDA8)
Store (VDAC, FDAC)
Store (VDB0, FDB0)
Store (VDB4, FDB4)
Store (VDB8, FDB8)
Store (VDBC, FDBC)
}
}
Method (PUPD, 2, Serialized)
{
If (LEqual (Arg0, 0x00))
{
PSSR (0x01)
P0SR (0x01)
Store (0x01, FLDS)
Add (Timer, 0x00989680, Local0)
While (LLessEqual (Timer, Local0))
{
If (LEqual (F214, 0x00))
{
Break
}
}
Store (0x00, FSQ1)
Store (0x01, FSQ2)
If (LEqual (Arg1, 0x04))
{
Store (0x01, B0PD)
Store (0x01, B1PD)
Store (0x01, B2PD)
Store (0x01, B3PD)
}
If (LEqual (Arg1, 0x02))
{
Store (0x01, B0PD)
Store (0x01, B1PD)
}
Store (0x01, C7AE)
}
Else
{
Store (0x00, C7AE)
PSSR (0x00)
P0SR (0x00)
Store (0x00, F006)
Store (0x00, F01E)
Store (0x00, F0AA)
Store (0x00, F0C0)
Store (0x00, F0D2)
Store (0x00, F1C4)
Store (0x00, F1D0)
Store (0x00, F1F0)
Store (0x00, FD9C)
Store (0x00, F0B2)
Store (0x00, FSQ1)
Store (0x00, FSQ2)
If (LEqual (Arg1, 0x04))
{
Store (0x00, B0PD)
Store (0x00, B1PD)
Store (0x00, B2PD)
Store (0x00, B3PD)
}
If (LEqual (Arg1, 0x02))
{
Store (0x00, B0PD)
Store (0x00, B1PD)
}
Store (0x00, FLDS)
Store (0x01, F508)
Add (Timer, 0x00989680, Local1)
While (LLessEqual (Timer, Local1))
{
If (LEqual (F11A, 0x00))
{
Break
}
}
}
}
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (EGNV, SystemMemory, GVNV (0x00020000), Field (EGNV, DWordAcc, Lock, Preserve)
{
EG00, 32768,
EG01, 32768,
EG02, 32768,
EG03, 32768,
EG04, 32768,
EG05, 32768,
EG06, 32768,
EG07, 32768,
EG08, 32768,
EG09, 32768,
EG0A, 32768,
EG0B, 32768,
EG0C, 32768,
EG0D, 32768,
EG0E, 32768,
EG0F, 32768,
EG10, 32768,
EG11, 32768,
EG12, 32768,
EG13, 32768,
EG14, 32768,
EG15, 32768,
EG16, 32768,
EG17, 32768,
EG18, 32768,
EG19, 32768,
EG1A, 32768,
EG1B, 32768,
EG1C, 32768,
EG1D, 32768,
EG1E, 32768,
EG1F, 32768
})
Name (VBUF, Buffer (0x1000) {})
Method (_ROM, 2, Serialized) // _ROM: Read-Only Memory
{
If (LEqual (Arg0, 0x00))
{
CPVB (ToBuffer (EG00), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x1000))
{
CPVB (ToBuffer (EG01), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x2000))
{
CPVB (ToBuffer (EG02), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x3000))
{
CPVB (ToBuffer (EG03), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x4000))
{
CPVB (ToBuffer (EG04), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x5000))
{
CPVB (ToBuffer (EG05), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x6000))
{
CPVB (ToBuffer (EG06), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x7000))
{
CPVB (ToBuffer (EG07), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x8000))
{
CPVB (ToBuffer (EG08), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x9000))
{
CPVB (ToBuffer (EG09), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0xA000))
{
CPVB (ToBuffer (EG0A), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0xB000))
{
CPVB (ToBuffer (EG0B), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0xC000))
{
CPVB (ToBuffer (EG0C), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0xD000))
{
CPVB (ToBuffer (EG0D), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0xE000))
{
CPVB (ToBuffer (EG0E), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0xF000))
{
CPVB (ToBuffer (EG0F), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00010000))
{
CPVB (ToBuffer (EG10), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00011000))
{
CPVB (ToBuffer (EG11), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00012000))
{
CPVB (ToBuffer (EG12), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00013000))
{
CPVB (ToBuffer (EG13), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00014000))
{
CPVB (ToBuffer (EG14), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00015000))
{
CPVB (ToBuffer (EG15), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00016000))
{
CPVB (ToBuffer (EG16), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00017000))
{
CPVB (ToBuffer (EG17), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00018000))
{
CPVB (ToBuffer (EG18), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x00019000))
{
CPVB (ToBuffer (EG19), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x0001A000))
{
CPVB (ToBuffer (EG1A), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x0001B000))
{
CPVB (ToBuffer (EG1B), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x0001C000))
{
CPVB (ToBuffer (EG1C), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x0001D000))
{
CPVB (ToBuffer (EG1D), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x0001E000))
{
CPVB (ToBuffer (EG1E), Arg0, Arg1)
Return (VBUF)
}
If (LEqual (Arg0, 0x0001F000))
{
CPVB (ToBuffer (EG1F), Arg0, Arg1)
Return (VBUF)
}
Return (VBUF)
}
Method (CPVB, 3, Serialized)
{
CopyObject (Arg0, VBUF)
}
Name (BRTN, Package (0x12)
{
0x50,
0x2F,
0x01,
0x04,
0x06,
0x09,
0x0E,
0x13,
0x1A,
0x21,
0x28,
0x2E,
0x34,
0x3A,
0x41,
0x47,
0x4E,
0x55
})
Method (ABCM, 1, NotSerialized)
{
Store (Arg0, BRTL)
If (BLCP (\_SB.PCI0.SBUS.BUS0.BLC0.BSET (Arg0), Return (Zero))) {}
Store (0x02, Local0)
While (LLess (Local0, 0x11))
{
If (LGreaterEqual (DerefOf (Index (BRTN, Local0)), Arg0))
{
Break
}
Increment (Local0)
}
Decrement (Local0)
Decrement (Local0)
ShiftLeft (Local0, 0x04, Local0)
Or (Local0, 0x04, Local0)
Acquire (MUTX, 0xFFFF)
Store (Local0, SSMY)
Store (0xBF, SSMP)
Release (MUTX)
Return (Zero)
}
Method (ABCL, 0, NotSerialized)
{
Store (DerefOf (Index (BRTN, 0x0F)), Index (BRTN, 0x00))
Store (DerefOf (Index (BRTN, 0x0A)), Index (BRTN, 0x01))
Return (BRTN)
}
Device (LCD)
{
Method (_ADR, 0, Serialized) // _ADR: Address
{
Return (0x80002400)
}
Method (_BCL, 0, NotSerialized) // _BCL: Brightness Control Levels
{
Return (ABCL ())
}
Method (_BCM, 1, NotSerialized) // _BCM: Brightness Control Method
{
ABCM (Arg0)
}
Method (_BQC, 0, NotSerialized) // _BQC: Brightness Query Current
{
Return (BRTL)
}
}
Method (_DOD, 0, NotSerialized) // _DOD: Display Output Devices
{
Return (Package (0x01)
{
0x80002400
})
}
Name (ATIB, Buffer (0x0100) {})
Method (ATIF, 2, Serialized)
{
If (LEqual (Arg0, 0x00))
{
Return (AF00 ())
}
If (LEqual (Arg0, 0x01))
{
Return (AF01 ())
}
If (LEqual (Arg0, 0x02))
{
Return (AF02 ())
}
Else
{
CreateWordField (ATIB, 0x00, SSZE)
CreateWordField (ATIB, 0x02, VERN)
CreateDWordField (ATIB, 0x04, NMSK)
CreateDWordField (ATIB, 0x08, SFUN)
Store (0x00, SSZE)
Store (0x00, VERN)
Store (0x00, NMSK)
Store (0x00, SFUN)
Return (ATIB)
}
}
Method (AF00, 0, NotSerialized)
{
CreateWordField (ATIB, 0x00, SSZE)
CreateWordField (ATIB, 0x02, VERN)
CreateDWordField (ATIB, 0x04, NMSK)
CreateDWordField (ATIB, 0x08, SFUN)
Store (0x0C, SSZE)
Store (0x01, VERN)
Store (0x0C, NMSK)
Store (0x03, SFUN)
Return (ATIB)
}
Method (AF01, 0, NotSerialized)
{
CreateWordField (ATIB, 0x00, SSZE)
CreateDWordField (ATIB, 0x02, VMSK)
CreateDWordField (ATIB, 0x06, FLGS)
Store (0x0A, SSZE)
Store (0x03, VMSK)
Store (0x01, FLGS)
Return (ATIB)
}
Method (AF02, 0, NotSerialized)
{
CreateWordField (ATIB, 0x00, SSZE)
CreateDWordField (ATIB, 0x02, PSBI)
CreateByteField (ATIB, 0x06, EXPM)
CreateByteField (ATIB, 0x07, THRM)
CreateByteField (ATIB, 0x08, THID)
CreateByteField (ATIB, 0x09, FPWR)
CreateByteField (ATIB, 0x0A, FPID)
CreateByteField (ATIB, 0x0B, SPWR)
CreateByteField (ATIB, 0x0C, PBBL)
Store (0x0D, SSZE)
Store (0x08, PSBI)
Store (0x00, FPWR)
Store (EGPS, FPID)
Return (ATIB)
}
Method (_PRW, 0, NotSerialized) // _PRW: Power Resources for Wake
{
If (OSDW)
{
Return (Package (0x02)
{
0x09,
0x04
})
}
Else
{
Return (Package (0x02)
{
0x09,
0x03
})
}
}
OperationRegion (PEGH, PCI_Config, 0x00, 0x40)
Field (PEGH, ByteAcc, NoLock, Preserve)
{
VID0, 16,
DID0, 16
}
OperationRegion (GBAR, SystemMemory, 0xE0008000, 0x0100)
Field (GBAR, DWordAcc, Lock, Preserve)
{
Offset (0xB0),
, 4,
LNKD, 1,
LCRL, 1,
Offset (0xB2),
, 4,
LSTS, 6,
, 1,
LTRN, 1,
Offset (0xD0),
LTLS, 4
}
Method (PWRD, 1, NotSerialized)
{
If (Arg0)
{
PUPD (0x00, 0x04)
Return (0x00)
}
Else
{
PUPD (0x01, 0x04)
While (LTRN)
{
Sleep (0x0A)
}
If (LEqual (LSTS, 0x08))
{
Return (0x00)
}
Else
{
Return (0x01)
}
}
}
Method (PWG1, 1, NotSerialized)
{
If (Arg0)
{
PUPD (0x00, 0x04)
Return (0x00)
}
Else
{
PUPD (0x01, 0x04)
Store (0x01, LTLS)
Store (0x01, LCRL)
While (LTRN)
{
Sleep (0x0A)
}
If (LEqual (LSTS, 0x08))
{
Return (0x00)
}
Else
{
Return (0x01)
}
}
}
Method (PWG3, 1, NotSerialized)
{
Store (0x03, LTLS)
Store (0x01, LCRL)
While (LTRN)
{
Sleep (0x0A)
}
If (LEqual (LSTS, 0x08))
{
Return (0x00)
}
Else
{
Return (0x01)
}
}
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
If (LEqual (Arg0, Buffer (0x10)
{
/* 0000 */ 0xC6, 0xB7, 0xB5, 0xA0, 0x18, 0x13, 0x1C, 0x44,
/* 0008 */ 0xB0, 0xC9, 0xFE, 0x69, 0x5E, 0xAF, 0x94, 0x9B
}))
{
If (LNotEqual (And (VID0, 0xFFFF), 0xFFFF))
{
Store (Package (0x02)
{
"hda-gfx",
Buffer (0x0A)
{
"onboard-1"
}
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3)
RefOf (Local0)
Return (Local0)
}
}
Return (0x80000002)
}
}
Device (HDAU)
{
Name (_ADR, 0x01) // _ADR: Address
OperationRegion (HDAH, PCI_Config, 0x00, 0x40)
Field (HDAH, ByteAcc, NoLock, Preserve)
{
VID0, 16,
DID0, 16
}
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
If (LEqual (Arg0, Buffer (0x10)
{
/* 0000 */ 0xC6, 0xB7, 0xB5, 0xA0, 0x18, 0x13, 0x1C, 0x44,
/* 0008 */ 0xB0, 0xC9, 0xFE, 0x69, 0x5E, 0xAF, 0x94, 0x9B
}))
{
If (LNotEqual (And (VID0, 0xFFFF), 0xFFFF))
{
Store (Package (0x02)
{
"hda-gfx",
Buffer (0x0A)
{
"onboard-1"
}
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3)
RefOf (Local0)
Return (Local0)
}
}
Return (0x80000002)
}
}
}
Scope (\_SB.PCI0)
{
Method (TGPE, 0, Serialized)
{
Notify (\_SB.PCI0.RP05, 0x02)
}
Method (DTBP, 0, Serialized)
{
If (LEqual (\_SB.PCI0.RP05.LDIS, 0x00))
{
Return (0x01)
}
Return (0x00)
}
Name (EJCD, 0x00)
Name (TBBT, 0x00)
Method (RMC1, 0, Serialized)
{
Store (0x01, \_SB.PCI0.RP05.LDIS)
Sleep (0x07D0)
Store (0x00, GP23)
}
Method (RMCR, 0, Serialized)
{
If (LNot (OSDW))
{
If (EJCD)
{
RMC1 ()
Return (Zero)
}
If (LAnd (LEqual (\_SB.PCI0.RP05.UPSB.DSB1.UPS0.AVND, 0xFFFF), LEqual (\_SB.PCI0.RP05.UPSB.DSB2.UPS0.AVND, 0xFFFF)))
{
RMC1 ()
Return (Zero)
}
Else
{
Store (0x01, TBBT)
}
}
Return (Zero)
}
Method (RMCW, 0, Serialized)
{
If (LNot (OSDW))
{
If (EJCD)
{
RMC1 ()
Return (Zero)
}
If (LAnd (TBBT, LNot (\_SB.PCI0.LPCB.RTC.ISTB)))
{
\_SB.PCI0.RP05.UPSB.DSB0.NHI0._EJ0 (0x01)
}
Else
{
If (LNot (TBBT))
{
RMC1 ()
}
}
}
Return (Zero)
}
Method (DTLK, 0, Serialized)
{
Store (0x01, \_SB.PCI0.RP05.LDIS)
Sleep (0x07D0)
Store (0x00, GP23)
}
Scope (\_SB.PCI0.RP05)
{
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
OperationRegion (A1E1, PCI_Config, 0x40, 0x40)
Field (A1E1, ByteAcc, NoLock, Preserve)
{
Offset (0x01),
Offset (0x02),
Offset (0x04),
Offset (0x08),
Offset (0x0A),
, 5,
TPEN, 1,
Offset (0x0C),
SSPD, 4,
, 16,
LACR, 1,
Offset (0x10),
, 4,
LDIS, 1,
LRTN, 1,
Offset (0x12),
CSPD, 4,
, 7,
LTRN, 1,
, 1,
LACT, 1,
Offset (0x14),
Offset (0x30),
TSPD, 4
}
OperationRegion (A1E2, PCI_Config, 0xA0, 0x08)
Field (A1E2, ByteAcc, NoLock, Preserve)
{
Offset (0x01),
Offset (0x02),
Offset (0x04),
PSTA, 2
}
OperationRegion (A1E3, PCI_Config, 0x0200, 0x20)
Field (A1E3, ByteAcc, NoLock, Preserve)
{
Offset (0x14),
Offset (0x16),
PSTS, 4
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
Device (UPSB)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
OperationRegion (A1E1, PCI_Config, 0xC0, 0x40)
Field (A1E1, ByteAcc, NoLock, Preserve)
{
Offset (0x01),
Offset (0x02),
Offset (0x04),
Offset (0x08),
Offset (0x0A),
, 5,
TPEN, 1,
Offset (0x0C),
SSPD, 4,
Offset (0x10),
, 4,
LDIS, 1,
LRTN, 1,
, 23,
LACT, 1,
Offset (0x30),
TSPD, 4
}
OperationRegion (A1E2, PCI_Config, 0x80, 0x08)
Field (A1E2, ByteAcc, NoLock, Preserve)
{
Offset (0x01),
Offset (0x02),
Offset (0x04),
PSTA, 2
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
Device (DSB0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
OperationRegion (A1E1, PCI_Config, 0xC0, 0x40)
Field (A1E1, ByteAcc, NoLock, Preserve)
{
Offset (0x01),
Offset (0x02),
Offset (0x04),
Offset (0x08),
Offset (0x0A),
, 5,
TPEN, 1,
Offset (0x0C),
Offset (0x10),
, 4,
LDIS, 1,
LRTN, 1,
, 23,
LACT, 1
}
OperationRegion (A1E2, PCI_Config, 0x80, 0x08)
Field (A1E2, ByteAcc, NoLock, Preserve)
{
Offset (0x01),
Offset (0x02),
Offset (0x04),
PSTA, 2
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
Device (NHI0)
{
Name (_ADR, 0x00) // _ADR: Address
Name (_STR, Unicode ("Thunderbolt")) // _STR: Description String
Method (_EJ0, 1, NotSerialized) // _EJx: Eject Device
{
Store (0x01, EJCD)
If (LNot (OSDW))
{
Store (0x01, GD24)
Sleep (0x64)
Sleep (0x64)
Store (0x0A, Local0)
While (LGreater (Local0, 0x00))
{
Decrement (Local0)
Sleep (0x64)
If (LEqual (GP24, 0x00))
{
Break
}
}
Store (0x03, \_SB.PCI0.RP05.PSTA)
Store (0x01, \_SB.PCI0.RP05.LDIS)
Add (Timer, 0x00989680, Local0)
While (LLessEqual (Timer, Local0))
{
If (LEqual (\_SB.PCI0.RP05.LACR, 0x01))
{
If (LEqual (\_SB.PCI0.RP05.LACT, 0x00))
{
Break
}
}
Else
{
If (LEqual (\_SB.PCI0.RP05.UPSB.AVND, 0xFFFFFFFF))
{
Break
}
}
Sleep (0x0A)
}
Store (0x00, GP23)
Sleep (0xFA)
Notify (\_SB.PCI0.RP05, 0x00)
}
}
Name (_GPE, 0x14) // _GPE: General Purpose Events
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (XDPG, 0, NotSerialized)
{
Return (GP33)
}
Method (XDPS, 1, Serialized)
{
If (LLessEqual (Arg0, 0x01))
{
Store (Arg0, GP33)
}
}
Method (TRPE, 2, Serialized)
{
If (OSDW)
{
If (LLessEqual (Arg0, 0x01))
{
If (LEqual (Arg0, 0x00))
{
Store (0x03, \_SB.PCI0.RP05.PSTA)
Store (0x01, \_SB.PCI0.RP05.LDIS)
Add (Timer, 0x00989680, Local0)
While (LLessEqual (Timer, Local0))
{
If (LEqual (\_SB.PCI0.RP05.LACR, 0x01))
{
If (LEqual (\_SB.PCI0.RP05.LACT, 0x00))
{
Break
}
}
Else
{
If (LEqual (\_SB.PCI0.RP05.UPSB.AVND, 0xFFFFFFFF))
{
Break
}
}
Sleep (0x0A)
}
Store (0x00, GP23)
}
Else
{
Store (0x00, Local0)
If (LEqual (GP23, 0x00))
{
Store (0x00, \_SB.PCI0.RP05.PSTA)
While (0x01)
{
If (LEqual (\_SB.PCI0.RP05.LDIS, 0x01))
{
Store (0x00, \_SB.PCI0.RP05.LDIS)
}
Store (0x01, GP23)
Store (0x00, Local1)
Add (Timer, 0x00989680, Local2)
While (LLessEqual (Timer, Local2))
{
If (LEqual (\_SB.PCI0.RP05.LACR, 0x00))
{
If (LNotEqual (\_SB.PCI0.RP05.LTRN, 0x01))
{
Break
}
}
Else
{
If (LAnd (LNotEqual (\_SB.PCI0.RP05.LTRN, 0x01), LEqual (\_SB.PCI0.RP05.LACT, 0x01)))
{
Break
}
}
Sleep (0x0A)
}
Sleep (Arg1)
While (LLessEqual (Timer, Local2))
{
If (LNotEqual (\_SB.PCI0.RP05.UPSB.AVND, 0xFFFFFFFF))
{
Store (0x01, Local1)
Break
}
Sleep (0x0A)
}
If (LEqual (Local1, 0x01))
{
Store (0x01, MABT)
Break
}
If (LEqual (Local0, 0x04))
{
Return (Zero)
}
Increment (Local0)
Store (0x00, GP23)
Sleep (0x03E8)
}
If (LEqual (\_SB.PCI0.RP05.CSPD, 0x01))
{
If (LEqual (\_SB.PCI0.RP05.SSPD, 0x02))
{
If (LEqual (\_SB.PCI0.RP05.UPSB.SSPD, 0x02))
{
If (LNotEqual (\_SB.PCI0.RP05.TSPD, 0x02))
{
Store (0x02, \_SB.PCI0.RP05.TSPD)
}
If (LNotEqual (\_SB.PCI0.RP05.UPSB.TSPD, 0x02))
{
Store (0x02, \_SB.PCI0.RP05.UPSB.TSPD)
}
Store (0x01, \_SB.PCI0.RP05.LRTN)
Add (Timer, 0x00989680, Local2)
While (LLessEqual (Timer, Local2))
{
If (LEqual (\_SB.PCI0.RP05.LACR, 0x00))
{
If (LAnd (LNotEqual (\_SB.PCI0.RP05.LTRN, 0x01), LNotEqual (\_SB.PCI0.RP05.UPSB.AVND, 0xFFFFFFFF)))
{
Store (0x01, Local1)
Break
}
}
Else
{
If (LAnd (LAnd (LNotEqual (\_SB.PCI0.RP05.LTRN, 0x01), LEqual (\_SB.PCI0.RP05.LACT, 0x01)),
LNotEqual (\_SB.PCI0.RP05.UPSB.AVND, 0xFFFFFFFF)))
{
Store (0x01, Local1)
Break
}
}
Sleep (0x0A)
}
}
}
}
}
}
}
}
Return (Zero)
}
Method (XRIP, 1, Serialized)
{
If (LLessEqual (Arg0, 0x01))
{
Store (Arg0, GI04)
}
}
Method (XRIO, 1, Serialized)
{
If (LLessEqual (Arg0, 0x01))
{
Store (Arg0, GD04)
}
}
Method (XRIL, 0, Serialized)
{
Return (GP04)
}
Name (XRIN, 0x14)
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
If (OSDW)
{
Store (Package (0x03)
{
"power-save",
0x01,
Buffer (0x01)
{
0x00
}
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3)
RefOf (Local0)
Return (Local0)
}
Return (Zero)
}
Method (SXFP, 1, Serialized)
{
If (LEqual (Arg0, 0x00))
{
Store (0x00, GP23)
}
}
Method (SXIO, 1, Serialized)
{
If (LLessEqual (Arg0, 0x01))
{
Store (Arg0, GD24)
}
}
Method (SXIL, 0, Serialized)
{
Return (GP24)
}
Method (SXLV, 1, Serialized)
{
If (LLessEqual (Arg0, 0x01))
{
Store (Arg0, GP24)
}
}
}
}
Device (DSB1)
{
Name (_ADR, 0x00030000) // _ADR: Address
Name (_SUN, 0x02) // _SUN: Slot User Number
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
Device (UPS0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (ARE0, PCI_Config, 0x00, 0x04)
Field (ARE0, ByteAcc, NoLock, Preserve)
{
AVND, 16
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DSB0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x3E),
, 6,
SBRS, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB3)
{
Name (_ADR, 0x00030000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (UPS0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (ARE0, PCI_Config, 0x00, 0x04)
Field (ARE0, ByteAcc, NoLock, Preserve)
{
AVND, 16
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DSB0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x3E),
, 6,
SBRS, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
}
}
Device (DSB3)
{
Name (_ADR, 0x00030000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB4)
{
Name (_ADR, 0x00040000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB5)
{
Name (_ADR, 0x00050000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
Device (DSB6)
{
Name (_ADR, 0x00060000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
}
Device (DSB4)
{
Name (_ADR, 0x00040000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (UPS0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (ARE0, PCI_Config, 0x00, 0x04)
Field (ARE0, ByteAcc, NoLock, Preserve)
{
AVND, 16
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DSB0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x3E),
, 6,
SBRS, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB3)
{
Name (_ADR, 0x00030000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB4)
{
Name (_ADR, 0x00040000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB5)
{
Name (_ADR, 0x00050000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
Device (DSB6)
{
Name (_ADR, 0x00060000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
}
Device (DSB5)
{
Name (_ADR, 0x00050000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
Device (DSB6)
{
Name (_ADR, 0x00060000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
}
Device (DSB2)
{
Name (_ADR, 0x00040000) // _ADR: Address
Name (_SUN, 0x03) // _SUN: Slot User Number
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
Device (UPS0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (ARE0, PCI_Config, 0x00, 0x04)
Field (ARE0, ByteAcc, NoLock, Preserve)
{
AVND, 16
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DSB0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x3E),
, 6,
SBRS, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB3)
{
Name (_ADR, 0x00030000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (UPS0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (ARE0, PCI_Config, 0x00, 0x04)
Field (ARE0, ByteAcc, NoLock, Preserve)
{
AVND, 16
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DSB0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x3E),
, 6,
SBRS, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
}
}
Device (DSB3)
{
Name (_ADR, 0x00030000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB4)
{
Name (_ADR, 0x00040000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB5)
{
Name (_ADR, 0x00050000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
Device (DSB6)
{
Name (_ADR, 0x00060000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
}
Device (DSB4)
{
Name (_ADR, 0x00040000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (UPS0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (ARE0, PCI_Config, 0x00, 0x04)
Field (ARE0, ByteAcc, NoLock, Preserve)
{
AVND, 16
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DSB0)
{
Name (_ADR, 0x00) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1,
Offset (0x3E),
, 6,
SBRS, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB3)
{
Name (_ADR, 0x00030000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB4)
{
Name (_ADR, 0x00040000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
Device (DEV0)
{
Name (_ADR, 0x00) // _ADR: Address
Method (_STA, 0, NotSerialized) // _STA: Status
{
Return (0x0F)
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
Device (DSB5)
{
Name (_ADR, 0x00050000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
Device (DSB6)
{
Name (_ADR, 0x00060000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
}
Device (DSB5)
{
Name (_ADR, 0x00050000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
Device (DSB6)
{
Name (_ADR, 0x00060000) // _ADR: Address
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
If (OSDW)
{
Return (0x01)
}
Return (0x00)
}
}
}
}
Device (DSB3)
{
Name (_ADR, 0x00050000) // _ADR: Address
Name (_SUN, 0x04) // _SUN: Slot User Number
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
}
Device (DSB4)
{
Name (_ADR, 0x00060000) // _ADR: Address
Name (_SUN, 0x05) // _SUN: Slot User Number
OperationRegion (A1E0, PCI_Config, 0x00, 0x40)
Field (A1E0, ByteAcc, NoLock, Preserve)
{
AVND, 32,
BMIE, 3,
Offset (0x18),
PRIB, 8,
SECB, 8,
SUBB, 8,
Offset (0x1E),
, 13,
MABT, 1
}
Method (_BBN, 0, NotSerialized) // _BBN: BIOS Bus Number
{
Return (SECB)
}
Method (_STA, 0, NotSerialized) // _STA: Status
{
If (OSDW)
{
Return (0x0F)
}
Else
{
Return (0x09)
}
}
Method (_RMV, 0, NotSerialized) // _RMV: Removal Status
{
Return (0x00)
}
}
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
If (OSDW)
{
If (LEqual (Arg0, Buffer (0x10)
{
/* 0000 */ 0xC6, 0xB7, 0xB5, 0xA0, 0x18, 0x13, 0x1C, 0x44,
/* 0008 */ 0xB0, 0xC9, 0xFE, 0x69, 0x5E, 0xAF, 0x94, 0x9B
}))
{
Store (Package (0x02)
{
"PCI-Thunderbolt",
0x01
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3)
RefOf (Local0)
Return (Local0)
}
}
Return (Zero)
}
}
}
}
}

SSDT-5

View File SSDT-5.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-5.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "SSDT"
* Length 0x000000B8 (184)
* Revision 0x01
* Checksum 0x25
* OEM ID "APPLE "
* OEM Table ID "Sdxc"
* OEM Revision 0x00001000 (4096)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-5.aml", "SSDT", 1, "APPLE ", "Sdxc", 0x00001000)
{
Scope (\_SB)
{
Name (SDTB, Buffer (0x82)
{
/* 0000 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0008 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0010 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0018 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0020 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0028 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0030 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0038 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0040 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0048 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0050 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0058 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0060 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0068 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0070 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0078 */ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
/* 0080 */ 0x00, 0x00
})
}
}

SSDT-6

View File SSDT-6.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-6.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "SSDT"
* Length 0x000006EF (1775)
* Revision 0x01
* Checksum 0xC0
* OEM ID "PmRef"
* OEM Table ID "Cpu0Ist"
* OEM Revision 0x00003000 (12288)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-6.aml", "SSDT", 1, "PmRef", "Cpu0Ist", 0x00003000)
{
External (_PR_.CPU0, DeviceObj)
External (CPLT, IntObj)
External (PDC0)
External (TCNT, IntObj)
Scope (\_PR.CPU0)
{
Method (_PPC, 0, NotSerialized) // _PPC: Performance Present Capabilites
{
Store (CPLT, Local0)
If (LLessEqual (Local0, 0x03))
{
Return (0x00)
}
Store (Subtract (Local0, 0x03), Local0)
Return (Local0)
}
Name (_PCT, Package (0x02) // _PCT: Performance Control
{
ResourceTemplate ()
{
Register (FFixedHW,
0x10, // Bit Width
0x00, // Bit Offset
0x0000000000000199, // Address
,)
},
ResourceTemplate ()
{
Register (FFixedHW,
0x10, // Bit Width
0x00, // Bit Offset
0x0000000000000198, // Address
,)
}
})
Name (_PSS, Package (0x0E) // _PSS: Performance Supported States
{
Package (0x06)
{
0x00000D49,
0x00014820,
0x0000000A,
0x0000000A,
0x00002600,
0x00002600
},
Package (0x06)
{
0x00000D48,
0x00014820,
0x0000000A,
0x0000000A,
0x00002200,
0x00002200
},
Package (0x06)
{
0x00000C80,
0x00012D71,
0x0000000A,
0x0000000A,
0x00002000,
0x00002000
},
Package (0x06)
{
0x00000BB8,
0x000113BB,
0x0000000A,
0x0000000A,
0x00001E00,
0x00001E00
},
Package (0x06)
{
0x00000A8C,
0x0000EEFE,
0x0000000A,
0x0000000A,
0x00001B00,
0x00001B00
},
Package (0x06)
{
0x000009C4,
0x0000D7A1,
0x0000000A,
0x0000000A,
0x00001900,
0x00001900
},
Package (0x06)
{
0x000008FC,
0x0000C138,
0x0000000A,
0x0000000A,
0x00001700,
0x00001700
},
Package (0x06)
{
0x00000834,
0x0000ABAA,
0x0000000A,
0x0000000A,
0x00001500,
0x00001500
},
Package (0x06)
{
0x0000076C,
0x000096FE,
0x0000000A,
0x0000000A,
0x00001300,
0x00001300
},
Package (0x06)
{
0x000006A4,
0x000085E5,
0x0000000A,
0x0000000A,
0x00001100,
0x00001100
},
Package (0x06)
{
0x00000578,
0x000069AD,
0x0000000A,
0x0000000A,
0x00000E00,
0x00000E00
},
Package (0x06)
{
0x000004B0,
0x000057ED,
0x0000000A,
0x0000000A,
0x00000C00,
0x00000C00
},
Package (0x06)
{
0x000003E8,
0x000046F7,
0x0000000A,
0x0000000A,
0x00000A00,
0x00000A00
},
Package (0x06)
{
0x00000320,
0x000036CF,
0x0000000A,
0x0000000A,
0x00000800,
0x00000800
}
})
Name (APSS, Package (0x1F)
{
Package (0x06)
{
0x00000ED8,
0x00014820,
0x0000000A,
0x0000000A,
0x00002600,
0x00002600
},
Package (0x06)
{
0x00000E74,
0x00014820,
0x0000000A,
0x0000000A,
0x00002500,
0x00002500
},
Package (0x06)
{
0x00000E10,
0x00014820,
0x0000000A,
0x0000000A,
0x00002400,
0x00002400
},
Package (0x06)
{
0x00000DAC,
0x00014820,
0x0000000A,
0x0000000A,
0x00002300,
0x00002300
},
Package (0x06)
{
0x00000D48,
0x00014820,
0x0000000A,
0x0000000A,
0x00002200,
0x00002200
},
Package (0x06)
{
0x00000CE4,
0x00012D71,
0x0000000A,
0x0000000A,
0x00002100,
0x00002100
},
Package (0x06)
{
0x00000C80,
0x000113BB,
0x0000000A,
0x0000000A,
0x00002000,
0x00002000
},
Package (0x06)
{
0x00000C1C,
0x0000EEFE,
0x0000000A,
0x0000000A,
0x00001F00,
0x00001F00
},
Package (0x06)
{
0x00000BB8,
0x0000D7A1,
0x0000000A,
0x0000000A,
0x00001E00,
0x00001E00
},
Package (0x06)
{
0x00000B54,
0x0000C138,
0x0000000A,
0x0000000A,
0x00001D00,
0x00001D00
},
Package (0x06)
{
0x00000AF0,
0x0000ABAA,
0x0000000A,
0x0000000A,
0x00001C00,
0x00001C00
},
Package (0x06)
{
0x00000A8C,
0x000096FE,
0x0000000A,
0x0000000A,
0x00001B00,
0x00001B00
},
Package (0x06)
{
0x00000A28,
0x000085E5,
0x0000000A,
0x0000000A,
0x00001A00,
0x00001A00
},
Package (0x06)
{
0x000009C4,
0x000069AD,
0x0000000A,
0x0000000A,
0x00001900,
0x00001900
},
Package (0x06)
{
0x00000960,
0x000057ED,
0x0000000A,
0x0000000A,
0x00001800,
0x00001800
},
Package (0x06)
{
0x000008FC,
0x000046F7,
0x0000000A,
0x0000000A,
0x00001700,
0x00001700
},
Package (0x06)
{
0x00000898,
0x000036CF,
0x0000000A,
0x0000000A,
0x00001600,
0x00001600
},
Package (0x06)
{
0x00000834,
0x00000000,
0x0000000A,
0x0000000A,
0x00001500,
0x00001500
},
Package (0x06)
{
0x000007D0,
0x00000000,
0x0000000A,
0x0000000A,
0x00001400,
0x00001400
},
Package (0x06)
{
0x0000076C,
0x00000000,
0x0000000A,
0x0000000A,
0x00001300,
0x00001300
},
Package (0x06)
{
0x00000708,
0x00000000,
0x0000000A,
0x0000000A,
0x00001200,
0x00001200
},
Package (0x06)
{
0x000006A4,
0x00000000,
0x0000000A,
0x0000000A,
0x00001100,
0x00001100
},
Package (0x06)
{
0x00000640,
0x00000000,
0x0000000A,
0x0000000A,
0x00001000,
0x00001000
},
Package (0x06)
{
0x000005DC,
0x00000000,
0x0000000A,
0x0000000A,
0x00000F00,
0x00000F00
},
Package (0x06)
{
0x00000578,
0x00000000,
0x0000000A,
0x0000000A,
0x00000E00,
0x00000E00
},
Package (0x06)
{
0x00000514,
0x00000000,
0x0000000A,
0x0000000A,
0x00000D00,
0x00000D00
},
Package (0x06)
{
0x000004B0,
0x00000000,
0x0000000A,
0x0000000A,
0x00000C00,
0x00000C00
},
Package (0x06)
{
0x0000044C,
0x00000000,
0x0000000A,
0x0000000A,
0x00000B00,
0x00000B00
},
Package (0x06)
{
0x000003E8,
0x00000000,
0x0000000A,
0x0000000A,
0x00000A00,
0x00000A00
},
Package (0x06)
{
0x00000384,
0x00000000,
0x0000000A,
0x0000000A,
0x00000900,
0x00000900
},
Package (0x06)
{
0x00000320,
0x00000000,
0x0000000A,
0x0000000A,
0x00000800,
0x00000800
}
})
Name (APSN, 0x04)
Name (APLF, 0x00)
Name (PSDF, 0x00)
Method (_PSD, 0, NotSerialized) // _PSD: Power State Dependencies
{
If (LNot (PSDF))
{
Store (TCNT, Index (DerefOf (Index (HPSD, 0x00)), 0x04))
Store (TCNT, Index (DerefOf (Index (SPSD, 0x00)), 0x04))
Store (Ones, PSDF)
}
If (And (PDC0, 0x0800))
{
Return (HPSD)
}
Return (SPSD)
}
Name (HPSD, Package (0x01)
{
Package (0x05)
{
0x05,
0x00,
0x00,
0xFE,
0x80
}
})
Name (SPSD, Package (0x01)
{
Package (0x05)
{
0x05,
0x00,
0x00,
0xFC,
0x80
}
})
}
}

SSDT-7

View File SSDT-7.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-7.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "SSDT"
* Length 0x00000B83 (2947)
* Revision 0x01
* Checksum 0x95
* OEM ID "PmRef"
* OEM Table ID "CpuPm"
* OEM Revision 0x00003000 (12288)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT-7.aml", "SSDT", 1, "PmRef", "CpuPm", 0x00003000)
{
External (_PR_.CPU0, DeviceObj)
External (_PR_.CPU0._PPC)
External (_PR_.CPU1, DeviceObj)
External (_PR_.CPU2, DeviceObj)
External (_PR_.CPU3, DeviceObj)
External (_PR_.CPU4, DeviceObj)
External (_PR_.CPU5, DeviceObj)
External (_PR_.CPU6, DeviceObj)
External (_PR_.CPU7, DeviceObj)
Scope (\)
{
Name (SSDT, Package (0x0C)
{
"CPU0IST ",
0x8B447190,
0x00000000,
"APIST ",
0x8CF8A190,
0x0000067C,
"CPU0CST ",
0x8CF89890,
0x000004F0,
"APCST ",
0x8CF88D90,
0x00000119
})
Name (\PDC0, 0x80000000)
Name (\PDC1, 0x80000000)
Name (\PDC2, 0x80000000)
Name (\PDC3, 0x80000000)
Name (\PDC4, 0x80000000)
Name (\PDC5, 0x80000000)
Name (\PDC6, 0x80000000)
Name (\PDC7, 0x80000000)
Name (\SDTL, 0x00)
}
Scope (\_PR)
{
OperationRegion (PPMT, SystemMemory, 0x8CD1BF90, 0x003A)
Field (PPMT, AnyAcc, Lock, Preserve)
{
PGRV, 8,
CFGD, 32,
Offset (0x06),
ACRT, 8,
APSV, 8,
AAC0, 8,
CPID, 32,
CPPC, 8,
CCTP, 8,
CLVL, 8,
CBMI, 8,
PL10, 16,
PL20, 16,
PLW0, 8,
CTC0, 8,
TAR0, 8,
PPC0, 8,
PL11, 16,
PL21, 16,
PLW1, 8,
CTC1, 8,
TAR1, 8,
PPC1, 8,
PL12, 16,
PL22, 16,
PLW2, 8,
CTC2, 8,
TAR2, 8,
PPC2, 8,
C3MW, 8,
C6MW, 8,
C7MW, 8,
CDMW, 8,
C3LT, 16,
C6LT, 16,
C7LT, 16,
CDLT, 16,
CDLV, 16,
CDPW, 16,
MPMF, 8
}
}
Scope (\_PR.CPU0)
{
Name (HI0, 0x00)
Name (HC0, 0x00)
Method (_PDC, 1, NotSerialized) // _PDC: Processor Driver Capabilities
{
If (CondRefOf (\_PR.CPU0._PPC))
{
Store (CPPC, \_PR.CPU0._PPC)
}
Store (CPDC (Arg0), Local0)
GCAP (Local0)
Return (Local0)
}
Method (_OSC, 4, NotSerialized) // _OSC: Operating System Capabilities
{
Store (COSC (Arg0, Arg1, Arg2, Arg3), Local0)
GCAP (Local0)
Return (Local0)
}
Method (CPDC, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, REVS)
CreateDWordField (Arg0, 0x04, SIZE)
Store (SizeOf (Arg0), Local0)
Store (Subtract (Local0, 0x08), Local1)
CreateField (Arg0, 0x40, Multiply (Local1, 0x08), TEMP)
Name (STS0, Buffer (0x04)
{
0x00, 0x00, 0x00, 0x00
})
Concatenate (STS0, TEMP, Local2)
Return (COSC (Buffer (0x10)
{
/* 0000 */ 0x16, 0xA6, 0x77, 0x40, 0x0C, 0x29, 0xBE, 0x47,
/* 0008 */ 0x9E, 0xBD, 0xD8, 0x70, 0x58, 0x71, 0x39, 0x53
}, REVS, SIZE, Local2))
}
Method (COSC, 4, NotSerialized)
{
CreateDWordField (Arg3, 0x00, STS0)
CreateDWordField (Arg3, 0x04, CAP0)
CreateDWordField (Arg0, 0x00, IID0)
CreateDWordField (Arg0, 0x04, IID1)
CreateDWordField (Arg0, 0x08, IID2)
CreateDWordField (Arg0, 0x0C, IID3)
Name (UID0, Buffer (0x10)
{
/* 0000 */ 0x16, 0xA6, 0x77, 0x40, 0x0C, 0x29, 0xBE, 0x47,
/* 0008 */ 0x9E, 0xBD, 0xD8, 0x70, 0x58, 0x71, 0x39, 0x53
})
CreateDWordField (UID0, 0x00, EID0)
CreateDWordField (UID0, 0x04, EID1)
CreateDWordField (UID0, 0x08, EID2)
CreateDWordField (UID0, 0x0C, EID3)
If (LNot (LAnd (LAnd (LEqual (IID0, EID0), LEqual (IID1, EID1)),
LAnd (LEqual (IID2, EID2), LEqual (IID3, EID3)))))
{
Store (0x06, STS0)
Return (Arg3)
}
If (LNotEqual (Arg1, 0x01))
{
Store (0x0A, STS0)
Return (Arg3)
}
Return (Arg3)
}
Method (GCAP, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, STS0)
CreateDWordField (Arg0, 0x04, CAP0)
If (LOr (LEqual (STS0, 0x06), LEqual (STS0, 0x0A)))
{
Return (Zero)
}
If (And (STS0, 0x01))
{
And (CAP0, 0x0BFF, CAP0)
Return (Zero)
}
Or (And (PDC0, 0x7FFFFFFF), CAP0, PDC0)
If (And (CFGD, 0x7A))
{
If (LAnd (LAnd (And (CFGD, 0x0200), And (PDC0, 0x18
)), LNot (And (SDTL, 0x02))))
{
Or (SDTL, 0x02, SDTL)
OperationRegion (CST0, SystemMemory, DerefOf (Index (SSDT, 0x07)), DerefOf (Index (SSDT, 0x08
)))
Load (CST0, HC0)
}
}
Return (Zero)
}
Method (DTGP, 5, NotSerialized)
{
If (LEqual (Arg0, Buffer (0x10)
{
/* 0000 */ 0xC6, 0xB7, 0xB5, 0xA0, 0x18, 0x13, 0x1C, 0x44,
/* 0008 */ 0xB0, 0xC9, 0xFE, 0x69, 0x5E, 0xAF, 0x94, 0x9B
}))
{
If (LEqual (Arg1, One))
{
If (LEqual (Arg2, Zero))
{
Store (Buffer (0x01)
{
0x03
}, Arg4)
Return (One)
}
If (LEqual (Arg2, One))
{
Return (One)
}
}
}
Store (Buffer (0x01)
{
0x00
}, Arg4)
Return (Zero)
}
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
Store ("Writing plugin-type to Registry!", Debug)
Store (Package (0x02)
{
"plugin-type",
0x01
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3, RefOf (Local0))
Return (Local0)
}
}
Scope (\_PR.CPU1)
{
Name (HI1, 0x00)
Name (HC1, 0x00)
Method (_PDC, 1, NotSerialized) // _PDC: Processor Driver Capabilities
{
Store (\_PR.CPU0.CPDC (Arg0), Local0)
GCAP (Local0)
Return (Local0)
}
Method (_OSC, 4, NotSerialized) // _OSC: Operating System Capabilities
{
Store (\_PR.CPU0.COSC (Arg0, Arg1, Arg2, Arg3), Local0)
GCAP (Local0)
Return (Local0)
}
Method (GCAP, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, STS1)
CreateDWordField (Arg0, 0x04, CAP1)
If (LOr (LEqual (STS1, 0x06), LEqual (STS1, 0x0A)))
{
Return (Zero)
}
If (And (STS1, 0x01))
{
And (CAP1, 0x0BFF, CAP1)
Return (Zero)
}
Or (And (PDC1, 0x7FFFFFFF), CAP1, PDC1)
If (LEqual (And (PDC1, 0x09), 0x09))
{
APPT ()
}
If (And (PDC1, 0x18))
{
APCT ()
}
Store (PDC1, PDC0)
Return (Zero)
}
Method (APCT, 0, NotSerialized)
{
If (LAnd (And (CFGD, 0x7A), LNot (And (SDTL, 0x20
))))
{
Or (SDTL, 0x20, SDTL)
OperationRegion (CST1, SystemMemory, DerefOf (Index (SSDT, 0x0A)), DerefOf (Index (SSDT, 0x0B
)))
Load (CST1, HC1)
}
}
Method (APPT, 0, NotSerialized)
{
If (LAnd (And (CFGD, 0x01), LNot (And (SDTL, 0x10
))))
{
Or (SDTL, 0x10, SDTL)
OperationRegion (IST1, SystemMemory, DerefOf (Index (SSDT, 0x04)), DerefOf (Index (SSDT, 0x05
)))
Load (IST1, HI1)
}
}
}
Scope (\_PR.CPU2)
{
Method (_PDC, 1, NotSerialized) // _PDC: Processor Driver Capabilities
{
Store (\_PR.CPU0.CPDC (Arg0), Local0)
GCAP (Local0)
Return (Local0)
}
Method (_OSC, 4, NotSerialized) // _OSC: Operating System Capabilities
{
Store (\_PR.CPU0.COSC (Arg0, Arg1, Arg2, Arg3), Local0)
GCAP (Local0)
Return (Local0)
}
Method (GCAP, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, STS2)
CreateDWordField (Arg0, 0x04, CAP2)
If (LOr (LEqual (STS2, 0x06), LEqual (STS2, 0x0A)))
{
Return (Zero)
}
If (And (STS2, 0x01))
{
And (CAP2, 0x0BFF, CAP2)
Return (Zero)
}
Or (And (PDC2, 0x7FFFFFFF), CAP2, PDC2)
If (LEqual (And (PDC2, 0x09), 0x09))
{
\_PR.CPU1.APPT ()
}
If (And (PDC2, 0x18))
{
\_PR.CPU1.APCT ()
}
Store (PDC2, PDC0)
Return (Zero)
}
}
Scope (\_PR.CPU3)
{
Method (_PDC, 1, NotSerialized) // _PDC: Processor Driver Capabilities
{
Store (\_PR.CPU0.CPDC (Arg0), Local0)
GCAP (Local0)
Return (Local0)
}
Method (_OSC, 4, NotSerialized) // _OSC: Operating System Capabilities
{
Store (\_PR.CPU0.COSC (Arg0, Arg1, Arg2, Arg3), Local0)
GCAP (Local0)
Return (Local0)
}
Method (GCAP, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, STS3)
CreateDWordField (Arg0, 0x04, CAP3)
If (LOr (LEqual (STS3, 0x06), LEqual (STS3, 0x0A)))
{
Return (Zero)
}
If (And (STS3, 0x01))
{
And (CAP3, 0x0BFF, CAP3)
Return (Zero)
}
Or (And (PDC3, 0x7FFFFFFF), CAP3, PDC3)
If (LEqual (And (PDC3, 0x09), 0x09))
{
\_PR.CPU1.APPT ()
}
If (And (PDC3, 0x18))
{
\_PR.CPU1.APCT ()
}
Store (PDC3, PDC0)
Return (Zero)
}
}
Scope (\_PR.CPU4)
{
Method (_PDC, 1, NotSerialized) // _PDC: Processor Driver Capabilities
{
Store (\_PR.CPU0.CPDC (Arg0), Local0)
GCAP (Local0)
Return (Local0)
}
Method (_OSC, 4, NotSerialized) // _OSC: Operating System Capabilities
{
Store (\_PR.CPU0.COSC (Arg0, Arg1, Arg2, Arg3), Local0)
GCAP (Local0)
Return (Local0)
}
Method (GCAP, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, STS4)
CreateDWordField (Arg0, 0x04, CAP4)
If (LOr (LEqual (STS4, 0x06), LEqual (STS4, 0x0A)))
{
Return (Zero)
}
If (And (STS4, 0x01))
{
And (CAP4, 0x0BFF, CAP4)
Return (Zero)
}
Or (And (PDC4, 0x7FFFFFFF), CAP4, PDC4)
If (LEqual (And (PDC4, 0x09), 0x09))
{
\_PR.CPU1.APPT ()
}
If (And (PDC4, 0x18))
{
\_PR.CPU1.APCT ()
}
Store (PDC4, PDC0)
Return (Zero)
}
}
Scope (\_PR.CPU5)
{
Method (_PDC, 1, NotSerialized) // _PDC: Processor Driver Capabilities
{
Store (\_PR.CPU0.CPDC (Arg0), Local0)
GCAP (Local0)
Return (Local0)
}
Method (_OSC, 4, NotSerialized) // _OSC: Operating System Capabilities
{
Store (\_PR.CPU0.COSC (Arg0, Arg1, Arg2, Arg3), Local0)
GCAP (Local0)
Return (Local0)
}
Method (GCAP, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, STS5)
CreateDWordField (Arg0, 0x04, CAP5)
If (LOr (LEqual (STS5, 0x06), LEqual (STS5, 0x0A)))
{
Return (Zero)
}
If (And (STS5, 0x01))
{
And (CAP5, 0x0BFF, CAP5)
Return (Zero)
}
Or (And (PDC5, 0x7FFFFFFF), CAP5, PDC5)
If (LEqual (And (PDC5, 0x09), 0x09))
{
\_PR.CPU1.APPT ()
}
If (And (PDC5, 0x18))
{
\_PR.CPU1.APCT ()
}
Store (PDC5, PDC0)
Return (Zero)
}
}
Scope (\_PR.CPU6)
{
Method (_PDC, 1, NotSerialized) // _PDC: Processor Driver Capabilities
{
Store (\_PR.CPU0.CPDC (Arg0), Local0)
GCAP (Local0)
Return (Local0)
}
Method (_OSC, 4, NotSerialized) // _OSC: Operating System Capabilities
{
Store (\_PR.CPU0.COSC (Arg0, Arg1, Arg2, Arg3), Local0)
GCAP (Local0)
Return (Local0)
}
Method (GCAP, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, STS6)
CreateDWordField (Arg0, 0x04, CAP6)
If (LOr (LEqual (STS6, 0x06), LEqual (STS6, 0x0A)))
{
Return (Zero)
}
If (And (STS6, 0x01))
{
And (CAP6, 0x0BFF, CAP6)
Return (Zero)
}
Or (And (PDC6, 0x7FFFFFFF), CAP6, PDC6)
If (LEqual (And (PDC6, 0x09), 0x09))
{
\_PR.CPU1.APPT ()
}
If (And (PDC6, 0x18))
{
\_PR.CPU1.APCT ()
}
Store (PDC6, PDC0)
Return (Zero)
}
}
Scope (\_PR.CPU7)
{
Method (_PDC, 1, NotSerialized) // _PDC: Processor Driver Capabilities
{
Store (\_PR.CPU0.CPDC (Arg0), Local0)
GCAP (Local0)
Return (Local0)
}
Method (_OSC, 4, NotSerialized) // _OSC: Operating System Capabilities
{
Store (\_PR.CPU0.COSC (Arg0, Arg1, Arg2, Arg3), Local0)
GCAP (Local0)
Return (Local0)
}
Method (GCAP, 1, NotSerialized)
{
CreateDWordField (Arg0, 0x00, STS7)
CreateDWordField (Arg0, 0x04, CAP7)
If (LOr (LEqual (STS7, 0x06), LEqual (STS7, 0x0A)))
{
Return (Zero)
}
If (And (STS7, 0x01))
{
And (CAP7, 0x0BFF, CAP7)
Return (Zero)
}
Or (And (PDC7, 0x7FFFFFFF), CAP7, PDC7)
If (LEqual (And (PDC7, 0x09), 0x09))
{
\_PR.CPU1.APPT ()
}
If (And (PDC7, 0x18))
{
\_PR.CPU1.APCT ()
}
Store (PDC7, PDC0)
Return (Zero)
}
}
}

SSDT

View File SSDT.dsl

/*
* Intel ACPI Component Architecture
* AML Disassembler version 20130823-32 [Sep 16 2013]
* Copyright (c) 2000 - 2013 Intel Corporation
*
* Disassembly of /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT.aml, Mon May 26 01:26:33 2014
*
* Original Table Header:
* Signature "SSDT"
* Length 0x0000025A (602)
* Revision 0x01
* Checksum 0x22
* OEM ID "APPLE "
* OEM Table ID "SataAhci"
* OEM Revision 0x00001000 (4096)
* Compiler ID "INTL"
* Compiler Version 0x20100915 (537921813)
*/
DefinitionBlock ("/Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/ACPI Tables/AML/SSDT.aml", "SSDT", 1, "APPLE ", "SataAhci", 0x00001000)
{
/*
* iASL Warning: There were 1 external control methods found during
* disassembly, but additional ACPI tables to resolve these externals
* were not specified. This resulting disassembler output file may not
* compile because the disassembler did not know how many arguments
* to assign to these methods. To specify the tables needed to resolve
* external control method references, use the one of the following
* example iASL invocations:
* iasl -e <ssdt1.aml,ssdt2.aml...> -d <dsdt.aml>
* iasl -e <dsdt.aml,ssdt2.aml...> -d <ssdt1.aml>
*/
External (DTGP, MethodObj) // Warning: Unresolved Method, guessing 4 arguments (may be incorrect, see warning above)
External (_SB_.PCI0.RP01.SSD0, DeviceObj)
External (_SB_.PCI0.SATA, DeviceObj)
External (GP08)
External (GTF0, IntObj)
Scope (\_SB.PCI0.SATA)
{
Device (PRT0)
{
Name (_ADR, 0xFFFF) // _ADR: Address
Name (_CID, "hdd-power-off") // _CID: Compatible ID
Method (_SDD, 1, NotSerialized) // _SDD: Set Device Data
{
Name (GBU0, Buffer (0x07)
{
0x00, 0x00, 0x00, 0x00, 0x00, 0xA0, 0x00
})
CreateByteField (GBU0, 0x00, GB00)
CreateByteField (GBU0, 0x01, GB01)
CreateByteField (GBU0, 0x02, GB02)
CreateByteField (GBU0, 0x03, GB03)
CreateByteField (GBU0, 0x04, GB04)
CreateByteField (GBU0, 0x05, GB05)
CreateByteField (GBU0, 0x06, GB06)
If (LEqual (SizeOf (Arg0), 0x0200))
{
CreateWordField (Arg0, 0x9C, W780)
If (And (W780, 0x08))
{
Store (0x10, GB00)
Store (0x03, GB01)
Store (0xEF, GB06)
}
Else
{
Store (0x90, GB00)
Store (0x03, GB01)
Store (0xEF, GB06)
}
}
Store (GBU0, GTF0)
}
Method (_PS0, 0, Serialized) // _PS0: Power State 0
{
Store (0x01, GP08)
Sleep (0x0A)
}
Method (_PS3, 0, Serialized) // _PS3: Power State 3
{
Store (0x00, GP08)
Sleep (0x7D)
}
Method (_GTF, 0, NotSerialized) // _GTF: Get Task File
{
Return (GTF0)
}
}
}
Scope (\_SB.PCI0.RP01.SSD0)
{
Device (PRT0)
{
Name (_ADR, 0xFFFF) // _ADR: Address
Method (_DSM, 4, NotSerialized) // _DSM: Device-Specific Method
{
Store (Package (0x02)
{
"io-device-location",
Buffer (0x04)
{
"SSD"
}
}, Local0)
DTGP (Arg0, Arg1, Arg2, Arg3)
RefOf (Local0)
Return (Local0)
}
Method (_SDD, 1, NotSerialized) // _SDD: Set Device Data
{
Name (GBU0, Buffer (0x07)
{
0x00, 0x00, 0x00, 0x00, 0x00, 0xA0, 0x00
})
CreateByteField (GBU0, 0x00, GB00)
CreateByteField (GBU0, 0x01, GB01)
CreateByteField (GBU0, 0x02, GB02)
CreateByteField (GBU0, 0x03, GB03)
CreateByteField (GBU0, 0x04, GB04)
CreateByteField (GBU0, 0x05, GB05)
CreateByteField (GBU0, 0x06, GB06)
If (LEqual (SizeOf (Arg0), 0x0200))
{
CreateWordField (Arg0, 0x9C, W780)
If (And (W780, 0x08))
{
Store (0x10, GB00)
Store (0x03, GB01)
Store (0xEF, GB06)
}
Else
{
Store (0x90, GB00)
Store (0x03, GB01)
Store (0xEF, GB06)
}
}
Store (GBU0, GTF0)
}
Method (_GTF, 0, NotSerialized) // _GTF: Get Task File
{
Return (GTF0)
}
}
}
}

Audio
Dumped using VoodooHDA's getdump tool

View VoodooHDAGetdump.txt File

VoodooHDA's getdump tool failed to produce a dump.
NOTE: AppleHDA was loaded when this dump was attempted.
If you wish to get a successful dump using VoodooHDA and it's associated getdump tool then AppleHDA will have to be disabled.
The simplest option to do that will be to add AppleHDADisabler.kext to your system, rebuild caches and reboot. Then try this dump again.

BIOS - System: Flashrom Log
Dumped using Flashrom Darwin Port, v0.9.6.1 r1589. OS X port by THe KiNG..

View flashrom_log.txt File

flashrom v0.9.6.1-runknown on Darwin 13.2.0 (x86_64)
flashrom was built with libpci 3.1.9, GCC 4.0.1 (Apple Inc. build 5488), little endian
Command line (6 args): /Applications/DarwinDumper_v2.8.8/DarwinDumper.app/Contents/Resources/Tools/flashrom -p internal -r /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/BIOS/System/biosbackup.rom -o /Applications/DarwinDumper_v2.8.8/DarwinDumperReports/000_2014-05-26_01-25-55_iMac14,2/DarwinDumper_2.8.8_Apple_X64_Mav_plievasabina/BIOS/System/flashrom_log.txt
Calibrating delay loop... OS timer resolution is 1 usecs, 2930M loops per second, 10 myus = 18 us, 100 myus = 93 us, 1000 myus = 929 us, 10000 myus = 8652 us, 4 myus = 3 us, OK.
Initializing internal programmer
Mapping low megabyte at 0x00000400, unaligned size 0xffc00.
Mapping low megabyte, 0xffc00 bytes at unaligned 0x00000400.
No coreboot table found.
dmidecode execution unsuccessful - continuing without DMI info
Found chipset "Intel Lynx Point" with PCI ID 8086:8c44.
This chipset is marked as untested. If you are using an up-to-date version
of flashrom *and* were (not) able to successfully update your firmware with it,
then please email a report to flashrom@flashrom.org including a verbose (-V) log.
Thank you!
Enabling flash write... enable_flash_ich_dc_spi: unknown ICH generation. Please report!
0xfff80000/0xffb80000 FWH IDSEL: 0x0
0xfff00000/0xffb00000 FWH IDSEL: 0x0
0xffe80000/0xffa80000 FWH IDSEL: 0x1
0xffe00000/0xffa00000 FWH IDSEL: 0x1
0xffd80000/0xff980000 FWH IDSEL: 0x2
0xffd00000/0xff900000 FWH IDSEL: 0x2
0xffc80000/0xff880000 FWH IDSEL: 0x3
0xffc00000/0xff800000 FWH IDSEL: 0x3
0xff700000/0xff300000 FWH IDSEL: 0x4
0xff600000/0xff200000 FWH IDSEL: 0x5
0xff500000/0xff100000 FWH IDSEL: 0x6
0xff400000/0xff000000 FWH IDSEL: 0x7
0xfff80000/0xffb80000 FWH decode enabled
0xfff00000/0xffb00000 FWH decode enabled
0xffe80000/0xffa80000 FWH decode enabled
0xffe00000/0xffa00000 FWH decode enabled
0xffd80000/0xff980000 FWH decode enabled
0xffd00000/0xff900000 FWH decode enabled
0xffc80000/0xff880000 FWH decode enabled
0xffc00000/0xff800000 FWH decode enabled
0xff700000/0xff300000 FWH decode disabled
0xff600000/0xff200000 FWH decode disabled
0xff500000/0xff100000 FWH decode disabled
0xff400000/0xff000000 FWH decode disabled
Maximum FWH chip size: 0x100000 bytes
BIOS_CNTL = 0x09: BIOS Lock Enable: disabled, BIOS Write Enable: enabled
Root Complex Register Block address = 0xfed1c000
GCS = 0xc21: BIOS Interface Lock-Down: enabled, Boot BIOS Straps: 0x3 (unknown)
Top Swap : not enabled
SPIBAR = 0xfed1c000 + 0x3800
0x04: 0xf008 (HSFS)
HSFS: FDONE=0, FCERR=0, AEL=0, BERASE=1, SCIP=0, FDOPSS=1, FDV=1, FLOCKDN=1
WARNING: SPI Configuration Lockdown activated.
Reading OPCODES... done
OP Type Pre-OP
op[0]: 0x9f, read w/o addr, none
op[1]: 0x02, write w/ addr, none
op[2]: 0x03, read w/ addr, none
op[3]: 0x01, write w/o addr, none
op[4]: 0x05, read w/o addr, none
op[5]: 0x20, write w/ addr, none
op[6]: 0xd8, write w/ addr, none
op[7]: 0xff, read w/o addr, none
Pre-OP 0: 0x06, Pre-OP 1: 0x06
0x06: 0x0004 (HSFC)
HSFC: FGO=0, FCYCLE=2, FDBC=0, SME=0
0x08: 0x00616257 (FADDR)
0x50: 0x00004aff (FRAP)
BMWAG 0x00, BMRAG 0x00, BRWA 0x4a, BRRA 0xff
0x54: 0x00000000 FREG0: WARNING: Flash Descriptor region (0x00000000-0x00000fff) is read-only.
0x58: 0x07ff0190 FREG1: BIOS region (0x00190000-0x007fffff) is read-write.
0x5C: 0x018f0002 FREG2: WARNING: Management Engine region (0x00002000-0x0018ffff) is read-only.
0x60: 0x00007fff FREG3: Gigabit Ethernet region is unused.
0x64: 0x00010001 FREG4: WARNING: Platform Data region (0x00001000-0x00001fff) is read-only.
0x74: 0x80010000 PR0: WARNING: 0x00000000-0x00001fff is read-only.
0x78: 0x860f0190 PR1: WARNING: 0x00190000-0x0060ffff is read-only.
0x7C: 0x9fff0632 PR2: WARNING: 0x00632000-0x01ffffff is read-only.
0x80: 0x00000000 (PR3 is unused)
0x84: 0x00000000 (PR4 is unused)
Please send a verbose log to flashrom@flashrom.org if this board is not listed on
http://flashrom.org/Supported_hardware#Supported_mainboards yet.
Writes have been disabled. You can enforce write support with the
ich_spi_force programmer option, but it will most likely harm your hardware!
If you force flashrom you will get no support if something breaks.
0x90: 0xc0 (SSFS)
SSFS: SCIP=0, FDONE=0, FCERR=0, AEL=0
0x91: 0xfc7f00 (SSFC)
SSFC: SCGO=0, ACS=0, SPOP=0, COP=0, DBC=63, SME=0, SCF=4
0x94: 0x0606 (PREOP)
0x96: 0x3c6c (OPTYPE)
0x98: 0x0103029f (OPMENU)
0x9C: 0xffd82005 (OPMENU+4)
0xA0: 0x00000000 (BBAR)
0xC4: 0x80802045 (LVSCC)
LVSCC: BES=0x1, WG=1, WSR=0, WEWS=0, EO=0x20, VCL=1
0xC8: 0x00000000 (UVSCC)
UVSCC: BES=0x0, WG=0, WSR=0, WEWS=0, EO=0x0, VCL=0
0xD0: 0x50444653 (FPB)
Reading flash descriptors mapped by the chipset via FDOC/FDOD... done.
=== Content Section ===
FLVALSIG 0x0ff0a55a
FLMAP0 0x03040003
FLMAP1 0x15100206
FLMAP2 0x00210120
--- Details ---
NR (Number of Regions): 4
FRBA (Flash Region Base Address): 0x040
NC (Number of Components): 1
FCBA (Flash Component Base Address): 0x030
ISL (ICH/PCH Strap Length): 21
FISBA/FPSBA (Flash ICH/PCH Strap Base Address): 0x100
NM (Number of Masters): 3
FMBA (Flash Master Base Address): 0x060
MSL/PSL (MCH/PROC Strap Length): 1
FMSBA (Flash MCH/PROC Strap Base Address): 0x200
=== Component Section ===
FLCOMP 0x64900044
FLILL 0x00000000
--- Details ---
Component 1 density: 8 MB
Component 2 is not used.
Read Clock Frequency: 20 MHz
Read ID and Status Clock Freq.: 50 MHz
Write and Erase Clock Freq.: 50 MHz
Fast Read is supported.
Fast Read Clock Frequency: 50 MHz
No forbidden opcodes.
=== Region Section ===
FLREG0 0x00000000
FLREG1 0x07ff0190
FLREG2 0x018f0002
FLREG3 0x00007fff
FLREG4 0x00010001
--- Details ---
Region 0 (Descr.) 0x00000000 - 0x00000fff
Region 1 (BIOS ) 0x00190000 - 0x007fffff
Region 2 (ME ) 0x00002000 - 0x0018ffff
Region 3 (GbE ) is unused.
Region 4 (Platf.) 0x00001000 - 0x00001fff
=== Master Section ===
FLMSTR1 0x0aff0000
FLMSTR2 0x0c0d0000
FLMSTR3 0xffff0118
--- Details ---
Descr. BIOS ME GbE Platf.
BIOS r rw r rw r
ME r rw rw
GbE rw rw rw rw rw
SPI Read Configuration: prefetching enabled, caching enabled, OK.
The following protocols are supported: FWH, SPI.
Probing for AMIC A25L05PT, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L05PU, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L10PT, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L10PU, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L20PT, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L20PU, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L40PT, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L40PU, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L80P, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L16PT, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L16PU, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L512, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L010, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L020, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L040, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L080, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L016, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25L032, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for AMIC A25LQ032, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF021, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF041A, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF081, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF081A, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF161, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF321, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF321A, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DF641(A), 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25DQ161, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25F512B, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25FS010, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT25FS040, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26DF041, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26DF081A, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26DF161, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26DF161A, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT26F004, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45CS1282, 16896 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB011D, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB021D, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB041D, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB081D, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB161D, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB321C, 4224 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB321D, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel AT45DB642D, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for EMST F25L008A, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B05, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B05T, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B10, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B10T, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B20T, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B40T, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B80T, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B16T, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B32T, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25B64T, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F05, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F10, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25F32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q80(A), 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q32(A/B), 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25Q128, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25QH16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon EN25QH32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for GigaDevice GD25Q128, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L512, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L1005, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L2005, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L4005, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L8005, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L1605, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L1635D, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L1635E, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L3205, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L3235D, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix MX25L6405, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Chip status register is 00
Chip status register: Status Register Write Disable (SRWD) is not set
Chip status register: Bit 6 is not set
Chip status register: Block Protect 3 (BP3) is not set
Chip status register: Block Protect 2 (BP2) is not set
Chip status register: Block Protect 1 (BP1) is not set
Chip status register: Block Protect 0 (BP0) is not set
Chip status register: Write Enable Latch (WEL) is not set
Chip status register: Write In Progress (WIP/BUSY) is not set
Found Macronix flash chip "MX25L6405" (8192 kB, SPI) at physical address 0xff800000.
Probing for Macronix MX25L12805, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE10, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx M25PE16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Numonyx N25Q064, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV010, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV016B, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV020, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV040, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV080B, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC Pm25LV512, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Sanyo LF25FW203A, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL004A, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL008A, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL016A, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL032A, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Spansion S25FL064A, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25LF040A, 512 kB: Invalid OPCODE 0xab, will not execute.
Probing for SST SST25LF080A, 1024 kB: Invalid OPCODE 0xab, will not execute.
Probing for SST SST25VF010, 128 kB: Invalid OPCODE 0x90, will not execute.
Probing for SST SST25VF016B, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25VF032B, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25VF064C, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25VF040, 512 kB: Invalid OPCODE 0x90, will not execute.
Probing for SST SST25VF040B, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST SST25VF040B.REMS, 512 kB: Invalid OPCODE 0x90, will not execute.
Probing for SST SST25VF080B, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P05-A, 64 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P05, 64 kB: Ignoring RES in favour of RDID.
Probing for ST M25P10-A, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P10, 128 kB: Ignoring RES in favour of RDID.
Probing for ST M25P20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P40-old, 512 kB: Ignoring RES in favour of RDID.
Probing for ST M25P80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25P128, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25PX16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25PX32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST M25PX64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25Q128, 16384 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X10, 128 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X20, 256 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X40, 512 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X80, 1024 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X16, 2048 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X32, 4096 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Winbond W25X64, 8192 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Unknown SFDP-capable chip, 0 kB: Invalid OPCODE 0x5a, will not execute.
Receiving SFDP signature failed.
Probing for AMIC unknown AMIC SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Atmel unknown Atmel SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Eon unknown Eon SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Macronix unknown Macronix SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for PMC unknown PMC SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for SST unknown SST SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for ST unknown ST SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Sanyo unknown Sanyo SPI chip, 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Generic unknown SPI chip (RDID), 0 kB: probe_spi_rdid_generic: id1 0xc2, id2 0x2017
Probing for Generic unknown SPI chip (REMS), 0 kB: Invalid OPCODE 0x90, will not execute.
Probing for Atmel AT49LH002, 256 kB: probe_82802ab: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 82802AB, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 82802AC, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm49FL002, 256 kB: probe_jedec_common: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm49FL004, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Sharp LHF00L04, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF002A/B, 256 kB: probe_jedec_common: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF003A/B, 384 kB: probe_jedec_common: id1 0xf0, id2 0xe2, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF004A/B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF004C, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF008A, 1024 kB: probe_jedec_common: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF008C, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF016C, 2048 kB: Chip size 2048 kB is bigger than supported size 1024 kB of chipset/board/programmer for FWH interface, probe/read/erase/write may fail. probe_82802ab: id1 0xf0, id2 0xe2, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW040A, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW040B, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW080A, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW080B, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW002, 256 kB: probe_82802ab: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW016, 2048 kB: Chip size 2048 kB is bigger than supported size 1024 kB of chipset/board/programmer for FWH interface, probe/read/erase/write may fail. probe_82802ab: id1 0xf0, id2 0xe2, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW040, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW080, 1024 kB: probe_82802ab: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FA, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FB, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FC, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W49V002FA, 256 kB: probe_jedec_common: id1 0x00, id2 0x00, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V080FA, 1024 kB: probe_jedec_common: id1 0x44, id2 0x24, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V080FA (dual mode), 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Found Macronix flash chip "MX25L6405" (8192 kB, SPI).
Reading flash... done.
Restoring MMIO space at 0x858a0
Restoring PCI config space for 00:1f:0 reg 0xdc

Bootloaders & Disk Sectors
disk0

APPLE HDD ST1000DM003 Media | 1 TB | GUID_partition_scheme | MBR boot code detected: None | View Disk Sectors

| DEVICE | TYPE | NAME | SIZE | PBR (Stage1) | BootFile (Stage 2) | UEFI BootFile
| disk0s1 | EFI | EFI | 209 MB | Apple EFI |  |
| disk0s2 | Apple_HFS | Macintosh HD | 999 GB |  |  |
| disk0s3 | Apple_Boot | Recovery HD | 650 MB |  |  |

disk1

WD My Passport 0812 Media | 500 GB | GUID_partition_scheme | MBR boot code detected: None | View Disk Sectors

| DEVICE | TYPE | NAME | SIZE | PBR (Stage1) | BootFile (Stage 2) | UEFI BootFile
| disk1s1 | EFI | EFI | 209 MB | Apple EFI |  |
| disk1s2 | Apple_HFS | OS X Snow Leopard Install Disk - 10.6.8 | 10 GB |  |  |
| disk1s3 | Apple_HFS | OS X Lion Install Disk - 10.7.5 | 10 GB |  |  |
| disk1s4 | Apple_HFS | OS X Mountain Lion Install Disk - 10.8.5 | 10 GB |  |  |
| disk1s5 | Apple_HFS | OS X 10.9 Install Disk - 10.9.3 | 10 GB |  |  |
| disk1s6 | Apple_HFS | OS X Install Disk - 10.10 | 10 GB |  |  |
| disk1s7 | Apple_HFS | BootTest | 27 GB |  |  |
| disk1s8 | Apple_HFS | SoftDisk | 149 GB |  |  |
| disk1s9 | Apple_HFS | DataDisk | 135 GB |  |  |
| disk1s10 | Microsoft Basic Data | 11111 | 135 GB | Windows NTFS NTLDR |  |

Bootloader Config .plist files
/disk0s2-Macintosh HD/Library/Preferences/SystemConfiguration/com.apple.Boot.plist : Apple

View com.apple.Boot.plist

<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE plist PUBLIC "-//Apple//DTD PLIST 1.0//EN" "http://www.apple.com/DTDs/PropertyList-1.0.dtd">
<plist version="1.0">
<dict>
<key>Kernel Flags</key>
<string></string>
</dict>
</plist>

/disk1s3-OS X Lion Install Disk - 10.7.5/Library/Preferences/SystemConfiguration/com.apple.Boot.plist : Apple

View com.apple.Boot.plist

<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE plist PUBLIC "-//Apple//DTD PLIST 1.0//EN" "http://www.apple.com/DTDs/PropertyList-1.0.dtd">
<plist version="1.0">
<dict>
<key>Kernel Flags</key>
<string>root-dmg=file:///BaseSystem.dmg</string>
<key>Kernel Cache</key>
<string>\kernelcache</string>
</dict>
</plist>

/disk1s4-OS X Mountain Lion Install Disk - 10.8.5/Library/Preferences/SystemConfiguration/com.apple.Boot.plist : Apple

View com.apple.Boot.plist

<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE plist PUBLIC "-//Apple//DTD PLIST 1.0//EN" "http://www.apple.com/DTDs/PropertyList-1.0.dtd">
<plist version="1.0">
<dict>
<key>Kernel Flags</key>
<string>root-dmg=file:///BaseSystem.dmg</string>
<key>Kernel Cache</key>
<string>\kernelcache</string>
</dict>
</plist>

/disk1s5-OS X 10.9 Install Disk - 10.9.3/Library/Preferences/SystemConfiguration/com.apple.Boot.plist : Apple

View com.apple.Boot.plist

<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE plist PUBLIC "-//Apple//DTD PLIST 1.0//EN" "http://www.apple.com/DTDs/PropertyList-1.0.dtd">
<plist version="1.0">
<dict>
<key>Kernel Cache</key>
<string>/.IABootFiles/kernelcache</string>
<key>Kernel Flags</key>
<string>container-dmg=file:///Install%20OS%20X%20Mavericks.app/Contents/SharedSupport/InstallESD.dmg root-dmg=file:///BaseSystem.dmg</string>
</dict>
</plist>

/disk1s7-BootTest/Library/Preferences/SystemConfiguration/com.apple.Boot.plist : Apple

View com.apple.Boot.plist

<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE plist PUBLIC "-//Apple//DTD PLIST 1.0//EN" "http://www.apple.com/DTDs/PropertyList-1.0.dtd">
<plist version="1.0">
<dict>
<key>Kernel Flags</key>
<string></string>
</dict>
</plist>

Device Properties
Dumped using gfxutil v0.71b by McMatrix from 2007

View device-properties.plist File

<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE plist PUBLIC "-//Apple//DTD PLIST 1.0//EN" "http://www.apple.com/DTDs/PropertyList-1.0.dtd">
<plist version="1.0">
<dict>
<key>PciRoot(0x0)/Pci(0x1,0x0)/Pci(0x0,0x0)</key>
<dict>
<key>@0,AAPL,boot-display</key>
<string></string>
<key>@0,EDID</key>
<data>
AP///////wAGEAWwAAAAABwWAQS1PCJ4Im+xp1VMniUMUFQAAAABAQEBAQEB
AQEBAQEBAQEBVl4AoKCgKVAwIDUAVVAhAAAaGh0AgFHQHCBAgDUAVVAhAAAc
AAAA/ABpTWFjCiAgICAgICAgAAAAAAAAAAAAAAAAAAAAAAAAAY4CAyjBIwkH
B4MBAABw+hAAABJ6Mfx4vbICEIh05Wr6EADb7vX3+P7/Vl4AoKCgKVAwIDUA
VVAhAAAaGh0AgFHQHCBAgDUAVVAhAAAcAAAAAAAAAAAAAAAAAAAAAAAAAAAA
AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAzA==
</data>
<key>@0,NVDA,UnderscanMin</key>
<data>
UgAAAA==
</data>
<key>@0,NVMT</key>
<data>
DgN/IAAAAAAACqAFoAowClAKAADJBaMFqAUAAGD/ZA4AAAABrwAAAAAAAAAA
AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAD//wAAAAAAAAAAAAABAAAAAAAA/wAA
AAC8AgFKCgQAAAADAAAACqAFAAqgBQ==
</data>
<key>@0,built-in</key>
<string></string>
<key>@0,compatible</key>
<string>NVDA,NVMac</string>
<key>@0,connector-type</key>
<data>
AAQAAA==
</data>
<key>@0,device_type</key>
<string>display</string>
<key>@0,display-cfg</key>
<data>
AwQIAA==
</data>
<key>@0,fboffset</key>
<data>
AAACAA==
</data>
<key>@0,name</key>
<string>NVDA,Display-A</string>
<key>@0,use-backlight-blanking</key>
<string></string>
<key>@1,NVDA,UnderscanMin</key>
<data>
UgAAAA==
</data>
<key>@1,can-hot-plug</key>
<string></string>
<key>@1,compatible</key>
<string>NVDA,NVMac</string>
<key>@1,connector-type</key>
<data>
AAQAAA==
</data>
<key>@1,device_type</key>
<string>display</string>
<key>@1,name</key>
<string>NVDA,Display-B</string>
<key>@2,NVDA,UnderscanMin</key>
<data>
UgAAAA==
</data>
<key>@2,compatible</key>
<string>NVDA,NVMac</string>
<key>@2,connector-type</key>
<data>
AAQAAA==
</data>
<key>@2,device_type</key>
<string>display</string>
<key>@2,name</key>
<string>NVDA,Display-C</string>
<key>@3,NVDA,UnderscanMin</key>
<data>
UgAAAA==
</data>
<key>NVCAP</key>
<data>
BQAAAAAAAQAGAAAAAAAADwAAAAA=
</data>
<key>NVDA,Features</key>
<data>
/xYgAQ==
</data>
<key>NVDA,invalid-config</key>
<data>
AAAAAA==
</data>
<key>VRAM,memvendorID</key>
<data>
AwA=
</data>
<key>VRAM,totalMB</key>
<data>
AAgAAA==
</data>
<key>VRAM,totalsize</key>
<data>
AAAAgAAAAAA=
</data>
<key>boot-gamma-restored</key>
<data>
AAAAAAAAAAA=
</data>
<key>device_type</key>
<string>NVDA,Parent</string>
<key>graphic-options</key>
<data>
DAAAAA==
</data>
<key>model</key>
<string>NVIDIA GeForce GTX 775M</string>
<key>rom-revision</key>
<string>3745</string>
<key>saved-config</key>
<data>
DwhMAyABAABgABAGsAUAAwJ/AAqgBaAKMABQAMkFAwAIAAgAVl4AAAAAAAAB
AAAAAAAAAAAEAAABCgoEAAAAAwAAAAAAAAAKoAUACqAFAAAAfn4AAQAAAAAA
AA8AgAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAQAAAAAAAAAAAAAAAAAA
AAAAAAAAAAAA/wAAAAAAAAAAAAAAAAAAAAIAAAAAAAAPAIAAAAAAAAAAAAAA
AAAAAAAAAAAAAAAAAAAAAAEAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAP8AAAAA
AAAAAAAAAAAAAAA=
</data>
<key>subsystem-id</key>
<data>
IAEAAA==
</data>
<key>vbios-revision</key>
<data>
AQDEBIA=
</data>
</dict>
<key>PciRoot(0x0)/Pci(0x1b,0x0)</key>
<dict>
<key>MaximumBootBeepVolume</key>
<string>M</string>
<key>MaximumBootBeepVolumeAlt</key>
<string>M</string>
<key>PinConfigurations</key>
<data>
AAGmkAABppAAAAAAAAAAAA==
</data>
<key>layout-id</key>
<data>
BwAAAA==
</data>
<key>multiEQDevicePresence</key>
<data>
AAABAA==
</data>
</dict>
<key>PciRoot(0x0)/Pci(0x1c,0x4)/Pci(0x0,0x0)/Pci(0x0,0x0)/Pci(0x0,0x0)</key>
<dict>
<key>TBTDPLowToHigh</key>
<data>
AQAAAA==
</data>
<key>ThunderboltConfig</key>
<data>
AAD//yUAAQAmAAIAJwABABYAAgABAAIA
</data>
<key>ThunderboltDROM</key>
<data>
6QBgnRsNAAEAzHwJbgFlAAEACgABCgiBgAKAAAAACIKQAYAAAAAIg4AEgAEA
AAiEkAOAAQAACIUAAAAAAAADhmADh4ADiKADicAFilAAAAWLUACCBYxQAIQN
AUFwcGxlIEluYy4ADAJNYWNpbnRvc2gA
</data>
<key>ThunderboltUUID</key>
<data>
Di6CEIxndVy6VKSUmGAKCA==
</data>
<key>linkDetails</key>
<data>
CAAAAAMAAAA=
</data>
<key>pathcr</key>
<data>
BAAAAAAAAAAAAAcAEAAQAAUAAAAAAAAAAAAHABAAEAABAAAACwAOAA4AAAAA
AAAAAgAAAAAAAAAAAAQAAgABAAMAAAAAAAAAAAAHAAIAAQA=
</data>
<key>sscOffset</key>
<data>
AAc=
</data>
</dict>
<key>PciRoot(0x0)/Pci(0x2,0x0)</key>
<dict>
<key>AAPL,ig-platform-id</key>
<data>
BAASBA==
</data>
</dict>
</dict>
</plist>

Disk Partition Tables
/dev/disk0

APPLE HDD ST1000DM003 Media | 1.0 TB (1953525168 Blocks * 512 byte sectors) | GUID Partition Table | Disk GUID:0000113e-72f2-0000-230c-000015480000

Start LBA
A
MBR Partition Map
GPT Partition Map
Loader
0
MBR
1
EFI Protective (ee)
Primary GPT Header
2
Primary GPT Table
34
40
EFI system partition (209.71MB)
Apple EFI
409640
Customer (999.34GB)
1952255592
Recovery HD (650.00MB)
1953525128
1953525135
Backup GPT Table
1953525167
Backup GPT Header

LBA 0

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 d238 0000 0000 00fe .........8...... 00001c0: ffff eefe ffff 0100 0000 af6d 7074 0000 ...........mpt.. 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 55aa ..............U.

Details

MBR Windows NT Signature: d2380000 MBR Partition Entry 1: 00feffffeefeffff01000000af6d7074 MBR Partition Entry 2: 00000000000000000000000000000000 MBR Partition Entry 3: 00000000000000000000000000000000 MBR Partition Entry 4: 00000000000000000000000000000000 MBR Signature: aa55 MBR Partition Entry: 00feffffeefeffff01000000af6d7074 ===================================================== MBR Partition Entry Status: 00 (Inactive) MBR Partition Entry Starting CHS: 1023:254:63 MBR Partition Entry Ending CHS: 1023:254:63 MBR Partition Entry Partition Type: ee (EFI Protective) MBR Partition Entry LBA of First Sector: 1 MBR Partition Entry No. Sectors in Partition: 1953525167 MBR Partition Size: 1.00TB

LBA 1

0000000: 4546 4920 5041 5254 0000 0100 5c00 0000 EFI PART....\... 0000010: 709d ced1 0000 0000 0100 0000 0000 0000 p............... 0000020: af6d 7074 0000 0000 2200 0000 0000 0000 .mpt...."....... 0000030: 8e6d 7074 0000 0000 3e11 0000 f272 0000 .mpt....>....r.. 0000040: 230c 0000 1548 0000 0200 0000 0000 0000 #....H.......... 0000050: 8000 0000 8000 0000 8798 e574 0000 0000 ...........t.... 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

Partition Table Revision: 00000100 Header Size: 92 Header Checksum: 709dced1 Middle Reserved Section (Should be zero): Yes Header LBA: 1 Backup LBA: 1953525167 First Logical Block: 34 Last Logical Block: 1953525134 Disk GUID: 0000113e-72f2-0000-230c-000015480000 Partition Array Starting LBA: 2 Partition Array Entries: 128 Partition Array Structure Size: 128 Partition Entry Array Checksum: 8798e574 Ending Reserved Section (Should be zero): Yes

LBA 2

0000000: 2873 2ac1 1ff8 d211 ba4b 00a0 c93e c93b (s*......K...>.; 0000010: 5c76 0000 221b 0000 335c 0000 4810 0000 .."...3\..H... 0000020: 2800 0000 0000 0000 2740 0600 0000 0000 (.......'@...... 0000030: 0000 0000 0000 0000 4500 4600 4900 2000 ........E.F.I. . 0000040: 7300 7900 7300 7400 6500 6d00 2000 7000 s.y.s.t.e.m. .p. 0000050: 6100 7200 7400 6900 7400 6900 6f00 6e00 a.r.t.i.t.i.o.n. 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000090: e03d 0000 8208 0000 8f5b 0000 fd01 0000 .=.......[...... 00000a0: 2840 0600 0000 0000 670e 5d74 0000 0000 (@......g.]t.... 00000b0: 0000 0000 0000 0000 4300 7500 7300 7400 ........C.u.s.t. 00000c0: 6f00 6d00 6500 7200 0000 0000 0000 0000 o.m.e.r......... 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 746f 6f42 0000 aa11 aa11 0030 6543 ecac tooB.......0eC.. 0000110: 65f0 1221 0285 f849 a348 fdeb 8d4f be3a e..!...I.H...O.: 0000120: 680e 5d74 0000 0000 876d 7074 0000 0000 h.]t.....mpt.... 0000130: 0000 0000 0000 0200 5200 6500 6300 6f00 ........R.e.c.o. 0000140: 7600 6500 7200 7900 2000 4800 4400 0000 v.e.r.y. .H.D... 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000200: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000210: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000220: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000230: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000240: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000250: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000260: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000270: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000280: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000290: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000300: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000310: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000320: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000330: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000340: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000350: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000360: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000370: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000380: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000390: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

Array Length:16384 bytes Array Block Count (512 bytes):32 ===================================================== Partition Type GUID: EFI System Partition Partition Unique GUID: 0000765c-1b22-0000-335c-000048100000 Partition Starting LBA: 40 Partition Ending LBA: 409639 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: EFI system partition Partition Reserved Byte: OK Partition Size: 209.71MB Partition Loader: Apple EFI ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 00003de0-0882-0000-8f5b-0000fd010000 Partition Starting LBA: 409640 Partition Ending LBA: 1952255591 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: Customer Partition Reserved Byte: OK Partition Size: 999.34GB ===================================================== Partition Type GUID: OSX Boot Partition Unique GUID: 2112f065-8502-49f8-a348-fdeb8d4fbe3a Partition Starting LBA: 1952255592 Partition Ending LBA: 1953525127 Partition UEFI Reserved Attributes: 0000000000000200 Partition Name: Recovery HD Partition Reserved Byte: OK Partition Size: 650.00MB

LBA 40

0000000: eb58 9042 5344 2020 342e 3400 0201 2000 .X.BSD 4.4... . 0000010: 0200 0000 00f0 0000 3f00 ff00 2800 0000 ........?...(... 0000020: 0040 0600 670c 0000 0000 0000 0200 0000 .@..g........... 0000030: 0100 0600 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 29f4 1160 2845 4649 2020 2020 2020 ..)..`(EFI 0000050: 2020 4641 5433 3220 2020 fa31 c08e d0bc FAT32 .1.... 0000060: 007c fb8e d8e8 0000 5e83 c619 bb07 00fc .|......^....... 0000070: ac84 c074 06b4 0ecd 10eb f530 e4cd 16cd ...t.......0.... 0000080: 190d 0a4e 6f6e 2d73 7973 7465 6d20 6469 ...Non-system di 0000090: 736b 0d0a 5072 6573 7320 616e 7920 6b65 sk..Press any ke 00000a0: 7920 746f 2072 6562 6f6f 740d 0a00 0000 y to reboot..... 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 55aa ..............U.

Details

LBA 409640

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 1952255592

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 1953525135

0000000: 2873 2ac1 1ff8 d211 ba4b 00a0 c93e c93b (s*......K...>.; 0000010: 5c76 0000 221b 0000 335c 0000 4810 0000 .."...3\..H... 0000020: 2800 0000 0000 0000 2740 0600 0000 0000 (.......'@...... 0000030: 0000 0000 0000 0000 4500 4600 4900 2000 ........E.F.I. . 0000040: 7300 7900 7300 7400 6500 6d00 2000 7000 s.y.s.t.e.m. .p. 0000050: 6100 7200 7400 6900 7400 6900 6f00 6e00 a.r.t.i.t.i.o.n. 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000090: e03d 0000 8208 0000 8f5b 0000 fd01 0000 .=.......[...... 00000a0: 2840 0600 0000 0000 670e 5d74 0000 0000 (@......g.]t.... 00000b0: 0000 0000 0000 0000 4300 7500 7300 7400 ........C.u.s.t. 00000c0: 6f00 6d00 6500 7200 0000 0000 0000 0000 o.m.e.r......... 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 746f 6f42 0000 aa11 aa11 0030 6543 ecac tooB.......0eC.. 0000110: 65f0 1221 0285 f849 a348 fdeb 8d4f be3a e..!...I.H...O.: 0000120: 680e 5d74 0000 0000 876d 7074 0000 0000 h.]t.....mpt.... 0000130: 0000 0000 0000 0200 5200 6500 6300 6f00 ........R.e.c.o. 0000140: 7600 6500 7200 7900 2000 4800 4400 0000 v.e.r.y. .H.D... 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000200: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000210: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000220: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000230: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000240: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000250: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000260: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000270: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000280: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000290: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000300: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000310: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000320: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000330: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000340: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000350: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000360: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000370: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000380: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000390: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

Array Length:16384 bytes Array Block Count (512 bytes):32 ===================================================== Partition Type GUID: EFI System Partition Partition Unique GUID: 0000765c-1b22-0000-335c-000048100000 Partition Starting LBA: 40 Partition Ending LBA: 409639 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: EFI system partition Partition Reserved Byte: OK Partition Size: 209.71MB Partition Loader: Apple EFI ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 00003de0-0882-0000-8f5b-0000fd010000 Partition Starting LBA: 409640 Partition Ending LBA: 1952255591 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: Customer Partition Reserved Byte: OK Partition Size: 999.34GB ===================================================== Partition Type GUID: OSX Boot Partition Unique GUID: 2112f065-8502-49f8-a348-fdeb8d4fbe3a Partition Starting LBA: 1952255592 Partition Ending LBA: 1953525127 Partition UEFI Reserved Attributes: 0000000000000200 Partition Name: Recovery HD Partition Reserved Byte: OK Partition Size: 650.00MB

LBA 1953525167

0000000: 4546 4920 5041 5254 0000 0100 5c00 0000 EFI PART....\... 0000010: 9225 5372 0000 0000 af6d 7074 0000 0000 .%Sr.....mpt.... 0000020: 0100 0000 0000 0000 2200 0000 0000 0000 ........"....... 0000030: 8e6d 7074 0000 0000 3e11 0000 f272 0000 .mpt....>....r.. 0000040: 230c 0000 1548 0000 8f6d 7074 0000 0000 #....H...mpt.... 0000050: 8000 0000 8000 0000 8798 e574 0000 0000 ...........t.... 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

Partition Table Revision: 00000100 Header Size: 92 Header Checksum: 92255372 Middle Reserved Section (Should be zero): Yes Header LBA: 1953525167 Backup LBA: 1 First Logical Block: 34 Last Logical Block: 1953525134 Disk GUID: 0000113e-72f2-0000-230c-000015480000 Partition Array Starting LBA: 1953525135 Partition Array Entries: 128 Partition Array Structure Size: 128 Partition Entry Array Checksum: 8798e574 Ending Reserved Section (Should be zero): Yes
/dev/disk1

WD My Passport 0812 Media | 500.1 GB (976707584 Blocks * 512 byte sectors) | GUID Partition Table | Disk GUID:2f85c6b6-a660-4080-9f7e-598ae3dced6a

Start LBA
A
MBR Partition Map
GPT Partition Map
Loader
0
MBR
1
EFI Protective (ee)
Primary GPT Header
2
Primary GPT Table
34
40
EFI System Partition (209.71MB)
Apple EFI
409640
10.6.8 (10.00GB)
19940896
20203040
10.7.5 (10.00GB)
39734296
39996440
10.8.5 (10.00GB)
59527696
59789840
10.9.3 (10.00GB)
79321096
79583240
10.10 (10.00GB)
99114496
99376640
TestBoot (27.78GB)
153647528
153909672
Soft (149.99GB)
446878416
447140560
DataDisk (135.50GB)
711792976
712056832
11111 (135.50GB)
Windows NTFS NTLDR
976705536
976707551
Backup GPT Table
976707583
Backup GPT Header

LBA 0

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 00fe ................ 00001c0: ffff eefe ffff 0100 0000 ff5f 373a 0000 ..........._7:.. 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 55aa ..............U.

Details

MBR Windows NT Signature: 00000000 MBR Partition Entry 1: 00feffffeefeffff01000000ff5f373a MBR Partition Entry 2: 00000000000000000000000000000000 MBR Partition Entry 3: 00000000000000000000000000000000 MBR Partition Entry 4: 00000000000000000000000000000000 MBR Signature: aa55 MBR Partition Entry: 00feffffeefeffff01000000ff5f373a ===================================================== MBR Partition Entry Status: 00 (Inactive) MBR Partition Entry Starting CHS: 1023:254:63 MBR Partition Entry Ending CHS: 1023:254:63 MBR Partition Entry Partition Type: ee (EFI Protective) MBR Partition Entry LBA of First Sector: 1 MBR Partition Entry No. Sectors in Partition: 976707583 MBR Partition Size: 500.07GB

LBA 1

0000000: 4546 4920 5041 5254 0000 0100 5c00 0000 EFI PART....\... 0000010: af04 cc91 0000 0000 0100 0000 0000 0000 ................ 0000020: ff5f 373a 0000 0000 2200 0000 0000 0000 ._7:...."....... 0000030: de5f 373a 0000 0000 b6c6 852f 60a6 8040 ._7:.......\`..@ 0000040: 9f7e 598a e3dc ed6a 0200 0000 0000 0000 .~Y....j........ 0000050: 8000 0000 8000 0000 2e3c 5a8a 0000 0000 ......... 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

Partition Table Revision: 00000100 Header Size: 92 Header Checksum: af04cc91 Middle Reserved Section (Should be zero): Yes Header LBA: 1 Backup LBA: 976707583 First Logical Block: 34 Last Logical Block: 976707550 Disk GUID: 2f85c6b6-a660-4080-9f7e-598ae3dced6a Partition Array Starting LBA: 2 Partition Array Entries: 128 Partition Array Structure Size: 128 Partition Entry Array Checksum: 2e3c5a8a Ending Reserved Section (Should be zero): Yes

LBA 2

0000000: 2873 2ac1 1ff8 d211 ba4b 00a0 c93e c93b (s*......K...>.; 0000010: 74f5 d314 4ea4 d14d 8b5c 5435 d901 f1d4 t...N..M.\T5.... 0000020: 2800 0000 0000 0000 2740 0600 0000 0000 (.......'@...... 0000030: 0000 0000 0000 0000 4500 4600 4900 2000 ........E.F.I. . 0000040: 5300 7900 7300 7400 6500 6d00 2000 5000 S.y.s.t.e.m. .P. 0000050: 6100 7200 7400 6900 7400 6900 6f00 6e00 a.r.t.i.t.i.o.n. 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000090: e8cb 7b27 608f d848 82c8 72f4 52e9 37ba ..{'`..H..r.R.7. 00000a0: 2840 0600 0000 0000 1f46 3001 0000 0000 (@.......F0..... 00000b0: 0000 0000 0000 0000 3100 3000 2e00 3600 ........1.0...6. 00000c0: 2e00 3800 0000 0000 0000 0000 0000 0000 ..8............. 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000110: 51ab 1a98 16d3 a34e b8f2 0ea2 e0ff 9808 Q......N........ 0000120: 2046 3401 0000 0000 174c 5e02 0000 0000 F4......L^..... 0000130: 0000 0000 0000 0000 3100 3000 2e00 3700 ........1.0...7. 0000140: 2e00 3500 0000 0000 0000 0000 0000 0000 ..5............. 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000190: 9094 7dfb 024d 7e4e 9265 5b3a 9d23 922c ..}..M~N.e[:.#., 00001a0: 184c 6202 0000 0000 0f52 8c03 0000 0000 .Lb......R...... 00001b0: 0000 0000 0000 0000 3100 3000 2e00 3800 ........1.0...8. 00001c0: 2e00 3500 0000 0000 0000 0000 0000 0000 ..5............. 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000200: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000210: ea92 d387 a085 854b 9279 b1cc 2a72 2229 .......K.y..*r") 0000220: 1052 9003 0000 0000 0758 ba04 0000 0000 .R.......X...... 0000230: 0000 0000 0000 0000 3100 3000 2e00 3900 ........1.0...9. 0000240: 2e00 3300 0000 0000 0000 0000 0000 0000 ..3............. 0000250: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000260: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000270: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000280: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000290: 65a4 637e 6b59 2849 922a 3902 aab6 a775 e.c~kY(I.*9....u 00002a0: 0858 be04 0000 0000 ff5d e805 0000 0000 .X.......]...... 00002b0: 0000 0000 0000 0000 3100 3000 2e00 3100 ........1.0...1. 00002c0: 3000 0000 0000 0000 0000 0000 0000 0000 0............... 00002d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000300: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000310: cb6c 3e9a 0247 5845 a1c1 4c62 177d b15d .l>..GXE..Lb.}.] 0000320: 005e ec05 0000 0000 a779 2809 0000 0000 .^.......y(..... 0000330: 0000 0000 0000 0000 5400 6500 7300 7400 ........T.e.s.t. 0000340: 4200 6f00 6f00 7400 0000 0000 0000 0000 B.o.o.t......... 0000350: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000360: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000370: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000380: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000390: fd1a ac56 8a5d 9145 a969 4b47 edf1 cdd1 ...V.].E.iKG.... 00003a0: a879 2c09 0000 0000 cfd2 a21a 0000 0000 .y,............. 00003b0: 0000 0000 0000 0000 5300 6f00 6600 7400 ........S.o.f.t. 00003c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

Array Length:16384 bytes Array Block Count (512 bytes):32 ===================================================== Partition Type GUID: EFI System Partition Partition Unique GUID: 14d3f574-a44e-4dd1-8b5c-5435d901f1d4 Partition Starting LBA: 40 Partition Ending LBA: 409639 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: EFI System Partition Partition Reserved Byte: OK Partition Size: 209.71MB Partition Loader: Apple EFI ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 277bcbe8-8f60-48d8-82c8-72f452e937ba Partition Starting LBA: 409640 Partition Ending LBA: 19940895 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.6.8 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 981aab51-d316-4ea3-b8f2-0ea2e0ff9808 Partition Starting LBA: 20203040 Partition Ending LBA: 39734295 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.7.5 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: fb7d9490-4d02-4e7e-9265-5b3a9d23922c Partition Starting LBA: 39996440 Partition Ending LBA: 59527695 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.8.5 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 87d392ea-85a0-4b85-9279-b1cc2a722229 Partition Starting LBA: 59789840 Partition Ending LBA: 79321095 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.9.3 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 7e63a465-596b-4928-922a-3902aab6a775 Partition Starting LBA: 79583240 Partition Ending LBA: 99114495 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.10 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 9a3e6ccb-4702-4558-a1c1-4c62177db15d Partition Starting LBA: 99376640 Partition Ending LBA: 153647527 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: TestBoot Partition Reserved Byte: OK Partition Size: 27.78GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 56ac1afd-5d8a-4591-a969-4b47edf1cdd1 Partition Starting LBA: 153909672 Partition Ending LBA: 446878415 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: Soft Partition Reserved Byte: OK Partition Size: 149.99GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: e7a5a3d0-be08-4412-9906-9f227f07d61d Partition Starting LBA: 447140560 Partition Ending LBA: 711792975 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: DataDisk Partition Reserved Byte: OK Partition Size: 135.50GB ===================================================== Partition Type GUID: Windows Basic Data Partition Unique GUID: 4e86257e-01df-4b8a-b212-9adf6670a3ed Partition Starting LBA: 712056832 Partition Ending LBA: 976705535 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 11111 Partition Reserved Byte: OK Partition Size: 135.50GB Partition Loader: Windows NTFS NTLDR

LBA 40

0000000: eb58 9042 5344 2020 342e 3400 0201 2000 .X.BSD 4.4... . 0000010: 0200 0000 00f0 0000 2000 1000 0000 0000 ........ ....... 0000020: 0040 0600 4f0c 0000 0000 0000 0200 0000 .@..O........... 0000030: 0100 0600 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 29ed 17e3 6745 4649 2020 2020 2020 ..)...gEFI 0000050: 2020 4641 5433 3220 2020 fa31 c08e d0bc FAT32 .1.... 0000060: 007c fb8e d8e8 0000 5e83 c619 bb07 00fc .|......^....... 0000070: ac84 c074 06b4 0ecd 10eb f530 e4cd 16cd ...t.......0.... 0000080: 190d 0a4e 6f6e 2d73 7973 7465 6d20 6469 ...Non-system di 0000090: 736b 0d0a 5072 6573 7320 616e 7920 6b65 sk..Press any ke 00000a0: 7920 746f 2072 6562 6f6f 740d 0a00 0000 y to reboot..... 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 55aa ..............U.

Details

LBA 409640

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 20203040

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 39996440

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 59789840

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 79583240

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 99376640

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 153909672

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 447140560

0000000: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000010: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000030: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000040: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000050: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

LBA 712056832

0000000: eb52 904e 5446 5320 2020 2000 0208 0000 .R.NTFS ..... 0000010: 0000 0000 00f8 0000 0000 0000 0000 0000 ................ 0000020: 0000 0000 8000 8000 ff37 c60f 0000 0000 .........7...... 0000030: 0400 0000 0000 0000 7f63 fc00 0000 0000 .........c...... 0000040: f600 0000 0100 0000 9479 1330 dd81 1742 .........y.0...B 0000050: 0000 0000 fa33 c08e d0bc 007c fb68 c007 .....3.....|.h.. 0000060: 1f1e 6866 00cb 8816 0e00 6681 3e03 004e ..hf......f.>..N 0000070: 5446 5375 15b4 41bb aa55 cd13 720c 81fb TFSu..A..U..r... 0000080: 55aa 7506 f7c1 0100 7503 e9d2 001e 83ec U.u.....u....... 0000090: 1868 1a00 b448 8a16 0e00 8bf4 161f cd13 .h...H.......... 00000a0: 9f83 c418 9e58 1f72 e13b 060b 0075 dba3 .....X.r.;...u.. 00000b0: 0f00 c12e 0f00 041e 5a33 dbb9 0020 2bc8 ........Z3... +. 00000c0: 66ff 0611 0003 160f 008e c2ff 0616 00e8 f............... 00000d0: 4000 2bc8 77ef b800 bbcd 1a66 23c0 752d @.+.w......f#.u- 00000e0: 6681 fb54 4350 4175 2481 f902 0172 1e16 f..TCPAu$....r.. 00000f0: 6807 bb16 6870 0e16 6809 0066 5366 5366 h...hp..h..fSfSf 0000100: 5516 1616 68b8 0166 610e 07cd 1ae9 6a01 U...h..fa.....j. 0000110: 9090 6660 1e06 66a1 1100 6603 061c 001e ..f`..f...f..... 0000120: 6668 0000 0000 6650 0653 6801 0068 1000 fh....fP.Sh..h.. 0000130: b442 8a16 0e00 161f 8bf4 cd13 6659 5b5a .B..........fY[Z 0000140: 6659 6659 1f0f 8216 0066 ff06 1100 0316 fYfY.....f...... 0000150: 0f00 8ec2 ff0e 1600 75bc 071f 6661 c3a0 ........u...fa.. 0000160: f801 e808 00a0 fb01 e802 00eb feb4 018b ................ 0000170: f0ac 3c00 7409 b40e bb07 00cd 10eb f2c3 ..<.t........... 0000180: 0d0a 4120 6469 736b 2072 6561 6420 6572 ..A disk read er 0000190: 726f 7220 6f63 6375 7272 6564 000d 0a42 ror occurred...B 00001a0: 4f4f 544d 4752 2069 7320 6d69 7373 696e OOTMGR is missin 00001b0: 6700 0d0a 424f 4f54 4d47 5220 6973 2063 g...BOOTMGR is c 00001c0: 6f6d 7072 6573 7365 6400 0d0a 5072 6573 ompressed...Pres 00001d0: 7320 4374 726c 2b41 6c74 2b44 656c 2074 s Ctrl+Alt+Del t 00001e0: 6f20 7265 7374 6172 740d 0a00 0000 0000 o restart....... 00001f0: 0000 0000 0000 0000 809d b2ca 0000 55aa ..............U.

Details

LBA 976707551

0000000: 2873 2ac1 1ff8 d211 ba4b 00a0 c93e c93b (s*......K...>.; 0000010: 74f5 d314 4ea4 d14d 8b5c 5435 d901 f1d4 t...N..M.\T5.... 0000020: 2800 0000 0000 0000 2740 0600 0000 0000 (.......'@...... 0000030: 0000 0000 0000 0000 4500 4600 4900 2000 ........E.F.I. . 0000040: 5300 7900 7300 7400 6500 6d00 2000 5000 S.y.s.t.e.m. .P. 0000050: 6100 7200 7400 6900 7400 6900 6f00 6e00 a.r.t.i.t.i.o.n. 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000090: e8cb 7b27 608f d848 82c8 72f4 52e9 37ba ..{'`..H..r.R.7. 00000a0: 2840 0600 0000 0000 1f46 3001 0000 0000 (@.......F0..... 00000b0: 0000 0000 0000 0000 3100 3000 2e00 3600 ........1.0...6. 00000c0: 2e00 3800 0000 0000 0000 0000 0000 0000 ..8............. 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000110: 51ab 1a98 16d3 a34e b8f2 0ea2 e0ff 9808 Q......N........ 0000120: 2046 3401 0000 0000 174c 5e02 0000 0000 F4......L^..... 0000130: 0000 0000 0000 0000 3100 3000 2e00 3700 ........1.0...7. 0000140: 2e00 3500 0000 0000 0000 0000 0000 0000 ..5............. 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000190: 9094 7dfb 024d 7e4e 9265 5b3a 9d23 922c ..}..M~N.e[:.#., 00001a0: 184c 6202 0000 0000 0f52 8c03 0000 0000 .Lb......R...... 00001b0: 0000 0000 0000 0000 3100 3000 2e00 3800 ........1.0...8. 00001c0: 2e00 3500 0000 0000 0000 0000 0000 0000 ..5............. 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000200: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000210: ea92 d387 a085 854b 9279 b1cc 2a72 2229 .......K.y..*r") 0000220: 1052 9003 0000 0000 0758 ba04 0000 0000 .R.......X...... 0000230: 0000 0000 0000 0000 3100 3000 2e00 3900 ........1.0...9. 0000240: 2e00 3300 0000 0000 0000 0000 0000 0000 ..3............. 0000250: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000260: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000270: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000280: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000290: 65a4 637e 6b59 2849 922a 3902 aab6 a775 e.c~kY(I.*9....u 00002a0: 0858 be04 0000 0000 ff5d e805 0000 0000 .X.......]...... 00002b0: 0000 0000 0000 0000 3100 3000 2e00 3100 ........1.0...1. 00002c0: 3000 0000 0000 0000 0000 0000 0000 0000 0............... 00002d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00002f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000300: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000310: cb6c 3e9a 0247 5845 a1c1 4c62 177d b15d .l>..GXE..Lb.}.] 0000320: 005e ec05 0000 0000 a779 2809 0000 0000 .^.......y(..... 0000330: 0000 0000 0000 0000 5400 6500 7300 7400 ........T.e.s.t. 0000340: 4200 6f00 6f00 7400 0000 0000 0000 0000 B.o.o.t......... 0000350: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000360: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000370: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000380: 0053 4648 0000 aa11 aa11 0030 6543 ecac .SFH.......0eC.. 0000390: fd1a ac56 8a5d 9145 a969 4b47 edf1 cdd1 ...V.].E.iKG.... 00003a0: a879 2c09 0000 0000 cfd2 a21a 0000 0000 .y,............. 00003b0: 0000 0000 0000 0000 5300 6f00 6600 7400 ........S.o.f.t. 00003c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00003f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

Array Length:16384 bytes Array Block Count (512 bytes):32 ===================================================== Partition Type GUID: EFI System Partition Partition Unique GUID: 14d3f574-a44e-4dd1-8b5c-5435d901f1d4 Partition Starting LBA: 40 Partition Ending LBA: 409639 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: EFI System Partition Partition Reserved Byte: OK Partition Size: 209.71MB Partition Loader: Apple EFI ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 277bcbe8-8f60-48d8-82c8-72f452e937ba Partition Starting LBA: 409640 Partition Ending LBA: 19940895 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.6.8 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 981aab51-d316-4ea3-b8f2-0ea2e0ff9808 Partition Starting LBA: 20203040 Partition Ending LBA: 39734295 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.7.5 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: fb7d9490-4d02-4e7e-9265-5b3a9d23922c Partition Starting LBA: 39996440 Partition Ending LBA: 59527695 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.8.5 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 87d392ea-85a0-4b85-9279-b1cc2a722229 Partition Starting LBA: 59789840 Partition Ending LBA: 79321095 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.9.3 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 7e63a465-596b-4928-922a-3902aab6a775 Partition Starting LBA: 79583240 Partition Ending LBA: 99114495 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 10.10 Partition Reserved Byte: OK Partition Size: 10.00GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 9a3e6ccb-4702-4558-a1c1-4c62177db15d Partition Starting LBA: 99376640 Partition Ending LBA: 153647527 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: TestBoot Partition Reserved Byte: OK Partition Size: 27.78GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: 56ac1afd-5d8a-4591-a969-4b47edf1cdd1 Partition Starting LBA: 153909672 Partition Ending LBA: 446878415 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: Soft Partition Reserved Byte: OK Partition Size: 149.99GB ===================================================== Partition Type GUID: HFS+ Partition Unique GUID: e7a5a3d0-be08-4412-9906-9f227f07d61d Partition Starting LBA: 447140560 Partition Ending LBA: 711792975 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: DataDisk Partition Reserved Byte: OK Partition Size: 135.50GB ===================================================== Partition Type GUID: Windows Basic Data Partition Unique GUID: 4e86257e-01df-4b8a-b212-9adf6670a3ed Partition Starting LBA: 712056832 Partition Ending LBA: 976705535 Partition UEFI Reserved Attributes: 0000000000000000 Partition Name: 11111 Partition Reserved Byte: OK Partition Size: 135.50GB Partition Loader: Windows NTFS NTLDR

LBA 976707583

0000000: 4546 4920 5041 5254 0000 0100 5c00 0000 EFI PART....\... 0000010: a589 9fc0 0000 0000 ff5f 373a 0000 0000 ........._7:.... 0000020: 0100 0000 0000 0000 2200 0000 0000 0000 ........"....... 0000030: de5f 373a 0000 0000 b6c6 852f 60a6 8040 ._7:.......\`..@ 0000040: 9f7e 598a e3dc ed6a df5f 373a 0000 0000 .~Y....j._7:.... 0000050: 8000 0000 8000 0000 2e3c 5a8a 0000 0000 ......... 0000060: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000070: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000080: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000090: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00000f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000100: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000110: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000120: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000130: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000140: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000150: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000160: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000170: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000180: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 0000190: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001a0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001b0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001c0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001d0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001e0: 0000 0000 0000 0000 0000 0000 0000 0000 ................ 00001f0: 0000 0000 0000 0000 0000 0000 0000 0000 ................

Details

Partition Table Revision: 00000100 Header Size: 92 Header Checksum: a5899fc0 Middle Reserved Section (Should be zero): Yes Header LBA: 976707583 Backup LBA: 1 First Logical Block: 34 Last Logical Block: 976707550 Disk GUID: 2f85c6b6-a660-4080-9f7e-598ae3dced6a Partition Array Starting LBA: 976707551 Partition Array Entries: 128 Partition Array Structure Size: 128 Partition Entry Array Checksum: 2e3c5a8a Ending Reserved Section (Should be zero): Yes
Disk & Volume UIDs
UUID's grabbed from diskutil info. Unique partition GUID's dumped from IOreg.

View UIDs.txt File

Device Name Volume UUID Unique partition GUID
disk0s1 /Volumes/EFI 0000765C-1B22-0000-335C-000048100000
disk0s2 /Volumes/Macintosh HD 0A72ACE6-3CA9-3689-92AB-46C63CC23C2E 00003DE0-0882-0000-8F5B-0000FD010000
disk0s3 /Volumes/Recovery HD 2E51F042-B45C-3F34-A887-BB8C024A12C1 2112F065-8502-49F8-A348-FDEB8D4FBE3A
disk1s1 /Volumes/EFI 14D3F574-A44E-4DD1-8B5C-5435D901F1D4
4E86257E-01DF-4B8A-B212-9ADF6670A3ED
disk1s2 /Volumes/OS X Snow Leopard Install Disk - 10.6.8 D9A569A2-4FEE-3DFD-8353-4D1595DDA64D 277BCBE8-8F60-48D8-82C8-72F452E937BA
disk1s3 /Volumes/OS X Lion Install Disk - 10.7.5 9F0ED271-9AB1-3A65-9BC6-A6D223414DCC 981AAB51-D316-4EA3-B8F2-0EA2E0FF9808
disk1s4 /Volumes/OS X Mountain Lion Install Disk - 10.8.5 B2B5E8ED-0B33-330C-A8D8-B271E7024B83 FB7D9490-4D02-4E7E-9265-5B3A9D23922C
disk1s5 /Volumes/OS X 10.9 Install Disk - 10.9.3 7197C1D7-0716-3A13-9CCB-D3D9111EC57F 87D392EA-85A0-4B85-9279-B1CC2A722229
disk1s6 /Volumes/OS X Install Disk - 10.10 244C6EAD-ACFB-3FE2-8810-8ECDDF728801 7E63A465-596B-4928-922A-3902AAB6A775
disk1s7 /Volumes/BootTest E2D015A7-BF58-3D07-AAE0-6595252DB26B 9A3E6CCB-4702-4558-A1C1-4C62177DB15D
disk1s8 /Volumes/SoftDisk 1523B934-0C60-358A-80A3-76F5737F3083 56AC1AFD-5D8A-4591-A969-4B47EDF1CDD1
disk1s9 /Volumes/DataDisk 8F3A3E46-17F4-3124-B994-0A95E73DD0D5 E7A5A3D0-BE08-4412-9906-9F227F07D61D
disk1s10 /Volumes/11111 4E86257E-01DF-4B8A-B212-9ADF6670A3ED

EDID
Dumped IODisplayEDID from ioreg and decoded using edid-decode by Adam Jackson.

View EDID.txt File

Extracted contents:
header: 00 ff ff ff ff ff ff 00
serial number: 06 10 05 b0 00 00 00 00 1c 16
version: 01 04
basic params: b5 3c 22 78 22
chroma info: 6f b1 a7 55 4c 9e 25 0c 50 54
established: 00 00 00
standard: 01 01 01 01 01 01 01 01 01 01 01 01 01 01 01 01
descriptor 1: 56 5e 00 a0 a0 a0 29 50 30 20 35 00 55 50 21 00 00 1a
descriptor 2: 1a 1d 00 80 51 d0 1c 20 40 80 35 00 55 50 21 00 00 1c
descriptor 3: 00 00 00 fc 00 69 4d 61 63 0a 20 20 20 20 20 20 20 20
descriptor 4: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
extensions: 01
checksum: 8e
Manufacturer: APP Model b005 Serial Number 0
Made week 28 of 2012
EDID version: 1.4
Digital display
10 bits per primary color channel
DisplayPort interface
Maximum image size: 60 cm x 34 cm
Gamma: 2.20
DPMS levels: Off
Supported color formats: RGB 4:4:4
First detailed timing is preferred timing
Established timings supported:
Standard timings supported:
Detailed mode: Clock 241.500 MHz, 597 mm x 336 mm
2560 2608 2640 2720 hborder 0
1440 1443 1448 1481 vborder 0
+hsync -vsync
Detailed mode: Clock 74.500 MHz, 597 mm x 336 mm
1280 1344 1472 1664 hborder 0
720 723 728 748 vborder 0
-hsync +vsync
Monitor name: iMac
Manufacturer-specified data, tag 0
Has 1 extension blocks
Checksum: 0x8e (valid)
CEA extension block
Extension version: 3
36 bytes of CEA data
Audio data block
Linear PCM, max channels 1
Supported sample rates (kHz): 48 44.1 32
Supported sample sizes (bits): 24 20 16
Speaker allocation data block
Vendor-specific data block, OUI 0010fa
Vendor-specific data block, OUI 0010fa
Underscans PC formats by default
Basic audio support
1 native detailed modes
Detailed mode: Clock 241.500 MHz, 597 mm x 336 mm
2560 2608 2640 2720 hborder 0
1440 1443 1448 1481 vborder 0
+hsync -vsync
Detailed mode: Clock 74.500 MHz, 597 mm x 336 mm
1280 1344 1472 1664 hborder 0
720 723 728 748 vborder 0
-hsync +vsync
Checksum: 0xcc (valid)
EDID block does NOT conform to EDID 1.3!
Missing monitor ranges

Firmware Memory Map
Script: FirmwareMemoryMap (formerly showbootermemorymap) by Amit Singh. Revised by bcc9, then by dmazar.

View FirmwareMemoryMap.txt File

BootArgs: Version=2, Revision=0, at 0xffffff800a062000
CommandLine:
Video: baseAddr=0x90020000, display=1, rowBytes=16384, width=2560, height=1440, depth=32
DevTree: addr=0xa067000, length=0x1a6c
Kernel image: kaddr=0x7500000, ksize=0x2c26000
EFI Runtime: Mode=64, PageStart=0xa069 (0xa069000), PageCount=0xba, SystemTable=0xa0bee10
MemoryMap: Size=0x2550, DescriptorSize=48, DescriptorVersion=1
Type Physical Start - Physical End Number of Pages Virtual Start Attribute
available 0000000000000000 - 0000000000057fff 0000000000000058 0000000000000000 080000000000000f
reserved 0000000000058000 - 0000000000058fff 0000000000000001 0000000000000000 080000000000000f
available 0000000000059000 - 000000000008efff 0000000000000036 0000000000000000 080000000000000f
reserved 000000000008f000 - 000000000008ffff 0000000000000001 0000000000000000 080000000000000f
available 0000000000090000 - 000000000009ffff 0000000000000010 0000000000000000 080000000000000f
reserved 00000000000a0000 - 00000000000bffff 0000000000000020 0000000000000000 0000000000000000
available 0000000000100000 - 00000000074fffff 0000000000007400 0000000000000000 000000000000000f
LoaderData 0000000007500000 - 0000000007512fff 0000000000000013 0000000000000000 000000000000000f
available 0000000007513000 - 00000000075fffff 00000000000000ed 0000000000000000 000000000000000f
LoaderData 0000000007600000 - 0000000007ba8fff 00000000000005a9 0000000000000000 000000000000000f
available 0000000007ba9000 - 0000000007bfffff 0000000000000057 0000000000000000 000000000000000f
LoaderData 0000000007c00000 - 000000000a068fff 0000000000002469 0000000000000000 000000000000000f
RT_data 000000000a069000 - 000000000a0befff 0000000000000056 ffffff800a069000 800000000000000f
RT_code 000000000a0bf000 - 000000000a0ecfff 000000000000002e ffffff800a0bf000 800000000000000f
LoaderData 000000000a0ed000 - 000000000a125fff 0000000000000039 0000000000000000 000000000000000f
available 000000000a126000 - 0000000089655fff 000000000007f530 0000000000000000 000000000000000f
LoaderCode 0000000089656000 - 00000000896d2fff 000000000000007d 0000000000000000 000000000000000f
available 00000000896d3000 - 00000000896edfff 000000000000001b 0000000000000000 000000000000000f
BS_data 00000000896ee000 - 00000000896effff 0000000000000002 0000000000000000 000000000000000f
available 00000000896f0000 - 00000000896f1fff 0000000000000002 0000000000000000 000000000000000f
BS_data 00000000896f2000 - 0000000089742fff 0000000000000051 0000000000000000 000000000000000f
LoaderCode 0000000089743000 - 0000000089743fff 0000000000000001 0000000000000000 000000000000000f
BS_data 0000000089744000 - 0000000089745fff 0000000000000002 0000000000000000 000000000000000f
available 0000000089746000 - 0000000089747fff 0000000000000002 0000000000000000 000000000000000f
BS_data 0000000089748000 - 0000000089749fff 0000000000000002 0000000000000000 000000000000000f
available 000000008974a000 - 000000008974bfff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008974c000 - 000000008b400fff 0000000000001cb5 0000000000000000 000000000000000f
BS_code 000000008b401000 - 000000008b411fff 0000000000000011 0000000000000000 000000000000000f
BS_data 000000008b412000 - 000000008b428fff 0000000000000017 0000000000000000 000000000000000f
BS_code 000000008b429000 - 000000008b42afff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b42b000 - 000000008b42cfff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b42d000 - 000000008b42efff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b42f000 - 000000008b435fff 0000000000000007 0000000000000000 000000000000000f
BS_code 000000008b436000 - 000000008b437fff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b438000 - 000000008b43afff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b43b000 - 000000008b442fff 0000000000000008 0000000000000000 000000000000000f
BS_data 000000008b443000 - 000000008b444fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b445000 - 000000008b445fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b446000 - 000000008b448fff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b449000 - 000000008b44ffff 0000000000000007 0000000000000000 000000000000000f
BS_data 000000008b450000 - 000000008b456fff 0000000000000007 0000000000000000 000000000000000f
BS_code 000000008b457000 - 000000008b45bfff 0000000000000005 0000000000000000 000000000000000f
BS_data 000000008b45c000 - 000000008b473fff 0000000000000018 0000000000000000 000000000000000f
BS_code 000000008b474000 - 000000008b477fff 0000000000000004 0000000000000000 000000000000000f
BS_data 000000008b478000 - 000000008b47bfff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008b47c000 - 000000008b486fff 000000000000000b 0000000000000000 000000000000000f
BS_data 000000008b487000 - 000000008b488fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b489000 - 000000008b489fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b48a000 - 000000008b48cfff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b48d000 - 000000008b48dfff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b48e000 - 000000008b491fff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008b492000 - 000000008b493fff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b494000 - 000000008b4d6fff 0000000000000043 0000000000000000 000000000000000f
BS_code 000000008b4d7000 - 000000008b4dffff 0000000000000009 0000000000000000 000000000000000f
BS_data 000000008b4e0000 - 000000008b4e3fff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008b4e4000 - 000000008b4e6fff 0000000000000003 0000000000000000 000000000000000f
BS_data 000000008b4e7000 - 000000008b521fff 000000000000003b 0000000000000000 000000000000000f
BS_code 000000008b522000 - 000000008b55afff 0000000000000039 0000000000000000 000000000000000f
BS_data 000000008b55b000 - 000000008b565fff 000000000000000b 0000000000000000 000000000000000f
BS_code 000000008b717000 - 000000008b717fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b718000 - 000000008b71afff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b71b000 - 000000008b71cfff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b71d000 - 000000008b722fff 0000000000000006 0000000000000000 000000000000000f
BS_code 000000008b723000 - 000000008b723fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b724000 - 000000008b724fff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b725000 - 000000008b725fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b726000 - 000000008b726fff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b727000 - 000000008b727fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b728000 - 000000008b739fff 0000000000000012 0000000000000000 000000000000000f
BS_code 000000008b73a000 - 000000008b747fff 000000000000000e 0000000000000000 000000000000000f
BS_data 000000008b748000 - 000000008b75bfff 0000000000000014 0000000000000000 000000000000000f
BS_code 000000008b75c000 - 000000008b75efff 0000000000000003 0000000000000000 000000000000000f
BS_data 000000008b75f000 - 000000008b764fff 0000000000000006 0000000000000000 000000000000000f
BS_code 000000008b765000 - 000000008b768fff 0000000000000004 0000000000000000 000000000000000f
BS_data 000000008b769000 - 000000008b791fff 0000000000000029 0000000000000000 000000000000000f
BS_code 000000008b792000 - 000000008b7a3fff 0000000000000012 0000000000000000 000000000000000f
BS_data 000000008b7a4000 - 000000008b7b5fff 0000000000000012 0000000000000000 000000000000000f
BS_code 000000008b7b6000 - 000000008b7bbfff 0000000000000006 0000000000000000 000000000000000f
BS_data 000000008b7bc000 - 000000008b7cdfff 0000000000000012 0000000000000000 000000000000000f
BS_code 000000008b7ce000 - 000000008b7cffff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b7d0000 - 000000008b7d3fff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008b7d4000 - 000000008b7dafff 0000000000000007 0000000000000000 000000000000000f
BS_data 000000008b7db000 - 000000008b7e7fff 000000000000000d 0000000000000000 000000000000000f
BS_code 000000008b7e8000 - 000000008b7e9fff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b7ea000 - 000000008b7eafff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b7eb000 - 000000008b7ebfff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b7ec000 - 000000008b7edfff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b7ee000 - 000000008b7eefff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b7ef000 - 000000008b806fff 0000000000000018 0000000000000000 000000000000000f
BS_code 000000008b807000 - 000000008b80efff 0000000000000008 0000000000000000 000000000000000f
BS_data 000000008b80f000 - 000000008b810fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b811000 - 000000008b811fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b812000 - 000000008b813fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b814000 - 000000008b824fff 0000000000000011 0000000000000000 000000000000000f
BS_data 000000008b825000 - 000000008b832fff 000000000000000e 0000000000000000 000000000000000f
BS_code 000000008b833000 - 000000008b833fff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b566000 - 000000008b58afff 0000000000000025 0000000000000000 000000000000000f
BS_data 000000008b58b000 - 000000008b5a7fff 000000000000001d 0000000000000000 000000000000000f
BS_code 000000008b5a8000 - 000000008b5c3fff 000000000000001c 0000000000000000 000000000000000f
BS_data 000000008b5c4000 - 000000008b5c5fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b5c6000 - 000000008b5c8fff 0000000000000003 0000000000000000 000000000000000f
BS_data 000000008b5c9000 - 000000008b5cafff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b5cb000 - 000000008b5cbfff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b5cc000 - 000000008b5cefff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b5cf000 - 000000008b5d8fff 000000000000000a 0000000000000000 000000000000000f
BS_data 000000008b5d9000 - 000000008b5d9fff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b5da000 - 000000008b5dafff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b5db000 - 000000008b5dcfff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b5dd000 - 000000008b5ddfff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b5de000 - 000000008b5e0fff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b5e1000 - 000000008b5e1fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b5e2000 - 000000008b5e4fff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b5e5000 - 000000008b5e7fff 0000000000000003 0000000000000000 000000000000000f
BS_data 000000008b5e8000 - 000000008b5ebfff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008b5ec000 - 000000008b5f5fff 000000000000000a 0000000000000000 000000000000000f
BS_data 000000008b5f6000 - 000000008b5f6fff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b5f7000 - 000000008b5f7fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b5f8000 - 000000008b5f8fff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b5f9000 - 000000008b5f9fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b5fa000 - 000000008b5fbfff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b5fc000 - 000000008b60bfff 0000000000000010 0000000000000000 000000000000000f
BS_data 000000008b60c000 - 000000008b621fff 0000000000000016 0000000000000000 000000000000000f
BS_code 000000008b622000 - 000000008b64efff 000000000000002d 0000000000000000 000000000000000f
BS_data 000000008b64f000 - 000000008b650fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b651000 - 000000008b652fff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b653000 - 000000008b655fff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b656000 - 000000008b66bfff 0000000000000016 0000000000000000 000000000000000f
BS_data 000000008b66c000 - 000000008b66ffff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008b670000 - 000000008b673fff 0000000000000004 0000000000000000 000000000000000f
BS_data 000000008b674000 - 000000008b67afff 0000000000000007 0000000000000000 000000000000000f
BS_code 000000008b67b000 - 000000008b67dfff 0000000000000003 0000000000000000 000000000000000f
BS_data 000000008b67e000 - 000000008b680fff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b681000 - 000000008b6affff 000000000000002f 0000000000000000 000000000000000f
BS_data 000000008b6b0000 - 000000008b6b4fff 0000000000000005 0000000000000000 000000000000000f
BS_code 000000008b6b5000 - 000000008b6cafff 0000000000000016 0000000000000000 000000000000000f
BS_data 000000008b6cb000 - 000000008b6ccfff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b6cd000 - 000000008b6cefff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b6cf000 - 000000008b6d0fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b6d1000 - 000000008b6d1fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b6d2000 - 000000008b6d7fff 0000000000000006 0000000000000000 000000000000000f
BS_code 000000008b6d8000 - 000000008b6ddfff 0000000000000006 0000000000000000 000000000000000f
BS_data 000000008b6de000 - 000000008b6dffff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b6e0000 - 000000008b6e5fff 0000000000000006 0000000000000000 000000000000000f
BS_data 000000008b6e6000 - 000000008b6e8fff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b6e9000 - 000000008b6e9fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b6ea000 - 000000008b6eafff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b6eb000 - 000000008b6ebfff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b6ec000 - 000000008b6f1fff 0000000000000006 0000000000000000 000000000000000f
BS_code 000000008b6f2000 - 000000008b6f3fff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b6f4000 - 000000008b6f6fff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b6f7000 - 000000008b6f7fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b6f8000 - 000000008b6f9fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b6fa000 - 000000008b6fcfff 0000000000000003 0000000000000000 000000000000000f
BS_data 000000008b6fd000 - 000000008b6fffff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b700000 - 000000008b701fff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b702000 - 000000008b708fff 0000000000000007 0000000000000000 000000000000000f
BS_code 000000008b709000 - 000000008b70afff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008b70b000 - 000000008b70dfff 0000000000000003 0000000000000000 000000000000000f
BS_code 000000008b70e000 - 000000008b711fff 0000000000000004 0000000000000000 000000000000000f
BS_data 000000008b712000 - 000000008b716fff 0000000000000005 0000000000000000 000000000000000f
BS_data 000000008b834000 - 000000008b834fff 0000000000000001 0000000000000000 000000000000000f
BS_code 000000008b835000 - 000000008b835fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b836000 - 000000008b837fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008b838000 - 000000008b838fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008b839000 - 000000008b83dfff 0000000000000005 0000000000000000 000000000000000f
BS_code 000000008b83e000 - 000000008b840fff 0000000000000003 0000000000000000 000000000000000f
BS_data 000000008b841000 - 000000008bc62fff 0000000000000422 0000000000000000 000000000000000f
BS_code 000000008bc63000 - 000000008bc63fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008bc64000 - 000000008bc67fff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008bc68000 - 000000008bc71fff 000000000000000a 0000000000000000 000000000000000f
BS_data 000000008bc72000 - 000000008bc75fff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008bc76000 - 000000008bc77fff 0000000000000002 0000000000000000 000000000000000f
BS_data 000000008bc78000 - 000000008bc7cfff 0000000000000005 0000000000000000 000000000000000f
BS_code 000000008bc7d000 - 000000008bc7dfff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008bc7e000 - 000000008bc85fff 0000000000000008 0000000000000000 000000000000000f
BS_code 000000008bc86000 - 000000008bc86fff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008bc87000 - 000000008bc88fff 0000000000000002 0000000000000000 000000000000000f
BS_code 000000008bc89000 - 000000008bc8dfff 0000000000000005 0000000000000000 000000000000000f
BS_data 000000008bc8e000 - 000000008bd39fff 00000000000000ac 0000000000000000 000000000000000f
BS_code 000000008bd3a000 - 000000008bd3afff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008bd3b000 - 000000008bd3efff 0000000000000004 0000000000000000 000000000000000f
BS_code 000000008bd3f000 - 000000008bd3ffff 0000000000000001 0000000000000000 000000000000000f
BS_data 000000008bd40000 - 000000008cd02fff 0000000000000fc3 0000000000000000 000000000000000f
available 000000008cd03000 - 000000008cd13fff 0000000000000011 0000000000000000 000000000000000f
ACPI_NVS 000000008cd14000 - 000000008cd52fff 000000000000003f 0000000000000000 000000000000000f
available 000000008cd53000 - 000000008cd60fff 000000000000000e 0000000000000000 000000000000000f
ACPI_recl 000000008cd61000 - 000000008cd8efff 000000000000002e 0000000000000000 000000000000000f
available 000000008cd8f000 - 000000008ce38fff 00000000000000aa 0000000000000000 000000000000000f
available 000000008ce39000 - 000000008ce8efff 0000000000000056 0000000000000000 000000000000000f
available 000000008ce8f000 - 000000008ced0fff 0000000000000042 0000000000000000 000000000000000f
available 000000008ced1000 - 000000008cefefff 000000000000002e 0000000000000000 000000000000000f
available 000000008ceff000 - 000000008cf87fff 0000000000000089 0000000000000000 000000000000000f
reserved 000000008cf88000 - 000000008cfeffff 0000000000000068 0000000000000000 000000000000000f
BS_data 000000008cff0000 - 000000008cffffff 0000000000000010 0000000000000000 000000000000000f
reserved 000000008d000000 - 000000008f9fffff 0000000000002a00 0000000000000000 0000000000000000
MemMapIO 00000000e00f8000 - 00000000e00f8fff 0000000000000001 ffffff800a0ed000 8000000000000001
MemMapIO 00000000fed1c000 - 00000000fed1ffff 0000000000000004 ffffff800a0ee000 8000000000000001
MemMapIO 00000000ffe10000 - 00000000ffe3ffff 0000000000000030 ffffff800a0f2000 8000000000000001
available 0000000100000000 - 000000026f5fffff 000000000016f600 0000000000000000 000000000000000f

I/O Kit Registry
Dumped using blackosx's ioregwv & viewed using IORegistry Web Viewer. To view this I/O Registry dump in it's own browser window/tab Click Here.
Property
Type
Value
Kernel Boot Messages
Dumped using OS X's BSD dmesg binary

View Boot-Messages.txt File

Longterm timer threshold: 1000 ms
PMAP: PCID enabled
PMAP: Supervisor Mode Execute Protection enabled
Darwin Kernel Version 13.2.0: Thu Apr 17 23:03:13 PDT 2014; root:xnu-2422.100.13~1/RELEASE_X86_64
vm_page_bootstrap: 1983731 free pages and 97037 wired pages
kext submap [0xffffff7f807a9000 - 0xffffff8000000000], kernel text [0xffffff8000200000 - 0xffffff80007a9000]
zone leak detection enabled
"vm_compressor_mode" is 4
standard timeslicing quantum is 10000 us
standard background quantum is 2500 us
mig_table_max_displ = 74
TSC Deadline Timer supported and enabled
AppleACPICPU: ProcessorId=1 LocalApicId=0 Enabled
AppleACPICPU: ProcessorId=2 LocalApicId=2 Enabled
AppleACPICPU: ProcessorId=3 LocalApicId=4 Enabled
AppleACPICPU: ProcessorId=4 LocalApicId=6 Enabled
AppleACPICPU: ProcessorId=5 LocalApicId=255 Disabled
AppleACPICPU: ProcessorId=6 LocalApicId=255 Disabled
AppleACPICPU: ProcessorId=7 LocalApicId=255 Disabled
AppleACPICPU: ProcessorId=8 LocalApicId=255 Disabled
calling mpo_policy_init for TMSafetyNet
Security policy loaded: Safety net for Time Machine (TMSafetyNet)
calling mpo_policy_init for Sandbox
Security policy loaded: Seatbelt sandbox policy (Sandbox)
calling mpo_policy_init for Quarantine
Security policy loaded: Quarantine policy (Quarantine)
Copyright (c) 1982, 1986, 1989, 1991, 1993
The Regents of the University of California. All rights reserved.
MAC Framework successfully initialized
using 16384 buffer headers and 10240 cluster IO buffer headers
AppleKeyStore starting (BUILT: Apr 17 2014 23:36:27)
IOAPIC: Version 0x20 Vectors 64:87
ACPI: sleep states S3 S4 S5
pci (build 23:24:05 Apr 17 2014), flags 0x63008, pfm64 (39 cpu) 0x7f80000000, 0x80000000
[ PCI configuration begin ]
console relocated to 0x7f80020000
[ PCI configuration end, bridges 12, devices 14 ]
AppleThunderboltNHIType2::setupPowerSavings - GPE based runtime power management
mcache: 4 CPU(s), 64 bytes CPU cache line size
mbinit: done [96 MB total pool size, (64/32) split]
Pthread support ABORTS when sync kernel primitives misused
rooting via boot-uuid from /chosen: 0A72ACE6-3CA9-3689-92AB-46C63CC23C2E
Waiting on <dict ID="0"><key>IOProviderClass</key><string ID="1">IOResources</string><key>IOResourceMatch</key><string ID="2">boot-uuid-media</string></dict>
com.apple.AppleFSCompressionTypeZlib kmod start
com.apple.AppleFSCompressionTypeDataless kmod start
com.apple.AppleFSCompressionTypeZlib load succeeded
com.apple.AppleFSCompressionTypeDataless load succeeded
srom rev:11
ARPT: 0.464445: ChangeVCO => vco:960, xtalF:40, frac: 98, ndivMode: 3, ndivint: 24
ARPT: 0.464454: Data written into the PLL_CNTRL_ADDR2: 00000c31
ARPT: 0.464473: Data written into the PLL_CNTRL_ADDR3 (Fractional): 0000100e
ARPT: 0.470550: BTCOEXIST off
ARPT: 0.470684: BRCM tunables:
ARPT: 0.470688: pullmode[1] txringsize[ 256] txsendqsize[1024] reapmin[ 32] reapcount[ 128]
ARPT: 0.471225: wl0: Broadcom BCM43a0, vendorID[0x14e4] BAR0[0xb1a00004]
6.30.223.154 (r420397)
Got boot device = IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/SATA@1F,2/AppleIntelPchSeriesAHCI/PRT0@0/IOAHCIDevice@0/AppleAHCIDiskDriver/IOAHCIBlockStorageDevice/IOBlockStorageDriver/APPLE HDD ST1000DM003 Media/IOGUIDPartitionScheme/Customer@2
BSD root: disk0s2, major 1, minor 2
Thunderbolt Self-Reset Count = 0xedefbe00
hfs: mounted Macintosh HD on device root_device
IOThunderboltSwitch<0xffffff801b1c5a00>(0x0)::listenerCallback - Thunderbolt HPD packet for route = 0x0 port = 11 unplug = 0
IOThunderboltSwitch<0xffffff801b1c5a00>(0x0)::listenerCallback - Thunderbolt HPD packet for route = 0x0 port = 12 unplug = 0
XCPM: registered
USBMSC Identifier (non-unique): 57584B314536334444534A4D 0x1058 0x812 0x1049, 3
com_sony_driver_dsccamDeviceInfo00 >> probe()
com_sony_driver_dsccamDeviceInfo00 : VENDOR_ID: WD
com_sony_driver_dsccamDeviceInfo00 << probe()
com_sony_driver_dsccamDeviceInfo00::probe fails
IO80211Controller::dataLinkLayerAttachComplete(): adding AppleEFINVRAM notification
IO80211Interface::efiNVRAMPublished():
flow_divert_kctl_disconnect (0): disconnecting group 1
NVDAStartup: Official
NVDAGK100HAL loaded and registered
SMC::smcReadKeyAction ERROR: smcReadData8 failed for key LsNM (kSMCKeyNotFound)
SMC::smcReadKeyAction ERROR LsNM kSMCKeyNotFound(0x84) fKeyHashTable=0x0
SMC::smcGetLightshowVers ERROR: smcReadKey LsNM failed (kSMCKeyNotFound)
SMC::smcPublishLightshowVersion ERROR: smcGetLightshowVers failed (kSMCKeyNotFound)
SMC::smcInitHelper ERROR: smcPublishLightshowVersion failed (kSMCKeyNotFound)
Previous Shutdown Cause: 0
IOBluetoothUSBDFU::probe
IOBluetoothUSBDFU::probe ProductID - 0x828D FirmwareVersion - 0x0079
**** [IOBluetoothHostControllerUSBTransport][start] -- completed -- result = TRUE -- 0x0400 ****
**** [BroadcomBluetoothHostControllerUSBTransport][start] -- Completed -- 0x0400 ****
init
probe
start
[IOBluetoothHCIController][staticBluetoothHCIControllerTransportShowsUp] -- Received Bluetooth Controller register service notification -- 0x0400
[IOBluetoothHCIController][start] -- completed
[IOBluetoothHCIController::setConfigState] calling registerService
**** [IOBluetoothHCIController][protectedBluetoothHCIControllerTransportShowsUp] -- Connected to the transport successfully -- 0xd9c0 -- 0xe800 -- 0x0400 ****
DSMOS has arrived
IOPPF - IODeviceTree:/efi/platform/StartupPowerEvents: 0x0
IOPPF - Found another boot volume.[AGPM Controller] build GPUDict by Vendor10deDevice119d
IOPPF: XCPM mode
hmm.. mismatch sizes: 3100 vs 20
Ethernet [AppleBCM5701Ethernet]: Link up on en0, 100-Megabit, Full-duplex, Symmetric flow-control, Debug [796d,0301,0de1,0300,45e1,0000]
0 [Level 5] [com.apple.message.domain com.apple.commssw.ethernet.broadcom.link] [com.apple.message.signature 100-Megabit] [com.apple.message.signature2 Full-duplex] [com.apple.message.signature3 Symmetric flow-control] [com.apple.message.signature4 EEE disabled]
0 [Level 5] [com.apple.message.domain com.apple.commssw.ethernet.broadcom.load] [com.apple.message.signature 0x14E4] [com.apple.message.signature2 0x1686] [com.apple.message.signature3 {Asymmetric-Pause=0}{Pause=1}{100baseTX-full-duplex=1}{100baseTX-half-duplex=1}{10baseT-full-duplex=1}{10baseT-half-duplex=1}{1000baseT-full-duplex=0}{100baseTX-EEE=0}{1000baseT-EEE=0}] [com.apple.message.signature4 1]
AirPort: Link Down on en1. Reason 8 (Disassociated because station leaving).
VM Swap Subsystem is ON
AirPort_Brcm4360_P2PInterface::init name <p2p0> role 1
AirPort_Brcm4360_P2PInterface::init() <p2p> role 1
_configureInterests - nElements <= 0!_configureInterests - nElements <= 0!en1: 802.11d country code set to 'GB'.
en1: Supported channels 1 2 3 4 5 6 7 8 9 10 11 12 13 36 40 44 48 52 56 60 64 100 104 108 112 116 120 124 128 132 136 140 149 153 157 161 165
hfs: mounted Recovery HD on device disk0s3
[BNBMouseDevice::init][80.14] init is complete
[BNBMouseDevice::handleStart][80.14] returning 1
[AppleMultitouchHIDEventDriver::start] entered
[AppleMultitouchDevice::start] entered
hfs: unmount initiated on Recovery HD on device disk0s3
AppleKeyStore:Sending lock change 0
pci pause: SDXC
0 [Level 5] [Facility messagetracer] [com.apple.message.domain com.apple.kernel.cs.mismatch] [com.apple.message.signature 1000] [com.apple.message.signature2 3345639bd98273913ff25086fe0151f45fea0fa3] [com.apple.message.signature3 38872323d4adae2cb310de88ceeeae695630ffd7] [com.apple.message.summarize YES]
0 [Level 5] [Facility messagetracer] [com.apple.message.domain com.apple.kernel.cs.invalidate] [com.apple.message.signature invalidate] [com.apple.message.signature4 525] [com.apple.message.signature3 ksadmin] [com.apple.message.summarize YES]
CODE SIGNING: cs_invalid_page(0x1000): p=525[ksadmin] final status 0x0, allowing (remove VALID) page
0 [Level 5] [Facility messagetracer] [com.apple.message.domain com.apple.kernel.cs.invalidate] [com.apple.message.signature invalidate] [com.apple.message.signature4 540] [com.apple.message.signature3 ksadmin] [com.apple.message.summarize YES]
CODE SIGNING: cs_invalid_page(0x1000): p=540[ksadmin] final status 0x0, allowing (remove VALID) page
hfs: mounted OS X Snow Leopard Install Disk - 10.6.8 on device disk1s2
hfs: mounted OS X Lion Install Disk - 10.7.5 on device disk1s3
hfs: mounted OS X Mountain Lion Install Disk - 10.8.5 on device disk1s4
hfs: mounted OS X 10.9 Install Disk - 10.9.3 on device disk1s5
hfs: mounted OS X Install Disk - 10.10 on device disk1s6
hfs: mounted BootTest on device disk1s7
hfs: mounted SoftDisk on device disk1s8
hfs: mounted DataDisk on device disk1s9
0 [Level 5] [Facility messagetracer] [com.apple.message.domain com.apple.kernel.cs.mismatch] [com.apple.message.signature 1000] [com.apple.message.signature2 53a18aae61685cc356b171ce37cc504048ed45a1] [com.apple.message.signature3 b928c695e1e1a867d5fc392eb8f09e460f3139af] [com.apple.message.summarize YES]
0 [Level 5] [Facility messagetracer] [com.apple.message.domain com.apple.kernel.cs.invalidate] [com.apple.message.signature invalidate] [com.apple.message.signature4 1092] [com.apple.message.signature3 GoogleSoftwareUp] [com.apple.message.summarize YES]
CODE SIGNING: cs_invalid_page(0x1000): p=1092[GoogleSoftwareUp] final status 0x0, allowing (remove VALID) page
TUFS: starting (version 2013.3.14, x86_64 (10.6+), built Mar 14 2013, 14:13:23)
hfs: mounted Tuxera NTFS on device disk2s1
hfs: unmount initiated on Tuxera NTFS on device disk2s1
considerRebuildOfPrelinkedKernel com.tuxera.filesystems.tufsfs.fusefs_txantfs triggered rebuild
RadeonPCI::start
Range[0] 100800000: 400000
Range[1] 108000000: 8000000
Range[2] 2000: 40
Range@0x10 100800000: 400000
Range@0x10 ( 100800000) mapped to kernel virtual address ffffff8115158000
ATI ROM start at 9d0000 mapped to kernel virtual address ffffff812b021000
ROM signature is read as: 0000ffff
Config register@0x4 = 00900407
RadeonPCIUserClient::initWithTask(type 23)
RadeonPCIUserClient::start
RadeonPCIUserClient::clientMemoryForType(100)
RadeonPCIUserClient::stop
RadeonPCI::start
Range[0] 101000000: 1000000
RadeonPCI::stop
RadeonPCI::stop
Can't unload kext com.dong.driver.RadeonPCI; classes have instances:
Kext com.dong.driver.RadeonPCI class RadeonPCI has 1 instance.
Range[1] 110000000: 10000000
Range[2] 102000000: 2000000
Range[3] 1000: 80
Range[4] 104000000: 80000
Range@0x10 101000000: 1000000
Range@0x10 ( 101000000) mapped to kernel virtual address ffffff8116715000
ATI ROM start at 11f0000 mapped to kernel virtual address ffffff812b021000
ROM signature is read as: 0000ffff
Config register@0x4 = 00100406
RadeonPCI: not registry member at registerService()

Kernel Info
Dumped using: uname -v, sysctl -a | grep cpu, sysctl -a | grep hw

View Kernel-Info.txt File

Darwin Kernel Version 13.2.0: Thu Apr 17 23:03:13 PDT 2014; root:xnu-2422.100.13~1/RELEASE_X86_64
hw.ncpu = 4
hw.cpufrequency = 3400000000
hw.availcpu = 4
hw.ncpu: 4
hw.activecpu: 4
hw.physicalcpu: 4
hw.physicalcpu_max: 4
hw.logicalcpu: 4
hw.logicalcpu_max: 4
hw.cputype: 7
hw.cpusubtype: 4
hw.cpu64bit_capable: 1
hw.cpufamily: 280134364
hw.cpufrequency: 3400000000
hw.cpufrequency_min: 3400000000
hw.cpufrequency_max: 3400000000
machdep.cpu.max_basic: 13
machdep.cpu.max_ext: 2147483656
machdep.cpu.vendor: GenuineIntel
machdep.cpu.brand_string: Intel(R) Core(TM) i5-4670 CPU @ 3.40GHz
machdep.cpu.family: 6
machdep.cpu.model: 60
machdep.cpu.extmodel: 3
machdep.cpu.extfamily: 0
machdep.cpu.stepping: 3
machdep.cpu.feature_bits: 3219913727 2147154943
machdep.cpu.leaf7_feature_bits: 12219
machdep.cpu.extfeature_bits: 739248384 33
machdep.cpu.signature: 198339
machdep.cpu.brand: 0
machdep.cpu.features: FPU VME DE PSE TSC MSR PAE MCE CX8 APIC SEP MTRR PGE MCA CMOV PAT PSE36 CLFSH DS ACPI MMX FXSR SSE SSE2 SS HTT TM PBE SSE3 PCLMULQDQ DTES64 MON DSCPL VMX SMX EST TM2 SSSE3 FMA CX16 TPR PDCM SSE4.1 SSE4.2 x2APIC MOVBE POPCNT AES PCID XSAVE OSXSAVE SEGLIM64 TSCTMR AVX1.0 RDRAND F16C
machdep.cpu.leaf7_features: SMEP ENFSTRG RDWRFSGS TSC_THREAD_OFFSET BMI1 HLE AVX2 BMI2 INVPCID RTM
machdep.cpu.extfeatures: SYSCALL XD 1GBPAGE EM64T LAHF RDTSCP TSCI
machdep.cpu.logical_per_package: 16
machdep.cpu.cores_per_package: 8
machdep.cpu.microcode_version: 16
machdep.cpu.processor_flag: 1
machdep.cpu.mwait.linesize_min: 64
machdep.cpu.mwait.linesize_max: 64
machdep.cpu.mwait.extensions: 3
machdep.cpu.mwait.sub_Cstates: 270624
machdep.cpu.thermal.sensor: 1
machdep.cpu.thermal.dynamic_acceleration: 1
machdep.cpu.thermal.invariant_APIC_timer: 1
machdep.cpu.thermal.thresholds: 2
machdep.cpu.thermal.ACNT_MCNT: 1
machdep.cpu.thermal.core_power_limits: 1
machdep.cpu.thermal.fine_grain_clock_mod: 1
machdep.cpu.thermal.package_thermal_intr: 1
machdep.cpu.thermal.hardware_feedback: 0
machdep.cpu.thermal.energy_policy: 1
machdep.cpu.xsave.extended_state: 7 832 832 0
machdep.cpu.arch_perf.version: 3
machdep.cpu.arch_perf.number: 8
machdep.cpu.arch_perf.width: 48
machdep.cpu.arch_perf.events_number: 7
machdep.cpu.arch_perf.events: 0
machdep.cpu.arch_perf.fixed_number: 3
machdep.cpu.arch_perf.fixed_width: 48
machdep.cpu.cache.linesize: 64
machdep.cpu.cache.L2_associativity: 8
machdep.cpu.cache.size: 256
machdep.cpu.tlb.inst.large: 8
machdep.cpu.tlb.data.small: 64
machdep.cpu.tlb.data.small_level1: 128
machdep.cpu.tlb.shared: 1024
machdep.cpu.address_bits.physical: 39
machdep.cpu.address_bits.virtual: 48
machdep.cpu.core_count: 4
machdep.cpu.thread_count: 4
machdep.xcpm.cpu_wakeup_energy_cost_selector: 0
hw.machine = x86_64
hw.model = iMac14,2
hw.ncpu = 4
hw.byteorder = 1234
hw.physmem = 2147483648
hw.usermem = 1219166208
hw.pagesize = 4096
hw.epoch = 0
hw.vectorunit = 1
hw.busfrequency = 100000000
hw.cpufrequency = 3400000000
hw.cachelinesize = 64
hw.l1icachesize = 32768
hw.l1dcachesize = 32768
hw.l2settings = 1
hw.l2cachesize = 262144
hw.l3settings = 1
hw.l3cachesize = 6291456
hw.tbfrequency = 1000000000
hw.memsize = 8589934592
hw.availcpu = 4
net.inet.ip.adj_clear_hwcksum: 0
net.link.generic.system.hwcksum_in_invalidated: 0
net.link.generic.system.hwcksum_dbg: 0
net.link.generic.system.hwcksum_dbg_mode: 0
net.link.generic.system.hwcksum_dbg_partial_forced: 0
net.link.generic.system.hwcksum_dbg_partial_forced_bytes: 0
net.link.generic.system.hwcksum_dbg_partial_rxoff_forced: 0
net.link.generic.system.hwcksum_dbg_partial_rxoff_adj: 0
net.link.generic.system.hwcksum_dbg_verified: 0
net.link.generic.system.hwcksum_dbg_bad_cksum: 0
net.link.generic.system.hwcksum_dbg_bad_rxoff: 0
net.link.generic.system.hwcksum_dbg_adjusted: 0
net.link.generic.system.hwcksum_dbg_finalized_hdr: 0
net.link.generic.system.hwcksum_dbg_finalized_data: 0
net.link.generic.system.hwcksum_tx: 1
net.link.generic.system.hwcksum_rx: 1
net.link.ether.inet.apple_hwcksum_tx: 1
net.link.ether.inet.apple_hwcksum_rx: 1
net.inet6.ip6.adj_clear_hwcksum: 0
hw.ncpu: 4
hw.byteorder: 1234
hw.memsize: 8589934592
hw.activecpu: 4
hw.physicalcpu: 4
hw.physicalcpu_max: 4
hw.logicalcpu: 4
hw.logicalcpu_max: 4
hw.cputype: 7
hw.cpusubtype: 4
hw.cpu64bit_capable: 1
hw.cpufamily: 280134364
hw.cacheconfig: 4 1 1 4 0 0 0 0 0 0
hw.cachesize: 8589934592 32768 262144 6291456 0 0 0 0 0 0
hw.pagesize: 4096
hw.busfrequency: 100000000
hw.busfrequency_min: 100000000
hw.busfrequency_max: 100000000
hw.cpufrequency: 3400000000
hw.cpufrequency_min: 3400000000
hw.cpufrequency_max: 3400000000
hw.cachelinesize: 64
hw.l1icachesize: 32768
hw.l1dcachesize: 32768
hw.l2cachesize: 262144
hw.l3cachesize: 6291456
hw.tbfrequency: 1000000000
hw.packages: 1
hw.optional.floatingpoint: 1
hw.optional.mmx: 1
hw.optional.sse: 1
hw.optional.sse2: 1
hw.optional.sse3: 1
hw.optional.supplementalsse3: 1
hw.optional.sse4_1: 1
hw.optional.sse4_2: 1
hw.optional.x86_64: 1
hw.optional.aes: 1
hw.optional.avx1_0: 1
hw.optional.rdrand: 1
hw.optional.f16c: 1
hw.optional.enfstrg: 1
hw.optional.fma: 1
hw.optional.avx2_0: 1
hw.optional.bmi1: 1
hw.optional.bmi2: 1
hw.optional.rtm: 1
hw.optional.hle: 1
machdep.pmap.hashwalks: 1332673

Kexts
Non Apple Kexts : 3

Terminal command issued: kextstat -l | egrep -v "com.apple"

IDX | REFS | ADDRESS | SIZE | WIRED | NAME | VERSION | LINKED AGAINST
128 | 0 | 0xffffff7f82879000 | 0x17000 | 0x17000 | com.tuxera.filesystems.tufsfs.fusefs_txantfs | (2013.3.14) | <7 5 4 3 1>
131 | 0 | 0xffffff7f828a6000 | 0x3000 | 0x3000 | com.dong.driver.RadeonPCI | (1.1.1d1) | <5 4 3>
132 | 0 | 0xffffff7f828a9000 | 0x4000 | 0x4000 | com.coresystems.driver.DirectHW | (1.3) | <7 5 4 3>

Apple Kexts : 118

Terminal command issued: kextstat -l | egrep "com.apple"

IDX | REFS | ADDRESS | SIZE | WIRED | NAME | VERSION | LINKED AGAINST
1 | 79 | 0xffffff7f807e3000 | 0x8d80 | 0x8d80 | com.apple.kpi.bsd | (13.2.0)
2 | 6 | 0xffffff7f80b67000 | 0x28c0 | 0x28c0 | com.apple.kpi.dsep | (13.2.0)
3 | 108 | 0xffffff7f807ac000 | 0x1dfb0 | 0x1dfb0 | com.apple.kpi.iokit | (13.2.0)
4 | 114 | 0xffffff7f807ca000 | 0xbf40 | 0xbf40 | com.apple.kpi.libkern | (13.2.0)
5 | 98 | 0xffffff7f807a9000 | 0x2d10 | 0x2d10 | com.apple.kpi.mach | (13.2.0)
6 | 39 | 0xffffff7f807d6000 | 0x7d90 | 0x7d90 | com.apple.kpi.private | (13.2.0)
7 | 59 | 0xffffff7f807de000 | 0x48e0 | 0x48e0 | com.apple.kpi.unsupported | (13.2.0)
8 | 0 | 0xffffff7f80bb4000 | 0xb000 | 0xb000 | com.apple.kec.pthread | (1) | <7 6 5 4 1>
9 | 2 | 0xffffff7f81226000 | 0x47000 | 0x47000 | com.apple.kec.corecrypto | (1.0) | <7 6 5 4 3 1>
10 | 19 | 0xffffff7f81548000 | 0x9000 | 0x9000 | com.apple.iokit.IOACPIFamily | (1.4) | <7 6 4 3>
11 | 32 | 0xffffff7f808be000 | 0x2b000 | 0x2b000 | com.apple.iokit.IOPCIFamily | (2.9) | <7 6 5 4 3>
12 | 2 | 0xffffff7f827ec000 | 0x59000 | 0x59000 | com.apple.driver.AppleACPIPlatform | (2.0) | <11 10 7 6 5 4 3 1>
13 | 1 | 0xffffff7f8126d000 | 0xb000 | 0xb000 | com.apple.driver.AppleFDEKeyStore | (28.30) | <9 7 6 5 4 3 1>
14 | 2 | 0xffffff7f81537000 | 0xf000 | 0xf000 | com.apple.iokit.IOReportFamily | (23) | <5 4 3>
15 | 7 | 0xffffff7f807ec000 | 0x25000 | 0x25000 | com.apple.iokit.IOStorageFamily | (1.9) | <7 6 5 4 3 1>
16 | 0 | 0xffffff7f815fc000 | 0x19000 | 0x19000 | com.apple.driver.DiskImages | (371.1) | <15 7 6 5 4 3 1>
17 | 0 | 0xffffff7f822cd000 | 0x14000 | 0x14000 | com.apple.driver.AppleKeyStore | (2) | <9 7 6 5 4 3 1>
18 | 0 | 0xffffff7f80b6a000 | 0x3000 | 0x3000 | com.apple.security.TMSafetyNet | (7) | <7 6 5 4 2 1>
19 | 2 | 0xffffff7f80b93000 | 0x5000 | 0x5000 | com.apple.kext.AppleMatch | (1.0.0d1) | <4 1>
20 | 1 | 0xffffff7f80b98000 | 0x14000 | 0x14000 | com.apple.security.sandbox | (278.11) | <19 7 6 5 4 3 2 1>
21 | 0 | 0xffffff7f80bac000 | 0x7000 | 0x7000 | com.apple.security.quarantine | (3) | <20 19 7 6 5 4 2 1>
22 | 0 | 0xffffff7f8285c000 | 0x8000 | 0x8000 | com.apple.nke.applicationfirewall | (153) | <7 6 5 4 3 1>
23 | 0 | 0xffffff7f827c0000 | 0x3000 | 0x3000 | com.apple.driver.AppleAPIC | (1.7) | <4 3>
24 | 2 | 0xffffff7f814c9000 | 0x4000 | 0x4000 | com.apple.iokit.IOSMBusFamily | (1.1) | <5 4 3>
25 | 0 | 0xffffff7f8284b000 | 0x7000 | 0x7000 | com.apple.driver.AppleACPIEC | (2.0) | <24 12 10 5 4 3>
26 | 0 | 0xffffff7f821f7000 | 0x4000 | 0x4000 | com.apple.driver.AppleSMBIOS | (2.1) | <7 4 3>
27 | 0 | 0xffffff7f824f0000 | 0x3000 | 0x3000 | com.apple.driver.AppleHPET | (1.8) | <10 7 5 4 3>
28 | 7 | 0xffffff7f81278000 | 0x72000 | 0x72000 | com.apple.iokit.IOHIDFamily | (2.0.0) | <13 7 6 5 4 3 2 1>
29 | 0 | 0xffffff7f82855000 | 0x4000 | 0x4000 | com.apple.driver.AppleACPIButtons | (2.0) | <28 12 10 7 6 5 4 3 1>
30 | 0 | 0xffffff7f82223000 | 0x7000 | 0x7000 | com.apple.driver.AppleRTC | (2.0) | <10 5 4 3 1>
31 | 1 | 0xffffff7f82793000 | 0x5000 | 0x5000 | com.apple.driver.AppleEFIRuntime | (2.0) | <7 6 5 4 3>
32 | 0 | 0xffffff7f82798000 | 0xa000 | 0xa000 | com.apple.driver.AppleEFINVRAM | (2.0) | <31 7 6 5 4 3>
33 | 10 | 0xffffff7f811a2000 | 0x61000 | 0x61000 | com.apple.iokit.IOUSBFamily | (677.4.0) | <11 7 5 4 3 1>
34 | 0 | 0xffffff7f8130d000 | 0x1d000 | 0x1d000 | com.apple.driver.AppleUSBXHCI | (677.4.0) | <33 11 7 5 4 3 1>
35 | 2 | 0xffffff7f817bb000 | 0x16000 | 0x16000 | com.apple.iokit.IOAHCIFamily | (2.6.5) | <5 4 3 1>
36 | 0 | 0xffffff7f827c5000 | 0x1a000 | 0x1a000 | com.apple.driver.AppleAHCIPort | (3.0.0) | <35 11 5 4 3 1>
37 | 7 | 0xffffff7f81161000 | 0x2d000 | 0x2d000 | com.apple.iokit.IONetworkingFamily | (3.2) | <7 6 5 4 3 1>
38 | 2 | 0xffffff7f815b4000 | 0x7000 | 0x7000 | com.apple.driver.mDNSOffloadUserClient | (1.0.1b5) | <37 4 3 1>
39 | 1 | 0xffffff7f815bb000 | 0x7000 | 0x7000 | com.apple.iokit.IOEthernetAVBController | (1.0.3b4) | <37 5 4 3 1>
40 | 0 | 0xffffff7f815c2000 | 0x38000 | 0x38000 | com.apple.iokit.AppleBCM5701Ethernet | (3.8.1b2) | <39 38 37 11 10 6 5 4 3 1>
41 | 0 | 0xffffff7f8220a000 | 0x12000 | 0x12000 | com.apple.driver.AppleSDXC | (1.5.2) | <15 11 5 4 3 1>
42 | 1 | 0xffffff7f81806000 | 0x79000 | 0x79000 | com.apple.iokit.IO80211Family | (630.35) | <37 7 6 5 4 3 1>
43 | 0 | 0xffffff7f81886000 | 0x3be000 | 0x3be000 | com.apple.driver.AirPort.Brcm4360 | (831.21.63) | <42 38 37 11 7 5 4 3 1>
44 | 7 | 0xffffff7f813c0000 | 0xd8000 | 0xd8000 | com.apple.iokit.IOThunderboltFamily | (3.2.7) | <5 4 3 1>
45 | 0 | 0xffffff7f82107000 | 0x18000 | 0x18000 | com.apple.driver.AppleThunderboltNHI | (2.0.1) | <44 11 10 5 4 3 1>
46 | 0 | 0xffffff7f817e1000 | 0x18000 | 0x18000 | com.apple.iokit.IOAHCIBlockStorage | (2.5.1) | <35 15 6 5 4 3 1>
47 | 0 | 0xffffff7f82049000 | 0x3000 | 0x3000 | com.apple.driver.XsanFilter | (404) | <15 5 4 3 1>
48 | 0 | 0xffffff7f81223000 | 0x3000 | 0x3000 | com.apple.iokit.IOUSBUserClient | (660.4.2) | <33 7 5 4 3 1>
49 | 0 | 0xffffff7f8136b000 | 0x18000 | 0x18000 | com.apple.driver.AppleUSBHub | (666.4.0) | <33 5 4 3 1>
50 | 0 | 0xffffff7f81ebc000 | 0x9000 | 0x9000 | com.apple.BootCache | (35) | <7 6 5 4 3 1>
51 | 0 | 0xffffff7f82784000 | 0x4000 | 0x4000 | com.apple.AppleFSCompression.AppleFSCompressionTypeZlib | (1.0.0d1) | <6 4 3 2 1>
52 | 0 | 0xffffff7f8278a000 | 0x3000 | 0x3000 | com.apple.AppleFSCompression.AppleFSCompressionTypeDataless | (1.0.0d1) | <7 6 4 3 2 1>
54 | 1 | 0xffffff7f81306000 | 0x7000 | 0x7000 | com.apple.driver.AppleUSBComposite | (656.4.1) | <33 4 3 1>
55 | 0 | 0xffffff7f820f5000 | 0x5000 | 0x5000 | com.apple.driver.AppleThunderboltPCIDownAdapter | (1.4.5) | <44 11 5 4 3 1>
56 | 3 | 0xffffff7f82145000 | 0xf000 | 0xf000 | com.apple.driver.AppleThunderboltDPAdapterFamily | (3.1.7) | <44 10 5 4 3 1>
57 | 1 | 0xffffff7f82154000 | 0xd000 | 0xd000 | com.apple.driver.AppleThunderboltDPOutAdapter | (3.1.7) | <56 44 5 4 3 1>
58 | 0 | 0xffffff7f8216e000 | 0x6000 | 0x6000 | com.apple.driver.AppleThunderboltDPInAdapter | (3.1.7) | <56 44 5 4 3 1>
59 | 3 | 0xffffff7f8087c000 | 0x2b000 | 0x2b000 | com.apple.iokit.IOSCSIArchitectureModelFamily | (3.6.6) | <5 4 3 1>
60 | 0 | 0xffffff7f8120f000 | 0x11000 | 0x11000 | com.apple.iokit.IOUSBMassStorageClass | (3.6.0) | <59 33 15 5 4 3 1>
61 | 0 | 0xffffff7f80b6d000 | 0x15000 | 0x15000 | com.apple.iokit.IOSCSIBlockCommandsDevice | (3.6.6) | <59 15 5 4 3 1>
63 | 0 | 0xffffff7f814e3000 | 0x7000 | 0x7000 | com.apple.iokit.SCSITaskUserClient | (3.6.6) | <59 15 5 4 3 1>
64 | 0 | 0xffffff7f81364000 | 0x7000 | 0x7000 | com.apple.driver.AppleUSBMergeNub | (650.4.0) | <54 33 4 3 1>
66 | 16 | 0xffffff7f80bc3000 | 0x38000 | 0x38000 | com.apple.iokit.IOGraphicsFamily | (2.4.1) | <11 7 5 4 3 1>
67 | 2 | 0xffffff7f8231c000 | 0x65000 | 0x65000 | com.apple.iokit.IOAcceleratorFamily2 | (98.20) | <66 11 7 6 5 4 3 1>
68 | 3 | 0xffffff7f80c16000 | 0x6000 | 0x6000 | com.apple.AppleGraphicsDeviceControl | (3.5.26) | <7 6 5 4 3 1>
69 | 0 | 0xffffff7f82406000 | 0x68000 | 0x68000 | com.apple.driver.AppleIntelFramebufferAzul | (8.2.6) | <68 67 66 14 11 10 7 6 5 4 3 1>
70 | 6 | 0xffffff7f80c06000 | 0x10000 | 0x10000 | com.apple.iokit.IONDRVSupport | (2.4.1) | <66 11 7 5 4 3>
71 | 1 | 0xffffff7f814b4000 | 0x13000 | 0x13000 | com.apple.iokit.IOSurface | (91.1) | <7 5 4 3 1>
72 | 0 | 0xffffff7f8238e000 | 0x51000 | 0x51000 | com.apple.driver.AppleIntelHD5000Graphics | (8.2.6) | <71 67 66 11 7 5 4 3 1>
74 | 2 | 0xffffff7f80c1c000 | 0x274000 | 0x274000 | com.apple.nvidia.driver.NVDAResman | (8.2.6) | <70 68 66 11 5 4 3 1>
75 | 4 | 0xffffff7f81551000 | 0xa000 | 0xa000 | com.apple.driver.IOPlatformPluginFamily | (5.7.0d11) | <10 7 6 5 4 3>
76 | 0 | 0xffffff7f822c5000 | 0x3000 | 0x3000 | com.apple.driver.AppleLPC | (1.7.0) | <75 11 5 4 3>
77 | 2 | 0xffffff7f82511000 | 0xc000 | 0xc000 | com.apple.iokit.IOHDAFamily | (2.6.1f2) | <5 4 3 1>
78 | 1 | 0xffffff7f82548000 | 0x1a000 | 0x1a000 | com.apple.driver.AppleHDAController | (2.6.1f2) | <77 66 11 7 6 5 4 3 1>
79 | 0 | 0xffffff7f80e9b000 | 0x1ad000 | 0x1ad000 | com.apple.nvidia.driver.NVDAGK100Hal | (8.2.6) | <74 11 4 3>
80 | 1 | 0xffffff7f81c9e000 | 0x59000 | 0x59000 | com.apple.iokit.IOAcceleratorFamily | (98.20) | <66 11 7 6 5 4 3 1>
81 | 0 | 0xffffff7f81d03000 | 0x8f000 | 0x8f000 | com.apple.GeForce | (8.2.6) | <80 74 70 66 11 7 5 4 3 1>
82 | 4 | 0xffffff7f8155b000 | 0x13000 | 0x13000 | com.apple.driver.AppleSMC | (3.1.8) | <10 7 5 4 3 1>
83 | 1 | 0xffffff7f81570000 | 0x11000 | 0x11000 | com.apple.driver.X86PlatformPlugin | (1.0.0) | <82 75 33 10 7 6 5 4 3 1>
86 | 2 | 0xffffff7f821e6000 | 0xe000 | 0xe000 | com.apple.driver.AppleSMBusController | (1.0.11d1) | <24 11 10 5 4 3>
87 | 0 | 0xffffff7f8228c000 | 0xd000 | 0xd000 | com.apple.driver.AppleMCCSControl | (1.1.12) | <86 66 11 10 7 5 4 3 1>
88 | 0 | 0xffffff7f820a6000 | 0x5000 | 0x5000 | com.apple.driver.AppleUpstreamUserClient | (3.5.13) | <66 11 10 7 5 4 3 1>
89 | 1 | 0xffffff7f82759000 | 0x5000 | 0x5000 | com.apple.driver.AppleBacklightExpert | (1.0.4) | <70 66 11 5 4 3>
90 | 0 | 0xffffff7f827b8000 | 0x5000 | 0x5000 | com.apple.driver.AppleBacklight | (170.3.5) | <89 70 66 11 5 4 3>
91 | 0 | 0xffffff7f82161000 | 0xd000 | 0xd000 | com.apple.driver.AppleThunderboltEDMSink | (2.1.3) | <57 56 44 5 4 3 1>
92 | 0 | 0xffffff7f82123000 | 0x17000 | 0x17000 | com.apple.driver.AppleThunderboltIP | (1.1.2) | <44 37 11 5 4 3 1>
94 | 0 | 0xffffff7f824cc000 | 0x3000 | 0x3000 | com.apple.driver.AppleHWAccess | (1) | <7 5 4 3>
95 | 0 | 0xffffff7f81dca000 | 0x5000 | 0x5000 | com.apple.Dont_Steal_Mac_OS_X | (7.0.0) | <82 7 4 3 1>
96 | 1 | 0xffffff7f81760000 | 0x1d000 | 0x1d000 | com.apple.iokit.IOBluetoothHostControllerUSBTransport | (4.2.4f1) | <33 11 10 7 5 4 3 1>
97 | 0 | 0xffffff7f8177d000 | 0x7000 | 0x7000 | com.apple.iokit.BroadcomBluetoothHostControllerUSBTransport | (4.2.4f1) | <96 33 11 10 7 5 4 3>
100 | 0 | 0xffffff7f821db000 | 0x5000 | 0x5000 | com.apple.driver.AppleSMCLMU | (2.0.4d1) | <82 66 5 4 3>
101 | 0 | 0xffffff7f821e3000 | 0x3000 | 0x3000 | com.apple.driver.AppleSMBusPCI | (1.0.12d1) | <11 5 4 3>
102 | 2 | 0xffffff7f81688000 | 0x9d000 | 0x9d000 | com.apple.iokit.IOBluetoothFamily | (4.2.4f1) | <33 14 7 5 4 3 1>
104 | 0 | 0xffffff7f81195000 | 0x7000 | 0x7000 | com.apple.iokit.IOUserEthernet | (1.0.0d1) | <37 6 5 4 3 1>
106 | 0 | 0xffffff7f8227a000 | 0x4000 | 0x4000 | com.apple.driver.ApplePlatformEnabler | (2.0.9d1) | <7 5 4 3>
107 | 0 | 0xffffff7f8273c000 | 0x12000 | 0x12000 | com.apple.driver.AGPM | (100.14.15) | <75 70 68 66 11 5 4 3>
108 | 0 | 0xffffff7f81581000 | 0x6000 | 0x6000 | com.apple.driver.X86PlatformShim | (1.0.0) | <83 82 75 7 4 3>
109 | 2 | 0xffffff7f81ed7000 | 0x12000 | 0x12000 | com.apple.kext.OSvKernDSPLib | (1.14) | <5 4>
110 | 3 | 0xffffff7f81ee9000 | 0x2f000 | 0x2f000 | com.apple.iokit.IOAudioFamily | (1.9.7fc2) | <109 5 4 3 1>
111 | 1 | 0xffffff7f82562000 | 0x2f000 | 0x2f000 | com.apple.vecLib.kext | (1.0.0) | <6 5 4 3>
112 | 1 | 0xffffff7f82591000 | 0xcd000 | 0xcd000 | com.apple.driver.DspFuncLib | (2.6.1f2) | <111 110 109 6 5 4 3 1>
113 | 0 | 0xffffff7f82667000 | 0x90000 | 0x90000 | com.apple.driver.AppleHDA | (2.6.1f2) | <112 110 78 77 70 66 6 5 4 3 1>
115 | 0 | 0xffffff7f82520000 | 0x16000 | 0x16000 | com.apple.driver.AppleMikeyDriver | (2.6.1f2) | <86 10 5 4 3 1>
116 | 0 | 0xffffff7f82281000 | 0x3000 | 0x3000 | com.apple.driver.AppleMikeyHIDDriver | (124) | <28 7 4 3 1>
117 | 0 | 0xffffff7f81f20000 | 0x5000 | 0x5000 | com.apple.driver.AudioAUUC | (1.60) | <110 66 11 10 7 5 4 3 1>
118 | 1 | 0xffffff7f814d2000 | 0xe000 | 0xe000 | com.apple.iokit.IOSerialFamily | (10.0.7) | <7 6 5 4 3 1>
119 | 0 | 0xffffff7f8174c000 | 0xa000 | 0xa000 | com.apple.iokit.IOBluetoothSerialManager | (4.2.4f1) | <118 7 5 4 3 1>
120 | 0 | 0xffffff7f824c3000 | 0x5000 | 0x5000 | com.apple.driver.AppleHWSensor | (1.9.5d0) | <5 4 3>
121 | 1 | 0xffffff7f820af000 | 0x17000 | 0x17000 | com.apple.driver.AppleMultitouchDriver | (245.13) | <28 5 4 3 1>
122 | 2 | 0xffffff7f81735000 | 0x12000 | 0x12000 | com.apple.driver.IOBluetoothHIDDriver | (4.2.4f1) | <102 28 5 4 3>
123 | 0 | 0xffffff7f827a2000 | 0xe000 | 0xe000 | com.apple.driver.AppleBluetoothMultitouch | (80.14) | <122 121 102 28 5 4 3>
124 | 1 | 0xffffff7f81ec7000 | 0x5000 | 0x5000 | com.apple.kext.triggers | (1.0) | <7 6 5 4 3 1>
125 | 0 | 0xffffff7f81ecc000 | 0x9000 | 0x9000 | com.apple.filesystems.autofs | (3.0) | <124 7 6 5 4 3 1>
126 | 1 | 0xffffff7f820ca000 | 0x7000 | 0x7000 | com.apple.driver.AppleHIDKeyboard | (170.15) | <28 4 3>
127 | 0 | 0xffffff7f8250b000 | 0x6000 | 0x6000 | com.apple.driver.AppleBluetoothHIDKeyboard | (170.15) | <126 122 28 4 3>
129 | 0 | 0xffffff7f82890000 | 0x8000 | 0x8000 | com.apple.driver.AppleIntelMCEReporter | (104) | <7 6 5 4 3>
130 | 0 | 0xffffff7f82898000 | 0xe000 | 0xe000 | com.apple.filesystems.msdosfs | (1.9) | <7 5 4 1>
133 | 0 | 0xffffff7f828ad000 | 0x3000 | 0x3000 | com.apple.nvidia.NVDAStartup | (8.2.6) | <11 4 3>

LSPCI (PCI vendor & device codes)
Tree (-nnvvt)

Dumped using pciutils v3.2.0 by Martin Mares. OS X port by THe KiNG. This version compiled by xsmile. View lspci tree (nnvvt).txt File

-[0000:00]-+-00.0 Intel Corporation 4th Gen Core Processor DRAM Controller [8086:0c00]
+-01.0-[01]--+-00.0 NVIDIA Corporation GK104M [GeForce GTX 775M Mac Edition] [10de:119d]
| \-00.1 NVIDIA Corporation GK104 HDMI Audio Controller [10de:0e0a]
+-02.0 Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor Integrated Graphics Controller [8086:0412]
+-14.0 Intel Corporation 8 Series/C220 Series Chipset Family USB xHCI [8086:8c31]
+-16.0 Intel Corporation 8 Series/C220 Series Chipset Family MEI Controller #1 [8086:8c3a]
+-1b.0 Intel Corporation 8 Series/C220 Series Chipset High Definition Audio Controller [8086:8c20]
+-1c.0-[02]--
+-1c.2-[03]----00.0 Broadcom Corporation BCM4360 802.11ac Wireless Network Adapter [14e4:43a0]
+-1c.3-[04]--+-00.0 Broadcom Corporation NetXtreme BCM57766 Gigabit Ethernet PCIe [14e4:1686]
| \-00.1 Broadcom Corporation BCM57765/57785 SDXC/MMC Card Reader [14e4:16bc]
+-1c.4-[05-ff]--
+-1f.0 Intel Corporation Z87 Express LPC Controller [8086:8c44]
+-1f.2 Intel Corporation 8 Series/C220 Series Chipset Family 6-port SATA Controller 1 [AHCI mode] [8086:8c02]
\-1f.3 Intel Corporation 8 Series/C220 Series Chipset Family SMBus Controller [8086:8c22]

Map (-M)

Dumped using pciutils v3.2.0 by Martin Mares. OS X port by THe KiNG. This version compiled by xsmile. View lspci map (M).txt File

00:00.0 Host bridge: Intel Corporation 4th Gen Core Processor DRAM Controller (rev 06)
00:01.0 PCI bridge: Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor PCI Express x16 Controller (rev 06)
## 00.01:0 is a bridge from 00 to 01-01
00:02.0 VGA compatible controller: Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor Integrated Graphics Controller (rev 06)
00:14.0 USB controller: Intel Corporation 8 Series/C220 Series Chipset Family USB xHCI (rev 05)
00:16.0 Communication controller: Intel Corporation 8 Series/C220 Series Chipset Family MEI Controller #1 (rev 05)
00:1b.0 Audio device: Intel Corporation 8 Series/C220 Series Chipset High Definition Audio Controller (rev 05)
00:1c.0 PCI bridge: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #1 (rev d5)
## 00.1c:0 is a bridge from 00 to 02-02
00:1c.2 PCI bridge: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #3 (rev d5)
## 00.1c:2 is a bridge from 00 to 03-03
00:1c.3 PCI bridge: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #4 (rev d5)
## 00.1c:3 is a bridge from 00 to 04-04
00:1c.4 PCI bridge: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #5 (rev d5)
## 00.1c:4 is a bridge from 00 to 05-ff
00:1f.0 ISA bridge: Intel Corporation Z87 Express LPC Controller (rev 05)
00:1f.2 SATA controller: Intel Corporation 8 Series/C220 Series Chipset Family 6-port SATA Controller 1 [AHCI mode] (rev 05)
00:1f.3 SMBus: Intel Corporation 8 Series/C220 Series Chipset Family SMBus Controller (rev 05)
01:00.0 VGA compatible controller: NVIDIA Corporation GK104M [GeForce GTX 775M Mac Edition] (rev a1)
01:00.1 Audio device: NVIDIA Corporation GK104 HDMI Audio Controller (rev a1)
03:00.0 Network controller: Broadcom Corporation BCM4360 802.11ac Wireless Network Adapter (rev 03)
04:00.0 Ethernet controller: Broadcom Corporation NetXtreme BCM57766 Gigabit Ethernet PCIe (rev 01)
04:00.1 SD Host controller: Broadcom Corporation BCM57765/57785 SDXC/MMC Card Reader (rev 01)
Summary of buses:
00: Primary host bus
1c.4 Bridge to 05-ff
1c.3 Bridge to 04-04
1c.2 Bridge to 03-03
1c.0 Bridge to 02-02
01.0 Bridge to 01-01
01: Entered via 00:01.0
03: Entered via 00:1c.2
04: Entered via 00:1c.3

Numbers & Names (-nnvv)

Dumped using pciutils v3.2.0 by Martin Mares. OS X port by THe KiNG. This version compiled by xsmile. View lspci (nnvv).txt File

00:00.0 Host bridge [0600]: Intel Corporation 4th Gen Core Processor DRAM Controller [8086:0c00] (rev 06)
Subsystem: Apple Inc. Device [106b:0123]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ >SERR- <PERR- INTx-
Latency: 0
Capabilities: [e0] Vendor Specific Information: Len=0c <?>
00:01.0 PCI bridge [0604]: Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor PCI Express x16 Controller [8086:0c01] (rev 06) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=01, subordinate=01, sec-latency=0
I/O behind bridge: 00001000-00001fff
Memory behind bridge: b0000000-b10fffff
Prefetchable memory behind bridge: 0000007f80000000-0000007f91ffffff
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [88] Subsystem: Apple Inc. Device [106b:0123]
Capabilities: [80] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [90] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [a0] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 256 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 256 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr- TransPend-
LnkCap: Port #2, Speed 8GT/s, Width x16, ASPM L0s L1, Latency L0 <256ns, L1 <8us
ClockPM- Surprise- LLActRep- BwNot+
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x16, TrErr- Train+ SlotClk+ DLActive- BWMgmt+ ABWMgmt+
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
Slot #1, PowerLimit 75.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
Changed: MRL- PresDet- LinkState-
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Not Supported, TimeoutDis- ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 8GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -3.5dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete+, EqualizationPhase1+
EqualizationPhase2+, EqualizationPhase3+, LinkEqualizationRequest-
00:02.0 VGA compatible controller [0300]: Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor Integrated Graphics Controller [8086:0412] (rev 06) (prog-if 00 [VGA controller])
Subsystem: Apple Inc. Device [106b:0123]
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin A routed to IRQ 16
Region 0: Memory at b1400000 (64-bit, non-prefetchable)
Region 2: Memory at 7f98000000 (64-bit, prefetchable)
Region 4: I/O ports at 2000
Capabilities: [90] MSI: Enable+ Count=1/1 Maskable- 64bit-
Address: fee00000 Data: 4075
Capabilities: [d0] Power Management version 2
Flags: PMEClk- DSI+ D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [a4] PCI Advanced Features
AFCap: TP+ FLR+
AFCtrl: FLR-
AFStatus: TP-
00:14.0 USB controller [0c03]: Intel Corporation 8 Series/C220 Series Chipset Family USB xHCI [8086:8c31] (rev 05) (prog-if 30 [XHCI])
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin A routed to IRQ 16
Region 0: Memory at b1c00000 (64-bit, non-prefetchable)
Capabilities: [70] Power Management version 2
Flags: PMEClk- DSI- D1- D2- AuxCurrent=375mA PME(D0-,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [80] MSI: Enable+ Count=1/8 Maskable- 64bit+
Address: 00000000fee00000 Data: 4072
00:16.0 Communication controller [0780]: Intel Corporation 8 Series/C220 Series Chipset Family MEI Controller #1 [8086:8c3a] (rev 05)
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin A routed to IRQ 16
Region 0: Memory at b1c15900 (64-bit, non-prefetchable)
Capabilities: [50] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [8c] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 4073
00:1b.0 Audio device [0403]: Intel Corporation 8 Series/C220 Series Chipset High Definition Audio Controller [8086:8c20] (rev 05)
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Interrupt: pin A routed to IRQ 22
Region 0: Memory at b1c10000 (64-bit, non-prefetchable)
Capabilities: [50] Power Management version 2
Flags: PMEClk- DSI- D1- D2- AuxCurrent=55mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [60] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 4074
Capabilities: [70] Express (v1) Root Complex Integrated Endpoint, MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE- FLReset+
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #0, Speed unknown, Width x0, ASPM unknown, Latency L0 <64ns, L1 <1us
ClockPM- Surprise- LLActRep- BwNot-
LnkCtl: ASPM Disabled; Disabled- Retrain- CommClk-
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed unknown, Width x0, TrErr- Train- SlotClk- DLActive- BWMgmt- ABWMgmt-
00:1c.0 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #1 [8086:8c10] (rev d5) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=02, subordinate=02, sec-latency=0
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [40] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #1, Speed 5GT/s, Width x2, ASPM L0s L1, Latency L0 <1us, L1 <4us
ClockPM- Surprise- LLActRep+ BwNot+
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk-
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x0, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug+ Surprise+
Slot #0, PowerLimit 0.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet- Interlock-
Changed: MRL- PresDet- LinkState-
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Range ABC, TimeoutDis+ ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
Capabilities: [80] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [90] Subsystem: Intel Corporation Device [8086:7270]
Capabilities: [a0] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
00:1c.2 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #3 [8086:8c14] (rev d5) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=03, subordinate=03, sec-latency=0
Memory behind bridge: b1800000-b1afffff
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [40] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal+ Fatal+ Unsupported+
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #3, Speed 5GT/s, Width x1, ASPM L0s L1, Latency L0 <512ns, L1 <16us
ClockPM- Surprise- LLActRep+ BwNot+
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive+ BWMgmt+ ABWMgmt-
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
Slot #2, PowerLimit 10.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
Changed: MRL- PresDet- LinkState-
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Range ABC, TimeoutDis+ ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
Capabilities: [80] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [90] Subsystem: Intel Corporation Device [8086:7270]
Capabilities: [a0] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
00:1c.3 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #4 [8086:8c16] (rev d5) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=04, subordinate=04, sec-latency=0
Prefetchable memory behind bridge: 0000007f92000000-0000007f920fffff
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [40] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal+ Fatal+ Unsupported+
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr+ UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #4, Speed 5GT/s, Width x1, ASPM L0s L1, Latency L0 <512ns, L1 <16us
ClockPM- Surprise- LLActRep+ BwNot+
LnkCtl: ASPM L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive+ BWMgmt+ ABWMgmt-
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
Slot #3, PowerLimit 10.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
Changed: MRL- PresDet- LinkState-
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Range ABC, TimeoutDis+ ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
Capabilities: [80] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [90] Subsystem: Intel Corporation Device [8086:7270]
Capabilities: [a0] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
00:1c.4 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #5 [8086:8c18] (rev d5) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=05, subordinate=ff, sec-latency=0
I/O behind bridge: 00003000-0000dfff
Memory behind bridge: b1d00000-dfffffff
Prefetchable memory behind bridge: 0000007fa0000000-0000007fffffffff
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [40] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal+ Fatal+ Unsupported+
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #5, Speed 5GT/s, Width x4, ASPM L0s L1, Latency L0 <1us, L1 <16us
ClockPM- Surprise- LLActRep+ BwNot+
LnkCtl: ASPM Disabled; RCB 64 bytes Disabled+ Retrain- CommClk-
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 5GT/s, Width x4, TrErr- Train- SlotClk+ DLActive- BWMgmt+ ABWMgmt-
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
Slot #4, PowerLimit 25.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
Changed: MRL- PresDet- LinkState+
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Range ABC, TimeoutDis+ ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
Capabilities: [80] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [90] Subsystem: Intel Corporation Device [8086:7270]
Capabilities: [a0] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D3 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
00:1f.0 ISA bridge [0601]: Intel Corporation Z87 Express LPC Controller [8086:8c44] (rev 05)
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Capabilities: [e0] Vendor Specific Information: Len=0c <?>
00:1f.2 SATA controller [0106]: Intel Corporation 8 Series/C220 Series Chipset Family 6-port SATA Controller 1 [AHCI mode] [8086:8c02] (rev 05) (prog-if 01 [AHCI 1.0])
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz+ UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin B routed to IRQ 19
Region 0: I/O ports at 2088
Region 1: I/O ports at 2094
Region 2: I/O ports at 2080
Region 3: I/O ports at 2090
Region 4: I/O ports at 2060
Region 5: Memory at b1c15000 (32-bit, non-prefetchable)
Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
Address: fee00000 Data: 4076
Capabilities: [70] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot+,D3cold-)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [a8] SATA HBA v1.0 BAR4 Offset=00000004
00:1f.3 SMBus [0c05]: Intel Corporation 8 Series/C220 Series Chipset Family SMBus Controller [8086:8c22] (rev 05)
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O+ Mem- BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap- 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Interrupt: pin C routed to IRQ 18
Region 0: Memory at b1c15800 (64-bit, non-prefetchable) [disabled]
Region 4: I/O ports at efa0
01:00.0 VGA compatible controller [0300]: NVIDIA Corporation GK104M [GeForce GTX 775M Mac Edition] [10de:119d] (rev a1) (prog-if 00 [VGA controller])
Subsystem: Apple Inc. Device [106b:0120]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin A routed to IRQ 16
Region 0: Memory at b0000000 (32-bit, non-prefetchable)
Region 1: Memory at 7f80000000 (64-bit, prefetchable)
Region 3: Memory at 7f90000000 (64-bit, prefetchable)
Region 5: I/O ports at 1000 [disabled]
Capabilities: [60] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [68] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 4079
Capabilities: [78] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 256 bytes, PhantFunc 0, Latency L0s unlimited, L1 <64us
ExtTag+ AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag+ PhantFunc- AuxPwr- NoSnoop+
MaxPayload 256 bytes, MaxReadReq 512 bytes
DevSta: CorrErr+ UncorrErr- FatalErr- UnsuppReq+ AuxPwr- TransPend-
LnkCap: Port #0, Speed 8GT/s, Width x16, ASPM L0s L1, Latency L0 <512ns, L1 <16us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x16, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range AB, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 8GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete+, EqualizationPhase1+
EqualizationPhase2+, EqualizationPhase3+, LinkEqualizationRequest+
Capabilities: [b4] Vendor Specific Information: Len=14 <?>
01:00.1 Audio device [0403]: NVIDIA Corporation GK104 HDMI Audio Controller [10de:0e0a] (rev a1)
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Interrupt: pin B routed to IRQ 17
Region 0: Memory at b1080000 (32-bit, non-prefetchable)
Capabilities: [60] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [68] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 407a
Capabilities: [78] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 256 bytes, PhantFunc 0, Latency L0s unlimited, L1 <64us
ExtTag+ AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag+ PhantFunc- AuxPwr- NoSnoop+
MaxPayload 256 bytes, MaxReadReq 512 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr- TransPend-
LnkCap: Port #0, Speed 8GT/s, Width x16, ASPM L0s L1, Latency L0 <512ns, L1 <4us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk-
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x16, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range AB, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete+, EqualizationPhase1+
EqualizationPhase2+, EqualizationPhase3+, LinkEqualizationRequest+
03:00.0 Network controller [0280]: Broadcom Corporation BCM4360 802.11ac Wireless Network Adapter [14e4:43a0] (rev 03)
Subsystem: Apple Inc. Device [106b:0111]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort+ <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Interrupt: pin A routed to IRQ 18
Region 0: Memory at b1a00000 (64-bit, non-prefetchable)
Region 2: Memory at b1800000 (64-bit, non-prefetchable)
Capabilities: [48] Power Management version 3
Flags: PMEClk- DSI- D1+ D2+ AuxCurrent=0mA PME(D0+,D1+,D2+,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable+ DSel=0 DScale=2 PME-
Capabilities: [58] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 407b
Capabilities: [68] Vendor Specific Information: Len=44 <?>
Capabilities: [ac] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 256 bytes, PhantFunc 0, Latency L0s <4us, L1 unlimited
ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
MaxPayload 128 bytes, MaxReadReq 1024 bytes
DevSta: CorrErr- UncorrErr+ FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #0, Speed 2.5GT/s, Width x1, ASPM L0s L1, Latency L0 <2us, L1 <32us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range ABCD, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
04:00.0 Ethernet controller [0200]: Broadcom Corporation NetXtreme BCM57766 Gigabit Ethernet PCIe [14e4:1686] (rev 01)
Subsystem: Broadcom Corporation NetXtreme BCM57766 Gigabit Ethernet PCIe [14e4:1686]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Interrupt: pin A routed to IRQ 19
Region 0: Memory at 7f92000000 (64-bit, prefetchable)
Region 2: Memory at 7f92010000 (64-bit, prefetchable)
Capabilities: [48] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable+ DSel=0 DScale=1 PME-
Capabilities: [50] Vital Product Data
Not readable
Capabilities: [58] MSI: Enable+ Count=1/8 Maskable- 64bit+
Address: 00000000fee00000 Data: 4077
Capabilities: [a0] MSI-X: Enable- Count=6 Masked-
Vector table: BAR=2 offset=00000000
PBA: BAR=2 offset=00000120
Capabilities: [ac] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
MaxPayload 128 bytes, MaxReadReq 4096 bytes
DevSta: CorrErr+ UncorrErr- FatalErr- UnsuppReq+ AuxPwr+ TransPend-
LnkCap: Port #0, Speed 2.5GT/s, Width x1, ASPM L0s L1, Latency L0 <2us, L1 <64us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range ABCD, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
04:00.1 SD Host controller [0805]: Broadcom Corporation BCM57765/57785 SDXC/MMC Card Reader [14e4:16bc] (rev 01) (prog-if 01)
Subsystem: Broadcom Corporation Device [14e4:0000]
Control: I/O- Mem+ BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Interrupt: pin B routed to IRQ 16
Region 0: Memory at 7f92020000 (64-bit, prefetchable)
Capabilities: [48] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D3 NoSoftRst+ PME-Enable+ DSel=0 DScale=1 PME-
Capabilities: [58] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 4078
Capabilities: [ac] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
MaxPayload 128 bytes, MaxReadReq 4096 bytes
DevSta: CorrErr+ UncorrErr+ FatalErr- UnsuppReq+ AuxPwr+ TransPend-
LnkCap: Port #0, Speed 2.5GT/s, Width x1, ASPM L0s L1, Latency L0 <2us, L1 <64us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range ABCD, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-

Bus centric view - Extended hex dump (-nnvvbxxxx)

Dumped using pciutils v3.2.0 by Martin Mares. OS X port by THe KiNG. This version compiled by xsmile. View lspci detailed (nnvvbxxxx).txt File

00:00.0 Host bridge [0600]: Intel Corporation 4th Gen Core Processor DRAM Controller [8086:0c00] (rev 06)
Subsystem: Apple Inc. Device [106b:0123]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ >SERR- <PERR- INTx-
Latency: 0
Capabilities: [e0] Vendor Specific Information: Len=0c <?>
00: 86 80 00 0c 06 00 90 20 06 00 00 06 00 00 00 00
10: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 6b 10 23 01
30: 00 00 00 00 e0 00 00 00 00 00 00 00 00 00 00 00
40: 01 90 d1 fe 00 00 00 00 01 00 d1 fe 00 00 00 00
50: 09 02 00 00 19 00 00 00 17 00 90 8f 01 00 00 8d
60: 01 00 00 e0 00 00 00 00 01 80 d1 fe 00 00 00 00
70: 00 00 00 ff 01 00 00 00 00 0c 00 ff 7f 00 00 00
80: 00 00 00 00 00 00 00 00 1a 00 00 00 00 00 00 00
90: 01 00 00 ff 01 00 00 00 01 00 50 6f 02 00 00 00
a0: 01 00 00 00 02 00 00 00 01 00 60 6f 02 00 00 00
b0: 01 00 a0 8d 01 00 80 8d 01 00 00 8d 01 00 a0 8f
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
e0: 09 00 0c 01 6d a0 04 62 d0 00 44 44 00 00 00 00
f0: 00 00 00 00 c8 0f 03 00 00 00 00 00 00 00 00 00
00:01.0 PCI bridge [0604]: Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor PCI Express x16 Controller [8086:0c01] (rev 06) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=01, subordinate=01, sec-latency=0
I/O behind bridge: 00001000-00001fff
Memory behind bridge: b0000000-b10fffff
Prefetchable memory behind bridge: 0000007f80000000-0000007f91ffffff
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [88] Subsystem: Apple Inc. Device [106b:0123]
Capabilities: [80] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [90] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [a0] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 256 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 256 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr- TransPend-
LnkCap: Port #2, Speed 8GT/s, Width x16, ASPM L0s L1, Latency L0 <256ns, L1 <8us
ClockPM- Surprise- LLActRep- BwNot+
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x16, TrErr- Train+ SlotClk+ DLActive- BWMgmt+ ABWMgmt+
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
Slot #1, PowerLimit 75.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
Changed: MRL- PresDet- LinkState-
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Not Supported, TimeoutDis- ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 8GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -3.5dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete+, EqualizationPhase1+
EqualizationPhase2+, EqualizationPhase3+, LinkEqualizationRequest-
00: 86 80 01 0c 07 00 10 00 06 00 04 06 40 00 81 00
10: 00 00 00 00 00 00 00 00 00 01 01 00 10 10 00 20
20: 00 b0 00 b1 01 80 f1 91 7f 00 00 00 7f 00 00 00
30: 00 00 00 00 88 00 00 00 00 00 00 00 10 01 00 00
40: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
50: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 0a
80: 01 90 03 c8 08 00 00 00 0d 80 00 00 6b 10 23 01
90: 05 a0 00 00 00 00 00 00 00 00 00 00 00 00 00 00
a0: 10 00 42 01 01 80 00 00 20 00 00 00 03 ad 61 02
b0: 43 00 01 d9 80 25 0c 00 00 00 40 00 00 00 00 00
c0: 00 00 00 00 80 0b 08 00 00 64 00 00 0e 00 00 00
d0: 43 00 1e 00 00 00 00 00 00 00 00 00 00 00 00 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 60 01 d0 4e 01 01 40 00 00 00 00 00 00 10 00
00:02.0 VGA compatible controller [0300]: Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor Integrated Graphics Controller [8086:0412] (rev 06) (prog-if 00 [VGA controller])
Subsystem: Apple Inc. Device [106b:0123]
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin A routed to IRQ 16
Region 0: Memory at b1400000 (64-bit, non-prefetchable)
Region 2: Memory at 7f98000000 (64-bit, prefetchable)
Region 4: I/O ports at 2000
Capabilities: [90] MSI: Enable+ Count=1/1 Maskable- 64bit-
Address: fee00000 Data: 4075
Capabilities: [d0] Power Management version 2
Flags: PMEClk- DSI+ D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [a4] PCI Advanced Features
AFCap: TP+ FLR+
AFCtrl: FLR-
AFStatus: TP-
00: 86 80 12 04 07 04 90 00 06 00 00 03 00 00 00 00
10: 04 00 40 b1 00 00 00 00 0c 00 00 98 7f 00 00 00
20: 01 20 00 00 00 00 00 00 00 00 00 00 6b 10 23 01
30: 00 00 00 00 90 00 00 00 00 00 00 00 10 01 00 00
40: 09 00 0c 01 6d a0 04 62 d0 00 44 44 00 00 00 00
50: 09 02 00 00 19 00 00 00 00 00 00 00 01 00 a0 8d
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
90: 05 d0 01 00 00 00 e0 fe 75 40 00 00 00 00 00 00
a0: 00 00 00 00 13 00 06 03 00 00 00 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 01 a4 22 00 00 00 00 00 00 00 00 00 00 00 00 00
e0: 00 00 00 00 00 00 00 00 00 80 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 00 00 06 00 90 81 d1 8c
00:14.0 USB controller [0c03]: Intel Corporation 8 Series/C220 Series Chipset Family USB xHCI [8086:8c31] (rev 05) (prog-if 30 [XHCI])
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin A routed to IRQ 16
Region 0: Memory at b1c00000 (64-bit, non-prefetchable)
Capabilities: [70] Power Management version 2
Flags: PMEClk- DSI- D1- D2- AuxCurrent=375mA PME(D0-,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [80] MSI: Enable+ Count=1/8 Maskable- 64bit+
Address: 00000000fee00000 Data: 4072
00: 86 80 31 8c 06 04 90 02 05 30 03 0c 00 00 00 00
10: 04 00 c0 b1 00 00 00 00 00 00 00 00 00 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 86 80 70 72
30: 00 00 00 00 70 00 00 00 00 00 00 00 10 01 00 00
40: fd 01 36 80 89 c6 0f 80 00 00 00 00 00 00 00 00
50: 9f 6e 88 07 00 00 00 00 00 00 00 00 00 00 00 00
60: 30 20 00 00 00 00 00 00 00 00 00 00 00 00 00 00
70: 01 80 c2 c1 08 00 00 00 00 00 00 00 00 00 00 00
80: 05 00 87 00 00 00 e0 fe 00 00 00 00 72 40 00 00
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
a0: 40 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00
b0: 0f 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 01 02 00 00 01 02 00 00 01 10 00 00 02 20 00 00
d0: ff 3f 00 00 ff 3f 00 00 3f 00 00 00 3f 00 00 00
e0: a0 00 00 00 00 00 00 00 00 00 00 00 d8 d8 d8 08
f0: 00 00 00 00 00 00 00 00 b1 0f 06 08 00 00 00 00
00:16.0 Communication controller [0780]: Intel Corporation 8 Series/C220 Series Chipset Family MEI Controller #1 [8086:8c3a] (rev 05)
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin A routed to IRQ 16
Region 0: Memory at b1c15900 (64-bit, non-prefetchable)
Capabilities: [50] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [8c] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 4073
00: 86 80 3a 8c 06 04 10 00 05 00 80 07 00 00 80 00
10: 04 59 c1 b1 00 00 00 00 00 00 00 00 00 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 86 80 70 72
30: 00 00 00 00 50 00 00 00 00 00 00 00 10 01 00 00
40: 55 02 00 1e 10 00 01 80 06 23 00 66 f0 1f 00 10
50: 01 8c 03 c8 08 00 00 00 00 00 00 00 00 00 00 00
60: 00 02 00 00 00 00 00 00 00 00 00 00 00 00 00 00
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
80: 00 00 00 00 00 00 00 00 00 00 00 00 05 00 81 00
90: 00 00 e0 fe 00 00 00 00 73 40 00 00 00 00 00 00
a0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 02 00 00 c0
c0: 72 eb 06 21 6f e5 72 fa e2 d4 7a c6 cb e1 06 27
d0: 99 21 4c 5a a7 7a 3f c4 fe 96 38 8a 8b 08 7e 6f
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00:1b.0 Audio device [0403]: Intel Corporation 8 Series/C220 Series Chipset High Definition Audio Controller [8086:8c20] (rev 05)
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Interrupt: pin A routed to IRQ 22
Region 0: Memory at b1c10000 (64-bit, non-prefetchable)
Capabilities: [50] Power Management version 2
Flags: PMEClk- DSI- D1- D2- AuxCurrent=55mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [60] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 4074
Capabilities: [70] Express (v1) Root Complex Integrated Endpoint, MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE- FLReset+
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #0, Speed unknown, Width x0, ASPM unknown, Latency L0 <64ns, L1 <1us
ClockPM- Surprise- LLActRep- BwNot-
LnkCtl: ASPM Disabled; Disabled- Retrain- CommClk-
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed unknown, Width x0, TrErr- Train- SlotClk- DLActive- BWMgmt- ABWMgmt-
00: 86 80 20 8c 06 04 10 00 05 00 03 04 40 00 00 00
10: 04 00 c1 b1 00 00 00 00 00 00 00 00 00 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 86 80 70 72
30: 00 00 00 00 50 00 00 00 00 00 00 00 16 01 00 00
40: 03 00 00 17 00 00 00 00 00 00 00 00 00 80 00 00
50: 01 60 42 c8 00 00 00 00 00 00 00 00 00 00 00 00
60: 05 70 81 00 00 00 e0 fe 00 00 00 00 74 40 00 00
70: 10 00 91 00 00 00 00 10 00 00 10 00 00 00 00 00
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
a0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 04 02 01 00 60 00 80 00 0c 85 82 10 00 31 02
d0: 00 0c 85 02 10 00 33 02 00 00 00 00 00 00 00 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 b1 0f 06 08 00 00 00 00
00:1c.0 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #1 [8086:8c10] (rev d5) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=02, subordinate=02, sec-latency=0
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [40] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #1, Speed 5GT/s, Width x2, ASPM L0s L1, Latency L0 <1us, L1 <4us
ClockPM- Surprise- LLActRep+ BwNot+
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk-
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x0, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug+ Surprise+
Slot #0, PowerLimit 0.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet- Interlock-
Changed: MRL- PresDet- LinkState-
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Range ABC, TimeoutDis+ ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
Capabilities: [80] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [90] Subsystem: Intel Corporation Device [8086:7270]
Capabilities: [a0] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
00: 86 80 10 8c 07 00 10 00 d5 00 04 06 40 00 81 00
10: 00 00 00 00 00 00 00 00 00 02 02 00 f0 00 00 20
20: f0 ff 00 00 f1 ff 01 00 00 00 00 00 00 00 00 00
30: 00 00 00 00 40 00 00 00 00 00 00 00 10 01 00 00
40: 10 80 42 01 00 80 00 00 00 00 10 00 22 4c 31 01
50: 03 00 01 10 60 00 04 00 00 00 00 00 00 00 00 00
60: 00 00 00 00 17 08 08 00 00 04 00 00 00 00 00 00
70: 02 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00
80: 05 90 00 00 00 00 00 00 00 00 00 00 00 00 00 00
90: 0d a0 00 00 86 80 70 72 00 00 00 00 00 00 00 00
a0: 01 00 03 c8 00 00 00 00 00 00 00 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 01 02 08 00 00 00 00 11 09 00 00 00 00
e0: 00 3f 00 00 00 00 00 00 03 00 00 00 00 00 00 00
f0: 50 00 00 00 80 f5 00 00 b1 0f 06 08 00 68 55 01
00:1c.2 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #3 [8086:8c14] (rev d5) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=03, subordinate=03, sec-latency=0
Memory behind bridge: b1800000-b1afffff
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [40] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal+ Fatal+ Unsupported+
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #3, Speed 5GT/s, Width x1, ASPM L0s L1, Latency L0 <512ns, L1 <16us
ClockPM- Surprise- LLActRep+ BwNot+
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive+ BWMgmt+ ABWMgmt-
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
Slot #2, PowerLimit 10.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
Changed: MRL- PresDet- LinkState-
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Range ABC, TimeoutDis+ ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
Capabilities: [80] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [90] Subsystem: Intel Corporation Device [8086:7270]
Capabilities: [a0] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
00: 86 80 14 8c 07 00 10 00 d5 00 04 06 40 00 81 00
10: 00 00 00 00 00 00 00 00 00 03 03 00 f0 00 00 20
20: 80 b1 a0 b1 f1 ff 01 00 ff ff ff ff 00 00 00 00
30: 00 00 00 00 40 00 00 00 00 00 00 00 12 03 00 00
40: 10 80 42 01 00 80 00 00 0e 00 10 00 12 3c 32 03
50: 43 00 11 70 00 b2 14 00 00 00 40 00 00 00 00 00
60: 00 00 00 00 17 08 00 00 00 04 00 00 00 00 00 00
70: 01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00
80: 05 90 00 00 00 00 00 00 00 00 00 00 00 00 00 00
90: 0d a0 00 00 86 80 70 72 00 00 00 00 00 00 00 00
a0: 01 00 03 c8 00 00 00 00 00 00 00 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 01 42 18 00 00 08 80 11 0b 00 00 00 00
e0: 00 03 00 00 03 90 03 90 13 00 00 00 00 00 00 00
f0: 50 00 00 00 40 00 00 0c b1 0f 06 08 00 28 00 03
00:1c.3 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #4 [8086:8c16] (rev d5) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=04, subordinate=04, sec-latency=0
Prefetchable memory behind bridge: 0000007f92000000-0000007f920fffff
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [40] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal+ Fatal+ Unsupported+
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr+ UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #4, Speed 5GT/s, Width x1, ASPM L0s L1, Latency L0 <512ns, L1 <16us
ClockPM- Surprise- LLActRep+ BwNot+
LnkCtl: ASPM L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive+ BWMgmt+ ABWMgmt-
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
Slot #3, PowerLimit 10.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
Changed: MRL- PresDet- LinkState-
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Range ABC, TimeoutDis+ ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
Capabilities: [80] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [90] Subsystem: Intel Corporation Device [8086:7270]
Capabilities: [a0] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
00: 86 80 16 8c 07 00 10 00 d5 00 04 06 40 00 81 00
10: 00 00 00 00 00 00 00 00 00 04 04 00 f0 00 00 20
20: f0 ff 00 00 01 92 01 92 7f 00 00 00 7f 00 00 00
30: 00 00 00 00 40 00 00 00 00 00 00 00 13 04 00 00
40: 10 80 42 01 00 80 00 00 0e 00 11 00 12 3c 32 04
50: 42 00 11 70 00 b2 1c 00 00 00 40 00 00 00 00 00
60: 00 00 00 00 17 08 00 00 00 04 00 00 00 00 00 00
70: 02 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00
80: 05 90 00 00 00 00 00 00 00 00 00 00 00 00 00 00
90: 0d a0 00 00 86 80 70 72 00 00 00 00 00 00 00 00
a0: 01 00 03 c8 00 00 00 00 00 00 00 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 01 42 18 00 00 08 80 11 0b 00 00 00 00
e0: 00 03 00 00 00 00 00 00 11 00 00 00 00 00 00 00
f0: 50 00 00 00 40 00 00 0c b1 0f 06 08 00 28 00 04
00:1c.4 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #5 [8086:8c18] (rev d5) (prog-if 00 [Normal decode])
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Bus: primary=00, secondary=05, subordinate=ff, sec-latency=0
I/O behind bridge: 00003000-0000dfff
Memory behind bridge: b1d00000-dfffffff
Prefetchable memory behind bridge: 0000007fa0000000-0000007fffffffff
Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
BridgeCtl: Parity- SERR- NoISA- VGA- MAbort- >Reset- FastB2B-
PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
Capabilities: [40] Express (v2) Root Port (Slot+), MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <64ns, L1 <1us
ExtTag- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal+ Fatal+ Unsupported+
RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
MaxPayload 128 bytes, MaxReadReq 128 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #5, Speed 5GT/s, Width x4, ASPM L0s L1, Latency L0 <1us, L1 <16us
ClockPM- Surprise- LLActRep+ BwNot+
LnkCtl: ASPM Disabled; RCB 64 bytes Disabled+ Retrain- CommClk-
ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 5GT/s, Width x4, TrErr- Train- SlotClk+ DLActive- BWMgmt+ ABWMgmt-
SltCap: AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
Slot #4, PowerLimit 25.000W; Interlock- NoCompl+
SltCtl: Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
SltSta: Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
Changed: MRL- PresDet- LinkState+
RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
RootCap: CRSVisible-
RootSta: PME ReqID 0000, PMEStatus- PMEPending-
DevCap2: Completion Timeout: Range ABC, TimeoutDis+ ARIFwd-
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
Capabilities: [80] MSI: Enable- Count=1/1 Maskable- 64bit-
Address: 00000000 Data: 0000
Capabilities: [90] Subsystem: Intel Corporation Device [8086:7270]
Capabilities: [a0] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D3 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
00: 86 80 18 8c 07 00 10 00 d5 00 04 06 40 00 81 00
10: 00 00 00 00 00 00 00 00 00 05 ff 00 30 d0 00 20
20: d0 b1 f0 df 01 a0 f1 ff 7f 00 00 00 7f 00 00 00
30: 00 00 00 00 40 00 00 00 00 00 00 00 10 01 00 00
40: 10 80 42 01 00 80 00 00 0e 00 10 00 42 4c 32 05
50: 10 00 42 50 00 fd 24 00 00 00 40 01 00 00 00 00
60: 00 00 00 00 17 08 00 00 00 00 00 00 00 00 00 00
70: 02 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
80: 05 90 00 00 00 00 00 00 00 00 00 00 00 00 00 00
90: 0d a0 00 00 86 80 70 72 00 00 00 00 00 00 00 00
a0: 01 00 03 c8 03 00 00 00 00 00 00 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 01 42 18 00 00 08 80 11 0b 00 00 00 00
e0: 00 3f 00 00 00 00 00 00 01 00 00 00 00 00 00 00
f0: 50 00 00 00 40 00 00 00 b1 0f 06 08 00 e8 00 05
00:1f.0 ISA bridge [0601]: Intel Corporation Z87 Express LPC Controller [8086:8c44] (rev 05)
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Capabilities: [e0] Vendor Specific Information: Len=0c <?>
00: 86 80 44 8c 07 00 10 02 05 00 01 06 00 00 80 00
10: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 86 80 70 72
30: 00 00 00 00 e0 00 00 00 00 00 00 00 00 00 00 00
40: 01 04 00 00 80 00 00 00 01 08 00 00 10 00 00 00
50: f8 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
60: 80 80 80 80 d0 00 00 00 80 80 80 80 f8 f0 00 00
70: 78 f0 78 f0 78 f0 78 f0 78 f0 78 f0 78 f0 78 f0
80: 70 00 0f 3f 81 06 0c 00 00 00 00 00 01 03 1c 00
90: 01 07 fc 00 00 00 00 00 01 00 f0 fe 00 00 00 00
a0: 08 5a a0 60 09 1c 06 00 00 46 00 00 00 00 00 80
b0: 00 00 00 00 00 00 00 00 80 8a 00 28 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 33 22 11 00 67 45 00 00 c0 ff 00 00 08 00 00 00
e0: 09 00 0c 10 00 00 00 00 01 e8 00 91 00 00 00 00
f0: 01 c0 d1 fe 00 00 00 00 b1 0f 06 08 00 00 00 00
00:1f.2 SATA controller [0106]: Intel Corporation 8 Series/C220 Series Chipset Family 6-port SATA Controller 1 [AHCI mode] [8086:8c02] (rev 05) (prog-if 01 [AHCI 1.0])
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz+ UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin B routed to IRQ 19
Region 0: I/O ports at 2088
Region 1: I/O ports at 2094
Region 2: I/O ports at 2080
Region 3: I/O ports at 2090
Region 4: I/O ports at 2060
Region 5: Memory at b1c15000 (32-bit, non-prefetchable)
Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
Address: fee00000 Data: 4076
Capabilities: [70] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot+,D3cold-)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [a8] SATA HBA v1.0 BAR4 Offset=00000004
00: 86 80 02 8c 07 04 b0 02 05 01 06 01 00 00 00 00
10: 89 20 00 00 95 20 00 00 81 20 00 00 91 20 00 00
20: 61 20 00 00 00 50 c1 b1 00 00 00 00 86 80 70 72
30: 00 00 00 00 80 00 00 00 00 00 00 00 13 02 00 00
40: 00 80 00 80 00 00 00 00 00 00 00 00 00 00 00 00
50: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
70: 01 a8 03 40 08 00 00 00 00 00 00 00 00 00 00 00
80: 05 70 01 00 00 00 e0 fe 76 40 00 00 00 00 00 00
90: 60 3e 01 81 83 01 00 3e 20 02 5c 20 20 00 00 80
a0: a8 00 00 00 00 00 00 00 12 00 10 00 48 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 b1 0f 06 08 00 00 00 00
00:1f.3 SMBus [0c05]: Intel Corporation 8 Series/C220 Series Chipset Family SMBus Controller [8086:8c22] (rev 05)
Subsystem: Intel Corporation Device [8086:7270]
Control: I/O+ Mem- BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
Status: Cap- 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Interrupt: pin C routed to IRQ 18
Region 0: Memory at b1c15800 (64-bit, non-prefetchable) [disabled]
Region 4: I/O ports at efa0
00: 86 80 22 8c 01 00 80 02 05 00 05 0c 00 00 00 00
10: 04 58 c1 b1 00 00 00 00 00 00 00 00 00 00 00 00
20: a1 ef 00 00 00 00 00 00 00 00 00 00 86 80 70 72
30: 00 00 00 00 00 00 00 00 00 00 00 00 12 03 00 00
40: 05 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
50: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
60: 03 04 04 00 00 00 08 08 00 00 00 00 00 00 00 00
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
80: 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
a0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 b1 0f 06 08 00 00 00 00
01:00.0 VGA compatible controller [0300]: NVIDIA Corporation GK104M [GeForce GTX 775M Mac Edition] [10de:119d] (rev a1) (prog-if 00 [VGA controller])
Subsystem: Apple Inc. Device [106b:0120]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0
Interrupt: pin A routed to IRQ 16
Region 0: Memory at b0000000 (32-bit, non-prefetchable)
Region 1: Memory at 7f80000000 (64-bit, prefetchable)
Region 3: Memory at 7f90000000 (64-bit, prefetchable)
Region 5: I/O ports at 1000 [disabled]
Capabilities: [60] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [68] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 4079
Capabilities: [78] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 256 bytes, PhantFunc 0, Latency L0s unlimited, L1 <64us
ExtTag+ AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag+ PhantFunc- AuxPwr- NoSnoop+
MaxPayload 256 bytes, MaxReadReq 512 bytes
DevSta: CorrErr+ UncorrErr- FatalErr- UnsuppReq+ AuxPwr- TransPend-
LnkCap: Port #0, Speed 8GT/s, Width x16, ASPM L0s L1, Latency L0 <512ns, L1 <16us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x16, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range AB, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 8GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete+, EqualizationPhase1+
EqualizationPhase2+, EqualizationPhase3+, LinkEqualizationRequest+
Capabilities: [b4] Vendor Specific Information: Len=14 <?>
00: de 10 9d 11 06 04 10 00 a1 00 00 03 00 00 80 00
10: 00 00 00 b0 0c 00 00 80 7f 00 00 00 0c 00 00 90
20: 7f 00 00 00 01 10 00 00 00 00 00 00 6b 10 20 01
30: 00 00 00 00 60 00 00 00 00 00 00 00 10 01 00 00
40: 6b 10 20 01 00 00 00 00 00 00 00 00 00 00 00 00
50: 01 00 00 00 00 00 00 00 ce d6 23 00 00 00 00 00
60: 01 68 03 00 08 00 00 00 05 78 81 00 00 00 e0 fe
70: 00 00 00 00 79 40 00 00 10 b4 02 00 e1 8d 2c 01
80: 30 29 09 00 03 3d 46 00 43 01 01 11 00 00 00 00
90: 00 00 00 00 00 00 00 00 00 00 00 00 13 00 00 00
a0: 00 00 00 00 0e 00 00 00 03 00 3f 00 00 00 00 00
b0: 00 00 00 00 09 00 14 01 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
01:00.1 Audio device [0403]: NVIDIA Corporation GK104 HDMI Audio Controller [10de:0e0a] (rev a1)
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Interrupt: pin B routed to IRQ 17
Region 0: Memory at b1080000 (32-bit, non-prefetchable)
Capabilities: [60] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
Capabilities: [68] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 407a
Capabilities: [78] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 256 bytes, PhantFunc 0, Latency L0s unlimited, L1 <64us
ExtTag+ AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag+ PhantFunc- AuxPwr- NoSnoop+
MaxPayload 256 bytes, MaxReadReq 512 bytes
DevSta: CorrErr- UncorrErr- FatalErr- UnsuppReq- AuxPwr- TransPend-
LnkCap: Port #0, Speed 8GT/s, Width x16, ASPM L0s L1, Latency L0 <512ns, L1 <4us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk-
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x16, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range AB, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete+, EqualizationPhase1+
EqualizationPhase2+, EqualizationPhase3+, LinkEqualizationRequest+
00: de 10 0a 0e 06 04 10 00 a1 00 03 04 40 00 80 00
10: 00 00 08 b1 00 00 00 00 00 00 00 00 00 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
30: 00 00 00 00 60 00 00 00 00 00 00 00 11 02 00 00
40: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
50: 00 00 00 00 00 00 00 00 ce d6 23 00 00 00 00 00
60: 01 68 03 00 08 00 00 00 05 78 81 00 00 00 e0 fe
70: 00 00 00 00 7a 40 00 00 10 00 02 00 e1 8d 2c 01
80: 30 29 00 00 03 3d 45 00 03 01 01 11 00 00 00 00
90: 00 00 00 00 00 00 00 00 00 00 00 00 13 00 00 00
a0: 00 00 00 00 0e 00 00 00 00 00 3f 00 00 00 00 00
b0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
03:00.0 Network controller [0280]: Broadcom Corporation BCM4360 802.11ac Wireless Network Adapter [14e4:43a0] (rev 03)
Subsystem: Apple Inc. Device [106b:0111]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort+ <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Interrupt: pin A routed to IRQ 18
Region 0: Memory at b1a00000 (64-bit, non-prefetchable)
Region 2: Memory at b1800000 (64-bit, non-prefetchable)
Capabilities: [48] Power Management version 3
Flags: PMEClk- DSI- D1+ D2+ AuxCurrent=0mA PME(D0+,D1+,D2+,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable+ DSel=0 DScale=2 PME-
Capabilities: [58] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 407b
Capabilities: [68] Vendor Specific Information: Len=44 <?>
Capabilities: [ac] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 256 bytes, PhantFunc 0, Latency L0s <4us, L1 unlimited
ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
MaxPayload 128 bytes, MaxReadReq 1024 bytes
DevSta: CorrErr- UncorrErr+ FatalErr- UnsuppReq- AuxPwr+ TransPend-
LnkCap: Port #0, Speed 2.5GT/s, Width x1, ASPM L0s L1, Latency L0 <2us, L1 <32us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L0s L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range ABCD, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
00: e4 14 a0 43 06 04 10 08 03 00 80 02 40 00 00 00
10: 04 00 a0 b1 00 00 00 00 04 00 80 b1 00 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 6b 10 11 01
30: 00 00 00 00 48 00 00 00 00 00 00 00 12 01 00 00
40: 00 00 00 00 00 00 00 00 01 58 03 fe 08 41 00 00
50: 00 00 00 00 00 00 00 00 05 68 81 00 00 00 e0 fe
60: 00 00 00 00 7b 40 00 00 09 ac 44 00 01 01 00 00
70: 00 10 10 18 00 00 00 00 00 00 00 00 00 00 00 00
80: 00 10 00 18 00 00 00 00 00 00 00 00 00 00 00 00
90: 04 00 00 00 00 02 00 00 00 00 00 00 00 00 00 00
a0: 00 00 00 00 00 00 00 00 40 00 03 00 10 00 02 00
b0: 81 8f 90 05 10 3c 12 00 11 dc 46 00 43 01 11 10
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 1f 08 08 00 00 04 00 00 00 00 00 00 01 00 01 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
04:00.0 Ethernet controller [0200]: Broadcom Corporation NetXtreme BCM57766 Gigabit Ethernet PCIe [14e4:1686] (rev 01)
Subsystem: Broadcom Corporation NetXtreme BCM57766 Gigabit Ethernet PCIe [14e4:1686]
Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Latency: 0, Cache Line Size: 256 bytes
Interrupt: pin A routed to IRQ 19
Region 0: Memory at 7f92000000 (64-bit, prefetchable)
Region 2: Memory at 7f92010000 (64-bit, prefetchable)
Capabilities: [48] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D0 NoSoftRst+ PME-Enable+ DSel=0 DScale=1 PME-
Capabilities: [50] Vital Product Data
Not readable
Capabilities: [58] MSI: Enable+ Count=1/8 Maskable- 64bit+
Address: 00000000fee00000 Data: 4077
Capabilities: [a0] MSI-X: Enable- Count=6 Masked-
Vector table: BAR=2 offset=00000000
PBA: BAR=2 offset=00000120
Capabilities: [ac] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
MaxPayload 128 bytes, MaxReadReq 4096 bytes
DevSta: CorrErr+ UncorrErr- FatalErr- UnsuppReq+ AuxPwr+ TransPend-
LnkCap: Port #0, Speed 2.5GT/s, Width x1, ASPM L0s L1, Latency L0 <2us, L1 <64us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range ABCD, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
00: e4 14 86 16 06 04 10 00 01 00 00 02 40 00 80 00
10: 0c 00 00 92 7f 00 00 00 0c 00 01 92 7f 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 e4 14 86 16
30: 00 00 00 00 48 00 00 00 00 00 00 00 13 01 00 00
40: 00 00 00 00 00 00 00 95 01 50 03 c8 08 21 00 16
50: 03 58 00 00 00 00 00 00 05 a0 87 00 00 00 e0 fe
60: 00 00 00 00 77 40 00 00 98 02 01 f0 d0 03 f8 01
70: 12 10 00 00 00 00 00 00 00 7c 00 00 00 00 00 00
80: 1a 00 60 16 f8 00 00 80 00 00 00 00 e1 03 00 00
90: 00 00 00 00 f8 01 00 00 00 00 00 00 df 01 00 00
a0: 11 ac 05 00 02 00 00 00 22 01 00 00 10 00 02 00
b0: 80 8d 90 05 10 5c 19 00 11 5c 47 00 42 01 11 10
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 1f 08 00 00 00 04 00 00 00 00 00 00 01 00 01 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 00 00 00 00 01 60 76 57
04:00.1 SD Host controller [0805]: Broadcom Corporation BCM57765/57785 SDXC/MMC Card Reader [14e4:16bc] (rev 01) (prog-if 01)
Subsystem: Broadcom Corporation Device [14e4:0000]
Control: I/O- Mem+ BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
Interrupt: pin B routed to IRQ 16
Region 0: Memory at 7f92020000 (64-bit, prefetchable)
Capabilities: [48] Power Management version 3
Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
Status: D3 NoSoftRst+ PME-Enable+ DSel=0 DScale=1 PME-
Capabilities: [58] MSI: Enable+ Count=1/1 Maskable- 64bit+
Address: 00000000fee00000 Data: 4078
Capabilities: [ac] Express (v2) Endpoint, MSI 00
DevCap: MaxPayload 128 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset-
DevCtl: Report errors: Correctable- Non-Fatal- Fatal- Unsupported-
RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
MaxPayload 128 bytes, MaxReadReq 4096 bytes
DevSta: CorrErr+ UncorrErr+ FatalErr- UnsuppReq+ AuxPwr+ TransPend-
LnkCap: Port #0, Speed 2.5GT/s, Width x1, ASPM L0s L1, Latency L0 <2us, L1 <64us
ClockPM+ Surprise- LLActRep- BwNot-
LnkCtl: ASPM L1 Enabled; RCB 64 bytes Disabled- Retrain- CommClk+
ExtSynch- ClockPM+ AutWidDis- BWInt- AutBWInt-
LnkSta: Speed 2.5GT/s, Width x1, TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
DevCap2: Completion Timeout: Range ABCD, TimeoutDis+
DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-, Selectable De-emphasis: -6dB
Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
Compliance De-emphasis: -6dB
LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete-, EqualizationPhase1-
EqualizationPhase2-, EqualizationPhase3-, LinkEqualizationRequest-
00: e4 14 bc 16 02 04 10 00 01 01 05 08 40 00 80 00
10: 0c 00 02 92 7f 00 00 00 00 00 00 00 00 00 00 00
20: 00 00 00 00 00 00 00 00 00 00 00 00 e4 14 00 00
30: 00 00 00 00 48 00 00 00 00 00 00 00 10 02 00 00
40: 00 00 00 00 00 00 00 00 01 58 03 c8 0b 21 00 00
50: 00 00 00 00 00 00 00 00 05 ac 81 00 00 00 e0 fe
60: 00 00 00 00 78 40 00 00 00 00 00 00 00 00 00 00
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
a0: 00 00 00 00 00 00 00 00 00 00 00 00 10 00 02 00
b0: 80 8d 90 05 10 5c 1b 00 11 5c 47 00 42 01 11 10
c0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
d0: 1f 00 00 00 00 00 00 00 00 00 00 00 00 00 01 00
e0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
f0: 00 00 00 00 00 00 00 00 00 00 00 00 01 60 76 57

NVRAM
Apple Specific Vars (dumped using an amended version of Apple's nvram tool with the -hp option)

View nvram_hexdump.txt File

------------------------------------------------------------------------------
efi-boot-device-data
------------------------------------------------------------------------------
000000: 02 01 0c 00 d0 41 03 0a 00 00 00 00 01 01 06 00 |.....A..........|
000010: 02 1f 03 12 0a 00 00 00 00 00 00 00 04 01 2a 00 |..............*.|
000020: 02 00 00 00 28 40 06 00 00 00 00 00 40 ce 56 74 |....(@......@.Vt|
000030: 00 00 00 00 e0 3d 00 00 82 08 00 00 8f 5b 00 00 |.....=.......[..|
000040: fd 01 00 00 02 02 7f ff 04 00 |..........|
------------------------------------------------------------------------------
backlight-level
------------------------------------------------------------------------------
000000: df 2c |.,|
------------------------------------------------------------------------------
efi-boot-device
------------------------------------------------------------------------------
000000: 3c 61 72 72 61 79 3e 3c 64 69 63 74 3e 3c 6b 65 |<array><dict><ke|
000010: 79 3e 49 4f 4d 61 74 63 68 3c 2f 6b 65 79 3e 3c |y>IOMatch</key><|
000020: 64 69 63 74 3e 3c 6b 65 79 3e 49 4f 50 72 6f 76 |dict><key>IOProv|
000030: 69 64 65 72 43 6c 61 73 73 3c 2f 6b 65 79 3e 3c |iderClass</key><|
000040: 73 74 72 69 6e 67 3e 49 4f 4d 65 64 69 61 3c 2f |string>IOMedia</|
000050: 73 74 72 69 6e 67 3e 3c 6b 65 79 3e 49 4f 50 72 |string><key>IOPr|
000060: 6f 70 65 72 74 79 4d 61 74 63 68 3c 2f 6b 65 79 |opertyMatch</key|
000070: 3e 3c 64 69 63 74 3e 3c 6b 65 79 3e 55 55 49 44 |><dict><key>UUID|
000080: 3c 2f 6b 65 79 3e 3c 73 74 72 69 6e 67 3e 30 30 |</key><string>00|
000090: 30 30 33 44 45 30 2d 30 38 38 32 2d 30 30 30 30 |003DE0-0882-0000|
0000a0: 2d 38 46 35 42 2d 30 30 30 30 46 44 30 31 30 30 |-8F5B-0000FD0100|
0000b0: 30 30 3c 2f 73 74 72 69 6e 67 3e 3c 2f 64 69 63 |00</string></dic|
0000c0: 74 3e 3c 2f 64 69 63 74 3e 3c 6b 65 79 3e 42 4c |t></dict><key>BL|
0000d0: 4c 61 73 74 42 53 44 4e 61 6d 65 3c 2f 6b 65 79 |LastBSDName</key|
0000e0: 3e 3c 73 74 72 69 6e 67 3e 64 69 73 6b 30 73 32 |><string>disk0s2|
0000f0: 3c 2f 73 74 72 69 6e 67 3e 3c 2f 64 69 63 74 3e |</string></dict>|
000100: 3c 2f 61 72 72 61 79 3e 00 |</array>.|
------------------------------------------------------------------------------
boot-gamma
------------------------------------------------------------------------------
000000: 10 06 00 00 05 b0 00 00 00 00 00 00 6e 00 00 00 |............n...|
000010: 00 00 00 00 07 00 04 04 db 05 0b 0b b2 0e 1e 1e |................|
000020: 95 24 36 36 6d 3e 57 57 4f 60 77 77 09 80 a1 a1 |.$66m>WWO`ww....|
000030: 87 a8 07 00 04 04 db 05 0b 0b b2 0e 1e 1e 95 24 |...............$|
000040: 36 36 6d 3e 57 57 4f 60 77 77 09 80 a1 a1 87 a8 |66m>WWO`ww......|
000050: 07 00 04 04 db 05 0b 0b b2 0e 1e 1e 95 24 36 36 |.............$66|
000060: 6d 3e 57 57 4f 60 77 77 09 80 a1 a1 87 a8 |m>WWO`ww......|
------------------------------------------------------------------------------
LocationServicesEnabled
------------------------------------------------------------------------------
000000: 01 |.|
------------------------------------------------------------------------------
display-config
------------------------------------------------------------------------------
000000: 00 00 25 01 73 08 ff ff 01 00 |..%.s.....|
------------------------------------------------------------------------------
EFIBluetoothDelay
------------------------------------------------------------------------------
000000: b8 0b |..|
------------------------------------------------------------------------------
fmm-mobileme-token-FMM
------------------------------------------------------------------------------
000000: 62 70 6c 69 73 74 30 30 d7 01 02 03 04 05 06 07 |bplist00........|
000010: 08 09 14 15 16 17 18 56 75 73 65 72 69 64 5f 10 |.......Vuserid_.|
000020: 13 64 61 74 61 63 6c 61 73 73 50 72 6f 70 65 72 |.dataclassProper|
000030: 74 69 65 73 59 61 75 74 68 54 6f 6b 65 6e 58 70 |tiesYauthTokenXp|
000040: 65 72 73 6f 6e 49 44 58 75 73 65 72 6e 61 6d 65 |ersonIDXusername|
000050: 5f 10 12 65 6e 61 62 6c 65 64 44 61 74 61 63 6c |_..enabledDatacl|
000060: 61 73 73 65 73 58 75 73 65 72 49 6e 66 6f 11 01 |assesXuserInfo..|
000070: f5 d1 0a 0b 5f 10 21 63 6f 6d 2e 61 70 70 6c 65 |...._.!com.apple|
000080: 2e 44 61 74 61 63 6c 61 73 73 2e 44 65 76 69 63 |.Dataclass.Devic|
000090: 65 4c 6f 63 61 74 6f 72 d4 0c 0d 0e 0f 10 11 12 |eLocator........|
0000a0: 13 56 61 70 73 45 6e 76 58 68 6f 73 74 6e 61 6d |.VapsEnvXhostnam|
0000b0: 65 5d 61 75 74 68 4d 65 63 68 61 6e 69 73 6d 56 |e]authMechanismV|
0000c0: 73 63 68 65 6d 65 5a 50 72 6f 64 75 63 74 69 6f |schemeZProductio|
0000d0: 6e 5f 10 13 70 31 32 2d 66 6d 69 70 2e 69 63 6c |n_..p12-fmip.icl|
0000e0: 6f 75 64 2e 63 6f 6d 55 74 6f 6b 65 6e 55 68 74 |oud.comUtokenUht|
0000f0: 74 70 73 5f 10 28 41 51 41 41 41 41 42 54 67 67 |tps_.(AQAAAABTgg|
000100: 6b 57 64 51 54 2d 59 4b 49 45 30 4a 73 56 56 70 |kWdQT-YKIE0JsVVp|
000110: 51 70 77 4b 54 67 30 39 4a 6d 76 7a 55 7e 5a 31 |QpwKTg09JmvzU~Z1|
000120: 33 36 30 36 33 39 34 36 37 5c 61 64 5f 70 40 6d |360639467d_p@m|
000130: 61 69 6c 2e 72 75 a1 0a d1 19 1a 5f 10 15 49 6e |ail.ru....._..In|
000140: 55 73 65 4f 77 6e 65 72 44 69 73 70 6c 61 79 4e |UseOwnerDisplayN|
000150: 61 6d 65 5d 50 6c 69 65 76 61 20 53 61 62 69 6e |ame]Plieva Sabin|
000160: 61 00 08 00 17 00 1e 00 34 00 3e 00 47 00 50 00 |a.......4.>.G.P.|
000170: 65 00 6e 00 71 00 74 00 98 00 a1 00 a8 00 b1 00 |e.n.q.t.........|
000180: bf 00 c6 00 d1 00 e7 00 ed 00 f3 01 1e 01 29 01 |..............).|
000190: 36 01 38 01 3b 01 53 00 00 00 00 00 00 02 01 00 |6.8.;.S.........|
0001a0: 00 00 00 00 00 00 1b 00 00 00 00 00 00 00 00 00 |................|
0001b0: 00 00 00 00 00 01 61 |......a|
------------------------------------------------------------------------------
prev-lang:kbd
------------------------------------------------------------------------------
000000: 72 75 3a 30 |ru:0|
------------------------------------------------------------------------------
SystemAudioVolume
------------------------------------------------------------------------------
000000: 4d |M|
------------------------------------------------------------------------------
bluetoothActiveControllerInfo
------------------------------------------------------------------------------
000000: 8d 82 ac 05 02 00 00 00 83 14 c8 e0 eb 2c 72 fe |.............,r.|
------------------------------------------------------------------------------
fmm-computer-name
------------------------------------------------------------------------------
000000: 69 4d 61 63 20 2d 20 50 6c 69 65 76 61 |iMac - Plieva|

UEFI Firmware Vars (dumped using an amended version of Apple's nvram tool with the -ha option)

View uefi_firmware_vars.txt File

------------------------------------------------------------------------------
AF9FFD67-EC10-488A-9DFC-6CBF5EE22C2E:AcpiGlobalVariable
------------------------------------------------------------------------------
000000: 00 b0 f8 8c 00 00 00 00 |........|
------------------------------------------------------------------------------
36C28AB5-6566-4C50-9EBD-CBB920F83843:current-network
------------------------------------------------------------------------------
000000: 00 00 00 00 00 00 00 00 04 00 05 00 07 00 00 00 |................|
000010: 69 4d 61 73 74 65 72 00 00 00 00 00 00 00 00 00 |iMaster.........|
000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000040: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000050: 05 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000060: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000070: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000080: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000090: 00 00 00 00 00 00 00 00 00 00 00 00 20 00 00 00 |............ ...|
0000a0: 6d a2 92 52 cf 5d f7 bd d6 69 0e 51 ea e5 ba 52 |m..R.]...i.Q...R|
0000b0: 7b ea 55 e4 21 78 96 10 c1 19 b2 1e 74 86 49 bc |{.U.!x......t.I.|
------------------------------------------------------------------------------
36C28AB5-6566-4C50-9EBD-CBB920F83843:preferred-count
------------------------------------------------------------------------------
000000: 01 00 00 00 00 00 00 00 |........|
------------------------------------------------------------------------------
36C28AB5-6566-4C50-9EBD-CBB920F83843:preferred-networks
------------------------------------------------------------------------------
000000: 00 00 00 00 00 00 00 00 04 00 05 00 07 00 00 00 |................|
000010: 69 4d 61 73 74 65 72 00 00 00 00 00 00 00 00 00 |iMaster.........|
000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000040: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000050: 05 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000060: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000070: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000080: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |................|
000090: 00 00 00 00 00 00 00 00 00 00 00 00 20 00 00 00 |............ ...|
0000a0: 6d a2 92 52 cf 5d f7 bd d6 69 0e 51 ea e5 ba 52 |m..R.]...i.Q...R|
0000b0: 7b ea 55 e4 21 78 96 10 c1 19 b2 1e 74 86 49 bc |{.U.!x......t.I.|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:ConOut
------------------------------------------------------------------------------
000000: 02 01 0c 00 d0 41 03 0a 00 00 00 00 01 01 06 00 |.....A..........|
000010: 00 01 01 01 06 00 00 00 03 0a 1c 00 fb ca d6 e9 |................|
000020: 8b e5 81 47 a8 f2 fb 2f 57 52 ca d6 00 00 00 00 |...G.../WR......|
000030: 00 00 00 00 03 0a 1a 00 24 ae 2d 95 1d a5 c8 49 |........$.-....I|
000040: 82 5d 91 68 1e 2c 6f 36 00 00 00 00 00 00 7f ff |.].h.,o6........|
000050: 04 00 |..|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:ConOutDev
------------------------------------------------------------------------------
000000: 02 01 0c 00 d0 41 03 0a 00 00 00 00 01 01 06 00 |.....A..........|
000010: 00 01 01 01 06 00 00 00 7f 01 04 00 02 01 0c 00 |................|
000020: d0 41 03 0a 00 00 00 00 01 01 06 00 00 02 7f 01 |.A..............|
000030: 04 00 02 01 0c 00 d0 41 03 0a 00 00 00 00 01 01 |.......A........|
000040: 06 00 00 01 01 01 06 00 00 00 03 0a 1c 00 fb ca |................|
000050: d6 e9 8b e5 81 47 a8 f2 fb 2f 57 52 ca d6 00 00 |.....G.../WR....|
000060: 00 00 00 00 00 00 03 0a 1a 00 24 ae 2d 95 1d a5 |..........$.-...|
000070: c8 49 82 5d 91 68 1e 2c 6f 36 00 00 00 00 00 00 |.I.].h.,o6......|
000080: 7f ff 04 00 |....|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:ErrOutDev
------------------------------------------------------------------------------
000000: 02 01 0c 00 d0 41 03 0a 00 00 00 00 01 01 06 00 |.....A..........|
000010: 00 01 01 01 06 00 00 00 03 0a 1c 00 fb ca d6 e9 |................|
000020: 8b e5 81 47 a8 f2 fb 2f 57 52 ca d6 00 00 00 00 |...G.../WR......|
000030: 00 00 00 00 03 0a 1a 00 24 ae 2d 95 1d a5 c8 49 |........$.-....I|
000040: 82 5d 91 68 1e 2c 6f 36 00 00 00 00 00 00 7f ff |.].h.,o6........|
000050: 04 00 |..|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:Lang
------------------------------------------------------------------------------
000000: 65 6e 67 |eng|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:LangCodes
------------------------------------------------------------------------------
000000: 65 6e 67 |eng|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:Timeout
------------------------------------------------------------------------------
000000: 05 00 |..|
------------------------------------------------------------------------------
E6C2F70A-B604-4877-85BA-DEEC89E117EB:PchInit
------------------------------------------------------------------------------
000000: 00 f0 fd 8c |....|
------------------------------------------------------------------------------
E6C2F70A-B604-4877-85BA-DEEC89E117EB:PchS3Peim
------------------------------------------------------------------------------
000000: c0 23 fe 8c 00 00 00 00 10 00 00 00 00 00 00 00 |.#..............|
------------------------------------------------------------------------------
4D1EDE05-38C7-4A6A-9CC6-4BCCA8B38C14:ROM
------------------------------------------------------------------------------
000000: 40 6c 8f e4 b9 d6 |@l....|
------------------------------------------------------------------------------
4D1EDE05-38C7-4A6A-9CC6-4BCCA8B38C14:MLB
------------------------------------------------------------------------------
000000: 43 30 32 33 32 38 35 30 30 31 33 46 43 33 46 41 |C0232850013FC3FA|
000010: 5a |Z|
------------------------------------------------------------------------------
4D1EDE05-38C7-4A6A-9CC6-4BCCA8B38C14:FirmwareFeatures
------------------------------------------------------------------------------
000000: 37 f5 03 e0 |7...|
------------------------------------------------------------------------------
4D1EDE05-38C7-4A6A-9CC6-4BCCA8B38C14:FirmwareFeaturesMask
------------------------------------------------------------------------------
000000: 37 ff 03 e0 |7...|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:BootOrder
------------------------------------------------------------------------------
000000: 80 00 |..|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:BootCurrent
------------------------------------------------------------------------------
000000: 80 00 |..|
------------------------------------------------------------------------------
8BE4DF61-93CA-11D2-AA0D-00E098032B8C:Boot0080
------------------------------------------------------------------------------
000000: 01 00 00 00 4a 00 4d 00 61 00 63 00 20 00 4f 00 |....J.M.a.c. .O.|
000010: 53 00 20 00 58 00 00 00 02 01 0c 00 d0 41 03 0a |S. .X........A..|
000020: 00 00 00 00 01 01 06 00 02 1f 03 12 0a 00 00 00 |................|
000030: 00 00 00 00 04 01 2a 00 02 00 00 00 28 40 06 00 |......*.....(@..|
000040: 00 00 00 00 40 ce 56 74 00 00 00 00 e0 3d 00 00 |....@.Vt.....=..|
000050: 82 08 00 00 8f 5b 00 00 fd 01 00 00 02 02 7f ff |.....[..........|
000060: 04 00 |..|

OpenCL
Dumped using opencl by cmf from 2009

View openCLinfo.txt File

1 OpenCL platform found!
[Platform 0]
Name: Apple
Vendor: Apple
Version: OpenCL 1.2 (Apr 25 2014 22:04:25)
Profile: FULL_PROFILE
Extensions: cl_APPLE_SetMemObjectDestructor cl_APPLE_ContextLoggingFunctions cl_APPLE_clut cl_APPLE_query_kernel_names cl_APPLE_gl_sharing cl_khr_gl_event
2 OpenCL devices found!
[Device 0]
Name: Intel(R) Core(TM) i5-4670 CPU @ 3.40GHz
Vendor: Intel
Type: CPU
Device Version: OpenCL 1.2
Driver Version: 1.1
Compute Units: 4
Work Group Size: 1024
Clock: 3400 MHz
Global Memory (Total): 8192 MB
Global Memory (Host): 8192 MB
Global Memory (PCIe): 0 MB
Local Memory: 32 KB
Cache Size: 0.0625 KB
Cache Line Size: 6291456 Bytes
Available: Yes
Double-Precision: Yes
Extensions:
cl_APPLE_SetMemObjectDestructor
cl_APPLE_ContextLoggingFunctions
cl_APPLE_clut
cl_APPLE_query_kernel_names
cl_APPLE_gl_sharing
cl_khr_gl_event
cl_khr_fp64
cl_khr_global_int32_base_atomics
cl_khr_global_int32_extended_atomics
cl_khr_local_int32_base_atomics
cl_khr_local_int32_extended_atomics
cl_khr_byte_addressable_store
cl_khr_int64_base_atomics
cl_khr_int64_extended_atomics
cl_khr_3d_image_writes
cl_khr_image2d_from_buffer
cl_APPLE_fp64_basic_ops
cl_APPLE_fixed_alpha_channel_orders
cl_APPLE_biased_fixed_point_image_formats
[Device 1]
Name: GeForce GTX 775M
Vendor: NVIDIA
Type: GPU
Device Version: OpenCL 1.2
Driver Version: 8.26.21 310.40.35f08
Compute Units: 7
Work Group Size: 1024
Clock: 797 MHz
Global Memory: 2048 MB
Local Memory: 48 KB
Cache Size: 0 KB
Cache Line Size: 0 Bytes
Available: Yes
Double-Precision: Yes
Extensions:
cl_APPLE_SetMemObjectDestructor
cl_APPLE_ContextLoggingFunctions
cl_APPLE_clut
cl_APPLE_query_kernel_names
cl_APPLE_gl_sharing
cl_khr_gl_event
cl_khr_byte_addressable_store
cl_khr_global_int32_base_atomics
cl_khr_global_int32_extended_atomics
cl_khr_local_int32_base_atomics
cl_khr_local_int32_extended_atomics
cl_APPLE_fp64_basic_ops
cl_khr_fp64
cl_khr_3d_image_writes
cl_khr_depth_images
cl_khr_gl_depth_images
cl_khr_gl_msaa_sharing
cl_khr_image2d_from_buffer

RTC
Dumped using cmosDumperForOsx by rafirafi, revised extensively by STLVNUB

View RTCDump.txt File

CMOS Dumper V0.1.:)
DSDT has RTC Length of 4. Dumped 256 Bytes.
--------------------------------------------------
0 1 2 3 4 5 6 7 8 9 A B C D E F |
--------------------------------------------------
0|34 44 26 31 21 22 00 25 05 14 26 02 50 80 ff ff |
1|ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff |
2|ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff |
3|ff ff 20 ff ff ff ff ff ff ff ff ff ff 00 f0 38 |
4|00 00 00 00 fe 00 00 00 00 00 00 00 00 00 00 00 |
5|00 00 00 00 00 00 00 ff 33 3a 80 00 04 00 00 00 |
6|54 4f 4f 42 00 00 00 02 00 00 1f 02 00 00 00 00 |
7|00 00 00 00 00 00 00 00 00 00 00 00 ff ff ff ff |
8|00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |
9|00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |
a|00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |
b|00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |
c|00 00 00 00 00 00 00 00 00 00 00 00 00 00 44 ec |
d|e9 51 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |
e|00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |
f|00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 |
--------------------------------------------------
By observtion of the CHANGED bytes from Sleep/Wake Cycles
You MAY get some idea as to why CMOS RESET bug exists!!!!

SMBIOS
Dumped using smbios-reader & dmidecode v2.11b. dmidecode compiled for OS X by Slice.

View SMBIOS.txt File

# dmidecode 2.11b
Handle 0x0000, DMI type 4, 35 bytes
0000: 04 23 00 00 04 03 cd 02 c3 06 03 00 ff fb eb bf
0010: 01 8a 19 00 48 0d 48 0d 41 2d 02 00 03 00 04 00
0020: 03 05 00
Processor Information
Socket Designation: U3E1
Type: Central Processor
Family: Core i5
Manufacturer: Intel(R) Corporation
ID: C3 06 03 00 FF FB EB BF
Signature: Type 0, Family 6, Model 60, Stepping 3
Flags:
FPU (Floating-point unit on-chip)
VME (Virtual mode extension)
DE (Debugging extension)
PSE (Page size extension)
TSC (Time stamp counter)
MSR (Model specific registers)
PAE (Physical address extension)
MCE (Machine check exception)
CX8 (CMPXCHG8 instruction supported)
APIC (On-chip APIC hardware supported)
SEP (Fast system call)
MTRR (Memory type range registers)
PGE (Page global enable)
MCA (Machine check architecture)
CMOV (Conditional move instruction supported)
PAT (Page attribute table)
PSE-36 (36-bit page size extension)
CLFSH (CLFLUSH instruction supported)
DS (Debug store)
ACPI (ACPI supported)
MMX (MMX technology supported)
FXSR (FXSAVE and FXSTOR instructions supported)
SSE (Streaming SIMD extensions)
SSE2 (Streaming SIMD extensions 2)
SS (Self-snoop)
HTT (Multi-threading)
TM (Thermal monitor supported)
PBE (Pending break enabled)
Version: Intel(R) Core(TM) i5-4670 CPU @ 3.40GHz
Voltage: 1.0 V
External Clock: 25 MHz
Max Speed: 3400 MHz
Current Speed: 3400 MHz
Status: Populated, Enabled
Upgrade: <OUT OF SPEC>
L1 Cache Handle: 0x0002
L2 Cache Handle: 0x0003
L3 Cache Handle: 0x0004
Serial Number: To Be Filled By O.E.M.
Asset Tag: To Be Filled By O.E.M.
Part Number: Not Specified
Handle 0x0001, DMI type 7, 19 bytes
0000: 07 13 01 00 00 80 01 80 00 80 00 40 00 40 00 00
0010: 05 04 07
Cache Information
Socket Designation: Not Specified
Configuration: Enabled, Not Socketed, Level 1
Operational Mode: Write Back
Location: Internal
Installed Size: 128 kB
Maximum Size: 128 kB
Supported SRAM Types:
Asynchronous
Installed SRAM Type: Asynchronous
Speed: Unknown
Error Correction Type: Single-bit ECC
System Type: Data
Associativity: 8-way Set-associative
Handle 0x0002, DMI type 7, 19 bytes
0000: 07 13 02 00 00 80 01 80 00 80 00 40 00 40 00 00
0010: 05 03 07
Cache Information
Socket Designation: Not Specified
Configuration: Enabled, Not Socketed, Level 1
Operational Mode: Write Back
Location: Internal
Installed Size: 128 kB
Maximum Size: 128 kB
Supported SRAM Types:
Asynchronous
Installed SRAM Type: Asynchronous
Speed: Unknown
Error Correction Type: Single-bit ECC
System Type: Instruction
Associativity: 8-way Set-associative
Handle 0x0003, DMI type 7, 19 bytes
0000: 07 13 03 00 00 81 01 00 04 00 04 40 00 40 00 00
0010: 05 05 07
Cache Information
Socket Designation: Not Specified
Configuration: Enabled, Not Socketed, Level 2
Operational Mode: Write Back
Location: Internal
Installed Size: 1024 kB
Maximum Size: 1024 kB
Supported SRAM Types:
Asynchronous
Installed SRAM Type: Asynchronous
Speed: Unknown
Error Correction Type: Single-bit ECC
System Type: Unified
Associativity: 8-way Set-associative
Handle 0x0004, DMI type 7, 19 bytes
0000: 07 13 04 00 00 82 01 00 18 00 18 40 00 40 00 00
0010: 05 05 09
Cache Information
Socket Designation: Not Specified
Configuration: Enabled, Not Socketed, Level 3
Operational Mode: Write Back
Location: Internal
Installed Size: 6144 kB
Maximum Size: 6144 kB
Supported SRAM Types:
Asynchronous
Installed SRAM Type: Asynchronous
Speed: Unknown
Error Correction Type: Single-bit ECC
System Type: Unified
Associativity: 12-way Set-associative
Handle 0x0005, DMI type 16, 15 bytes
0000: 10 0f 05 00 03 03 03 00 00 00 01 fe ff 04 00
Physical Memory Array
Location: System Board Or Motherboard
Use: System Memory
Error Correction Type: None
Maximum Capacity: 16 GB
Error Information Handle: Not Provided
Number Of Devices: 4
Handle 0x0006, DMI type 130, 186 bytes
0000: 82 ba 06 00 07 00 00 00 b0 00 92 12 0b 03 04 21
0010: 02 01 03 11 01 08 0a 00 fe 00 69 78 69 30 69 11
0020: 18 81 20 08 3c 3c 00 f0 83 81 00 00 00 00 00 00
0030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0040: 00 00 00 00 00 00 2f 11 61 00 00 00 00 00 00 00
0050: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0060: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0070: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 02
0080: fe 4b 13 23 47 21 08 c0 82 d5 45 42 4a 34 30 55
0090: 47 38 45 46 55 35 2d 47 4e 4c 2d 46 30 20 02 fe
00a0: 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00
00b0: 00 00 00 00 13 20 81 02 02 11
Apple specific SPD
000082ba060007000000b00092120b030421
00100201031101080a00fe00697869306911
0020188120083c3c00f08381000000000000
003000000000000000000000000000000000
00400000000000002f116100000000000000
005000000000000000000000000000000000
006000000000000000000000000000000000
007000000000000000000000000000000002
0080fe4b1323472108c082d545424a343055
00904738454655352d474e4c2d46302002fe
00a000000000000000000100000000000000
00b0000000001320810202110000111b0700
00c00500ffff0000000000100d0001021880
00d00040060304050644494d4d300042414e
00e04b203000307830324645003078343732
00f0313038433000556e6b6e6f776e003078
Handle 0x0007, DMI type 17, 27 bytes
0000: 11 1b 07 00 05 00 ff ff 00 00 00 00 00 10 0d 00
0010: 01 02 18 80 00 40 06 03 04 05 06
Memory Device
Array Handle: 0x0005
Error Information Handle: No Error
Total Width: Unknown
Data Width: Unknown
Size: 4096 MB
Form Factor: SODIMM
Set: None
Locator: DIMM0
Bank Locator: BANK 0
Type: DDR3
Type Detail: Synchronous
Speed: 1600 MHz (0.6 ns)
Manufacturer: 0x02FE
Serial Number: 0x472108C0
Asset Tag: Unknown
Part Number: 0x45424A3430554738454655352D474E4C2D46
Handle 0x0008, DMI type 130, 186 bytes
0000: 82 ba 08 00 09 00 00 00 b0 00 92 12 0b 03 04 21
0010: 02 01 03 11 01 08 0a 00 fe 00 69 78 69 30 69 11
0020: 18 81 20 08 3c 3c 00 f0 83 81 00 00 00 00 00 00
0030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0040: 00 00 00 00 00 00 2f 11 61 00 00 00 00 00 00 00
0050: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0060: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0070: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 02
0080: fe 4b 13 23 dc ec 06 fc 82 d5 45 42 4a 34 30 55
0090: 47 38 45 46 55 35 2d 47 4e 4c 2d 46 30 20 02 fe
00a0: 00 00 00 00 00 00 01 00 01 00 00 00 00 00 00 00
00b0: 00 00 00 00 13 20 81 02 02 11
Apple specific SPD
000082ba080009000000b00092120b030421
00100201031101080a00fe00697869306911
0020188120083c3c00f08381000000000000
003000000000000000000000000000000000
00400000000000002f116100000000000000
005000000000000000000000000000000000
006000000000000000000000000000000000
007000000000000000000000000000000002
0080fe4b1323dcec06fc82d545424a343055
00904738454655352d474e4c2d46302002fe
00a000000000000001000100000000000000
00b0000000001320810202110000111b0900
00c00500ffff0000000000100d0001021880
00d00040060304050644494d4d300042414e
00e04b203100307830324645003078444345
00f0433036464300556e6b6e6f776e003078
Handle 0x0009, DMI type 17, 27 bytes
0000: 11 1b 09 00 05 00 ff ff 00 00 00 00 00 10 0d 00
0010: 01 02 18 80 00 40 06 03 04 05 06
Memory Device
Array Handle: 0x0005
Error Information Handle: No Error
Total Width: Unknown
Data Width: Unknown
Size: 4096 MB
Form Factor: SODIMM
Set: None
Locator: DIMM0
Bank Locator: BANK 1
Type: DDR3
Type Detail: Synchronous
Speed: 1600 MHz (0.6 ns)
Manufacturer: 0x02FE
Serial Number: 0xDCEC06FC
Asset Tag: Unknown
Part Number: 0x45424A3430554738454655352D474E4C2D46
Handle 0x000A, DMI type 17, 27 bytes
0000: 11 1b 0a 00 05 00 ff ff 00 00 00 00 00 00 0d 00
0010: 01 02 02 00 00 00 00 00 00 03 00
Memory Device
Array Handle: 0x0005
Error Information Handle: No Error
Total Width: Unknown
Data Width: Unknown
Size: No Module Installed
Form Factor: SODIMM
Set: None
Locator: DIMM1
Bank Locator: BANK 0
Type: Unknown
Type Detail: None
Speed: Unknown
Manufacturer: Not Specified
Serial Number: Not Specified
Asset Tag: Unknown
Part Number: Not Specified
Handle 0x000B, DMI type 17, 27 bytes
0000: 11 1b 0b 00 05 00 ff ff 00 00 00 00 00 00 0d 00
0010: 01 02 02 00 00 00 00 00 00 03 00
Memory Device
Array Handle: 0x0005
Error Information Handle: No Error
Total Width: Unknown
Data Width: Unknown
Size: No Module Installed
Form Factor: SODIMM
Set: None
Locator: DIMM1
Bank Locator: BANK 1
Type: Unknown
Type Detail: None
Speed: Unknown
Manufacturer: Not Specified
Serial Number: Not Specified
Asset Tag: Unknown
Part Number: Not Specified
Handle 0x000C, DMI type 19, 15 bytes
0000: 13 0f 0c 00 00 00 00 00 ff ff 7f 00 05 00 00
Memory Array Mapped Address
Starting Address: 0x00000000000
Ending Address: 0x001FFFFFFFF
Range Size: 8 GB
Physical Array Handle: 0x0005
Partition Width: 0
Handle 0x000D, DMI type 0, 24 bytes
0000: 00 18 0d 00 01 02 00 00 03 7f 80 98 01 00 00 00
0010: 00 00 c1 02 00 01 ff ff
BIOS Information
Vendor: Apple Inc.
Version: IM142.88Z.0108.B00.1306271125
Release Date: 06/27/2013
ROM Size: 8192 kB
Characteristics:
PCI is supported
BIOS is upgradeable
BIOS shadowing is allowed
Boot from CD is supported
Selectable boot is supported
ACPI is supported
IEEE 1394 boot is supported
Smart battery is supported
Function key-initiated network boot is supported
BIOS Revision: 0.1
Handle 0x000E, DMI type 1, 27 bytes
0000: 01 1b 0e 00 01 02 03 04 a4 0f de 17 38 14 7e 54
0010: bf 68 ac 3a 13 8c a5 df 06 05 06
System Information
Manufacturer: Apple Inc.
Product Name: iMac14,2
Version: 1.0
Serial Number: C02L346HF8J5
UUID: A40FDE17-3814-7E54-BF68-AC3A138CA5DF
Wake-up Type: Power Switch
SKU Number: System SKU#
Family: iMac
Handle 0x000F, DMI type 2, 16 bytes
0000: 02 10 0f 00 01 02 03 04 05 09 06 10 00 0a 00 00
0010:
Base Board Information
Manufacturer: Apple Inc.
Product Name: Mac-27ADBB7B4CEE8E61
Version: iMac14,2
Serial Number: C0232850013FC3FAZ
Asset Tag: Base Board Asset Tag#
Features:
Board is a hosting board
Board is replaceable
Location In Chassis: Part Component
Chassis Handle: 0x0010
Type: Motherboard
Contained Object Handles: 0
Handle 0x0010, DMI type 3, 21 bytes
0000: 03 15 10 00 01 0d 02 03 00 03 03 01 01 00 00 00
0010: 00 00 00 00 00
Chassis Information
Manufacturer: Apple Inc.
Type: All In One
Lock: Not Present
Version: Mac-27ADBB7B4CEE8E61
Serial Number: C02L346HF8J5
Asset Tag: Not Specified
Boot-up State: Safe
Power Supply State: Safe
Thermal State: Other
Security Status: Other
OEM Information: 0x00000000
Height: Unspecified
Number Of Power Cords: Unspecified
Contained Elements: 0
Handle 0x0011, DMI type 8, 9 bytes
0000: 08 09 11 00 01 ff 02 00 ff
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: Other
External Reference Designator: Mini DisplayPort
External Connector Type: None
Port Type: Other
Handle 0x0012, DMI type 8, 9 bytes
0000: 08 09 12 00 01 ff 02 00 ff
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: Other
External Reference Designator: FireWire 800
External Connector Type: None
Port Type: Other
Handle 0x0013, DMI type 8, 9 bytes
0000: 08 09 13 00 01 00 02 0b 1f
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: None
External Reference Designator: Ethernet
External Connector Type: RJ-45
Port Type: Network Port
Handle 0x0014, DMI type 8, 9 bytes
0000: 08 09 14 00 01 00 02 12 10
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: None
External Reference Designator: USB0
External Connector Type: Access Bus (USB)
Port Type: USB
Handle 0x0015, DMI type 8, 9 bytes
0000: 08 09 15 00 01 00 02 12 10
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: None
External Reference Designator: USB1
External Connector Type: Access Bus (USB)
Port Type: USB
Handle 0x0016, DMI type 8, 9 bytes
0000: 08 09 16 00 01 00 02 12 10
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: None
External Reference Designator: USB2
External Connector Type: Access Bus (USB)
Port Type: USB
Handle 0x0017, DMI type 8, 9 bytes
0000: 08 09 17 00 01 00 02 12 10
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: None
External Reference Designator: USB3
External Connector Type: Access Bus (USB)
Port Type: USB
Handle 0x0018, DMI type 8, 9 bytes
0000: 08 09 18 00 01 00 02 1f 1d
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: None
External Reference Designator: Audio Line In
External Connector Type: Mini Jack (headphones)
Port Type: Audio Port
Handle 0x0019, DMI type 8, 9 bytes
0000: 08 09 19 00 01 00 02 1f 1d
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: None
External Reference Designator: Audio Line Out
External Connector Type: Mini Jack (headphones)
Port Type: Audio Port
Handle 0x001A, DMI type 8, 9 bytes
0000: 08 09 1a 00 01 16 02 00 ff
Port Connector Information
Internal Reference Designator: SATA Port A
Internal Connector Type: On Board IDE
External Reference Designator: None
External Connector Type: None
Port Type: Other
Handle 0x001B, DMI type 8, 9 bytes
0000: 08 09 1b 00 01 16 02 00 ff
Port Connector Information
Internal Reference Designator: SATA Port B
Internal Connector Type: On Board IDE
External Reference Designator: None
External Connector Type: None
Port Type: Other
Handle 0x001C, DMI type 8, 9 bytes
0000: 08 09 1c 00 01 00 02 ff ff
Port Connector Information
Internal Reference Designator: None
Internal Connector Type: None
External Reference Designator: None
External Connector Type: Other
Port Type: Other
Handle 0x001D, DMI type 8, 9 bytes
0000: 08 09 1d 00 01 ff 02 00 ff
Port Connector Information
Internal Reference Designator: Speaker
Internal Connector Type: Other
External Reference Designator: None
External Connector Type: None
Port Type: Other
Handle 0x001E, DMI type 8, 9 bytes
0000: 08 09 1e 00 01 ff 02 00 ff
Port Connector Information
Internal Reference Designator: FHB
Internal Connector Type: Other
External Reference Designator: None
External Connector Type: None
Port Type: Other
Handle 0x001F, DMI type 9, 13 bytes
0000: 09 0d 1f 00 01 a5 08 03 03 00 00 04 06
System Slot Information
Designation: AirPort
Type: x1 PCI Express
Current Usage: Available
Length: Short
ID: 0
Characteristics:
3.3 V is provided
Hot-plug devices are supported
SMBus signal is supported
Handle 0x0020, DMI type 9, 13 bytes
0000: 09 0d 20 00 01 06 05 03 04 02 00 04 07
System Slot Information
Designation: Thunderbolt Slot 1
Type: 32-bit PCI
Current Usage: Available
Length: Long
ID: 2
Characteristics:
3.3 V is provided
PME signal is supported
Hot-plug devices are supported
SMBus signal is supported
Handle 0x0021, DMI type 9, 13 bytes
0000: 09 0d 21 00 01 06 05 03 04 03 00 04 07
System Slot Information
Designation: Thunderbolt Slot 2
Type: 32-bit PCI
Current Usage: Available
Length: Long
ID: 3
Characteristics:
3.3 V is provided
PME signal is supported
Hot-plug devices are supported
SMBus signal is supported
Handle 0x0022, DMI type 9, 13 bytes
0000: 09 0d 22 00 01 06 05 03 04 04 00 04 07
System Slot Information
Designation: Thunderbolt Slot 3
Type: 32-bit PCI
Current Usage: Available
Length: Long
ID: 4
Characteristics:
3.3 V is provided
PME signal is supported
Hot-plug devices are supported
SMBus signal is supported
Handle 0x0023, DMI type 9, 13 bytes
0000: 09 0d 23 00 01 06 05 03 04 05 00 04 07
System Slot Information
Designation: Thunderbolt Slot 4
Type: 32-bit PCI
Current Usage: Available
Length: Long
ID: 5
Characteristics:
3.3 V is provided
PME signal is supported
Hot-plug devices are supported
SMBus signal is supported
Handle 0x0024, DMI type 10, 6 bytes
0000: 0a 06 24 00 83 00
On Board Device Information
Type: Video
Status: Enabled
Description: Not Specified
Handle 0x0025, DMI type 10, 6 bytes
0000: 0a 06 25 00 87 01
On Board Device Information
Type: Sound
Status: Enabled
Description: Azalia Audio Codec
Handle 0x0026, DMI type 10, 6 bytes
0000: 0a 06 26 00 85 01
On Board Device Information
Type: Ethernet
Status: Enabled
Description: Caesar IV Ethernet Controller
Handle 0x0027, DMI type 10, 6 bytes
0000: 0a 06 27 00 81 01
On Board Device Information
Type: Other
Status: Enabled
Description: SATA
Handle 0x0028, DMI type 11, 5 bytes
0000: 0b 05 28 00 03
OEM Strings
String 1: Apple ROM Version. BIOS ID: IM142. Built by: root@sa
String 2: umon. Date: Thu Jun 27 11:23:19 PDT 2013. Revision:
String 3: svn 31588 (B&I). Buildcave ID: 896. ROM Version: 0108_B00
Handle 0x0029, DMI type 12, 5 bytes
0000: 0c 05 29 00 00
System Configuration Options
Handle 0x002A, DMI type 13, 22 bytes
0000: 0d 16 2a 00 01 00 00 00 00 00 00 00 00 00 00 00
0010: 00 00 00 00 00 00
BIOS Language Information
Installable Languages: 1
<BAD INDEX>
Currently Installed Language: Not Specified
Handle 0x002B, DMI type 32, 20 bytes
0000: 20 14 2b 00 00 00 00 00 00 00 00 00 00 00 00 00
0010: 00 00 00 00
System Boot Information
Status: No errors detected
Handle 0x002C, DMI type 131, 6 bytes
0000: 83 06 2c 00 05 06
Apple specific Processor Type
cpu=0605
Handle 0x002D, DMI type 128, 88 bytes
0000: 80 58 2d 00 04 00 00 00 37 f5 03 e0 37 ff 03 e0
0010: 02 00 00 03 00 00 00 00 00 00 99 ff ff ff b2 ff
0020: 00 00 b3 ff ff ff b5 ff 00 00 b6 ff ff ff dd ff
0030: 00 00 e1 ff ff ff e3 ff 00 00 00 00 00 00 00 00
0040: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0050: 00 00 00 00 00 00 00 00
Apple specific FirmwareVolume
FirmwareFeatures: e003f537
FirmwareFeaturesMask: e003ff37
Region Type:02 Start:ff990000 End:ffb2ffff
Region Type:00 Start:ffb30000 End:ffb5ffff
Region Type:00 Start:ffb60000 End:ffddffff
Region Type:03 Start:ffe10000 End:ffe3ffff
Handle 0x002E, DMI type 133, 12 bytes
0000: 85 0c 2e 00 01 00 00 00 00 00 00 00
OEM-specific Type
Header and Data:
85 0C 2E 00 01 00 00 00 00 00 00 00
Handle 0xFFFD, DMI type 127, 4 bytes
0000: 7f 04 fd ff
End Of Table

SMC
SMC Keys. Dumped using SMC_util2 (Former Apple System Management Control (SMC) tool 0.01) by usr-sse2.

View SMC-keys.txt File

Num: b0=0 b1=0 b2=2 b3=2e size=4
#KEY [ui32] 46 (bytes 00 00 02 2e)
$Adr [ui32] 0 (bytes 00 00 03 00)
$Num [ui8 ] 1 (bytes 01)
+LKS [flag] (bytes 01)
ADC0 [ui16] 121 (bytes 0e 79)
ADC1 [ui16] 180 (bytes 03 b4)
ADC2 [ui16] 133 (bytes 0e 85)
ADC3 [ui16] 80 (bytes 00 50)
ADC4 [ui16] 65 (bytes 07 41)
ADC5 [ui16] 205 (bytes 00 cd)
ADC6 [ui16] 71 (bytes 07 47)
ADC7 [ui16] 103 (bytes 01 67)
ADC8 [ui16] 117 (bytes 0e 75)
ADC9 [ui16] 149 (bytes 00 95)
ADCa [ui16] 143 (bytes 08 8f)
ADCb [ui16] 50 (bytes 03 32)
ADCc [ui16] 19 (bytes 04 13)
ADCd [ui16] 28 (bytes 00 1c)
ADCe [ui16] 198 (bytes 0e c6)
ADCf [ui16] 58 (bytes 02 3a)
ADCg [ui16] 0 (bytes 00 00)
ADCh [ui16] 29 (bytes 05 1d)
ADCi [ui16] 244 (bytes 00 f4)
ADCj [ui16] 0 (bytes 00 00)
ADCk [ui16] 2 (bytes 00 02)
ADCl [ui16] 255 (bytes 0f ff)
ADCm [ui16] 0 (bytes 00 00)
ADCn [ui16] 0 (bytes 00 00)
ADSC [hex_] (bytes 33)
AL! [ui16] 0 (bytes 00 00)
ALI0 [{ali] (bytes 07 01 02 00)
ALI1 [{ali] (bytes 00 00 00 00)
ALIT [ui8 ] (bytes 01)
ALP0 [{alp] (bytes 13 33 0a 00)
ALP1 [{alp] (bytes 00 00 00 00)
ALRV [ui16] 1 (bytes 00 01)
ALSC [{alc] (bytes 00 c7 00 96 03 e8 00 0f 00 01 01 5e 1d 03 01 06)
ALSF [fp1f] (bytes 31 cb)
ALSL [ui16] 40 (bytes 00 28)
ALV0 [{alv] (bytes 01 01 01 55 00 8c 00 0a 23 50)
ALV1 [{alv] (bytes 00 01 00 00 00 00 00 00 00 00)
AUPO [ui8 ] 0 (bytes 00)
BATP [flag] (bytes 00)
BEMB [flag] (bytes 00)
BNum [ui8 ] 0 (bytes 00)
BSIn [hex_] (bytes 42)
CLKT [ui32] 72 (bytes 00 00 14 48)
CLSD [ui16] 0 (bytes 00 00)
CLWK [ui16] 255 (bytes ff ff)
CPL1 [sp96] (bytes 00 00)
CPL2 [sp96] (bytes 00 00)
CPL3 [ui32] 0 (bytes 00 00 00 00)
CRCA [ui32] 96 (bytes 7a 0f 09 60)
CRCB [ui32] 74 (bytes 41 a8 ce 4a)
CRCC [ui32] 8 (bytes 78 14 8c 08)
CRCF [ui32] 110 (bytes ac 2b e8 6e)
CRCK [ui32] 0 (bytes 00 00 00 00)
CRCR [ui32] 8 (bytes 39 cf aa 08)
CRCU [ui32] 185 (bytes be de dc b9)
CRCa [ui32] 96 (bytes 7a 0f 09 60)
CRCb [ui32] 74 (bytes 41 a8 ce 4a)
CRCc [ui32] 8 (bytes 78 14 8c 08)
CRCr [ui32] 8 (bytes 39 cf aa 08)
CRCu [ui32] 185 (bytes be de dc b9)
DBGP [ui8 ] 2 (bytes 02)
DICT [flag] (bytes 00)
DID0 [ui32] 3 (bytes 18 05 00 03)
DID1 [ui32] 52 (bytes 10 ec a8 34)
DM0C [hex_] (bytes 01 02)
DM0F [ui8 ] 0 (bytes 00)
DM0I [{hdi] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
DM0M [ui8 ] 0 (bytes 00)
DM0P [ui8 ] 1 (bytes 01)
DM0S [ui8 ] 1 (bytes 01)
DM0T [hex_] (bytes 80 80)
DM0b [ui32] 0 (bytes 00 00 00 00)
DM0g [ui32] 22 (bytes 00 00 00 16)
DM0h [ui8 ] (bytes 00)
DM1C [hex_] (bytes 01 04)
DM1F [ui8 ] 0 (bytes 00)
DM1I [{hdi] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
DM1M [ui8 ] 0 (bytes 00)
DM1P [ui8 ] 3 (bytes 03)
DM1S [ui8 ] 0 (bytes 00)
DM1T [hex_] (bytes 80 80)
DM1b [ui32] 0 (bytes 00 00 00 00)
DM1g [ui32] 0 (bytes 00 00 00 00)
DM1h [ui8 ] (bytes 00)
DMP! [hex_] (bytes 00)
DMS! [hex_] (bytes 00)
DPLM [{lim] (bytes 00 00 00 00 00)
DT0A [sp78] (bytes 00 00)
DT0B [sp78] (bytes 00 00)
DT0C [sp78] (bytes 00 00)
DT1A [sp78] (bytes 00 00)
DT1B [sp78] (bytes 00 00)
DT1C [sp78] (bytes 00 00)
DULI [ui8 ] 0 (bytes 00)
DULT [ui8 ] 70 (bytes 46)
DURR [ui8 ] 4 (bytes 04)
DUSR [ui8 ] 0 (bytes 00)
DUST [ui8 ] 0 (bytes 00)
DUTC [flag] (bytes 00)
DUTI [ui8 ] 0 (bytes 00)
DUTT [ui8 ] 45 (bytes 2d)
ECIP [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
ECIT [ui8 ] 0 (bytes 00)
EECC [ui32] 0 (bytes 00 00 00 00)
ENV0 [ui8 ] 3 (bytes 03)
EPCA [ui32] 0 (bytes 00 00 b0 00)
EPCF [flag] (bytes 01)
EPCI [ui32] 0 (bytes 07 80 f0 00)
EPCV [ui16] 1 (bytes 00 01)
EPMA [ch8*] (bytes 00 00 a8 10)
EPMI [ui8 ] 0 (bytes 00)
EPUA [ui32] 0 (bytes 00 00 a8 00)
EPUF [flag] (bytes 01)
EPUI [ui32] 1 (bytes 07 80 00 01)
EPUV [ui16] 1 (bytes 00 01)
EVCT [hex_] (bytes 06 06)
EVHF [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
EVMD [ui32] 0 (bytes 00 00 00 00)
EVRD [ch8*] (bytes f6 06 02 00 00 01 3f 57 93 03 82 01 06 01 3f 5d 94 03 82 01 06 01 3f 5d 93 04 00 02 02 01 3f 5e)
EVSL [ui8 ] 0 (bytes 00)
F0Ac [fpe2] 1201 (bytes 12 c4)
F0ID [{fds] (bytes 00 00 10 00 4d 61 69 6e 20 00 00 00 00 00 00 00)
F0Mn [fpe2] 1200 (bytes 12 c0)
F0Mt [ui16] 0 (bytes 00 00)
F0Mx [fpe2] 2640 (bytes 29 40)
F0Tg [fpe2] 1200 (bytes 12 c0)
FNum [ui8 ] 1 (bytes 01)
FPDc [fp79] (bytes 21 34)
FRmn [ui16] 0 (bytes 00 00)
FRmp [ui16] 0 (bytes 00 00)
FS! [ui16] 0 (bytes 00 00)
FSDc [ui16] 0 (bytes 69 00)
G3AO [ui32] 0 (bytes 00 00 00 00)
G3WD [flag] (bytes 00)
GCID [hex_] (bytes 11 9d 10 de)
GT0C [ui16] 0 (bytes 00 00)
GT0R [ui8 ] 0 (bytes 00)
GTHR [ui8 ] 1 (bytes 01)
HBKP [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
HBKT [ui32] 0 (bytes 00 05 46 00)
HC0N [ui8 ] 27 (bytes 1b)
HC0T [ui8 ] 4 (bytes 04)
HDBS [ui8 ] 0 (bytes 00)
HDST [hex_] (bytes 00 00 00 00)
HDSW [hex_] (bytes 00 01 00 01)
HE0N [ui8 ] 14 (bytes 0e)
HE0T [ui8 ] 0 (bytes 00)
HE1N [ui8 ] 0 (bytes 00)
HE1T [ui8 ] 0 (bytes 00)
HI0N [ui8 ] 23 (bytes 17)
HI0T [ui8 ] 0 (bytes 00)
HI1N [ui8 ] 0 (bytes 00)
HI1T [ui8 ] 0 (bytes 00)
HNVD [ui16] 0 (bytes 00 00)
IC0C [sp78] (bytes 12 81)
IC0M [sp5a] (bytes 01 10)
ID2E [sp78] (bytes 07 91)
ID2F [sp78] (bytes 07 92)
ID2I [sp78] (bytes 06 57)
ID2J [sp78] (bytes 00 02)
ID2L [ui16] 0 (bytes 04 00)
ID2R [sp69] (bytes 0c af)
ID2S [si16] (bytes 99 cc)
ID2T [sp78] (bytes 00 09)
IG0C [sp87] (bytes 00 ba)
IG0F [sp3c] (bytes 02 bb)
IG1C [sp4b] (bytes 02 30)
IH02 [sp3c] (bytes 03 2e)
IH05 [sp2d] (bytes 07 59)
IH1R [sp3c] (bytes 00 10)
IM0R [sp5a] (bytes 01 9b)
IW0R [sp3c] (bytes 00 00)
KDD0 [hex_] (bytes 19 99 36 36 a2 fb 3f 93 1a 81 14 fe b1 f3 e5 29 91 42 a0 28 82 5d 09 d5 14 78 f6 24 00 00 3e 8a)
KDD1 [hex_] (bytes 00 00 00 00 00 00 da 96 00 00 00 00 6a 21 00 00 00 00 00 00 00 00 00 00 00 00 00 00 da 26 00 00)
KDFT [ui8 ] 1 (bytes 01)
KDTP [ui8 ] 1 (bytes 01)
LAcN [ui8 ] 0 (bytes 00)
LAtN [ui16] 0 (bytes 00 00)
LC2D [ui16] 195 (bytes 00 c3)
LC2E [ui16] 195 (bytes 00 c3)
LCCC [ui8 ] 0 (bytes 00)
LCCN [ui8 ] 4 (bytes 04)
LCCQ [ui8 ] 4 (bytes 04)
LCKA [ui8 ] 70 (bytes 46)
LCKN [ui8 ] 222 (bytes de)
LCLD [ui16] 0 (bytes 00 00)
LCLG [ui8 ] 0 (bytes 00)
LCSA [ui8 ] 0 (bytes 00)
LCTN [ui8 ] 21 (bytes 15)
LCTQ [ui8 ] 205 (bytes cd)
LDEN [ui16] 0 (bytes 00 00)
LDI2 [ui8 ] 1 (bytes 01)
LDKN [ui8 ] 2 (bytes 02)
LDLG [ui8 ] 0 (bytes 00)
LDLT [ui8 ] 1 (bytes 01)
LDS4 [ui8 ] 0 (bytes 00)
LDSP [flag] (bytes 00)
LDT1 [ui8 ] 0 (bytes 00)
LDT2 [ui16] 0 (bytes 00 00)
LDT4 [ui32] 0 (bytes 00 00 00 00)
LDTF [ui16] 0 (bytes 00 00)
LDWE [ui32] 0 (bytes 00 00 05 00)
LPMC [ui32] 1 (bytes 00 00 00 01)
MACA [ui32] 0 (bytes 00 00 00 00)
MACM [flag] (bytes 01)
MACR [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
MDMT [flag] (bytes 00)
MDSC [hex_] (bytes 05)
MSAL [hex_] (bytes 4b)
MSAc [fp88] (bytes 00 00)
MSAf [fp6a] (bytes 00 00)
MSAg [fp88] (bytes 00 00)
MSAi [fp88] (bytes 00 00)
MSDV [hex_] (bytes a2)
MSDW [flag] (bytes 00)
MSFC [ui8 ] 0 (bytes 00)
MSFD [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
MSFW [flag] (bytes 00)
MSG3 [flag] (bytes 00)
MSGA [fp6a] (bytes 00 00)
MSLD [ui8 ] 0 (bytes 00)
MSLF [ui8 ] 0 (bytes 00)
MSLG [ui8 ] 0 (bytes 00)
MSLP [ui8 ] 0 (bytes 00)
MSLS [ui8 ] 0 (bytes 00)
MSLT [flt ] (bytes 00 00 00 00)
MSLU [flt ] (bytes 00 00 00 00)
MSPA [fp6a] (bytes 00 00)
MSPB [flag] (bytes 00)
MSPC [ui8 ] 27 (bytes 1b)
MSPE [ui8 ] 14 (bytes 0e)
MSPI [ui8 ] 23 (bytes 17)
MSPP [ui8 ] 0 (bytes 00)
MSPS [hex_] (bytes 00 02)
MSPT [ui8 ] 45 (bytes 1f 17 00 09 0e)
MSPV [ui8 ] 2 (bytes 02)
MSRC [ui32] 2 (bytes 00 00 00 02)
MSSD [si8 ] (bytes 00)
MSSF [ui32] 0 (bytes 00 00 00 00)
MSSG [ui32] 0 (bytes 00 00 00 00)
MSSP [si8 ] (bytes 05)
MSSR [flag] (bytes 01)
MSSS [{mss] (bytes 00)
MSTC [ui16] 0 (bytes 00 00)
MSTD [ui16] 0 (bytes 00 00)
MSTS [ui8 ] 4 (bytes 04)
MSTc [ui8 ] 0 (bytes 00)
MSTe [ui8 ] 0 (bytes 00)
MSTf [ui8 ] 0 (bytes 00)
MSTi [ui8 ] 0 (bytes 00)
MSTj [ui8 ] 0 (bytes 00)
MSWd [flag] (bytes 01)
MSWo [flag] (bytes 01)
MSWr [ui8 ] 0 (bytes 00)
MSXC [ch8*] (bytes 00 00 00 00)
MSXD [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
MSXH [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
MSXK [ch8*] (bytes 01 02 03 04 05 06 07 08 09 0a 0b 0c 0d 0e 0f 10 11 12 13 14 15 16 17 18 19 1a 1b 1c 1d 1e 1f 20)
MSXL [ch8*] (bytes 00 00 fd e8 00 00 fd e8 00 00 fd e8 00 00 fd e8)
MSXN [ui8 ] 58 (bytes 3a)
MSXP [ui32] 0 (bytes 00 00 00 00)
MSXS [ch8*] (bytes 01 02 03 04)
MSXT [ui32] 255 (bytes ff ff ff ff)
MSXb [ui8 ] 0 (bytes 00)
MSXc [ch8*] (bytes 00 00 00 00)
MSXd [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
MSXh [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
MSXk [ch8*] (bytes 01 02 03 04 05 06 07 08 09 0a 0b 0c 0d 0e 0f 10 11 12 13 14 15 16 17 18 19 1a 1b 1c 1d 1e 1f 20)
MSXl [ch8*] (bytes 00 00 fd e8 00 00 fd e8 00 00 fd e8 00 00 fd e8)
MSXm [ui16] 8 (bytes 00 08)
MSXn [ui8 ] 65 (bytes 41)
MSXs [ui32] 4 (bytes 01 02 03 04)
MSa! [hex_] (bytes 00)
MSac [ui8 ] 0 (bytes 00)
MSaf [ui8 ] 0 (bytes 00)
MSag [ui8 ] 0 (bytes 00)
MSah [ui8 ] 0 (bytes 00)
MSai [ui8 ] 0 (bytes 00)
MSap [ui8 ] 0 (bytes 00)
MSt0 [flt ] (bytes 00 00 00 00)
MSt1 [flt ] (bytes 00 00 00 00)
MSt2 [flt ] (bytes 00 00 00 00)
MSt3 [flt ] (bytes 00 00 00 00)
MSt4 [flt ] (bytes 00 00 00 00)
NATJ [ui8 ] 0 (bytes 00)
NATi [ui16] 0 (bytes 00 00)
NOPB [ui8 ] 0 (bytes 00)
NTOK [ui8 ] 0 (bytes 00)
ONMI [ui8 ] 0 (bytes 00)
OOBC [ui8 ] (bytes 00 00)
OOBR [ui8 ] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
OOBS [ui8 ] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
OOBT [ui8 ] (bytes 00 00)
OOBW [ui8 ] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
PC0C [sp96] (bytes 08 31)
PC0M [sp96] (bytes 00 19)
PCPC [sp96] (bytes 06 ad)
PCPG [sp96] (bytes 00 00)
PCPL [sp96] (bytes 15 00)
PCPR [sp96] (bytes 08 4a)
PCPT [sp96] (bytes 08 90)
PCTR [sp96] (bytes 09 bf)
PD2R [sp96] (bytes 13 07)
PDTR [sp96] (bytes 13 07)
PDTx [sp96] (bytes 00 62)
PG0C [sp96] (bytes 00 4e)
PG0F [sp96] (bytes 00 82)
PG1C [sp96] (bytes 00 d2)
PGPR [sp96] (bytes 00 00)
PGTR [sp96] (bytes 02 c2)
PH02 [sp96] (bytes 00 98)
PH05 [sp96] (bytes 00 4a)
PH0F [sp78] (bytes 08 0f)
PH0R [sp96] (bytes 00 e3)
PH1F [sp78] (bytes 00 00)
PH1R [sp96] (bytes 00 00)
PM0R [sp96] (bytes 00 26)
PM0f [sp2d] (bytes 00 8d)
PSTR [sp96] (bytes 13 07)
PW0R [sp96] (bytes 00 00)
PZ0E [flt ] (bytes 00 00 20 43)
PZ0F [flt ] (bytes c5 c6 4c 42)
PZ0G [sp96] (bytes 0c 82)
PZ0T [flt ] (bytes 00 00 00 00)
PZ1E [flt ] (bytes 00 00 b4 42)
PZ1F [flt ] (bytes 0a 03 20 42)
PZ1G [sp96] (bytes 09 bf)
PZ1T [flt ] (bytes 00 00 00 00)
PZ2E [flt ] (bytes 00 00 d2 42)
PZ2F [flt ] (bytes c1 16 33 41)
PZ2G [sp96] (bytes 02 c2)
PZ2T [flt ] (bytes 00 00 00 00)
PZ3E [flt ] (bytes 00 00 ac 42)
PZ3F [flt ] (bytes 67 6a 9a 3f)
PZ3G [sp96] (bytes 00 4e)
PZ3T [flt ] (bytes 00 00 00 00)
PZ4E [flt ] (bytes f9 ff 05 42)
PZ4F [flt ] (bytes 91 ba 00 40)
PZ4G [sp96] (bytes 00 82)
PZ4T [flt ] (bytes 00 00 00 00)
PZ5E [flt ] (bytes 00 00 9b 43)
PZ5F [flt ] (bytes 00 70 b3 42)
PZ5G [sp96] (bytes 15 6c)
PZ5T [flt ] (bytes 00 00 00 00)
RBr [ch8*] (bytes 6a 31 36 6a 31 37 00 00)
REV [{rev] (bytes 02 15 0f 00 00 00)
RMde [char] (bytes 41)
RPlt [ch8*] (bytes 6a 31 37 00 00 00 00 00)
RSvn [ui32] 0 (bytes 00 00 00 00)
RVBF [{rev] (bytes 02 15 0f 00 00 00)
RVCR [{rev] (bytes ff ff ff ff ff ff)
RVUF [{rev] (bytes 02 15 0f 00 00 00)
SAS! [hex_] (bytes 00 3e ff ff)
SBF [hex_] (bytes 00 00 00 00)
SBFC [flag] (bytes 00)
SBFD [hex_] (bytes 00 00 0f c0)
SBFE [flag] (bytes 01)
SBFF [hex_] (bytes 00 00 00 00)
SBFL [hex_] (bytes 00 00 00 00)
SBFN [hex_] (bytes 00 00 00 00)
SBFU [hex_] (bytes 00 00 0f d8)
SBFV [hex_] (bytes 00 3f f0 3f)
SC0F [sp78] (bytes fc 00)
SC0W [sp78] (bytes fe 00)
SCIA [ui16] 248 (bytes 03 f8)
SCIB [ui32] 0 (bytes 00 01 c2 00)
SCII [ui8 ] 3 (bytes 03)
SCIL [ui8 ] 0 (bytes 00)
SCXC [sp78] (bytes 64 00)
SDAS [ui16] 0 (bytes 00 00)
SDPE [ui8 ] 0 (bytes 00)
SFBR [ui8 ] 6 (bytes 06)
SG0F [sp78] (bytes 5f 00)
SG0W [sp78] (bytes 64 00)
SH0F [sp78] (bytes 06 00)
SH0W [sp78] (bytes 00 00)
SH1F [sp78] (bytes 0f 00)
SH1W [sp78] (bytes 00 00)
SIP [ui8 ] (bytes 01)
SIPB [flag] (bytes 00)
SIS! [hex_] (bytes 00 00 00 00)
SIT! [hex_] (bytes 00 00 00 00)
SIU! [hex_] (bytes 00 00 00 00)
SL0F [sp78] (bytes 32 00)
SL0P [sp78] (bytes 3a 00)
SL0S [sp78] (bytes 3c 00)
SL0W [sp78] (bytes 34 00)
SM0F [sp78] (bytes 53 00)
SM0W [sp78] (bytes 59 00)
SMBC [ch8*] (bytes 00 00 00 00 00 00)
SMBG [ui8 ] 0 (bytes 00)
SMBR [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
SMBS [ch8*] (bytes 00 00)
SMBW [ch8*] (bytes 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00)
SPDO [ui8 ] 1 (bytes 01)
SPH0 [ui16] 0 (bytes 00 00)
SPHR [ui32] 0 (bytes 00 00 00 00)
SPHS [ui8 ] 0 (bytes 00)
SPHT [ui16] 0 (bytes 00 00)
SPHZ [ui8 ] (bytes 00)
SPT! [hex_] (bytes 00)
SPU! [hex_] (bytes 00 00 00 00)
SPV! [hex_] (bytes 00 00 00 00)
SRS! [hex_] (bytes 00 00 00 00)
SRT! [hex_] (bytes 00 00 00 00)
SS0F [sp78] (bytes 32 00)
SS0W [sp78] (bytes 34 00)
STC0 [ui8 ] 1 (bytes 01)
STC1 [ui8 ] 0 (bytes 00)
STC2 [ui8 ] 2 (bytes 02)
STDK [ui16] 0 (bytes 00 00)
STFD [flag] (bytes 00)
Sp2F [sp78] (bytes 5a 00)
Sp2P [sp78] (bytes 61 00)
Sp2S [sp78] (bytes 66 00)
Sp2W [sp78] (bytes 5c 00)
SpCC [fp6a] (bytes 64 6b)
SpCI [ui8 ] (bytes 0e)
SpCP [fp6a] (bytes 6b 1c)
SpCS [si16] (bytes 0e c5)
SpCT [fpc4] (bytes 27 63)
TA0P [sp78] (bytes 0f c0)
TA0V [sp78] (bytes 18 f5)
TA0p [sp78] (bytes 23 c0)
TC0E [sp78] (bytes db 82)
TC0F [sp78] (bytes dd 68)
TC0J [sp78] (bytes 01 e6)
TC0L [ui16] 26 (bytes 00 1a)
TC0P [sp78] (bytes 32 e0)
TC0T [sp78] (bytes 00 29)
TC0c [sp78] (bytes 41 00)
TC0p [sp78] (bytes 32 e0)
TC1c [sp78] (bytes 3f 00)
TC2c [sp78] (bytes 3f 00)
TC3c [sp78] (bytes 3d 00)
TCGc [sp78] (bytes 3a 00)
TCSc [sp78] (bytes 3b 00)
TCXR [sp78] (bytes dc c0)
TCXc [sp78] (bytes 40 c0)
TCXr [sp78] (bytes dc c0)
TG0D [sp78] (bytes 34 00)
TG0E [sp78] (bytes 34 f1)
TG0F [sp78] (bytes 36 1a)
TG0J [sp78] (bytes 01 29)
TG0L [ui16] 32 (bytes 00 20)
TG0P [sp78] (bytes 2c 80)
TG0T [sp78] (bytes ff f7)
TG0d [sp78] (bytes 2b 00)
TG0p [sp78] (bytes 2c 80)
TH0A [sp78] (bytes 81 00)
TH0B [sp78] (bytes 81 00)
TH0C [sp78] (bytes 81 00)
TH0F [sp78] (bytes 81 00)
TH0O [sp78] (bytes f9 00)
TH0P [sp78] (bytes f9 00)
TH0R [sp78] (bytes 81 00)
TH0a [sp78] (bytes 81 00)
TH0b [sp78] (bytes 81 00)
TH0c [sp78] (bytes 81 00)
TH0e [sp78] (bytes 00 00)
TH0o [hex_] (bytes 00 07)
TH1A [sp78] (bytes 81 00)
TH1B [sp78] (bytes 81 00)
TH1C [sp78] (bytes 81 00)
TH1F [sp78] (bytes 81 00)
TH1O [sp78] (bytes 09 00)
TH1P [sp78] (bytes 81 00)
TH1R [sp78] (bytes 81 00)
TH1a [sp78] (bytes 81 00)
TH1b [sp78] (bytes 81 00)
TH1c [sp78] (bytes 81 00)
TH1o [hex_] (bytes 00 80)
TL0P [sp78] (bytes 25 60)
TL0V [sp78] (bytes 22 eb)
TL0p [sp78] (bytes 25 60)
TL1P [sp78] (bytes 26 80)
TL1V [sp78] (bytes 20 fc)
TL1p [sp78] (bytes 26 80)
TL1v [sp78] (bytes 20 fc)
TL2p [sp87] (bytes c0 80)
TL3p [spa5] (bytes f0 20)
TM0P [sp78] (bytes 27 e0)
TM0V [sp78] (bytes 27 62)
TM0p [sp78] (bytes 27 e0)
TM1P [sp78] (bytes 22 20)
TM1a [sp78] (bytes 27 e4)
TM1p [sp78] (bytes 22 20)
TM2P [sp78] (bytes 24 60)
TM2a [sp78] (bytes 27 62)
TM2b [sp78] (bytes 2a 62)
TM2c [sp78] (bytes 27 62)
TM2d [sp78] (bytes 2a 62)
TM2p [sp78] (bytes 24 60)
TM3P [sp78] (bytes 25 e0)
TM3a [sp78] (bytes 24 62)
TM3b [sp78] (bytes 22 62)
TM3c [sp78] (bytes 26 73)
TM3d [sp78] (bytes 24 62)
TM3p [sp78] (bytes 25 e0)
TM4a [sp78] (bytes 27 a6)
TMXP [sp78] (bytes 27 e0)
TPCD [sp78] (bytes 2e 00)
TS0V [sp78] (bytes 23 5a)
Tb0P [sp78] (bytes 2a a0)
Tb0p [sp78] (bytes 2a a0)
Tm0P [sp78] (bytes 28 80)
Tm0p [sp78] (bytes 28 80)
Tm1P [sp78] (bytes 2a 00)
Tm1p [sp78] (bytes 2a 00)
Tm2P [sp78] (bytes 2f 40)
Tm2p [sp78] (bytes 2f 40)
Tp2F [sp78] (bytes 26 d5)
Tp2H [sp78] (bytes 26 e0)
Tp2h [sp78] (bytes 26 e0)
UBDC [flag] (bytes 00)
UFIS [ui32] 0 (bytes 00 00 00 00)
UPRC [ui16] 1 (bytes 00 01)
UREV [ui8 ] (bytes a3)
URPP [ui32] 51 (bytes 00 00 00 33)
URWD [ui32] 0 (bytes 00 00 00 00)
USR0 [ui32] 255 (bytes ff ff ff ff)
USR1 [ui32] 255 (bytes ff ff ff ff)
USR2 [ui32] 255 (bytes ff ff ff ff)
USR3 [ui32] 144 (bytes 01 2b 27 90)
VC0C [sp2d] (bytes 38 af)
VC0M [sp2d] (bytes 2f e2)
VD2R [sp4b] (bytes 60 00)
VG0C [sp2d] (bytes 1a e4)
VG0F [sp4b] (bytes 5f c5)
VG1C [sp4b] (bytes 60 52)
VH05 [sp3c] (bytes 51 38)
VL3t [si16] (bytes ff 81)
VM0R [sp2d] (bytes 30 09)
VR1R [sp2d] (bytes 21 b6)
VR3R [sp3c] (bytes 34 cc)
WCPW [ui8 ] 0 (bytes 00)
WIr0 [si8 ] (bytes 05)
WIw0 [si8 ] (bytes 02)
WIz0 [ui8 ] 2 (bytes 02)
WKEN [ui8 ] 0 (bytes 00)
ZPEN [hex_] (bytes 3f)
hSci [ui8 ] 0 (bytes 00)
hSdn [flt ] (bytes 00 00 00 00)
hSei [ui8 ] 0 (bytes 00 00)
hSii [ui8 ] 0 (bytes 00)
hSij [ui8 ] 0 (bytes 00)
hSta [ui8 ] 2 (bytes 01 01 02)
hSup [flt ] (bytes 00 00 00 00)
mSTC [flt ] (bytes 00 00 00 00)
mSTD [flt ] (bytes 00 00 00 00)
mSTK [flt ] (bytes 00 00 00 00)
zDBG [ui8 ] (bytes 00)
zDSF [flag] (bytes 00)
zMOJ [flag] (bytes 01)

SMC Fans. Dumped using SMC_util2 (Former Apple System Management Control (SMC) tool 0.01) by usr-sse2.

View SMC-fans.txt File

Total fans in system: 1
Fan #0:
Actual speed : 1202 Key[F0Ac]
Minimum speed: 1200
Maximum speed: 2640
Safe speed : 0
Target speed : 1200
Mode : auto

System Profiler
Dumped using /usr/sbin/system_profiler -detailLevel mini

View System-Profiler.txt File

Audio:
Intel High Definition Audio:
Audio ID: 7
Headphone:
Connection: Combination Output
Speaker:
Connection: Internal
Internal Microphone:
Connection: Internal
S/PDIF Optical Digital Audio Output:
Connection: Combination Output
External Microphone / iPhone Headset:
Connection: Combination Output
HDMI / DisplayPort Output:
Connection: Display
Devices:
Built-in Microphone:
Default Input Device: Yes
Input Channels: 2
Manufacturer: Apple Inc.
Current SampleRate: 32000
Transport: Built-in
Built-in Output:
Default Output Device: Yes
Default System Output Device: Yes
Manufacturer: Apple Inc.
Output Channels: 2
Current SampleRate: 44100
Transport: Built-in
Bluetooth:
Apple Bluetooth Software Version: 4.2.4f1 13674
Hardware Settings:
Manufacturer: Broadcom
Chipset: 20702B0
Firmware Version: v79 c8652
Connectable: Yes
Auto Seek Keyboard: On
Auto Seek Pointing: On
Remote wake: On
Vendor ID: 0x05AC
Product ID: 0x828D
Devices (Paired, Configured, etc):
Apple Magic Mouse:
Major Type: Mouse
Minor Type: Peripheral
Services: Apple Magic Mouse
Manufacturer: Apple (0x3, 0x31C)
Battery Level: 95%
Firmware Version: 0x0306
Vendor ID: 0x05AC
Product ID: 0x030D
Host Connectable: Yes
EDR Supported: No
eSCO Supported: No
SSP Supported: No
Apple Wireless Keyboard:
Major Type: Keyboard
Minor Type: Peripheral
Services: Apple Wireless Keyboard
Manufacturer: Apple (0x3, 0x31C)
Battery Level: 100%
Firmware Version: 0x0050
Vendor ID: 0x05AC
Product ID: 0x0256
Host Connectable: Yes
EDR Supported: No
eSCO Supported: No
SSP Supported: No
Camera:
HD-камера FaceTime (встроенная):
Model ID: UVC Camera VendorID_1452 ProductID_34065
Unique ID: 0x1470000005ac8511
Card Reader:
Built in SD Card Reader:
Vendor ID: 0x14e4
Device ID: 0x16bc
Subsystem Vendor ID: 0x14e4
Subsystem ID: 0x0000
Revision: 0x0001
Link Width: x1
Link Speed: 2.5 GT/s
Diagnostics:
Power On Self-Test:
Last Run: 5/26/14, 1:21 AM
Result: Passed
Ethernet Cards:
Broadcom 57766-A1:
Name: ethernet
Type: Ethernet Controller
Bus: PCI
Vendor ID: 0x14e4
Device ID: 0x1686
Subsystem Vendor ID: 0x14e4
Subsystem ID: 0x1686
Revision ID: 0x0001
Link Width: x1
BSD name: en0
Kext name: AppleBCM5701Ethernet.kext
Firmware version: 57766a-v1.13, 0x010e63c4
Location: /System/Library/Extensions/IONetworkingFamily.kext/Contents/PlugIns/AppleBCM5701Ethernet.kext
mDNS offload capable: 10:dd:b1:ea:91:fa
Version: 3.8.1b2
Graphics/Displays:
NVIDIA GeForce GTX 775M:
Chipset Model: NVIDIA GeForce GTX 775M
Type: GPU
Bus: PCIe
PCIe Lane Width: x16
VRAM (Total): 2048 MB
Vendor: NVIDIA (0x10de)
Device ID: 0x119d
Revision ID: 0x00a2
ROM Revision: 3745
Displays:
iMac:
Display Type: LCD
Resolution: 2560 x 1440
Pixel Depth: 32-Bit Color (ARGB8888)
Main Display: Yes
Mirror: Off
Online: Yes
Built-In: Yes
Hardware:
Hardware Overview:
Model Name: iMac
Model Identifier: iMac14,2
Processor Name: Intel Core i5
Processor Speed: 3.4 GHz
Number of Processors: 1
Total Number of Cores: 4
L2 Cache (per Core): 256 KB
L3 Cache: 6 MB
Memory: 8 GB
Boot ROM Version: IM142.0108.B00
SMC Version (system): 2.15f0
Memory:
Memory Slots:
ECC: Disabled
BANK 0/DIMM0:
Size: 4 GB
Type: DDR3
Speed: 1600 MHz
Status: OK
Manufacturer: 0x02FE
Part Number: 0x45424A3430554738454655352D474E4C2D46
BANK 1/DIMM0:
Size: 4 GB
Type: DDR3
Speed: 1600 MHz
Status: OK
Manufacturer: 0x02FE
Part Number: 0x45424A3430554738454655352D474E4C2D46
BANK 0/DIMM1:
Size: Empty
Type: Empty
Speed: Empty
Status: Empty
Manufacturer: Empty
Part Number: Empty
BANK 1/DIMM1:
Size: Empty
Type: Empty
Speed: Empty
Status: Empty
Manufacturer: Empty
Part Number: Empty
Network:
Bluetooth DUN:
Type: PPP (PPPSerial)
Hardware: Modem
BSD Device Name: Bluetooth-Modem
Service Order: 0
Ethernet:
Type: Ethernet
Hardware: Ethernet
BSD Device Name: en0
Service Order: 1
Wi-Fi:
Type: AirPort
Hardware: AirPort
BSD Device Name: en1
Service Order: 2
Bluetooth PAN:
Type: Ethernet
Hardware: Ethernet
BSD Device Name: en2
Service Order: 3
Printer Software:
PPDs:
PPDs:
Path: /Library/Printers/PPDs/Contents/Resources/HP 910.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP 915.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Business Inkjet 2250.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Business Inkjet 2280.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/hp business inkjet 2300.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Business Inkjet 2600.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Business Inkjet 2800.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Business Inkjet 3000.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP CM8050 CM8060 MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/hp color LaserJet 2500.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 2550.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 2600.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 2605.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 2700.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 2800.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 3000.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP color LaserJet 3500.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP color LaserJet 3550.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 3600.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/hp color LaserJet 3700.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 3800.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 4500.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 4550.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp color LaserJet 4600.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp color LaserJet 4650.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 4700.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 4730 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp color LaserJet 5500.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 5550.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 5M.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 8500.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet 8550.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/hp color LaserJet 9500 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp color LaserJet 9500.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM1015.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM1312 MFP Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM1312 MFP Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM2320 MFP Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM2320 MFP Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM3530 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM4540 MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM4730 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM6030 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM6040 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CM6049 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP1510 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP2020 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP2020d Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP3505.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP3525.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP4005.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP4020 CP4520 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP5220 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP5220d Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP5520 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet CP6015.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet flow MFP M880.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet M750.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet M855.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet Pro MFP M176.ppd.gz
Version: 1.0.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet Pro MFP M177.ppd.gz
Version: 1.0.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LaserJet.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Color LJ Pro MFP M177 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 111 Roll.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 111 Tray.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP designjet 130.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP designjet 130nr.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 4020 PS3.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 4520 PS3.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 4520mfp PS3.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 500 plus C7769F.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 500 plus C7770F.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 500ps plus C7769G.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 500ps plus C7770G.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 510 24in.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 510 42in.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 510ps 24in.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet 510ps 42in.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1100 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1100 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1100ps 24in.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1100ps 44in.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1120 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1120 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1120ps 24in.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1120ps 44in.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T120.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1200 PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1200 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1300 PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1300 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1500 PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T1500 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T2300 PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T2300 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T2500 PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T2500 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T520 24in.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T520 36in.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T610 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T610 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T620 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T7100ps Monochrome.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T7100ps.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T770 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T770 PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T770 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T770ps 24in.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T790 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T790 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T790ps 24in.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T790ps 44in.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T920 PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet T920 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z2100 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z2100 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3100 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3100 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3100ps 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3100ps 24in Photo.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3100ps 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3100ps 44in Photo.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3200 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3200 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3200ps 24in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3200ps 24in Photo.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3200ps 44in PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z3200ps 44in Photo.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z5200 PostScript PCL3.ppd.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z5200 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z5400 PostScript.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z6100ps 42in Photo.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z6100ps 60in Photo.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z6200ps 42in Photo.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Designjet Z6200ps 60in Photo.gz
Version: 26.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 1000 J110 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 1010 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 1050 J410 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 1510 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 2000 J210 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 2020 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 2050 J510 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 2510 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 2520 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 2540 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 2640 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3000 J310 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3050 J610 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3050A J611 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3070 B611 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP deskjet 3320.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP deskjet 3420.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP deskjet 3500.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3510 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3520 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3540 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP deskjet 3600.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3740.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3840.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 3900.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 4510 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 460.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 4610 series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 4610 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 4620 series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 4620 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 4640 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 5400 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 5520 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 5700.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 5900 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 6500.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 6520 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 6600.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 6800.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 6940 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 6980 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet 9800.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D1300 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D1400 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D1500 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D1600 series.ppd.gz
Version: 3.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D2300 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D2400 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D2500 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D2600 series.ppd.gz
Version: 3.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D4100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D4200 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D4300 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D5500 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet D730.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F2100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F2200 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F2400 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F300 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F4100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F4200 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F4400 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F4500 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet F735.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet Ink Adv 2010 K010 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet Ink Adv 2060 K110.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet Ink Advant K109a-z.ppd.gz
Version: 3.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet Ink Advant K209a-z.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet Ink Advantage 2640 All-in-One Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Deskjet Ink Advantage 4640 e-All-in-One Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Envy 100 D410 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP ENVY 110 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP ENVY 120 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP ENVY 4500 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP ENVY 5530 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 100 color MFP M175.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1010.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1012.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1015.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1022.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1150.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1160 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1200.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1220.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp LaserJet 1300 series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 1320 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 200 color M251.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 200 color MFP M275.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 200 color MFP M276 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 200 color MFP M276.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 2100 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 2200.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp LaserJet 2300.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 2410.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 2420.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 2430.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp LaserJet 3015.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp LaserJet 3020 3030.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 3050.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 3052.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 3200.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 3300 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp LaserJet 3380.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 3390.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4 Plus.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 400 M401.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 400 M401dne.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 400 MFP M425 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 400 MFP M425.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4000 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4050 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4100 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4100 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp LaserJet 4200 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4240.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4250.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/hp LaserJet 4300 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4345 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4350.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4ML.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4MP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4Si v2011.110.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 4V.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 500 color M551.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 500 color MFP M570 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 500 color MFP M570.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 500 color MFP M575.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 500 MFP M525.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5000 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5100 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5200.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5200L.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5200LX.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5M.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5MP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5Si Mopier.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 5Si.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 600 M601 M602 M603.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 6MP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 700 color MFP M775.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 700 M712.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 8000 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 8100 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 8150 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 9000 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 9000 Series.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 9040 9050 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 9040.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 9050.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet 9055 9065 MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CM1410 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CM1410 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet color flow MFP M575.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP 1025.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP 1025nw.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1021.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1022.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1022nw.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1023.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1025.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1025nw.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1027nw.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1028.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1028nw.gz
Version: 2.0.20120620
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet CP1520 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet flow MFP M525.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet flow MFP M830.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M1005.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M1120.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M1319f.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M1522 MFP Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M1522 MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M1530 MFP Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M1536dnf MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M2727 MFP Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M2727 MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M3027 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M3035 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M4345 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M4349 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M4555 MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M5025 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M5035 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M5039 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M806.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M9040 M9050 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet M9059 MFP.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet MFP M725.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P1005.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P1006.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P1007.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P1008.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P1009.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P1505.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P1505n.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P2014.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P2015.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P2035.gz
Version: 1.4.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P2055.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P2055d.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P3004.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P3005.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P3010 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet P4010_P4510 Series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet Pro MFP M125-M126.ppd.gz
Version: 1.0.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet Pro MFP M127-M128.ppd.gz
Version: 1.0.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet Pro MFP M435.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet Pro MFP M521 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LaserJet Pro MFP M521.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LJ 300 color MFP M375 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LJ 300-400 color M351-M451.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LJ 300-400 color MFP M375-M475.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP LJ 400 color MFP M475 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP LJ Pro MFP M127-M128 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Mopier 240.gz
Version: 19.8
Path: /Library/Printers/PPDs/Contents/Resources/HP Mopier 320.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 100 Mobile L411.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 150 Mobile L511.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 2620 All-in-One Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 2620 series.ppd.gz
Version: 2.3.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4000 K210.ppd.gz
Version: 3.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 4100 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP officejet 4100 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 4105 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP officejet 4105.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 4200 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP officejet 4200 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 4300 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4300 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4400 K410.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 4500 G510a-f Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4500 G510a-f.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 4500 G510g-m Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4500 G510g-m.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 4500 G510n-z Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4500 G510n-z.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4500 K710 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4500 K710.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4610 series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4610 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4620 series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4620 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4630 e-All-in-One Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 4630 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 5500 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP officejet 5500 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 5600 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 5600 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6000 E609a.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6000 E609n.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 6100 Series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6100.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6200 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6200 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6300 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6300 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6500 E709a Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6500 E709a.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6500 E709n Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6500 E709n.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 6500 E710a-f Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6500 E710a-f.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 6500 E710n-z Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6500 E710n-z.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6600 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6600.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6700 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 6700.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 7000 E809a.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 7110 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 7200 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 7200 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 7300 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 7300 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 7400 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 7400 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet 7500 E910 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 7500 E910.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 7610 series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet 7610 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/hp officejet 9100 series.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet H470.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J3600 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J3600 series.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J4500 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J4500 series.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J4660 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J4660 series.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet J4680 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J4680 series.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet J5700 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J5700 series.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J6400 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet J6400 series.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet K7100.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 251dw Printer.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 276dw MFP Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 276dw MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 3610.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 3620 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 3620.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8000 A809.ppd.gz
Version: 3.3.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8000 Enterprise A811a.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8100.ppd.gz
Version: 3.3.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8500 A909a Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8500 A909a.ppd.gz
Version: 3.3.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8500 A909g Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8500 A909g.ppd.gz
Version: 3.3.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8500 A909n Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8500 A909n.ppd.gz
Version: 3.3.3
Path: /Library/Printers/PPDs/Contents/Resources/HP OfficeJet Pro 8500 A910 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8500 A910.ppd.gz
Version: 3.3.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8600 Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro 8600.ppd.gz
Version: 3.3.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro K5300.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro K5400.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro K550.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro K850.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro K8600.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7300 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7300.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7400.ppd.gz
Version: 4.0.6
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7500 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7500.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7600 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7600.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7700 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro L7700.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro X451-X551 Printer.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro X476-X576 MFP Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Officejet Pro X476-X576 MFP.gz
Version: 19.9
Path: /Library/Printers/PPDs/Contents/Resources/HP photosmart 140 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP photosmart 240 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 2570 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 2600 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 2600 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 2700 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 2700 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 3100 series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 3100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 320 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 3200 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 330 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 3300 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 3300 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 370 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 380 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 420 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 470 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 5510 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 5510d series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 5520 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 6510 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 6520 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP photosmart 7200 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 7400 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 7510 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 7520 series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 7520 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP photosmart 7600 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP photosmart 7700 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 7800 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP photosmart 7900 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 8000 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 8100 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 8200 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 8400 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart 8700 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A310 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A320 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A430 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A440 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A510 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A520 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A530,A630.ppd.gz
Version: 1.1.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A610 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A620 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A640.ppd.gz
Version: 1.1.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A710 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart A820 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart B010 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart B109a-m.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart B110 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart B8500 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C309a series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C309a series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C3100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4200 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4340 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4340 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4380 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4400 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4500 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4600 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C4700 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C5100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C5200 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C5300 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C5500 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C6100 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C6100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C6200 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C6300 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C7100 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C7100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C7200 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C7200 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart C8100 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D110 series.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D5060 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D5100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D5300 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D5400 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D6100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D7100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D7200 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D7300 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D7400 series.ppd.gz
Version: 5.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart D7500 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart eStn C510 Japan.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart eStn C510 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Ink Adv K510.ppd.gz
Version: 3.2.1
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Plus B209a-m.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Plus B210 series.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Prem C310 Japan.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Prem C310 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Prem C410 Japan Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Prem C410 Japan.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Prem C410 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Prem C410 series.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Prem-Web C309n-s Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Prem-Web C309n-s.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Premium C309g-m.ppd.gz
Version: 4.1.2
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Pro B8300 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Pro B8800 series.ppd.gz
Version: 4.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Pro B9100 series.ppd.gz
Version: 4.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP Photosmart Wireless B109n-z.ppd.gz
Version: 4.2.4
Path: /Library/Printers/PPDs/Contents/Resources/HP psc 1000 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP psc 1100 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP psc 1200 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP psc 1300 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP psc 1310 series .ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 1400 series.ppd.gz
Version: 2.0.4
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 1500 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 1600 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 2100 Series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 2150 Series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 2170 Series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 2200 Series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP psc 2300 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 2350 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 2400 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP psc 2400 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/HP PSC 2500 Series Fax.ppd.gz
Version: 5.11.0
Path: /Library/Printers/PPDs/Contents/Resources/HP psc 2500 series.ppd.gz
Version: 2.0.3
Path: /Library/Printers/PPDs/Contents/Resources/hp1100.ppd.gz
Version: 6.9
Path: /Library/Printers/PPDs/Contents/Resources/hp1100w.ppd.gz
Version: 6.9
Path: /Library/Printers/PPDs/Contents/Resources/hp1130.ppd.gz
Version: 1.7
Path: /Library/Printers/PPDs/Contents/Resources/hp1210nf.ppd.gz
Version: 1.7
Path: /Library/Printers/PPDs/Contents/Resources/hp1210nfFax.ppd.gz
Version: 1.4
Path: /Library/Printers/PPDs/Contents/Resources/hp1560.ppd.gz
Version: 6.9
Path: /Library/Printers/PPDs/Contents/Resources/hp1600dn.ppd.gz
Version: 6.9
Printers:
Printers:
Path: /Library/Printers/Canon/BJPrinter/Frameworks/BJCommand2.framework/Versions/A/Resources/Info.plist
Version: 8.1.0
Path: /Library/Printers/Canon/BJPrinter/Frameworks/BJEssential2.framework/Versions/A/Resources/Info.plist
Version: 4.1.3
Path: /Library/Printers/Canon/BJPrinter/Frameworks/BJExtDDI.framework/Versions/A/Resources/Info.plist
Version: 4.0.1
Path: /Library/Printers/Canon/BJPrinter/Frameworks/BJPDELocalizedString2.framework/Versions/A/Resources/Info.plist
Version: 2.1.3
Path: /Library/Printers/Canon/BJPrinter/Frameworks/BJPrinterUtility2.framework/Versions/A/Resources/Info.plist
Version: 7.47.1
Path: /Library/Printers/Canon/BJPrinter/Frameworks/BJStatus2.framework/Versions/A/Resources/Info.plist
Version: 7.42.2
Path: /Library/Printers/Canon/BJPrinter/Plugins/BJNP/canonijnetwork.bundle/Contents/Info.plist
Version: 1.6.7
Path: /Library/Printers/Canon/BJPrinter/Plugins/BJNP/CIJNetworkIOM.plugin/Contents/Info.plist
Version: 10.44.0
Path: /Library/Printers/Canon/BJPrinter/Plugins/BJNP/CIJNetworkPBM.plugin/Contents/Info.plist
Version: 1.1.0
Path: /Library/Printers/Canon/BJPrinter/Plugins/BJUSB/BJUSBIOM.plugin/Contents/Info.plist
Version: 1.5.0
Path: /Library/Printers/Canon/BJPrinter/Plugins/BJUSB/BJUSBPBM.plugin/Contents/Info.plist
Version: 1.4.7
Path: /Library/Printers/Canon/BJPrinter/Plugins/BJUSB/CIJUSBClassDriver.plugin/Contents/Info.plist
Version: 1.1.5
Path: /Library/Printers/Canon/BJPrinter/Plugins/BJUSB/CIJUSBClassDriver2.plugin/Contents/Info.plist
Version: 1.1.0
Path: /Library/Printers/Canon/BJPrinter/Plugins/CIJUtility/CIJUtilityControl.bundle/Contents/Info.plist
Version: 1.3.1
Path: /Library/Printers/Canon/BJPrinter/Plugins/IJBluetooth/IJBluetoothIOM.plugin/Contents/Info.plist
Version: 1.0.12
Path: /Library/Printers/Canon/BJPrinter/Utilities/BJPrinterUtility2.app/Contents/Info.plist
Version: 7.27.2
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Info.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/172CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/173CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/174CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/175CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/205CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/206CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/213CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/217CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/218CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/220CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/221CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/237CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/238CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/250CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/252CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/253CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/254CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/256CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/257CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/258CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/260CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/261CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/262CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/263CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/264CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/265CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/266CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/267CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/270CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/271CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/272CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/273CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/274CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/275CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/276CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/278CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/279CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/280CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/281CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/282CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/283CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/284CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/285CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/286CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/287CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/288CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/289CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/290CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/291CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/292CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/293CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/294CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/295CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/296CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/297CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/298CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/300CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/301CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/302CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/303CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/309CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/310CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/311CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/312CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/315CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/316CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/317CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/318CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/319CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/320CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/321CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/323CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/324CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/325CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/326CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/327CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/328CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/329CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/331CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/332CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/333CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/334CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/335CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/336CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/337CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/338CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/339CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/340CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/341CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/342CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/346CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/347CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/348CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/349CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/352CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/353CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/354CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/356CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/357CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/358CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/359CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/360CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/361CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/362CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/363CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/364CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/365CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/366CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/367CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/369CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/370CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/373CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/374CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/375CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/376CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/377CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/378CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/380CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/381CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/382CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/383CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/384CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/385CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/386CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/387CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/388CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/389CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/390CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/391CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/392CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/393CIJPrinterInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJBatteryLevelInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJChangeBJCartridgeInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJChangeInkTankInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJCleaningInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJCustomSettingInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJInkCartridgeInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJInkInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJInkUsageControlInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeBatteryLevelInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeCartridgeInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeChangeBJCartridgeInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeChangeInkTankInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeCleaningInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeCustomSettingInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeHelpInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeInkInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeInkUsageControlInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizePaperAllocationInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizePaperSourceSettingInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizePowerSettingInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeRemainingInkLevelSettingInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeSelectInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeSilentModeInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJLocalizeTestPrintInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJPaperAllocationInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJPaperSourceSettingInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJPowerSettingInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJRemainingInkLevelSettingInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJSilentModeInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/BJPrinter/Utilities/CanonIJPrinterUtility.app/Contents/Resources/CIJTestPrintInfo.plist
Version: 10.51.7
Path: /Library/Printers/Canon/IJScanner/Frameworks/Caddis_09.framework/Versions/A/Resources/Info.plist
Version: 1.0.5
Path: /Library/Printers/Canon/IJScanner/Frameworks/SGSM5_09.framework/Versions/A/Resources/Info.plist
Version: 6.2.0
Path: /Library/Printers/Canon/IJScanner/Plugins/ag07_09.plugin/Contents/Info.plist
Version: 7.1.4
Path: /Library/Printers/Canon/IJScanner/Plugins/ag08_09.plugin/Contents/Info.plist
Version: 7.2.4
Path: /Library/Printers/Canon/IJScanner/Plugins/cncl09_09.plugin/Contents/Info.plist
Version: 3.7.1
Path: /Library/Printers/Canon/IJScanner/Plugins/cnq2413_09.plugin/Contents/Info.plist
Version: 2.0.0
Path: /Library/Printers/Canon/IJScanner/Plugins/cnq2414_09.plugin/Contents/Info.plist
Version: 1.0.2
Path: /Library/Printers/Canon/IJScanner/Plugins/cnq4807_09.plugin/Contents/Info.plist
Version: 2.1.0
Path: /Library/Printers/Canon/IJScanner/Plugins/cnq4808_09.plugin/Contents/Info.plist
Version: 2.0.0
Path: /Library/Printers/Canon/IJScanner/Plugins/cnq4809_09.plugin/Contents/Info.plist
Version: 1.0.2
Path: /Library/Printers/Canon/IJScanner/Plugins/cnq9601_09.plugin/Contents/Info.plist
Version: 2.0.0
Path: /Library/Printers/Canon/IJScanner/Plugins/ijfshlib_09.plugin/Contents/Info.plist
Version: 1.1.4
Path: /Library/Printers/Canon/IJScanner/Plugins/mld07_09.plugin/Contents/Info.plist
Version: 1.1.3
Path: /Library/Printers/Canon/IJScanner/Plugins/mld08_09.plugin/Contents/Info.plist
Version: 3.0.3
Path: /Library/Printers/Canon/IJScanner/Plugins/mld09_09.plugin/Contents/Info.plist
Version: 6.2.0
Path: /Library/Printers/Canon/IJScanner/Plugins/mld9601_09.plugin/Contents/Info.plist
Version: 3.1.3
Path: /Library/Printers/Canon/IJScanner/Plugins/sfusb_09.plugin/Contents/Info.plist
Version: 1.2.1
Path: /Library/Printers/Canon/IJScanner/Plugins/sgusb_09.plugin/Contents/Info.plist
Version: 1.4.0
Path: /Library/Printers/Canon/IJScanner/Plugins/smac_09.plugin/Contents/Info.plist
Version: 1.2.5
Path: /Library/Printers/Canon/IJScanner/Plugins/zoom_09.plugin/Contents/Info.plist
Version: 1.1.1
Path: /Library/Printers/hp/cups/CompactPhotosmart.driver/Contents/Info.plist
Version: 4.0.3
Path: /Library/Printers/hp/cups/Designjet1PS.driver/Contents/Info.plist
Version: 1.5.0
Path: /Library/Printers/hp/cups/Designjet1Raster.driver/Contents/Info.plist
Version: 1.5.0
Path: /Library/Printers/hp/cups/Designjet1Raster.driver/Contents/PlugIns/DesignjetDMFInfo.bundle/Contents/Info.plist
Version: 1.5.0
Path: /Library/Printers/hp/cups/Deskjet.driver/Contents/Info.plist
Version: 4.0.4
Path: /Library/Printers/hp/cups/filters/commandtohp.filter/Contents/Info.plist
Version: 2.2.1
Path: /Library/Printers/hp/cups/filters/commandtohp.filter/Contents/PlugIns/reportlevels.plugin/Contents/Info.plist
Version: 2.2.1
Path: /Library/Printers/hp/cups/filters/commandtohp.filter/Contents/PlugIns/reporttrays.plugin/Contents/Info.plist
Version: 2.2.1
Path: /Library/Printers/hp/cups/filters/pdftopdf.filter/Contents/Info.plist
Version: 2.5.2
Path: /Library/Printers/hp/cups/filters/pdftopdf.filter/Contents/PlugIns/mh_one_button.plugin/Contents/Info.plist
Version: 2.5.2
Path: /Library/Printers/hp/cups/filters/pdftopdf.filter/Contents/PlugIns/mh_pre_one_button.plugin/Contents/Info.plist
Version: 2.5.2
Path: /Library/Printers/hp/cups/filters/raster2pclm.filter/Contents/Info.plist
Version: 1.0.0
Path: /Library/Printers/hp/cups/Inkjet.driver/Contents/Info.plist
Version: 4.0.4
Path: /Library/Printers/hp/cups/Inkjet1.driver/Contents/Info.plist
Version: 3.2.1
Path: /Library/Printers/hp/cups/Inkjet2.driver/Contents/Info.plist
Version: 4.0.4
Path: /Library/Printers/hp/cups/Inkjet3.driver/Contents/Info.plist
Version: 3.3.3
Path: /Library/Printers/hp/cups/Inkjet4.driver/Contents/Info.plist
Version: 4.1.2
Path: /Library/Printers/hp/cups/Inkjet5.driver/Contents/Info.plist
Version: 3.0.4
Path: /Library/Printers/hp/cups/Inkjet6.driver/Contents/Info.plist
Version: 2.0.3
Path: /Library/Printers/hp/cups/Inkjet7.driver/Contents/Info.plist
Version: 2.0.4
Path: /Library/Printers/hp/cups/Inkjet8.driver/Contents/Info.plist
Version: 4.2.4
Path: /Library/Printers/hp/cups/Inkjet9.driver/Contents/Info.plist
Version: 2.3.1
Path: /Library/Printers/hp/cups/Laserjet.driver/Contents/Info.plist
Version: 2.0.3
Path: /Library/Printers/hp/cups/Officejet.driver/Contents/Info.plist
Version: 4.0.6
Path: /Library/Printers/hp/cups/Photosmart.driver/Contents/Info.plist
Version: 5.0.4
Path: /Library/Printers/hp/cups/PhotosmartPro.driver/Contents/Info.plist
Version: 4.0.3
Path: /Library/Printers/hp/cups/tools/autosetup.tool/Contents/Info.plist
Version: 1.3.1
Path: /Library/Printers/hp/cups/tools/DesignjetAutoSetup.tool/Contents/Info.plist
Version: 1.5.0
Path: /Library/Printers/hp/cups/tools/epcl2ppd.tool/Contents/Info.plist
Version: 1.0.0
Path: /Library/Printers/hp/Fax/fax.backend/Contents/Info.plist
Version: 5.11.0
Path: /Library/Printers/hp/Fax/rastertofax.filter/Contents/Info.plist
Version: 5.11.0
Path: /Library/Printers/hp/filter/hpPostProcessing.bundle/Contents/Info.plist
Version: 19.9.0
Path: /Library/Printers/hp/filter/hpPreProcessing.filter/Contents/Info.plist
Version: 1.5.2
Path: /Library/Printers/hp/filter/hprastertojpeg.driver/Contents/Info.plist
Version: 1.1.0
Path: /Library/Printers/hp/Frameworks/Crossbow.framework/Versions/D/Resources/Info.plist
Version: 2.0
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/ClientUI.framework/Versions/4.0/PlugIns/ClientUI.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/ClientUI.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Configure.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Core.framework/Versions/4.0/PlugIns/bluetooth.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Core.framework/Versions/4.0/PlugIns/CFXmlParser.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Core.framework/Versions/4.0/PlugIns/libXmlParser.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Core.framework/Versions/4.0/PlugIns/network.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Core.framework/Versions/4.0/PlugIns/NSXMLParser.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Core.framework/Versions/4.0/PlugIns/usb.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Core.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/DataStore.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/DeviceID.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Fax.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/HDT.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/HTTP.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/PML.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Scan.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/CDPrintingStatus.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/CoversStatus.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/DeviceAlerts.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/DeviceStatus.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/DeviceTrays.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/EstimatedPagesStatus.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/JobsStatus.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/SpecialtyPrintingStatus.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/PlugIns/SuppliesStatus.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/Status.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Frameworks/XMLServices.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/PlugIns/statusclient.bundle/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Resources/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Runtime/hpdot4d.app/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDeviceModel.framework/Versions/4.0/Runtime/HPIOPrinterClassDriver.plugin/Contents/Info.plist
Version: 4.8.1
Path: /Library/Printers/hp/Frameworks/HPDriverCore.framework/Versions/A/Frameworks/DCCommunicationServices.framework/Versions/A/Resources/DCCSDMFLoader.bundle/Contents/Info.plist
Version: 1.8.2
Path: /Library/Printers/hp/Frameworks/HPDriverCore.framework/Versions/A/Frameworks/DCCommunicationServices.framework/Versions/A/Resources/Info.plist
Version: 1.8.2
Path: /Library/Printers/hp/Frameworks/HPDriverCore.framework/Versions/A/Frameworks/DCCore.framework/Versions/A/Resources/Info.plist
Version: 1.8.2
Path: /Library/Printers/hp/Frameworks/HPDriverCore.framework/Versions/A/Frameworks/DCJobSettings.framework/Versions/A/Resources/Info.plist
Version: 1.8.2
Path: /Library/Printers/hp/Frameworks/HPDriverCore.framework/Versions/A/Frameworks/DCPPDGeneration.framework/Versions/A/Resources/Info.plist
Version: 1.8.2
Path: /Library/Printers/hp/Frameworks/HPDriverCore.framework/Versions/A/Frameworks/DCPPDUpdating.framework/Versions/A/Resources/Info.plist
Version: 1.8.2
Path: /Library/Printers/hp/Frameworks/HPDriverCore.framework/Versions/A/Frameworks/DCXMLRepository.framework/Versions/A/Resources/Info.plist
Version: 1.8.2
Path: /Library/Printers/hp/Frameworks/HPDriverCore.framework/Versions/A/Resources/Info.plist
Version: 1.8.2
Path: /Library/Printers/hp/Frameworks/HPSmartPrint.framework/Versions/A/Resources/Info.plist
Version: 5.12.0
Path: /Library/Printers/hp/Frameworks/Interlaken.framework/Versions/DI_ILLN.A.03.00.011/Resources/Info.plist
Version: 03.00.011
Path: /Library/Printers/hp/Frameworks/Interlaken.framework/Versions/DI_ILLN.A.04.02.001/Resources/Info.plist
Version: 04.02.001
Path: /Library/Printers/hp/Frameworks/Matterhorn.framework/Versions/DI_MH.A.05.03.006/Resources/Info.plist
Version: 05.03.006
Path: /Library/Printers/hp/Frameworks/Matterhorn.framework/Versions/DI_MH.A.06.04.008/Resources/Info.plist
Version: 06.04.008
Path: /Library/Printers/hp/Frameworks/ResourceManager.framework/Versions/DI_RM.A.04.08.004/Resources/Info.plist
Version: 04.08.004
Path: /Library/Printers/hp/laserjet/cp1020series/hpcp1020.plugin/Contents/Info.plist
Version: 1.1.20120809
Path: /Library/Printers/hp/laserjet/cp1020series/hpcp1020filter.plugin/Contents/Info.plist
Version: 1.0.20120809
Path: /Library/Printers/hp/laserjet/cp1020series/hpcp1020jbig.plugin/Contents/Info.plist
Version: 1.0.20120615
Path: /Library/Printers/hp/laserjet/cp1020series/hpcp1020pq.plugin/Contents/Info.plist
Version: 1.0.20110211
Path: /Library/Printers/hp/laserjet/hplaserjetzjs.bundle/Contents/Info.plist
Version: 1.4.0
Path: /Library/Printers/hp/laserjet/M1130_1210series/HP LaserJet Professional Utility.app/Contents/Info.plist
Version: 5.0
Path: /Library/Printers/hp/laserjet/M1130_1210series/HPM1210_1130Raster.bundle/Contents/Info.plist
Version: 6.0
Path: /Library/Printers/hp/laserjet/p1100_1560_1600series/HP LaserJet Professional Utility.app/Contents/Info.plist
Version: 5.0
Path: /Library/Printers/hp/laserjet/p1100_1560_1600series/hpRaster.bundle/Contents/Info.plist
Version: 6.0
Path: /Library/Printers/hp/PDEs/DesignjetPDE.plugin/Contents/Info.plist
Version: 1.5.0
Path: /Library/Printers/hp/PDEs/DesignjetPDE.plugin/Contents/PlugIns/SmartPrintDesignjet.plugin/Contents/Info.plist
Version: 1.5.0
Path: /Library/Printers/hp/PDEs/DesignjetPDE.plugin/Contents/Resources/Controllers/ConceptPreviewInfo.plist
Version: 1.5.0
Path: /Library/Printers/hp/PDEs/FaxPDE.plugin/Contents/Info.plist
Version: 5.11.0
Path: /Library/Printers/hp/PDEs/hpcp1020PDE.plugin/Contents/Info.plist
Version: 2.1.0
Path: /Library/Printers/hp/PDEs/hpcp1020PDE.plugin/Contents/PlugIns/SmartPrintCP1020.plugin/Contents/Info.plist
Version: 2.1.0
Path: /Library/Printers/hp/PDEs/hpPostScriptPDE.plugin/Contents/Info.plist
Version: 19.9.0
Path: /Library/Printers/hp/PDEs/hpPostScriptPDE.plugin/Contents/PlugIns/SmartPrintPostScript.plugin/Contents/Info.plist
Version: 19.9.0
Path: /Library/Printers/hp/PDEs/PDE.plugin/Contents/Info.plist
Version: 4.6.0
Path: /Library/Printers/hp/PDEs/PDE.plugin/Contents/PlugIns/SmartPrint.plugin/Contents/Info.plist
Version: 5.1.0
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Frameworks/HPEventStore.framework/Versions/A/Resources/HPStoreModel.momd/VersionInfo.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Frameworks/HPEventStore.framework/Versions/A/Resources/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Frameworks/HSDCommonLib.framework/Versions/A/Resources/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Library/LoginItems/HP Device Monitor.app/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Library/LoginItems/HP Device Monitor.app/Contents/Resources/HP Alerts.app/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Library/LoginItems/HP Device Monitor.app/Contents/Resources/HP Alerts.app/Contents/PlugIns/AlertMessagePlugin.AlertHandler/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Library/LoginItems/HP Device Monitor.app/Contents/Resources/HP Alerts.app/Contents/PlugIns/HPACfEventPlugin.AlertHandler/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Library/LoginItems/HP Device Monitor.app/Contents/Resources/HP Alerts.app/Contents/PlugIns/HPOutOfPaperEventPlugin.AlertHandler/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Library/LoginItems/HP Device Monitor.app/Contents/Resources/HP Alerts.app/Contents/PlugIns/HPSuppliesStatusEventPlugin.AlertHandler/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Library/LoginItems/HP Device Monitor.app/Contents/Resources/HP Email Alerts.app/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HP Utility.app/Contents/Library/LoginItems/HP Device Monitor.app/Contents/Resources/HP Fax Archive.app/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/AddCustomPaper.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/AdminDisabledFeatures.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/AlertsManagementAssistant.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ArbitraryCommand.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/AssignICCProfile.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/AutomaticPenAlignment.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/AutoOff.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/AutoWirelessConnect.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/BasicFaxSettings.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Bluetooth.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/CalibrateDisplay.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/CleanBackPageSmear.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ClosedLoopCalibration.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ColorCalibration.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ColorCleaning.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ColorUsage.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ConfigurationPage.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ConsumableLevel.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ContactSupport.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ControlPanelGuide.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ControlPanelLanguage.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/CreatePaperPreset.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DateTime.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DesignjetAssistant.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DesignjetStoredJobs.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DeviceDiscoveryAssistant.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DirectPrint.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DMF.discovery/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DMF.transport/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DownloadDriversAndSoftware.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/DPOF.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Duplex.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/EconomodeToner.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/eFax.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/EmailAlerts.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/EmailNotifications.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ePrintMobile.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxArchive.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxArchive.task/Contents/PlugIns/DeviceSetupDMFFaxArchive.plugin/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxArchive.task/Contents/PlugIns/DeviceSetupDMFFaxArchive.plugin/Contents/Resources/FaxCallerIDInfo.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxBlocking.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxBlocking.task/Contents/PlugIns/DeviceSetupDMFFaxBlocking.plugin/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxBlocking.task/Contents/PlugIns/DeviceSetupDMFFaxBlocking.plugin/Contents/Resources/FaxCallerIDInfo.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxBlocking.task/Contents/Resources/FaxCallerIDInfo.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxForwarding.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxLogs.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxLogs.task/Contents/PlugIns/DeviceSetupDMFFaxLogs.plugin/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxLogs.task/Contents/PlugIns/DeviceSetupDMFFaxLogs.plugin/Contents/Resources/FaxCallerIDInfo.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxLogs.task/Contents/Resources/FaxCallerIDInfo.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxSpeedDials.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxSpeedDials.task/Contents/PlugIns/DeviceSetupDMFFaxSpeedDials.plugin/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FaxSpeedDials.task/Contents/PlugIns/DeviceSetupDMFFaxSpeedDials.plugin/Contents/Resources/FaxCallerIDInfo.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FileUpload.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/FirmwareUpdate.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/HPColorCenter.assistant/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/HPePrinterCenter.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ImportPreset.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/IPSettings.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/IQTroubleshooting.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/JobAccounting.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/JobQueue.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/LineFeedCalibration.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ManageCustomPapers.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ManagePapers.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Marketsplash.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Message Center.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Message Center.task/Contents/PlugIns/AlertMessagePlugin.EventHandler/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Message Center.task/Contents/PlugIns/HPACfEventPlugin.EventHandler/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Message Center.task/Contents/PlugIns/HPOutOfPaperEventPlugin.EventHandler/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Message Center.task/Contents/PlugIns/HPSuppliesStatusEventPlugin.EventHandler/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Message Center.task/Contents/Resources/HPMessageCenterBridge.app/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/NetworkSettings.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/OnlineInformation.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/OutputDevices.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PantoneEmulation.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PaperFeedCleaning.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PaperHandling.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PenAlignment.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PowerManagement.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PrinterDocumentation.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PrinterSettings.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PrinterStatus.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PrinterStatus.task/Contents/Resources/DetailsViewInfo.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PrinterUsage.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PrintingKnowledgeCenter.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/PrintQueueSetupAssistant.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ProfPhotographyCenter.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ProtectDirectPorts.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ProxySettings.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/QualityCalibration.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/QualityDiagnostics.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/RegionUnlock.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Resolution.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ResourcesLocking.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/RestrictColor.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ScanShortcutsManager.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ScanToEmail.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ScanToNetwork.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/ScanToNetworkFolder.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SecureUpgrade.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SemiAutomaticPenAlignment.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SkewTest.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/StoredJobs.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SubmitJob.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SummaryAssistant.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SuppliesManagement.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SuppliesManagementCLT2.0.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SupplyInfo.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/SystemMaintenance.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/TestPage.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/TestPaperFeed.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/TravelInfo.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/TraysConfiguration.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/Universal.monitor/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/UpdateFirmware.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/UploadFonts.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/UserRolesManagement.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/WebRegistrationAssistant.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/WebServer.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/WebServicesAssistant.task/Contents/Info.plist
Version: 5.19.2
Path: /Library/Printers/hp/Utilities/HPPU Plugins/WirelessDirectPrintAssistant.task/Contents/Info.plist
Version: 5.19.2
Image Capture Devices:
Image Capture Devices:
Path: /Library/Image Capture/Devices/Canon IJScanner2.app/Contents/Info.plist
Version: 1.5.1
Path: /Library/Image Capture/Devices/Canon IJScanner2.app/Contents/Resources/DeviceInfo.plist
Version: 1.5.1
Path: /Library/Image Capture/Devices/Canon IJScanner2.app/Contents/Resources/DeviceMatchingInfo.plist
Version: 1.5.1
Path: /Library/Image Capture/Devices/Canon IJScanner4.app/Contents/Info.plist
Version: 2.3.0
Path: /Library/Image Capture/Devices/Canon IJScanner4.app/Contents/Resources/DeviceInfo.plist
Version: 2.3.0
Path: /Library/Image Capture/Devices/Canon IJScanner4.app/Contents/Resources/DeviceMatchingInfo.plist
Version: 2.3.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/Info.plist
Version: 5.6.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/.ICASingle.bundle/Contents/Info.plist
Version: 5.3.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/DDC.bundle/Contents/Info.plist
Version: 1.1.2
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/FIT.bundle/Contents/Info.plist
Version: 3.7.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/ImageFilter.bundle/Contents/Info.plist
Version: 3.2.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 1D.bundle/Contents/Info.plist
Version: 1.0.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 23.bundle/Contents/Info.plist
Version: 1.0.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 30.bundle/Contents/Info.plist
Version: 1.0.4
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 32.bundle/Contents/Info.plist
Version: 1.0.2
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 41.bundle/Contents/Info.plist
Version: 1.1.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 43.bundle/Contents/Info.plist
Version: 1.1.4
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 52.bundle/Contents/Info.plist
Version: 1.1.2
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 54.bundle/Contents/Info.plist
Version: 1.0.9
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 5A.bundle/Contents/Info.plist
Version: 1.0.4
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 66.bundle/Contents/Info.plist
Version: 1.0.10
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 68.bundle/Contents/Info.plist
Version: 1.1.3
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 6E.bundle/Contents/Info.plist
Version: 1.0.3
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 7A.bundle/Contents/Info.plist
Version: 1.0.6
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 7C.bundle/Contents/Info.plist
Version: 1.0.9
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 7E.bundle/Contents/Info.plist
Version: 1.0.3
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 86.bundle/Contents/Info.plist
Version: 1.0.2
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 8B.bundle/Contents/Info.plist
Version: 1.0.3
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 94.bundle/Contents/Info.plist
Version: 1.2.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter 95.bundle/Contents/Info.plist
Version: 1.2.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter A1.bundle/Contents/Info.plist
Version: 1.0.6
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter AD.bundle/Contents/Info.plist
Version: 1.1.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter C2.bundle/Contents/Info.plist
Version: 1.0.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter C3.bundle/Contents/Info.plist
Version: 1.0.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/PlugIns/Interpreter DD.bundle/Contents/Info.plist
Version: 1.0.1
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/Resources/DeviceInfo.plist
Version: 5.6.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/Resources/DeviceMatchingInfo.plist
Version: 5.6.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/Resources/HardwareInfo.plist
Version: 5.6.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/Resources/ModelInfo.plist
Version: 5.6.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/Resources/ProfileInfo.plist
Version: 5.6.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/Resources/RegionCodeInfo.plist
Version: 5.6.0
Path: /Library/Image Capture/Devices/EPSON Scanner.app/Contents/Resources/ResolutionInfo.plist
Version: 5.6.0
Path: /Library/Image Capture/Devices/HP M1130_M1210 Scanner.app/Contents/Info.plist
Version: 1.0
Path: /Library/Image Capture/Devices/HP M1130_M1210 Scanner.app/Contents/Resources/DeviceInfo.plist
Version: 1.0
Path: /Library/Image Capture/Devices/HP M1130_M1210 Scanner.app/Contents/Resources/DeviceMatchingInfo.plist
Version: 1.0
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Frameworks/HPScanServices.framework/Versions/A/PlugIns/HPDOT4Scan.bundle/Contents/Info.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Frameworks/HPScanServices.framework/Versions/A/PlugIns/HPDOT4Scan.bundle/Contents/Resources/HPAiOTulip.bundle/Contents/Info.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Frameworks/HPScanServices.framework/Versions/A/PlugIns/HPDOT4Scan.bundle/Contents/Resources/HPAiOTulip.bundle/Contents/Resources/ModelInfo.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Frameworks/HPScanServices.framework/Versions/A/PlugIns/HPLEDMScan.bundle/Contents/Info.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Frameworks/HPScanServices.framework/Versions/A/PlugIns/HPSOAPScan.bundle/Contents/Info.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Frameworks/HPScanServices.framework/Versions/A/Resources/Info.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Info.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Resources/DeviceInfo.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HP Scanner 3.app/Contents/Resources/DeviceMatchingInfo.plist
Version: 4.4.2
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/Frameworks/HPScan.framework/Versions/A/Resources/DestinationInfo.plist
Version: 2.3.5
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/Frameworks/HPScan.framework/Versions/A/Resources/Info.plist
Version: 2.3.5
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/Frameworks/HPScan.framework/Versions/A/Resources/ProfileInfo.plist
Version: 2.3.5
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/Frameworks/HPScan.framework/Versions/A/Resources/TulipInfo.plist
Version: 2.3.5
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/Info.plist
Version: 1.10.1
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/PlugIns/HPAiOScan.bundle/Contents/Info.plist
Version: 2.3.0
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/PlugIns/HPAiOScan.bundle/Contents/Resources/DeviceInfo.plist
Version: 2.3.0
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/PlugIns/HPAiOScan.bundle/Contents/Resources/ModelInfo.plist
Version: 2.3.0
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/Resources/DeviceInfo.plist
Version: 1.10.1
Path: /Library/Image Capture/Devices/HPScanner.app/Contents/Resources/DeviceMatchingInfo.plist
Version: 1.10.1
Image Capture Support:
Image Capture Support:
Extensions:
Extensions:
Path: /System/Library/Extensions/AppleMobileDevice.kext
Version: 3.3.0
Path: /System/Library/Extensions/AppleStorageDrivers.kext/Contents/PlugIns/AppleATAPIStorage.kext
Version: 3.4.1
Path: /System/Library/Extensions/AppleStorageDrivers.kext/Contents/PlugIns/AppleXserveRAID.kext
Version: 3.4.1
Path: /System/Library/Extensions/AppleStorageDrivers.kext/Contents/PlugIns/FireWireStorageDeviceSpecifics.kext
Version: 3.4.1
Path: /System/Library/Extensions/AppleStorageDrivers.kext/Contents/PlugIns/SonyXDCAMDriver.kext
Version: 3.4.1
Path: /System/Library/Extensions/AppleStorageDrivers.kext/Contents/PlugIns/USBStorageDeviceSpecifics.kext
Version: 3.4.1
Path: /System/Library/Extensions/AppleTopCase.kext
Version: 10.21
Path: /System/Library/Extensions/AppleUSBTopCase.kext
Version: 240.2
Path: /System/Library/Extensions/CellPhoneHelper.kext
Version: 1.3.2
Path: /System/Library/Extensions/hp_designjet_series.kext
Version: 2.4.0
Path: /System/Library/Extensions/hp_Deskjet_io_enabler.kext
Version: 4.0.4
Path: /System/Library/Extensions/hp_fax_io.kext
Version: 5.11.0
Path: /System/Library/Extensions/hp_Inkjet1_io_enabler.kext
Version: 3.2.1
Path: /System/Library/Extensions/hp_Inkjet2_io_enabler.kext
Version: 4.0.4
Path: /System/Library/Extensions/hp_Inkjet3_io_enabler.kext
Version: 3.3.3
Path: /System/Library/Extensions/hp_Inkjet4_io_enabler.kext
Version: 4.1.2
Path: /System/Library/Extensions/hp_Inkjet5_io_enabler.kext
Version: 3.0.4
Path: /System/Library/Extensions/hp_Inkjet7_io_enabler.kext
Version: 2.0.4
Path: /System/Library/Extensions/hp_Inkjet8_io_enabler.kext
Version: 4.2.4
Path: /System/Library/Extensions/hp_Inkjet9_io_enabler.kext
Version: 2.3.1
Path: /System/Library/Extensions/hp_Inkjet_io_enabler.kext
Version: 4.0.4
Path: /System/Library/Extensions/hp_io_printerclassdriver_enabler.kext
Version: 19.9.0
Path: /System/Library/Extensions/hp_Laserjet_io_enabler.kext
Version: 2.0.3
Path: /System/Library/Extensions/hp_Officejet_io_enabler.kext
Version: 4.0.6
Path: /System/Library/Extensions/hp_Photosmart_io_enabler.kext
Version: 5.0.4
Path: /System/Library/Extensions/hp_PhotosmartPro_io_enabler.kext
Version: 4.0.3
Path: /System/Library/Extensions/hp_psa640_io_enabler.kext
Version: 1.1.0
Path: /System/Library/Extensions/hp_qc_io_enabler.kext
Version: 1.1.0
Path: /System/Library/Extensions/IOHIDFamily.kext/Contents/PlugIns/IOHIDEventDriver.kext
Version: 2.0.0
Path: /System/Library/Extensions/IOHIDFamily.kext/Contents/PlugIns/IOHIDEventDriverSafeBoot.kext
Version: 2.0.0
Path: /System/Library/Extensions/IOHIDFamily.kext/Contents/PlugIns/IOHIDUserClient.kext
Version: 2.0.0
Path: /System/Library/Extensions/IOStreamFamily.kext/Contents/PlugIns/IOStreamUserClient.kext
Version: 1.1.0
Path: /System/Library/Extensions/IOUSBFamily.kext/Contents/PlugIns/IOUSBHIDDriverSafeBoot.kext
Version: 650.4.0
Path: /System/Library/Extensions/IOVideoFamily.kext/Contents/PlugIns/IOVideoDeviceUserClient.kext
Version: 1.2.0
Printers:
HP LaserJet 1020:
Status: Idle
Print Server: Local
Driver Version: 1.4.0
Default: Yes
Shared: No
URI: usb://Hewlett-Packard/HP%20LaserJet%201020?serial=FN0LBSX
PPD: HP LaserJet 1022, 1.4.0
PPD File Version: 1.4.0
PostScript Version: (3010.000) 853
CUPS Version: 1.7.2 (cups-372.4)
Scanning support: No
Printer Commands: none
CUPS filters:
rasterToHPZJS:
Bundle: hplaserjetzjs.bundle
Path: /Library/Printers/hp/laserjet/hplaserjetzjs.bundle/Contents/MacOS/rasterToHPZJS
Permissions: rwxr-xr-x
Version: 1.4.0
Fax support: No
PDEs:
SATA/SATA Express:
Intel 8 Series Chipset:
Vendor: Intel
Product: 8 Series Chipset
Link Speed: 6 Gigabit
Negotiated Link Speed: 3 Gigabit
Physical Interconnect: SATA
Description: AHCI Version 1.30 Supported
APPLE HDD ST1000DM003:
Capacity: 1 TB (1,000,204,886,016 bytes)
Model: APPLE HDD ST1000DM003
Revision: AP18
Native Command Queuing: Yes
Queue Depth: 32
Removable Media: No
Detachable Drive: No
BSD Name: disk0
Rotational Rate: 7200
Medium Type: Rotational
Partition Map Type: GPT (GUID Partition Table)
S.M.A.R.T. status: Verified
Software:
System Software Overview:
System Version: OS X 10.9.3 (13D65)
Kernel Version: Darwin 13.2.0
Time since boot: 5 minutes
Thunderbolt:
Thunderbolt Bus:
Vendor Name: Apple Inc.
Device Name: iMac
UID: 0x0001000D1B9D6000
Firmware Version: 23.10
Domain UUID: 0E2E8210-8C67-755C-BA54-A49498600A08
Port:
Status: No device connected
Link Status: 0x101
Receptacle: 1
Link Controller Firmware Version: 0.12.3
Port:
Status: No device connected
Link Status: 0x101
Receptacle: 2
Link Controller Firmware Version: 0.12.3
USB:
USB 3.0 SuperSpeed Bus:
Host Controller Location: Built-in USB
Host Controller Driver: AppleUSBXHCI
PCI Device ID: 0x8c31
PCI Revision ID: 0x0005
PCI Vendor ID: 0x8086
Bus Number: 0x0a
My Passport 0812:
Product ID: 0x0812
Vendor ID: 0x1058 (Western Digital Technologies, Inc.)
Version: 10.49
Serial Number: 57584B314536334444534A4D
Speed: Up to 5 Gb/sec
Manufacturer: Western Digital
Location ID: 0x15100000 / 2
Current Available (mA): 900
Current Required (mA): 224
Capacity: 500.07 GB (500,074,283,008 bytes)
Removable Media: Yes
Detachable Drive: Yes
BSD Name: disk1
Partition Map Type: GPT (GUID Partition Table)
S.M.A.R.T. status: Not Supported
USB 3.0 Hi-Speed Bus:
Host Controller Location: Built-in USB
Host Controller Driver: AppleUSBXHCI
PCI Device ID: 0x8c31
PCI Revision ID: 0x0005
PCI Vendor ID: 0x8086
Bus Number: 0x0a
BRCM20702 Hub:
Product ID: 0x4500
Vendor ID: 0x0a5c (Broadcom Corp.)
Version: 1.00
Speed: Up to 12 Mb/sec
Manufacturer: Apple Inc.
Location ID: 0x14800000 / 4
Current Available (mA): 500
Current Required (mA): 94
Bluetooth USB Host Controller:
Product ID: 0x828d
Vendor ID: 0x05ac (Apple Inc.)
Version: 0.79
Speed: Up to 12 Mb/sec
Manufacturer: Apple Inc.
Location ID: 0x14830000 / 7
Current Available (mA): 500
Current Required (mA): 0
FaceTime HD Camera (Built-in):
Product ID: 0x8511
Vendor ID: 0x05ac (Apple Inc.)
Version: 72.30
Serial Number: CCGD6E10YJFDYPF0
Speed: Up to 480 Mb/sec
Manufacturer: Apple Inc.
Location ID: 0x14700000 / 3
Current Available (mA): 500
Current Required (mA): 500
HP LaserJet 1020:
Product ID: 0x2b17
Vendor ID: 0x03f0 (Hewlett Packard)
Version: 1.00
Serial Number: FN0LBSX
Speed: Up to 480 Mb/sec
Manufacturer: Hewlett-Packard
Location ID: 0x14600000 / 1
Current Available (mA): 500
Current Required (mA): 98
1284 Device ID: MFG:Hewlett-Packard;MDL:HP LaserJet 1020;CMD:ACL;CLS:PRINTER;DES:HP LaserJet 1020;FWVER:20050309;
Wi-Fi:
Software Versions:
CoreWLAN: 4.3.3 (433.48)
CoreWLANKit: 3.3.2 (332.36)
Menu Extra: 9.3.2 (932.35)
System Information: 9.0 (900.8)
IO80211 Family: 6.3 (630.35)
Diagnostics: 3.0 (300.40)
AirPort Utility: 6.3.2 (632.3)
Interfaces:
en1:
Card Type: AirPort Extreme (0x14E4, 0x111)
Firmware Version: Broadcom BCM43xx 1.0 (6.30.223.154.63)
MAC Address: c8:e0:eb:2c:72:fd
Locale: ETSI
Country Code: GB
Supported PHY Modes: 802.11 a/b/g/n/ac
Supported Channels: 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 36, 40, 44, 48, 52, 56, 60, 64, 100, 104, 108, 112, 116, 120, 124, 128, 132, 136, 140, 149, 153, 157, 161, 165
Wake On Wireless: Supported
AirDrop: Supported
Status: Not Associated