[
{"data":{"title":"IOPowerManagement"},"attr":{"id":"9143","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"9145","ColType":"Number","ColValue":"2"}},{"data":{"title":"DevicePowerState"},"attr":{"id":"9147","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"9149","ColType":"Number","ColValue":"3"}},{"data":{"title":"DriverPowerState"},"attr":{"id":"9151","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"9153","ColType":"Number","ColValue":"65536"}}]},
{"data":{"title":"locationID"},"attr":{"id":"9155","ColType":"Number","ColValue":"1510998016"}},
{"data":{"title":"kUSBBusCurrentAllocation"},"attr":{"id":"9157","ColType":"Number","ColValue":"0"}},
{"data":{"title":"kUSBSleepPortCurrentLimit"},"attr":{"id":"9159","ColType":"Number","ColValue":"1000"}},
{"data":{"title":"port"},"attr":{"id":"9161","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"port-statistics"},"attr":{"id":"9163","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"kPortStatRemoteWakeCount"},"attr":{"id":"9165","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationCount"},"attr":{"id":"9167","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationDuringResetCount"},"attr":{"id":"9169","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatAddressFailureCount"},"attr":{"id":"9171","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationDuringResumeCount"},"attr":{"id":"9173","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationRecoveryDuringResetCount"},"attr":{"id":"9175","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatOverCurrentCount"},"attr":{"id":"9177","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEnumerationFailureCount"},"attr":{"id":"9179","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationCurrentConnectCount"},"attr":{"id":"9181","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatPowerStateTime"},"attr":{"id":"9183","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"kPowerStateSleep"},"attr":{"id":"9185","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateOn"},"attr":{"id":"9187","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateOff"},"attr":{"id":"9189","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateSuspended"},"attr":{"id":"9191","ColType":"String","ColValue":"66948ms (100%)"}}]},{"data":{"title":"kPortStatConnectCount"},"attr":{"id":"9193","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"kUSBWakePortCurrentLimit"},"attr":{"id":"9195","ColType":"Number","ColValue":"1500"}},
{"data":{"title":"IOGeneralInterest"},"attr":{"id":"9197","ColType":"String","ColValue":"IOCommand is not serializable"}},
{"data":{"title":"port-status"},"attr":{"id":"9199","ColType":"Number","ColValue":"1"}},
{"data":{"title":"kUSBBusCurrentSleepAllocation"},"attr":{"id":"9201","ColType":"Number","ColValue":"0"}}
]
