[
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5749","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5750","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5751","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5753","ColType":"Number","ColValue":"4193239040"}},{"data":{"title":"length"},"attr":{"id":"5755","ColType":"Number","ColValue":"16384"}}]}]},{"data":{"title":"1"},"attr":{"id":"5756","ColType":"String","ColValue":"IOSubMemoryDescriptor is not serializable"}}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"5758","ColType":"Number","ColValue":"72"}},
{"data":{"title":"device-id"},"attr":{"id":"5760","ColType":"Data","ColValue":"&lt;64430000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"5762","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"5764","ColType":"Data","ColValue":"&lt;\"ethernet\"&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"5766","ColType":"String","ColValue":"ethernet"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5768","ColType":"Data","ColValue":"&lt;ab110000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5770","ColType":"Data","ColValue":"&lt;12000000&gt;"}},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"5772","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIPMCSState"},"attr":{"id":"5774","ColType":"Number","ColValue":"8451"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5776","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5778","ColType":"Data","ColValue":"&lt;43100000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5780","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5781","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"5782","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5784","ColType":"Number","ColValue":"502801"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"5786","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5787","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"5789","ColType":"String","ColValue":"ethernet 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"5791","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5792","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5793","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"5794","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5795","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5796","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5797","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"5798","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5799","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5800","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5801","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"5802","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5803","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5804","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5805","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"5806","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5807","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5808","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5809","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"5810","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5811","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"5813","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"5815","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"5817","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5819","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5821","ColType":"String","ColValue":"4:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5823","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"model"},"attr":{"id":"5825","ColType":"String","ColValue":"Marvell Yukon Gigabit Adapter 88E8056 Singleport Copper SA"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5827","ColType":"Number","ColValue":"17"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5829","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5831","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5833","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5835","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"5837","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5839","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5841","ColType":"Data","ColValue":"&lt;00000200&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"5843","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"5845","ColType":"Data","ColValue":"&lt;\"pci1043,81f8\",\"pci11ab,4364\",\"pciclass,020000\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"5847","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"5849","ColType":"Data","ColValue":"&lt;f8810000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"5851","ColType":"Data","ColValue":"&lt;100004820000000000c0eff90000000000400000180004810000000000d800000000000000010000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5853","ColType":"Data","ColValue":"&lt;000004000000000000000000000000000000000010000402000000000000000000000000004000001800040100000000000000000000000000010000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5855","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5856","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"5857","ColType":"Data","ColValue":"&lt;0400000000000100&gt;"}}]}
]
