[
{"data":{"title":"built-in"},"attr":{"id":"2770","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"layout-id"},"attr":{"id":"2772","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"2774","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2775","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2776","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"2778","ColType":"Number","ColValue":"4178051072"}},{"data":{"title":"length"},"attr":{"id":"2780","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"hda-gfx"},"attr":{"id":"2782","ColType":"Data","ColValue":"&lt;\"onboard-1\"&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"2784","ColType":"Data","ColValue":"&lt;0a0e0000&gt;"}},
{"data":{"title":"PinConfigurations"},"attr":{"id":"2786","ColType":"Data","ColValue":"&lt;e0005628&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"2788","ColType":"Number","ColValue":"2"}},
{"data":{"title":"name"},"attr":{"id":"2790","ColType":"Data","ColValue":"&lt;\"pci10de,e0a\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"2792","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/P0P3@60000/HDAU@1"}},
{"data":{"title":"IOName"},"attr":{"id":"2794","ColType":"String","ColValue":"pci10de,e0a"}},
{"data":{"title":"vendor-id"},"attr":{"id":"2796","ColType":"Data","ColValue":"&lt;de100000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"2798","ColType":"Data","ColValue":"&lt;a1000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"2800","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIPMCSState"},"attr":{"id":"2802","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"2804","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"2806","ColType":"Data","ColValue":"&lt;62140000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"2808","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2809","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"2810","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"2812","ColType":"Number","ColValue":"21314819"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"2814","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2815","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"2817","ColType":"String","ColValue":"HDAU 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"2819","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2820","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2821","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"2822","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"2823","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"2824","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2825","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"2826","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"2827","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"2828","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2829","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"2830","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"2831","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"2832","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2833","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"2834","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"2835","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"2836","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2837","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"2838","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"2839","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"2841","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"2843","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"2845","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"2847","ColType":"Number","ColValue":"3"}},
{"data":{"title":"pcidebug"},"attr":{"id":"2849","ColType":"String","ColValue":"1:0:1"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"2851","ColType":"Number","ColValue":"4225"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"2853","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"2855","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"2857","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"2859","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"2861","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"2863","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"2865","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"2867","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"2869","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"2871","ColType":"Data","ColValue":"&lt;\"pci1462,2842\",\"pci10de,e0a\",\"pciclass,040300\",\"HDAU\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"2873","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"2875","ColType":"Data","ColValue":"&lt;42280000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"2877","ColType":"Data","ColValue":"&lt;1001018200000000000008f90000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"2879","ColType":"Data","ColValue":"&lt;00010100000000000000000000000000000000001001010200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"2881","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"2882","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"2883","ColType":"Data","ColValue":"&lt;0200000000000100&gt;"}}]}
]
