[
{"data":{"title":"IODeviceMemory"},"attr":{"id":"3420","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3421","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3422","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"3424","ColType":"Number","ColValue":"4194287616"}},{"data":{"title":"length"},"attr":{"id":"3426","ColType":"Number","ColValue":"16384"}}]}]},{"data":{"title":"1"},"attr":{"id":"3427","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3428","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"3430","ColType":"Number","ColValue":"4194271232"}},{"data":{"title":"length"},"attr":{"id":"3432","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"layout-id"},"attr":{"id":"3434","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"PinConfigurations"},"attr":{"id":"3436","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"3438","ColType":"Data","ColValue":"&lt;12000000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"3440","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"3442","ColType":"Data","ColValue":"&lt;\"pci1102,12\"&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"3444","ColType":"String","ColValue":"pci1102,12"}},
{"data":{"title":"vendor-id"},"attr":{"id":"3446","ColType":"Data","ColValue":"&lt;02110000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"3448","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"IOPCIPMCSState"},"attr":{"id":"3450","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"3452","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"3454","ColType":"Data","ColValue":"&lt;02110000&gt;"}},
{"data":{"title":"MaximumBootBeepVolume"},"attr":{"id":"3456","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"3458","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3459","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"3460","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"3462","ColType":"Number","ColValue":"146449"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"3464","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3465","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"3467","ColType":"String","ColValue":"pci1102,12 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"3469","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3470","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3471","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"3472","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3473","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"3474","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3475","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"3476","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3477","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"3478","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3479","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"3480","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3481","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"3482","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3483","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"3484","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3485","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"3486","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3487","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"3488","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3489","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"3491","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"3493","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"3495","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"3497","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"3499","ColType":"String","ColValue":"5:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"3501","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"3503","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"3505","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"3507","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"3509","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"3511","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"3513","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"3515","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"3517","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"3519","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"3521","ColType":"Data","ColValue":"&lt;\"pci1102,10\",\"pci1102,12\",\"pciclass,040300\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"3523","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"3525","ColType":"Data","ColValue":"&lt;10000000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"3527","ColType":"Data","ColValue":"&lt;100005820000000000c0fff9000000000040000018000582000000000080fff90000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"3529","ColType":"Data","ColValue":"&lt;000005000000000000000000000000000000000010000502000000000000000000000000004000001800050200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"3531","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3532","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"3533","ColType":"Data","ColValue":"&lt;0500000000000100&gt;"}}]}
]
