[
{"data":{"title":"built-in"},"attr":{"id":"5138","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"layout-id"},"attr":{"id":"5140","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5142","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5143","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5144","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5146","ColType":"Number","ColValue":"4178051072"}},{"data":{"title":"length"},"attr":{"id":"5148","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"hda-gfx"},"attr":{"id":"5150","ColType":"Data","ColValue":"&lt;\"onboard-1\"&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"5152","ColType":"Data","ColValue":"&lt;0a0e0000&gt;"}},
{"data":{"title":"PinConfigurations"},"attr":{"id":"5154","ColType":"Data","ColValue":"&lt;e0005628&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"5156","ColType":"Number","ColValue":"2"}},
{"data":{"title":"name"},"attr":{"id":"5158","ColType":"Data","ColValue":"&lt;\"pci10de,e0a\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5160","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/P0P3@60000/HDAU@1"}},
{"data":{"title":"IOName"},"attr":{"id":"5162","ColType":"String","ColValue":"pci10de,e0a"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5164","ColType":"Data","ColValue":"&lt;de100000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5166","ColType":"Data","ColValue":"&lt;a1000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5168","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIPMCSState"},"attr":{"id":"5170","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5172","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5174","ColType":"Data","ColValue":"&lt;62140000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5176","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5177","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"5178","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5180","ColType":"Number","ColValue":"21314819"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"5182","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5183","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"5185","ColType":"String","ColValue":"HDAU 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"5187","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5188","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5189","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"5190","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5191","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5192","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5193","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"5194","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5195","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5196","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5197","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"5198","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5199","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5200","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5201","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"5202","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5203","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5204","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5205","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"5206","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5207","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"5209","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"5211","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"5213","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5215","ColType":"Number","ColValue":"3"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5217","ColType":"String","ColValue":"1:0:1"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5219","ColType":"Number","ColValue":"4225"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5221","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5223","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5225","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5227","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5229","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"5231","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5233","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5235","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"5237","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"5239","ColType":"Data","ColValue":"&lt;\"pci1462,2842\",\"pci10de,e0a\",\"pciclass,040300\",\"HDAU\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"5241","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"5243","ColType":"Data","ColValue":"&lt;42280000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"5245","ColType":"Data","ColValue":"&lt;1001018200000000000008f90000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5247","ColType":"Data","ColValue":"&lt;00010100000000000000000000000000000000001001010200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5249","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5250","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"5251","ColType":"Data","ColValue":"&lt;0200000000000100&gt;"}}]}
]
