[
{"data":{"title":"IODeviceMemory"},"attr":{"id":"13371","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13372","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13373","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"13375","ColType":"Number","ColValue":"4193239040"}},{"data":{"title":"length"},"attr":{"id":"13377","ColType":"Number","ColValue":"16384"}}]}]},{"data":{"title":"1"},"attr":{"id":"13378","ColType":"String","ColValue":"IOSubMemoryDescriptor is not serializable"}}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"13380","ColType":"Number","ColValue":"72"}},
{"data":{"title":"device-id"},"attr":{"id":"13382","ColType":"Data","ColValue":"&lt;64430000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"13384","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"13386","ColType":"Data","ColValue":"&lt;\"ethernet\"&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"13388","ColType":"String","ColValue":"ethernet"}},
{"data":{"title":"vendor-id"},"attr":{"id":"13390","ColType":"Data","ColValue":"&lt;ab110000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"13392","ColType":"Data","ColValue":"&lt;12000000&gt;"}},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"13394","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIPMCSState"},"attr":{"id":"13396","ColType":"Number","ColValue":"8451"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"13398","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"13400","ColType":"Data","ColValue":"&lt;43100000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"13402","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13403","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"13404","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"13406","ColType":"Number","ColValue":"502801"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"13408","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13409","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"13411","ColType":"String","ColValue":"ethernet 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"13413","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13414","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13415","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"13416","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"13417","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"13418","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13419","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"13420","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"13421","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"13422","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13423","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"13424","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"13425","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"13426","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13427","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"13428","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"13429","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"13430","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13431","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"13432","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"13433","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"13435","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"13437","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"13439","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"13441","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"13443","ColType":"String","ColValue":"4:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"13445","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"model"},"attr":{"id":"13447","ColType":"String","ColValue":"Marvell Yukon Gigabit Adapter 88E8056 Singleport Copper SA"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"13449","ColType":"Number","ColValue":"17"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"13451","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"13453","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"13455","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"13457","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"13459","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"13461","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"13463","ColType":"Data","ColValue":"&lt;00000200&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"13465","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"13467","ColType":"Data","ColValue":"&lt;\"pci1043,81f8\",\"pci11ab,4364\",\"pciclass,020000\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"13469","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"13471","ColType":"Data","ColValue":"&lt;f8810000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"13473","ColType":"Data","ColValue":"&lt;100004820000000000c0eff90000000000400000180004810000000000d800000000000000010000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"13475","ColType":"Data","ColValue":"&lt;000004000000000000000000000000000000000010000402000000000000000000000000004000001800040100000000000000000000000000010000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"13477","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13478","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"13479","ColType":"Data","ColValue":"&lt;0400000000000100&gt;"}}]}
]
