[
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5438","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5439","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5440","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5442","ColType":"Number","ColValue":"4194287616"}},{"data":{"title":"length"},"attr":{"id":"5444","ColType":"Number","ColValue":"16384"}}]}]},{"data":{"title":"1"},"attr":{"id":"5445","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5446","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5448","ColType":"Number","ColValue":"4194271232"}},{"data":{"title":"length"},"attr":{"id":"5450","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"layout-id"},"attr":{"id":"5452","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"PinConfigurations"},"attr":{"id":"5454","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"5456","ColType":"Data","ColValue":"&lt;12000000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"5458","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"5460","ColType":"Data","ColValue":"&lt;\"pci1102,12\"&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"5462","ColType":"String","ColValue":"pci1102,12"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5464","ColType":"Data","ColValue":"&lt;02110000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5466","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"IOPCIPMCSState"},"attr":{"id":"5468","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5470","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5472","ColType":"Data","ColValue":"&lt;02110000&gt;"}},
{"data":{"title":"MaximumBootBeepVolume"},"attr":{"id":"5474","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5476","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5477","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"5478","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5480","ColType":"Number","ColValue":"146449"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"5482","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5483","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"5485","ColType":"String","ColValue":"pci1102,12 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"5487","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5488","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5489","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"5490","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5491","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5492","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5493","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"5494","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5495","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5496","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5497","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"5498","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5499","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5500","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5501","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"5502","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5503","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5504","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5505","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"5506","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5507","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"5509","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"5511","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"5513","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5515","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5517","ColType":"String","ColValue":"5:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5519","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5521","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5523","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5525","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5527","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5529","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"5531","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5533","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5535","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"5537","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"5539","ColType":"Data","ColValue":"&lt;\"pci1102,10\",\"pci1102,12\",\"pciclass,040300\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"5541","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"5543","ColType":"Data","ColValue":"&lt;10000000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"5545","ColType":"Data","ColValue":"&lt;100005820000000000c0fff9000000000040000018000582000000000080fff90000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5547","ColType":"Data","ColValue":"&lt;000005000000000000000000000000000000000010000502000000000000000000000000004000001800050200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5549","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5550","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"5551","ColType":"Data","ColValue":"&lt;0500000000000100&gt;"}}]}
]
