[
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5346","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5347","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}}]},
{"data":{"title":"built-in"},"attr":{"id":"5349","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"5351","ColType":"Number","ColValue":"160"}},
{"data":{"title":"device-id"},"attr":{"id":"5353","ColType":"Data","ColValue":"&lt;423a0000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"5355","ColType":"Data","ColValue":"&lt;\"pci-bridge\"&gt;"}},
{"data":{"title":"IOPCIConfigured"},"attr":{"id":"5357","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"#size-cells"},"attr":{"id":"5359","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5361","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/POP5@1c0001"}},
{"data":{"title":"IOName"},"attr":{"id":"5363","ColType":"String","ColValue":"pci-bridge"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5365","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5367","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5369","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIPMCSState"},"attr":{"id":"5371","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5373","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIExpressSlotStatus"},"attr":{"id":"5375","ColType":"Number","ColValue":"328"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5377","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5378","ColType":"String","ColValue":"io-apic-0"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5380","ColType":"Number","ColValue":"34679825"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5382","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5384","ColType":"String","ColValue":"0:28:1(5:5)"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5386","ColType":"Number","ColValue":"12305"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5388","ColType":"Number","ColValue":"321"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5390","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5392","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5394","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5396","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"5398","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5400","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5402","ColType":"Data","ColValue":"&lt;00040600&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"5404","ColType":"Data","ColValue":"&lt;\"pci8086,3a42\",\"pciclass,060400\",\"POP5\"&gt;"}},
{"data":{"title":"IOPCIExpressSlotCapabilities"},"attr":{"id":"5406","ColType":"Number","ColValue":"1376"}},
{"data":{"title":"IODTPersist"},"attr":{"id":"5408","ColType":"Number","ColValue":"0"}},
{"data":{"title":"#address-cells"},"attr":{"id":"5410","ColType":"Data","ColValue":"&lt;03000000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5412","ColType":"Data","ColValue":"&lt;00e1000000000000000000000000000000000000&gt;"}},
{"data":{"title":"ranges"},"attr":{"id":"5414","ColType":"Data","ColValue":"&lt;00000082000000000000f0f900000082000000000000f0f90000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000&gt;"}}
]
