[
{"data":{"title":"assigned-addresses"},"attr":{"id":"6163","ColType":"Data","ColValue":"&lt;100003820000000000c0dff90000000000400000180003810000000000c800000000000000010000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"6165","ColType":"String","ColValue":"3:0:0"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"6167","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"6169","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6170","ColType":"Data","ColValue":"&lt;1300000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"6171","ColType":"Data","ColValue":"&lt;0600000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"6173","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/P0P7@1c0003/GIGE@0"}},
{"data":{"title":"model"},"attr":{"id":"6175","ColType":"String","ColValue":"Marvell Yukon Gigabit Adapter 88E8056 Singleport Copper SA"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"6177","ColType":"Number","ColValue":"72"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"6179","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6180","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"6181","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"6183","ColType":"Number","ColValue":"17"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"6185","ColType":"Number","ColValue":"1"}},
{"data":{"title":"AAPL,slot-name"},"attr":{"id":"6187","ColType":"Data","ColValue":"&lt;\"Ethernet\"&gt;"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"6189","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"6191","ColType":"Data","ColValue":"&lt;43100000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"6193","ColType":"Data","ColValue":"&lt;ab110000&gt;"}},
{"data":{"title":"empty"},"attr":{"id":"6195","ColType":"Number","ColValue":"0"}},
{"data":{"title":"name"},"attr":{"id":"6197","ColType":"Data","ColValue":"&lt;\"ethernet\"&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"6199","ColType":"Data","ColValue":"&lt;\"pci1043,81f8\",\"pci11ab,4364\",\"pciclass,020000\",\"GIGE\"&gt;"}},
{"data":{"title":"IOPCIPMCSState"},"attr":{"id":"6201","ColType":"Number","ColValue":"8451"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"6203","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"6205","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"6207","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"6209","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"6211","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"6213","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"6215","ColType":"Data","ColValue":"&lt;12000000&gt;"}},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"6217","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"6219","ColType":"Number","ColValue":"502801"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"6221","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"built-in"},"attr":{"id":"6223","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"6225","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"6227","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6228","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6229","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"6231","ColType":"Number","ColValue":"4192190464"}},{"data":{"title":"length"},"attr":{"id":"6233","ColType":"Number","ColValue":"16384"}}]}]},{"data":{"title":"1"},"attr":{"id":"6234","ColType":"String","ColValue":"IOSubMemoryDescriptor is not serializable"}}]},
{"data":{"title":"IOName"},"attr":{"id":"6236","ColType":"String","ColValue":"ethernet"}},
{"data":{"title":"acpi-device"},"attr":{"id":"6238","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"6240","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"6242","ColType":"Data","ColValue":"&lt;f8810000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"6244","ColType":"Data","ColValue":"&lt;000003000000000000000000000000000000000010000302000000000000000000000000004000001800030100000000000000000000000000010000&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"6246","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6247","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"6249","ColType":"String","ColValue":"GIGE 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"6251","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6252","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6253","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"6254","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6255","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"6256","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6257","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"6258","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6259","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"6260","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6261","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"6262","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6263","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"6264","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6265","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"6266","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6267","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"6268","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6269","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"6270","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6271","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"6273","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"6275","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"6277","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"6279","ColType":"Data","ColValue":"&lt;00000200&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"6281","ColType":"Data","ColValue":"&lt;64430000&gt;"}}
]
