[
{"data":{"title":"AHCI Port ESATA"},"attr":{"id":"5870","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"AHCI-Built-In"},"attr":{"id":"5872","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AHCI Port Hot Plug"},"attr":{"id":"5874","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"IOMaximumSegmentByteCountRead"},"attr":{"id":"5876","ColType":"Number","ColValue":"4194304"}},
{"data":{"title":"Physical Interconnect Location"},"attr":{"id":"5878","ColType":"String","ColValue":"Internal"}},
{"data":{"title":"64-bit"},"attr":{"id":"5880","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AHCI Port SNotification"},"attr":{"id":"5882","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"Protocol Characteristics"},"attr":{"id":"5884","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"Physical Interconnect Location"},"attr":{"id":"5886","ColType":"String","ColValue":"Internal"}},{"data":{"title":"Physical Interconnect"},"attr":{"id":"5888","ColType":"String","ColValue":"SATA"}}]},
{"data":{"title":"AHCI Port ALPM"},"attr":{"id":"5890","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"Trace ID"},"attr":{"id":"5892","ColType":"Number","ColValue":"2032192"}},
{"data":{"title":"AHCI Port Optimized Device Number"},"attr":{"id":"5894","ColType":"Number","ColValue":"0"}},
{"data":{"title":"Controller Characteristics"},"attr":{"id":"5896","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"Product Name"},"attr":{"id":"5898","ColType":"String","ColValue":"ESB2 AHCI"}},{"data":{"title":"Port Description"},"attr":{"id":"5900","ColType":"String","ColValue":"AHCI Version 1.20 Supported"}},{"data":{"title":"Vendor Name"},"attr":{"id":"5902","ColType":"String","ColValue":"Intel"}},{"data":{"title":"Port Speed"},"attr":{"id":"5904","ColType":"String","ColValue":"3 Gigabit"}}]},
{"data":{"title":"IOMaximumSegmentCountWrite"},"attr":{"id":"5906","ColType":"Number","ColValue":"256"}},
{"data":{"title":"IOMaximumSegmentCountRead"},"attr":{"id":"5908","ColType":"Number","ColValue":"256"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5910","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5912","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5914","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5916","ColType":"Number","ColValue":"2"}},{"data":{"title":"DriverPowerState"},"attr":{"id":"5918","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5920","ColType":"Number","ColValue":"32768"}}]},
{"data":{"title":"AHCI-Ejectable"},"attr":{"id":"5922","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"IOMaximumSegmentByteCountWrite"},"attr":{"id":"5924","ColType":"Number","ColValue":"4194304"}}
]
