[
{"data":{"title":"IOPowerManagement"},"attr":{"id":"9207","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"9209","ColType":"Number","ColValue":"2"}},{"data":{"title":"DevicePowerState"},"attr":{"id":"9211","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"9213","ColType":"Number","ColValue":"3"}},{"data":{"title":"DriverPowerState"},"attr":{"id":"9215","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"9217","ColType":"Number","ColValue":"65536"}}]},
{"data":{"title":"locationID"},"attr":{"id":"9219","ColType":"Number","ColValue":"1512046592"}},
{"data":{"title":"kUSBBusCurrentAllocation"},"attr":{"id":"9221","ColType":"Number","ColValue":"0"}},
{"data":{"title":"kUSBSleepPortCurrentLimit"},"attr":{"id":"9223","ColType":"Number","ColValue":"1000"}},
{"data":{"title":"port"},"attr":{"id":"9225","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"port-statistics"},"attr":{"id":"9227","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"kPortStatRemoteWakeCount"},"attr":{"id":"9229","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationCount"},"attr":{"id":"9231","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationDuringResetCount"},"attr":{"id":"9233","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatAddressFailureCount"},"attr":{"id":"9235","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationDuringResumeCount"},"attr":{"id":"9237","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationRecoveryDuringResetCount"},"attr":{"id":"9239","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatOverCurrentCount"},"attr":{"id":"9241","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEnumerationFailureCount"},"attr":{"id":"9243","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationCurrentConnectCount"},"attr":{"id":"9245","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatPowerStateTime"},"attr":{"id":"9247","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"kPowerStateSleep"},"attr":{"id":"9249","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateOn"},"attr":{"id":"9251","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateOff"},"attr":{"id":"9253","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateSuspended"},"attr":{"id":"9255","ColType":"String","ColValue":"68713ms (100%)"}}]},{"data":{"title":"kPortStatConnectCount"},"attr":{"id":"9257","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"kUSBWakePortCurrentLimit"},"attr":{"id":"9259","ColType":"Number","ColValue":"1500"}},
{"data":{"title":"IOGeneralInterest"},"attr":{"id":"9261","ColType":"String","ColValue":"IOCommand is not serializable"}},
{"data":{"title":"port-status"},"attr":{"id":"9263","ColType":"Number","ColValue":"1"}},
{"data":{"title":"kUSBBusCurrentSleepAllocation"},"attr":{"id":"9265","ColType":"Number","ColValue":"0"}}
]
