[
{"data":{"title":"IOPowerManagement"},"attr":{"id":"4437","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"4439","ColType":"Number","ColValue":"2"}},{"data":{"title":"DevicePowerState"},"attr":{"id":"4441","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"4443","ColType":"Number","ColValue":"3"}},{"data":{"title":"DriverPowerState"},"attr":{"id":"4445","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"4447","ColType":"Number","ColValue":"65536"}}]},
{"data":{"title":"locationID"},"attr":{"id":"4449","ColType":"Number","ColValue":"1510998016"}},
{"data":{"title":"kUSBBusCurrentAllocation"},"attr":{"id":"4451","ColType":"Number","ColValue":"0"}},
{"data":{"title":"kUSBSleepPortCurrentLimit"},"attr":{"id":"4453","ColType":"Number","ColValue":"1000"}},
{"data":{"title":"port"},"attr":{"id":"4455","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"port-statistics"},"attr":{"id":"4457","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"kPortStatRemoteWakeCount"},"attr":{"id":"4459","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationCount"},"attr":{"id":"4461","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationDuringResetCount"},"attr":{"id":"4463","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatAddressFailureCount"},"attr":{"id":"4465","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationDuringResumeCount"},"attr":{"id":"4467","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationRecoveryDuringResetCount"},"attr":{"id":"4469","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatOverCurrentCount"},"attr":{"id":"4471","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEnumerationFailureCount"},"attr":{"id":"4473","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationCurrentConnectCount"},"attr":{"id":"4475","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatPowerStateTime"},"attr":{"id":"4477","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"kPowerStateSleep"},"attr":{"id":"4479","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateOn"},"attr":{"id":"4481","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateOff"},"attr":{"id":"4483","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateSuspended"},"attr":{"id":"4485","ColType":"String","ColValue":"69931ms (100%)"}}]},{"data":{"title":"kPortStatConnectCount"},"attr":{"id":"4487","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"kUSBWakePortCurrentLimit"},"attr":{"id":"4489","ColType":"Number","ColValue":"1500"}},
{"data":{"title":"IOGeneralInterest"},"attr":{"id":"4491","ColType":"String","ColValue":"IOCommand is not serializable"}},
{"data":{"title":"port-status"},"attr":{"id":"4493","ColType":"Number","ColValue":"1"}},
{"data":{"title":"kUSBBusCurrentSleepAllocation"},"attr":{"id":"4495","ColType":"Number","ColValue":"0"}}
]
