[
{"data":{"title":"AHCI Port ESATA"},"attr":{"id":"9812","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"AHCI-Built-In"},"attr":{"id":"9814","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AHCI Port Hot Plug"},"attr":{"id":"9816","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"IOMaximumSegmentByteCountRead"},"attr":{"id":"9818","ColType":"Number","ColValue":"4194304"}},
{"data":{"title":"Physical Interconnect Location"},"attr":{"id":"9820","ColType":"String","ColValue":"Internal"}},
{"data":{"title":"64-bit"},"attr":{"id":"9822","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AHCI Port SNotification"},"attr":{"id":"9824","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"Protocol Characteristics"},"attr":{"id":"9826","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"Physical Interconnect Location"},"attr":{"id":"9828","ColType":"String","ColValue":"Internal"}},{"data":{"title":"Physical Interconnect"},"attr":{"id":"9830","ColType":"String","ColValue":"SATA"}}]},
{"data":{"title":"AHCI Port ALPM"},"attr":{"id":"9832","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"Trace ID"},"attr":{"id":"9834","ColType":"Number","ColValue":"2032176"}},
{"data":{"title":"AHCI Port Optimized Device Number"},"attr":{"id":"9836","ColType":"Number","ColValue":"0"}},
{"data":{"title":"Controller Characteristics"},"attr":{"id":"9838","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"Product Name"},"attr":{"id":"9840","ColType":"String","ColValue":"ESB2 AHCI"}},{"data":{"title":"Port Description"},"attr":{"id":"9842","ColType":"String","ColValue":"AHCI Version 1.20 Supported"}},{"data":{"title":"Vendor Name"},"attr":{"id":"9844","ColType":"String","ColValue":"Intel"}},{"data":{"title":"Port Speed"},"attr":{"id":"9846","ColType":"String","ColValue":"3 Gigabit"}}]},
{"data":{"title":"IOMaximumSegmentCountWrite"},"attr":{"id":"9848","ColType":"Number","ColValue":"256"}},
{"data":{"title":"IOMaximumSegmentCountRead"},"attr":{"id":"9850","ColType":"Number","ColValue":"256"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"9852","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"9854","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"9856","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"9858","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"9860","ColType":"Number","ColValue":"2"}},{"data":{"title":"DriverPowerState"},"attr":{"id":"9862","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"9864","ColType":"Number","ColValue":"32768"}}]},
{"data":{"title":"AHCI-Ejectable"},"attr":{"id":"9866","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"IOMaximumSegmentByteCountWrite"},"attr":{"id":"9868","ColType":"Number","ColValue":"4194304"}}
]
