[
{"data":{"title":"AHCI Port ESATA"},"attr":{"id":"5926","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"AHCI-Built-In"},"attr":{"id":"5928","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AHCI Port Hot Plug"},"attr":{"id":"5930","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"IOMaximumSegmentByteCountRead"},"attr":{"id":"5932","ColType":"Number","ColValue":"4194304"}},
{"data":{"title":"Physical Interconnect Location"},"attr":{"id":"5934","ColType":"String","ColValue":"Internal"}},
{"data":{"title":"64-bit"},"attr":{"id":"5936","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AHCI Port SNotification"},"attr":{"id":"5938","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"Protocol Characteristics"},"attr":{"id":"5940","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"Physical Interconnect Location"},"attr":{"id":"5942","ColType":"String","ColValue":"Internal"}},{"data":{"title":"Physical Interconnect"},"attr":{"id":"5944","ColType":"String","ColValue":"SATA"}}]},
{"data":{"title":"AHCI Port ALPM"},"attr":{"id":"5946","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"Trace ID"},"attr":{"id":"5948","ColType":"Number","ColValue":"2032208"}},
{"data":{"title":"AHCI Port Optimized Device Number"},"attr":{"id":"5950","ColType":"Number","ColValue":"0"}},
{"data":{"title":"Controller Characteristics"},"attr":{"id":"5952","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"Product Name"},"attr":{"id":"5954","ColType":"String","ColValue":"ESB2 AHCI"}},{"data":{"title":"Port Description"},"attr":{"id":"5956","ColType":"String","ColValue":"AHCI Version 1.20 Supported"}},{"data":{"title":"Vendor Name"},"attr":{"id":"5958","ColType":"String","ColValue":"Intel"}},{"data":{"title":"Port Speed"},"attr":{"id":"5960","ColType":"String","ColValue":"3 Gigabit"}}]},
{"data":{"title":"IOMaximumSegmentCountWrite"},"attr":{"id":"5962","ColType":"Number","ColValue":"256"}},
{"data":{"title":"IOMaximumSegmentCountRead"},"attr":{"id":"5964","ColType":"Number","ColValue":"256"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5966","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5968","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5970","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5972","ColType":"Number","ColValue":"2"}},{"data":{"title":"DriverPowerState"},"attr":{"id":"5974","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5976","ColType":"Number","ColValue":"32768"}}]},
{"data":{"title":"AHCI-Ejectable"},"attr":{"id":"5978","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"IOMaximumSegmentByteCountWrite"},"attr":{"id":"5980","ColType":"Number","ColValue":"4194304"}}
]
