[
{"data":{"title":"AHCI Port ESATA"},"attr":{"id":"5796","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"AHCI-Built-In"},"attr":{"id":"5798","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AHCI Port Hot Plug"},"attr":{"id":"5800","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"IOMaximumSegmentByteCountRead"},"attr":{"id":"5802","ColType":"Number","ColValue":"4194304"}},
{"data":{"title":"Physical Interconnect Location"},"attr":{"id":"5804","ColType":"String","ColValue":"Internal"}},
{"data":{"title":"64-bit"},"attr":{"id":"5806","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AHCI Port SNotification"},"attr":{"id":"5808","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"Protocol Characteristics"},"attr":{"id":"5810","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"Physical Interconnect Location"},"attr":{"id":"5812","ColType":"String","ColValue":"Internal"}},{"data":{"title":"Physical Interconnect"},"attr":{"id":"5814","ColType":"String","ColValue":"SATA"}}]},
{"data":{"title":"AHCI Port ALPM"},"attr":{"id":"5816","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"Trace ID"},"attr":{"id":"5818","ColType":"Number","ColValue":"2032176"}},
{"data":{"title":"AHCI Port Optimized Device Number"},"attr":{"id":"5820","ColType":"Number","ColValue":"0"}},
{"data":{"title":"Controller Characteristics"},"attr":{"id":"5822","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"Product Name"},"attr":{"id":"5824","ColType":"String","ColValue":"ESB2 AHCI"}},{"data":{"title":"Port Description"},"attr":{"id":"5826","ColType":"String","ColValue":"AHCI Version 1.20 Supported"}},{"data":{"title":"Vendor Name"},"attr":{"id":"5828","ColType":"String","ColValue":"Intel"}},{"data":{"title":"Port Speed"},"attr":{"id":"5830","ColType":"String","ColValue":"3 Gigabit"}}]},
{"data":{"title":"IOMaximumSegmentCountWrite"},"attr":{"id":"5832","ColType":"Number","ColValue":"256"}},
{"data":{"title":"IOMaximumSegmentCountRead"},"attr":{"id":"5834","ColType":"Number","ColValue":"256"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5836","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5838","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5840","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5842","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"5844","ColType":"Number","ColValue":"2"}},{"data":{"title":"DriverPowerState"},"attr":{"id":"5846","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5848","ColType":"Number","ColValue":"32768"}}]},
{"data":{"title":"AHCI-Ejectable"},"attr":{"id":"5850","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"IOMaximumSegmentByteCountWrite"},"attr":{"id":"5852","ColType":"Number","ColValue":"4194304"}}
]
